(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 31)
    (no_connects 0)
    (area 129.54 88.9 160.020001 113.12963)
    (thickness 1.6002)
    (drawings 10)
    (tracks 136)
    (zones 0)
    (modules 17)
    (nets 15)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.96 3.96)
    (pad_drill 1.9)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 130.81 110.49)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 /~RESET~)
  (net 7 "Net-(U2-Pad2)")
  (net 8 "Net-(U2-Pad5)")
  (net 9 /MOSI)
  (net 10 /MISO)
  (net 11 /SCK)
  (net 12 "Net-(R1-Pad2)")
  (net 13 "Net-(R3-Pad1)")
  (net 14 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /~RESET~)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5782C5C7)
    (at 152.654 100.584 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5782BD6F)
    (at 140.208 101.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -4.826 1.778) (layer F.SilkS))
    (fp_text value ICM7555 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57805090)
    (at 135.636 107.95 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5782DDFB)
    (at 142.24 95.25 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.032 0 360) (layer F.SilkS))
    (fp_text value Red (at 0 1.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5782DE07)
    (at 147.32 95.25 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.032 0 360) (layer F.SilkS))
    (fp_text value Green (at 0 1.5 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5780509F)
    (at 140.716 107.95 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5781D57C)
    (at 138.176 107.95 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 470K (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5781D591)
    (at 143.256 107.95 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 68 (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5781D596)
    (at 147.574 107.95 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 56 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BlinkyFeet:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5782C5EF)
    (at 149.098 101.6)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -3.302 -1.778) (layer F.SilkS))
    (fp_text value ATTINY85-M (at 0 3.33) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /~RESET~))
    (pad 2 smd rect (at -1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 12 smd rect (at 1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 13 smd rect (at 1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCK))
    (pad 15 smd rect (at 1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 16 smd rect (at 1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 0 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "BlinkyFeet:AVR 1996 dilated" (layer F.Cu) (tedit 0)
    (at 153.67 94.488)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BlinkyFeet:ISP_Pogo_5-thru (layer F.Cu) (tedit 57869202)
    (at 156.464 106.172 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -1.778 5.08 270) (layer F.SilkS) hide)
    (fp_text value ISP (at -2.286 -0.508 360) (layer F.SilkS))
    (pad 1 smd rect (at 0 0 270) (size 1.2 1.2) (layers F.Cu F.Mask)
      (net 10 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MOSI))
    (pad 5 smd oval (at 0 5.08 270) (size 1 1) (layers F.Cu F.Mask)
      (net 6 /~RESET~))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module "BlinkyFeet:AVR 1996" (layer F.Cu) (tedit 0)
    (at 153.67 94.488)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module BlinkyFeet:Big_Pad_Battery (layer B.Cu) (tedit 57A2B902)
    (at 144.78 100.33 180)
    (fp_text reference BT1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value CR2032 (at 0.75 0 180) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at -10.8 0 180) (size 4 4) (drill 1.9) (layers *.Cu *.Mask B.SilkS)
      (net 1 VCC))
    (pad 2 smd rect (at 0 0 180) (size 3.96 3.96) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 10.8 0 180) (size 3.96 3.96) (drill 1.9) (layers *.Cu *.Mask B.SilkS)
      (net 1 VCC))
    (model ${KIPRJMOD}/../FreeCAD/BK-913.wrl
      (at (xyz 0 0 0.161417))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module BlinkyFeet:Nixon-left (layer B.Cu) (tedit 0)
    (at 137.668 107.95 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module BlinkyFeet:Clinton-right (layer B.Cu) (tedit 0)
    (at 151.892 107.95 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module "BlinkyFeet:555 1971" (layer F.Cu) (tedit 0)
    (at 136.144 94.488)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "Blink Eras 1.1" (at 144.78 109.728) (layer B.SilkS))
  (gr_line (start 132.08 110.49) (end 157.48 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 91.44) (end 130.81 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 90.17) (end 132.08 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 109.22) (end 158.75 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.08 109.22) (end 132.08 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.08 91.44) (end 130.81 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.48 109.22) (end 158.75 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.48 91.44) (end 157.48 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 111.76) (xy 129.54 111.76) (xy 129.54 88.9) (xy 160.02 88.9) (xy 160.02 111.76)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 111.76) (xy 129.54 111.76) (xy 129.54 88.9) (xy 160.02 88.9) (xy 160.02 111.76)
      )
    )
  )
)
