(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 15)
    (no_connects 0)
    (area 125.73 100.33 155.528334 117.705)
    (thickness 1.6)
    (drawings 15)
    (tracks 37)
    (zones 0)
    (modules 9)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J2-Pad3)")
  (net 5 "Net-(J2-Pad5)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 "Net-(J3-Pad2)")
  (net 10 "Net-(J3-Pad4)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(C1-Pad1)")
  (net 13 "Net-(C2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left (layer B.Cu) (tedit 5A06B4E0)
    (at 130.937 109.22)
    (descr "surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J3 (at -0.635 5.08) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at 0 5.08) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at 0 0) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at 0 -5.08) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.54) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at 0 -2.54) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5A06B4EA)
    (at 142.24 111.76 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 2.794 7.874 180) (layer F.SilkS))
    (fp_text value ATTINY85-20PU (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 5 thru_hole rect (at 7.62 7.62 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad5)"))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C2-Pad1)"))
    (pad 6 thru_hole rect (at 7.62 5.08 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 3 thru_hole rect (at 0 5.08 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad1)"))
    (pad 7 thru_hole rect (at 7.62 2.54 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 4 thru_hole rect (at 0 7.62 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole rect (at 7.62 0 180) (size 2.4 1.25) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left (layer F.Cu) (tedit 5A06B4E2)
    (at 130.937 109.22)
    (descr "surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J2 (at -0.635 -5.08) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -5.08) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at 0 0) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad3)"))
    (pad 5 smd rect (at 0 5.08) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at 0 -2.54) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 4 smd rect (at 0 2.54) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5A08D8C9)
    (at 149.225 111.76 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 2.921 2.413 540) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A06B4E7)
    (at 142.24 114.3 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5A06BF96)
    (at 145.161 106.68)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.26) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5A06BF90)
    (at 145.161 109.22)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 2.54 0) (layer F.SilkS))
    (fp_text value C_Small (at 2.5 2.26) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A06BFC6)
    (at 150.114 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at -5.08 0.127) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5A06BFCA)
    (at 145.161 104.14)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 2.54 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2017 (at 147.574 106.807 270) (layer B.SilkS))
  (gr_line (start 151.384 102.87) (end 148.082 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.082 115.57) (end 151.384 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "KEY OTHER\nSIDE" (at 138.303 109.093 270) (layer B.SilkS))
  (gr_text "TINY\n85" (at 145.669 112.268) (layer F.SilkS))
  (gr_line (start 129.032 115.57) (end 129.032 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.384 102.87) (end 151.384 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.574 115.57) (end 148.082 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.574 102.87) (end 148.082 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 115.57) (end 129.032 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 102.87) (end 129.032 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.32 102.87) (end 147.574 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.32 115.57) (end 147.574 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.32 102.87) (end 129.286 102.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.286 115.57) (end 147.32 115.57) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 153.67 116.84) (xy 125.73 116.84) (xy 125.73 100.33) (xy 153.67 100.33)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 152.4 115.57) (xy 152.4 101.6) (xy 127 101.6) (xy 127 115.57)
      )
    )
  )
)
