(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(3 "In3.Cu" signal)
		(4 "In4.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(C10-Pad2)")
	(net 3 "Net-(U2-SS_TR)")
	(net 4 "Net-(U2-FB)")
	(net 5 "Net-(U5-SS_TR)")
	(net 6 "Net-(U5-FB)")
	(net 7 "Net-(U6-SS_TR)")
	(net 8 "Net-(C25-Pad2)")
	(net 9 "Net-(U6-FB)")
	(net 10 "Net-(U7-SS_TR)")
	(net 11 "Net-(U7-FB)")
	(net 12 "Net-(U2-SW)")
	(net 13 "Net-(U5-SW)")
	(net 14 "Net-(U6-SW)")
	(net 15 "Net-(U7-SW)")
	(net 16 "Net-(P1-P2)")
	(net 17 "Net-(P1-P3)")
	(net 18 "Net-(P1-P1)")
	(net 19 "Net-(P2-P5)")
	(net 20 "Net-(P2-P4)")
	(net 21 "Net-(P4-P4)")
	(net 22 "Net-(P4-P5)")
	(net 23 "Net-(P4-P3)")
	(net 24 "Net-(Q1-D)")
	(net 25 "Net-(U2-COMP_FSET)")
	(net 26 "Net-(U2-PG)")
	(net 27 "Net-(U5-COMP_FSET)")
	(net 28 "Net-(U5-PG)")
	(net 29 "Net-(U6-PG)")
	(net 30 "Net-(U7-PG)")
	(net 31 "Net-(U6-COMP_FSET)")
	(net 32 "Net-(U7-COMP_FSET)")
	(net 33 "unconnected-(U1-NC-Pad11)")
	(net 34 "unconnected-(U1-NC-Pad2)")
	(net 35 "unconnected-(U1-NC-Pad17)")
	(net 36 "unconnected-(U1-NC-Pad9)")
	(net 37 "unconnected-(U1-NC-Pad21)")
	(net 38 "unconnected-(U1-NC-Pad13)")
	(net 39 "unconnected-(U1-NC-Pad19)")
	(net 40 "unconnected-(U3-N_C-Pad4)")
	(net 41 "unconnected-(U4-NC-Pad5)")
	(net 42 "unconnected-(U4-CE-Pad6)")
	(net 43 "unconnected-(U8-NC-Pad5)")
	(net 44 "unconnected-(U8-CE-Pad6)")
	(net 45 "/5.6v")
	(net 46 "Net-(C13-Pad2)")
	(net 47 "/3.3v")
	(net 48 "Net-(C19-Pad2)")
	(net 49 "/1.8v")
	(net 50 "/1.3v")
	(net 51 "Net-(C31-Pad2)")
	(net 52 "/1.0v")
	(net 53 "/2.5v")
	(net 54 "/1.1v")
	(net 55 "/1.2v")
	(net 56 "Net-(R15-Pad2)")
	(net 57 "/Vin")
	(net 58 "Net-(P2-P1)")
	(net 59 "Net-(P2-P2)")
	(net 60 "Net-(P2-P3)")
	(net 61 "unconnected-(U4-pad-Pad7)")
	(net 62 "unconnected-(U8-pad-Pad7)")
	(net 63 "Net-(U1-VCC)")
	(net 64 "Net-(U1-SW4)")
	(net 65 "Net-(U1-CBOOT)")
	(net 66 "Net-(U1-FB)")
	(net 67 "Net-(U1-SW1)")
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 161.036 72.898)
		(property "Reference" "TP21"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 120.015 94.107 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R5"
			(at 0 -0.9144 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-COMP_FSET)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:RWY0009A-MFG"
		(layer "F.Cu")
		(at 121.383949 97.334748 180)
		(tags "TPS62813QWRWYRQ1 ")
		(property "Reference" "U2"
			(at 1.749949 -1.725252 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS62813QWRWYRQ1"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RWY0009A-MFG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62813-q1.pdf?ts=1732709405459&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RWY0009A-MFG")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -0.568749 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 16 "Net-(P1-P2)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 0.193748) (xy -0.581251 0.143749) (xy -0.581251 -0.006251) (xy -0.531251 -0.056251)
						(xy -0.206251 -0.056254) (xy -0.156251 -0.106251) (xy -0.156251 -0.531251) (xy -0.106248 -0.581251)
						(xy 0.143749 -0.581251) (xy 0.193748 -0.531251) (xy 0.193748 0.143751) (xy 0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -0.55 -1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 16 "Net-(P1-P2)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 0 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 12 "Net-(U2-SW)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd custom
			(at -0.568749 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 -0.193748) (xy -0.581251 -0.143749) (xy -0.581251 0.006251) (xy -0.531251 0.056251)
						(xy -0.206251 0.056251) (xy -0.156248 0.106251) (xy -0.156251 0.531251) (xy -0.106248 0.581251)
						(xy 0.143749 0.581251) (xy 0.193748 0.531251) (xy 0.193748 -0.143751) (xy 0.143751 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "5" smd circle
			(at -0.55 1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 0 1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U2-SS_TR)")
			(pinfunction "SS_TR")
			(pintype "unspecified")
		)
		(pad "7" smd circle
			(at 0.55 1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 25 "Net-(U2-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
		)
		(pad "7" smd custom
			(at 0.568747 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 25 "Net-(U2-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 -0.193748) (xy 0.581253 -0.143749) (xy 0.581253 0.006251) (xy 0.531253 0.056251)
						(xy 0.206253 0.056251) (xy 0.15625 0.106251) (xy 0.156253 0.531251) (xy 0.10625 0.581251) (xy -0.143747 0.581251)
						(xy -0.193749 0.531251) (xy -0.193746 -0.143751) (xy -0.143749 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "8" smd circle
			(at 0.55 -1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "8" smd custom
			(at 0.568747 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 0.193748) (xy 0.581253 0.143749) (xy 0.581253 -0.006251) (xy 0.531253 -0.056251)
						(xy 0.206253 -0.056251) (xy 0.15625 -0.106251) (xy 0.156253 -0.531251) (xy 0.10625 -0.581251)
						(xy -0.143747 -0.581251) (xy -0.193749 -0.531251) (xy -0.193746 0.143751) (xy -0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd rect
			(at 0 -1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-PG)")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_qfn/TPS62813QWRWYRQ1.STEP"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_qfn:xc6601"
		(layer "F.Cu")
		(at 134.874 87.884 90)
		(property "Reference" "U8"
			(at 1.651 -1.651 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 4.5 -5.1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:xc6601"
			(at 4.5 -6.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.torexsemi.com/system/files/series/xc6601.pdf"
			(at 4.5 -6.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 4.5 -6.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.5 -3.6 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 -0.55 270)
			(size 0.45 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pinfunction "VBIAS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -0.975 0 90)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.975 0.5 90)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pinfunction "VIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.975 0.5 90)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/1.1v")
			(pinfunction "Vout")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0.975 0 90)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(U8-NC-Pad5)")
			(pinfunction "NC")
			(pintype "output+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0.975 -0.5 90)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "unconnected-(U8-CE-Pad6)")
			(pinfunction "CE")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd custom
			(at 0 0 90)
			(size 1 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "unconnected-(U8-pad-Pad7)")
			(pinfunction "pad")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_rect
					(start -0.4 -0.845)
					(end 0.402329 0.845)
					(width 0.1)
					(fill yes)
				)
			)
		)
		(model "${T_LIBS}/3d/t_qfn/xc6601.stp"
			(offset
				(xyz 0.05 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 136.647876 96.896876 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C23"
			(at 1.655124 -0.131124 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:DBV0005A_L"
		(layer "F.Cu")
		(at 126.233001 89.728002)
		(tags "LP5907MFX-2.5/NOPB ")
		(property "Reference" "U3"
			(at -2.789001 -1.971002 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LP5907MFX-2.5/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:DBV0005A_L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp5907.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DBV0005A_N DBV0005A_M DBV0005A_L")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.275001 -0.950001 90)
			(size 0.549999 0.800001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.275001 0 90)
			(size 0.549999 0.800001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.275001 0.949998 90)
			(size 0.549999 0.800001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 1.274999 0.949998 90)
			(size 0.549999 0.800001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "unconnected-(U3-N_C-Pad4)")
			(pinfunction "N_C")
			(pintype "unspecified+no_connect")
		)
		(pad "5" smd rect
			(at 1.274999 -0.950001 90)
			(size 0.549999 0.800001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/2.5v")
			(pinfunction "VOUT")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_qfn/LP5907MFX-2.5_NOPB.step"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 141.224 95.758)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C26"
			(at 2.921 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:IND_XGL3520_COC"
		(layer "F.Cu")
		(at 151.887876 97.531876)
		(tags "XGL3520-102MEC ")
		(property "Reference" "L5"
			(at 5.588 1.397 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Ind4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:IND_XGL3520_COC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(U7-SW)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/1.0v")
			(pinfunction "2")
			(pintype "input")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 150.368 94.361)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C34"
			(at 1.905 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/1.0v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 137.959876 93.509876 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R22"
			(at 0.291876 -0.926876 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U6-COMP_FSET)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 111.76 101.092 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C2"
			(at -1.524 -0.381 180)
			(layer "F.SilkS")
		)
		(property "Value" "10nf"
			(at 0 0.4826 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 108.966 101.727 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R1"
			(at -1.651 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(Q1-D)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 136.906 100.203 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R13"
			(at 0 -0.9144 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "Net-(P2-P2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U6-PG)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 104.521 98.044)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C10"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U1-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 114.935 102.87 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R7"
			(at 1.397 -0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(Q1-D)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:xc6601"
		(layer "F.Cu")
		(at 134.153 91.186 180)
		(property "Reference" "U4"
			(at -1.483 -1.651 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 4.5 -5.1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:xc6601"
			(at 4.5 -6.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://product.torexsemi.com/system/files/series/xc6601.pdf"
			(at 4.5 -6.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 4.5 -6.1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.5 -3.6 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 -0.55)
			(size 0.45 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pinfunction "VBIAS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -0.975 0 180)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.975 0.5 180)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pinfunction "VIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.975 0.5 180)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/1.2v")
			(pinfunction "Vout")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0.975 0 180)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "unconnected-(U4-NC-Pad5)")
			(pinfunction "NC")
			(pintype "output+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0.975 -0.5 180)
			(size 0.45 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "unconnected-(U4-CE-Pad6)")
			(pinfunction "CE")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd custom
			(at 0 0 180)
			(size 1 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "unconnected-(U4-pad-Pad7)")
			(pinfunction "pad")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_rect
					(start -0.4 -0.845)
					(end 0.402329 0.845)
					(width 0.1)
					(fill yes)
				)
			)
		)
		(model "${T_LIBS}/3d/t_qfn/xc6601.stp"
			(offset
				(xyz 0.05 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 103.124 72.898)
		(property "Reference" "TP20"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 124.206 95.334)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C15"
			(at 2.032 0.043 180)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:CONN_1729128_PXC"
		(layer "F.Cu")
		(at 107.95 116.967)
		(tags "1729128 ")
		(property "Reference" "J1"
			(at 2.54 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1729128"
			(at 2.54 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:CONN_1729128_PXC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "1729128"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_1729128_PXC")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/Vin")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_connectors/1729128.step"
			(offset
				(xyz -2.5 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 150.363876 95.118876)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C33"
			(at 2.036124 0.004124 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/1.0v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 108.9914 94.742)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C7"
			(at -1.2954 -0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U1-SW4)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U1-CBOOT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 113.411 92.583)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C6"
			(at 0 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 120.396 88.646)
		(property "Reference" "TP3"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/3.3v")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 134.747 89.662)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C41"
			(at 1.651 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 145.791876 96.769876 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C29"
			(at 1.651 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 130.048 93.091)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C19"
			(at 1.651 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U5-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(C19-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 138.933876 100.579876 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R27"
			(at -1.778 0.254 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(P4-P5)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
		(layer "F.Cu")
		(at 108.105 71.882)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "P1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONN_01X05"
			(at 0 12.49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.33 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(P1-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(P1-P2)")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(P1-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P5")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 103.759 91.313)
		(property "Reference" "TP2"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(R15-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 141.224 93.98)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C28"
			(at 2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 139.441876 92.112876)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C25"
			(at 2.798124 -0.042 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U6-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(C25-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:IND_XGL5030_3.1_COC"
		(layer "F.Cu")
		(at 115.951 98.044)
		(tags "XGL5030-183MEC ")
		(property "Reference" "L1"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uh"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:IND_XGL5030_3.1_COC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.8034 0)
			(size 1.0414 4.191)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(U1-SW1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.8034 0)
			(size 1.0414 4.191)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "2")
			(pintype "input")
		)
	)
	(footprint "t_sot:SOT-323"
		(layer "F.Cu")
		(at 116.84 102.489)
		(property "Reference" "Q1"
			(at 1.778 0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "BSS84"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SOT-323"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.7 1)
			(size 0.45 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(P4-P3)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.7 1)
			(size 0.45 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1)
			(size 0.45 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT-323_DIO.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 134.62 85.598)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C37"
			(at 0 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/1.1v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 132.715 95.885)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C20"
			(at 1.651 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/1.8v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 124.248 96.223)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C16"
			(at 1.99 -0.084 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 106.426 96.012)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C5"
			(at 0 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U1-VCC)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 124.206 94.572)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C14"
			(at 2.032 -0.084 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:CONN_1729047_PXC"
		(layer "F.Cu")
		(at 140.89 117.094 180)
		(tags "1729047 ")
		(property "Reference" "P5"
			(at 10 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X05"
			(at 10 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:CONN_1729047_PXC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/1.0v")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/1.2v")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/1.1v")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.000001 0 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.000001 0 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P5")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_connectors/1729047.step"
			(offset
				(xyz -2.5 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:IND_XGL3520_COC"
		(layer "F.Cu")
		(at 125.349 98.552)
		(tags "XGL3520-102MEC ")
		(property "Reference" "L2"
			(at -0.254 2.667 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Ind4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:IND_XGL3520_COC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U2-SW)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pinfunction "2")
			(pintype "input")
		)
	)
	(footprint "t_passive_smd:cap_1206"
		(layer "F.Cu")
		(at 109.347 92.583 180)
		(descr "SMT capacitor, 1206")
		(property "Reference" "C3"
			(at -0.254 2.032 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 -1.6002 180)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1206"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_1206.stp"
			(offset
				(xyz -0.599999991 -0.5499999917 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 130.048 92.202)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R12"
			(at 1.778 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U5-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(C19-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 147.400876 93.277874 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C30"
			(at -3.683 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7nf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U7-SS_TR)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 122.428 91.821)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R8"
			(at 1.524 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 128.016 98.086 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C17"
			(at -1.566 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 132.715 94.996)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C22"
			(at 1.778 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/1.8v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 147.908876 90.864874)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R16"
			(at 1.824124 0.067126 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U7-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 106.341 98.933 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R25"
			(at 2.963 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U1-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 150.241 93.599)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C32"
			(at 1.778 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/1.0v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:IND_XGL3520_COC"
		(layer "F.Cu")
		(at 133.604 98.552)
		(tags "XGL3520-102MEC ")
		(property "Reference" "L3"
			(at -0.635 2.667 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Ind4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:IND_XGL3520_COC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(U5-SW)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/1.8v")
			(pinfunction "2")
			(pintype "input")
		)
	)
	(footprint "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
		(layer "F.Cu")
		(at 119.253 83.058 90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "P4"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONN_01X05"
			(at 0 12.49 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.33 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(P4-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(P4-P4)")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(P4-P5)")
			(pinfunction "P5")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 131.826 90.424)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C40"
			(at -1.524 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:IND_XGL3520_COC"
		(layer "F.Cu")
		(at 142.362876 98.171)
		(tags "XGL3520-102MEC ")
		(property "Reference" "L4"
			(at -1.27 2.667 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ind4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:IND_XGL3520_COC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(U6-SW)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.0541 0)
			(size 0.7112 3.0734)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pinfunction "2")
			(pintype "input")
		)
	)
	(footprint "t_misc:cap_0603"
		(layer "F.Cu")
		(at 114.046 94.361)
		(descr "SMT resistor, 0603")
		(property "Reference" "C8"
			(at 0.762 -1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "47uf"
			(at 0 0.6096 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1206"
		(layer "F.Cu")
		(at 111.887 102.87 180)
		(descr "SMT capacitor, 1206")
		(property "Reference" "C4"
			(at 0.0254 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 -1.6002 180)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1206"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_1206.stp"
			(offset
				(xyz -0.599999991 -0.5499999917 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 146.469876 91.245874 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R33"
			(at -0.381 0.974 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/1.0v")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 127.889 87.503 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C36"
			(at 0.127 1.905 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/2.5v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 129.54 94.488 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C18"
			(at -3.937 0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7nf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U5-SS_TR)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 117.348 91.567)
		(property "Reference" "TP4"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(C13-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 119.634 97.409 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C11"
			(at -1.651 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 128.524 92.456 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R31"
			(at 0 1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(C19-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/1.8v")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 120.904 94.107 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C12"
			(at -2.159 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7nf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U2-SS_TR)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 106.299 90.17)
		(property "Reference" "TP1"
			(at -1.778 -0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/5.6v")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
		(layer "F.Cu")
		(at 110.805 71.882)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "P2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONN_01X05"
			(at 0 12.49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_connectors:Pin_Header_Straight_1x05_Pitch2.54mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.33 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(P2-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(P2-P2)")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(P2-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(P2-P4)")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(P2-P5)")
			(pinfunction "P5")
			(pintype "passive")
		)
	)
	(footprint "t_qfn:RWY0009A-MFG"
		(layer "F.Cu")
		(at 138.492127 96.844128 180)
		(tags "TPS62813QWRWYRQ1 ")
		(property "Reference" "U6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS62813QWRWYRQ1"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RWY0009A-MFG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62813-q1.pdf?ts=1732709405459&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RWY0009A-MFG")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -0.568749 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(P4-P5)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 0.193748) (xy -0.581251 0.143749) (xy -0.581251 -0.006251) (xy -0.531251 -0.056251)
						(xy -0.206251 -0.056254) (xy -0.156251 -0.106251) (xy -0.156251 -0.531251) (xy -0.106248 -0.581251)
						(xy 0.143749 -0.581251) (xy 0.193748 -0.531251) (xy 0.193748 0.143751) (xy 0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -0.55 -1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(P4-P5)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 0 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 14 "Net-(U6-SW)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd custom
			(at -0.568749 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 9 "Net-(U6-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 -0.193748) (xy -0.581251 -0.143749) (xy -0.581251 0.006251) (xy -0.531251 0.056251)
						(xy -0.206251 0.056251) (xy -0.156248 0.106251) (xy -0.156251 0.531251) (xy -0.106248 0.581251)
						(xy 0.143749 0.581251) (xy 0.193748 0.531251) (xy 0.193748 -0.143751) (xy 0.143751 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "5" smd circle
			(at -0.55 1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 9 "Net-(U6-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 0 1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U6-SS_TR)")
			(pinfunction "SS_TR")
			(pintype "unspecified")
		)
		(pad "7" smd circle
			(at 0.55 1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 31 "Net-(U6-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
		)
		(pad "7" smd custom
			(at 0.568747 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 31 "Net-(U6-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 -0.193748) (xy 0.581253 -0.143749) (xy 0.581253 0.006251) (xy 0.531253 0.056251)
						(xy 0.206253 0.056251) (xy 0.15625 0.106251) (xy 0.156253 0.531251) (xy 0.10625 0.581251) (xy -0.143747 0.581251)
						(xy -0.193749 0.531251) (xy -0.193746 -0.143751) (xy -0.143749 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "8" smd circle
			(at 0.55 -1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "8" smd custom
			(at 0.568747 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 0.193748) (xy 0.581253 0.143749) (xy 0.581253 -0.006251) (xy 0.531253 -0.056251)
						(xy 0.206253 -0.056251) (xy 0.15625 -0.106251) (xy 0.156253 -0.531251) (xy 0.10625 -0.581251)
						(xy -0.143747 -0.581251) (xy -0.193749 -0.531251) (xy -0.193746 0.143751) (xy -0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd rect
			(at 0 -1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U6-PG)")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_qfn/TPS62813QWRWYRQ1.STEP"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_qfn:RWY0009A-MFG"
		(layer "F.Cu")
		(at 147.569876 96.380875 180)
		(tags "TPS62813QWRWYRQ1 ")
		(property "Reference" "U7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS62813QWRWYRQ1"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RWY0009A-MFG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62813-q1.pdf?ts=1732709405459&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RWY0009A-MFG")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -0.568749 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 21 "Net-(P4-P4)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 0.193748) (xy -0.581251 0.143749) (xy -0.581251 -0.006251) (xy -0.531251 -0.056251)
						(xy -0.206251 -0.056254) (xy -0.156251 -0.106251) (xy -0.156251 -0.531251) (xy -0.106248 -0.581251)
						(xy 0.143749 -0.581251) (xy 0.193748 -0.531251) (xy 0.193748 0.143751) (xy 0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -0.55 -1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 21 "Net-(P4-P4)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 0 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 15 "Net-(U7-SW)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd custom
			(at -0.568749 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 11 "Net-(U7-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 -0.193748) (xy -0.581251 -0.143749) (xy -0.581251 0.006251) (xy -0.531251 0.056251)
						(xy -0.206251 0.056251) (xy -0.156248 0.106251) (xy -0.156251 0.531251) (xy -0.106248 0.581251)
						(xy 0.143749 0.581251) (xy 0.193748 0.531251) (xy 0.193748 -0.143751) (xy 0.143751 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "5" smd circle
			(at -0.55 1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 11 "Net-(U7-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 0 1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U7-SS_TR)")
			(pinfunction "SS_TR")
			(pintype "unspecified")
		)
		(pad "7" smd circle
			(at 0.55 1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 32 "Net-(U7-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
		)
		(pad "7" smd custom
			(at 0.568747 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 32 "Net-(U7-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 -0.193748) (xy 0.581253 -0.143749) (xy 0.581253 0.006251) (xy 0.531253 0.056251)
						(xy 0.206253 0.056251) (xy 0.15625 0.106251) (xy 0.156253 0.531251) (xy 0.10625 0.581251) (xy -0.143747 0.581251)
						(xy -0.193749 0.531251) (xy -0.193746 -0.143751) (xy -0.143749 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "8" smd circle
			(at 0.55 -1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "8" smd custom
			(at 0.568747 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 0.193748) (xy 0.581253 0.143749) (xy 0.581253 -0.006251) (xy 0.531253 -0.056251)
						(xy 0.206253 -0.056251) (xy 0.15625 -0.106251) (xy 0.156253 -0.531251) (xy 0.10625 -0.581251)
						(xy -0.143747 -0.581251) (xy -0.193749 -0.531251) (xy -0.193746 0.143751) (xy -0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd rect
			(at 0 -1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U7-PG)")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_qfn/TPS62813QWRWYRQ1.STEP"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 128.905 100.584 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R11"
			(at 0 -0.9144 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "Net-(P2-P3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U5-PG)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 139.822876 93.509876 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R21"
			(at 1.561876 1.147124 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U6-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:RWY0009A-MFG"
		(layer "F.Cu")
		(at 129.794 97.633001 180)
		(tags "TPS62813QWRWYRQ1 ")
		(property "Reference" "U5"
			(at 1.651 -2.061999 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS62813QWRWYRQ1"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:RWY0009A-MFG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62813-q1.pdf?ts=1732709405459&ref_url=https%253A%252F%252Fwww.mouser.co.uk%252F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RWY0009A-MFG")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1 -4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -0.568749 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 18 "Net-(P1-P1)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 0.193748) (xy -0.581251 0.143749) (xy -0.581251 -0.006251) (xy -0.531251 -0.056251)
						(xy -0.206251 -0.056254) (xy -0.156251 -0.106251) (xy -0.156251 -0.531251) (xy -0.106248 -0.581251)
						(xy 0.143749 -0.581251) (xy 0.193748 -0.531251) (xy 0.193748 0.143751) (xy 0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -0.55 -1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 18 "Net-(P1-P1)")
			(pinfunction "MODE_SYNC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0 0 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 13 "Net-(U5-SW)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 0.499999 180)
			(size 2.3 0.249999)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd custom
			(at -0.568749 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 6 "Net-(U5-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.531251 -0.193748) (xy -0.581251 -0.143749) (xy -0.581251 0.006251) (xy -0.531251 0.056251)
						(xy -0.206251 0.056251) (xy -0.156248 0.106251) (xy -0.156251 0.531251) (xy -0.106248 0.581251)
						(xy 0.143749 0.581251) (xy 0.193748 0.531251) (xy 0.193748 -0.143751) (xy 0.143751 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "5" smd circle
			(at -0.55 1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 6 "Net-(U5-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 0 1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U5-SS_TR)")
			(pinfunction "SS_TR")
			(pintype "unspecified")
		)
		(pad "7" smd circle
			(at 0.55 1.4 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 27 "Net-(U5-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
		)
		(pad "7" smd custom
			(at 0.568747 1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 27 "Net-(U5-COMP_FSET)")
			(pinfunction "COMP_FSET")
			(pintype "unspecified")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 -0.193748) (xy 0.581253 -0.143749) (xy 0.581253 0.006251) (xy 0.531253 0.056251)
						(xy 0.206253 0.056251) (xy 0.15625 0.106251) (xy 0.156253 0.531251) (xy 0.10625 0.581251) (xy -0.143747 0.581251)
						(xy -0.193749 0.531251) (xy -0.193746 -0.143751) (xy -0.143749 -0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "8" smd circle
			(at 0.55 -1.425 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "8" smd custom
			(at 0.568747 -1.068748 180)
			(size 0.327607 0.327607)
			(layers "F.Cu" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "EN")
			(pintype "input")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.531253 0.193748) (xy 0.581253 0.143749) (xy 0.581253 -0.006251) (xy 0.531253 -0.056251)
						(xy 0.206253 -0.056251) (xy 0.15625 -0.106251) (xy 0.156253 -0.531251) (xy 0.10625 -0.581251)
						(xy -0.143747 -0.581251) (xy -0.193749 -0.531251) (xy -0.193746 0.143751) (xy -0.143749 0.193751)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd rect
			(at 0 -1.325001 180)
			(size 0.249999 0.650001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U5-PG)")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_qfn/TPS62813QWRWYRQ1.STEP"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0603"
		(layer "F.Cu")
		(at 117.602 94.361 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C9"
			(at 0.508 0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "47uf"
			(at 0 0.6096 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 104.775 96.52 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R4"
			(at -1.524 0.381 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(R15-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 106.426 96.901)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R15"
			(at -3.683 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(R15-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 123.571 89.662 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C35"
			(at -0.127 0.889 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 148.839876 100.198876 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R28"
			(at -1.778 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(P4-P4)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 145.241876 88.197874 -90)
		(property "Reference" "TP9"
			(at -2.032 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(C31-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_connectors:CONN_1729047_PXC"
		(layer "F.Cu")
		(at 118.778 73.152)
		(tags "1729047 ")
		(property "Reference" "P3"
			(at -4.478 -2.794 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X05"
			(at 10 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:CONN_1729047_PXC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/5.6v")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/3.3v")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/2.5v")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.000001 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/1.8v")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.000001 0)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/1.3v")
			(pinfunction "P5")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_connectors/1729047.step"
			(offset
				(xyz -2.5 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 136.779 87.757 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C38"
			(at -1.651 -0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 146.511876 93.277874 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R23"
			(at 0.381 -0.889 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U7-COMP_FSET)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 106.934 101.6 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R2"
			(at -1.778 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(P2-P5)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 103.124 103.378)
		(property "Reference" "TP22"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 120.269 100.076 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R6"
			(at 0.635 -1.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(P2-P4)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-PG)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 125.222 86.614)
		(property "Reference" "TP6"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(C19-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 132.715 94.234)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C21"
			(at 1.651 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/1.8v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 137.917876 91.477876 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R32"
			(at -1.778 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(C25-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:VQFN22_RYF_TEX"
		(layer "F.Cu")
		(at 110.2614 98.044)
		(tags "LM64460APPQRYFRQ1 ")
		(property "Reference" "U1"
			(at -4.4704 -4.191 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LM64460APPQRYFRQ1"
			(at 0 -3.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_qfn:VQFN22_RYF_TEX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VQFN22_RYF_TEX")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.6924 -3.048 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.6924 -3.048 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.939999 -1.750441 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.939999 -1.750441 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -0.5 -5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.575001 -1.500378 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U1-CBOOT)")
			(pinfunction "CBOOT")
			(pintype "power_in")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.127 -0.381) (xy -0.127 -0.381) (xy -0.127 0.381) (xy 0.635 0.380998) (xy 0.635 0.126998)
						(xy 0.127 0.126998)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd rect
			(at -1.325 -1.75 180)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U1-CBOOT)")
			(pinfunction "CBOOT")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.575001 -1.000252 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "unconnected-(U1-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -1.575001 -0.500126 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/5.6v")
			(pinfunction "BIAS")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.575001 0 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U1-VCC)")
			(pinfunction "VCC")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -1.575001 0.500126 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U1-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -1.575001 1.000252 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(P2-P5)")
			(pinfunction "PGOOD")
			(pintype "output")
		)
		(pad "7" smd custom
			(at -1.575001 1.500378 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(P1-P3)")
			(pinfunction "MODE/SYNC")
			(pintype "input")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.127 -0.381) (xy 0.127 0.381) (xy -0.635 0.380998) (xy -0.635 0.126998) (xy -0.127 0.126998)
						(xy -0.127 -0.381)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "7" smd rect
			(at -1.325 1.75 180)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(P1-P3)")
			(pinfunction "MODE/SYNC")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -0.750189 1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(Q1-D)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -0.250063 1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "unconnected-(U1-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd rect
			(at 0.250063 1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pinfunction "VIN2")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at 0.750189 1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "unconnected-(U1-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" smd rect
			(at 1.325 1.75 180)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PGND2")
			(pintype "power_out")
		)
		(pad "12" smd custom
			(at 1.575001 1.500378 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PGND2")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.127 0.381) (xy 0.127 -0.381) (xy -0.635 -0.380998) (xy -0.635 -0.126998) (xy -0.127 -0.126998)
						(xy -0.127 0.381)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "13" smd rect
			(at 1.575001 1.000252 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "unconnected-(U1-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "14" smd rect
			(at 1.575001 0.500126 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(U1-SW1)")
			(pinfunction "SW1")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 1.575001 0 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(U1-SW1)")
			(pinfunction "SW2")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at 1.575001 -0.500126 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(U1-SW1)")
			(pinfunction "SW3")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 1.575001 -1.000252 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "unconnected-(U1-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at 1.325 -1.75 180)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PGND1")
			(pintype "power_out")
		)
		(pad "18" smd custom
			(at 1.575001 -1.500378 90)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PGND1")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.635 -0.380998) (xy -0.127 -0.381) (xy -0.127 0.381) (xy 0.127 0.381) (xy 0.127 -0.126998)
						(xy 0.635 -0.126998)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "19" smd rect
			(at 0.750189 -1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "unconnected-(U1-NC-Pad19)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 0.250063 -1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pinfunction "VIN1")
			(pintype "power_in")
		)
		(pad "21" smd rect
			(at -0.250063 -1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "unconnected-(U1-NC-Pad21)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "22" smd rect
			(at -0.750189 -1.825)
			(size 0.254 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U1-SW4)")
			(pinfunction "SW4")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at 0 0)
			(size 1.7018 2.2098)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(model "${T_LIBS}/3d/t_qfn/LM64460APPQRYFRQ1.STEP"
			(offset
				(xyz 0 0 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 141.219876 88.937876)
		(property "Reference" "TP7"
			(at -1.778 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(C25-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 147.908876 91.880874)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C31"
			(at 1.697124 0.067126 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U7-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 147.527876 99.119874 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R14"
			(at 1.223876 -0.956126 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "Net-(P2-P1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U7-PG)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 122.682 100.584 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R18"
			(at -1.905 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(P1-P2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 160.909 103.378)
		(property "Reference" "TP23"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 138.176 86.614)
		(property "Reference" "TP8"
			(at -1.651 -0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/1.3v")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 131.826 89.535)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C42"
			(at -1.524 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/1.2v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 129.667 86.614)
		(property "Reference" "TP5"
			(at 0 -1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/1.8v")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 116.967 104.521)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R24"
			(at 1.778 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(P4-P3)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 148.289876 87.562874 -90)
		(property "Reference" "TP10"
			(at -1.905 0.508 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/1.0v")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 132.588 88.392)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C39"
			(at -1.905 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 138.806876 93.509876 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C24"
			(at -3.556 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7nf"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U6-SS_TR)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 111.252 95.123 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C1"
			(at 0.127 0.762 180)
			(layer "F.SilkS")
		)
		(property "Value" "10nf"
			(at 0 0.4826 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/Vin")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 120.015 92.075 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R30"
			(at 0 1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/3.3v")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 128.651 94.488 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R10"
			(at 0.254 -0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(U5-COMP_FSET)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 148.289876 93.277874 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R20"
			(at 0.059874 0.935124 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U7-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 130.556 100.838 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R26"
			(at -1.778 -0.127 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(P1-P1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 130.429 94.488 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R29"
			(at 0.127 0.889 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U5-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 107.823 101.981 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R17"
			(at -1.905 0.085 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(P1-P3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 141.224 94.869)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C27"
			(at 2.921 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/1.3v")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 139.441876 91.223876)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R19"
			(at 1.782124 -0.672876 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U6-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(C25-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 121.92 94.107 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R9"
			(at 0.127 0.889 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 106.426 97.917)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R3"
			(at -3.429 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res2"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206 SM0402")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(R15-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U1-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:cap_0402"
		(layer "F.Cu")
		(at 122.428 92.71)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C13"
			(at 1.778 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "10pf"
			(at 0 0.4826 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Root")
		(sheetfile "power supply test.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-FB)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 99.314 67.945)
		(end 165.354 122.301)
		(locked yes)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "1.1v\n"
		(at 131.064 111.125 270)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 126.238 111.125 270)
		(layer "F.SilkS")
	)
	(gr_text "5.6 sync\n"
		(at 105.41 77.089 0)
		(layer "F.SilkS")
	)
	(gr_text "U6 pgood"
		(at 113.792 74.549 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3 sync\n"
		(at 106.68 74.422 90)
		(layer "F.SilkS")
	)
	(gr_text "1.8 sync\n"
		(at 108.077 70.231 0)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 118.999 81.153 270)
		(layer "F.SilkS")
	)
	(gr_text "2.5v\n"
		(at 128.524 78.486 270)
		(layer "F.SilkS")
	)
	(gr_text "U7 pgood"
		(at 113.919 71.882 0)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 106.299 82.169 0)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 121.031 110.998 270)
		(layer "F.SilkS")
	)
	(gr_text "1.3v\n"
		(at 138.557 78.613 270)
		(layer "F.SilkS")
	)
	(gr_text "1.2v\n\n"
		(at 135.255 111.125 270)
		(layer "F.SilkS")
	)
	(gr_text "1.0v\n"
		(at 140.716 110.617 270)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 106.299 79.502 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3v\n"
		(at 123.063 78.613 270)
		(layer "F.SilkS")
	)
	(gr_text "U2 pgood"
		(at 113.665 79.629 0)
		(layer "F.SilkS")
	)
	(gr_text "1.8v\n"
		(at 134.112 78.613 270)
		(layer "F.SilkS")
	)
	(gr_text "VIN\n"
		(at 106.807 111.252 90)
		(layer "F.SilkS")
	)
	(gr_text "5.6v\n"
		(at 118.237 78.486 270)
		(layer "F.SilkS")
	)
	(gr_text "1.3 sync\n"
		(at 129.54 80.518 270)
		(layer "F.SilkS")
	)
	(gr_text "U1 pgood"
		(at 113.538 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "Q1 gate"
		(at 124.333 80.518 270)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 112.776 111.379 90)
		(layer "F.SilkS")
	)
	(gr_text "U5 pgood"
		(at 113.792 77.216 0)
		(layer "F.SilkS")
	)
	(gr_text "gnd\n"
		(at 121.539 81.026 270)
		(layer "F.SilkS")
	)
	(gr_text "1.0 sync\n"
		(at 127.127 80.391 270)
		(layer "F.SilkS")
	)
	(gr_text_box "SK 1715\nYTH 18/12/24\n"
		(start 101.092 84.201)
		(end 114.3 87.884)
		(layer "F.SilkS")
		(border yes)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "x1")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.681 95.631) (xy 113.776582 95.631) (xy 113.157 95.758) (xy 113.157 95.123) (xy 115.313892 95.130905)
				(xy 116.713 95.123) (xy 116.713 100.457) (xy 114.554 100.33)
			)
		)
	)
	(zone
		(net 67)
		(net_name "Net-(U1-SW1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.633 97.409) (xy 114.3 97.409) (xy 114.3 98.806) (xy 111.633 98.679)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/5.6v")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.889 97.663) (xy 131.191 97.663) (xy 131.318 102.235) (xy 127.889 102.235)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/5.6v")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads thru_hole_only
			(clearance 0.1524)
		)
		(min_thickness 0.1778)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 105.537 69.469) (xy 121.666 69.723) (xy 119.253 97.536) (xy 147.447 96.774) (xy 148.209 103.759)
				(xy 104.14 105.156)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/5.6v")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.763 97.155) (xy 139.065 97.155) (xy 139.192 101.727) (xy 135.763 101.727)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/5.6v")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.1778)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.060876 97.023876) (xy 142.108876 97.023876) (xy 141.219876 99.944876) (xy 138.806876 101.595876)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "In1.Cu" "In3.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.203 68.58) (xy 164.465 68.961) (xy 164.084 121.793) (xy 139.666222 121.648231) (xy 99.822 121.412)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/Vin")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.937781 95.297218) (xy 111.621781 93.138218) (xy 111.367781 120.697218) (xy 102.235 120.777)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/3.3v")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.1778)
		)
		(min_thickness 0.1778)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.0249 71.758951) (xy 124.9619 72.520951) (xy 135.5029 89.157951) (xy 135.5029 95.380951)
				(xy 125.984 100.33) (xy 118.6119 90.173951)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/1.3v")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.832204 71.236867) (xy 147.610204 99.049867) (xy 141.768204 98.668867) (xy 134.747 91.313)
				(xy 136.942204 71.829867)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/1.8v")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.461 71.374) (xy 137.287 73.787) (xy 137.414 100.711) (xy 127.635 93.853)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/1.1v")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.65617 86.995) (xy 135.02117 85.217) (xy 128.651 88.138) (xy 129.622348 112.137667) (xy 128.905 117.475)
				(xy 129.94117 120.015) (xy 133.49717 118.999) (xy 130.95717 89.281)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/1.2v")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.831962 89.582819) (xy 137.419962 88.947819) (xy 138.816962 115.363819) (xy 135.763 121.031)
				(xy 132.715 114.3) (xy 131.577962 89.836819)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/1.0v")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.319 116.713) (xy 145.415 101.854) (xy 145.542 89.789) (xy 148.082 85.344) (xy 153.67 93.726)
				(xy 155.617507 96.603323) (xy 153.966507 116.161323) (xy 139.319 121.031)
			)
		)
	)
)
