<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="43.18" y1="17.78" x2="1.27" y2="17.78" width="0" layer="20"/>
<wire x1="1.27" y1="17.78" x2="0" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="0" y1="16.51" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="43.18" y2="0" width="0" layer="20"/>
<wire x1="43.18" y1="0" x2="44.45" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="44.45" y1="1.27" x2="44.45" y2="16.51" width="0" layer="20"/>
<wire x1="44.45" y1="16.51" x2="43.18" y2="17.78" width="0" layer="20" curve="90"/>
<text>5V</text>
<text>GND</text>
<text>DAT</text>
<text>CLK</text>
<text>LAT</text>
<text>Revision 1.0</text>
<text>SPI LCD Backpack</text>
<hole x="42.164" y="5.461" drill="3.2"/>
<hole x="2.286" y="4.953" drill="3.2"/>
<text>ScareTronix (c)2011-2013</text>
<text>1</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TC33X">
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="74xx-us">
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="transistor">
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
<package name="1X16_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="74xx-us" package="SO16" value="74LS595D">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05" value="M5PTH">
<attribute name="NAME"/>
</element>
<element name="Q1" library="transistor" package="SOT23-BEC" value="MMBT2222">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="CONTRAST" library="adafruit" package="TC33X" value="10K">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="A/3216-18R" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X16_LONGPADS" value="M16LONGPADS">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="10"/>
<contactref element="CONTRAST" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="15"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="1"/>
<contactref element="Q1" pad="E"/>
<contactref element="CONTRAST" pad="3"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="RS">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="E">
<contactref element="J2" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DB4">
<contactref element="J2" pad="11"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="DB6">
<contactref element="J2" pad="13"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="DB7">
<contactref element="J2" pad="14"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="DB5">
<contactref element="J2" pad="12"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="Q1" pad="C"/>
<contactref element="J2" pad="16"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="B"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="LITE">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="CONTRAST" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="DATA">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="LATCH">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
