(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "RC12-3")
		(date "2024-12-11")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J1-Pin_7)")
	(net 3 "Net-(J1-Pin_8)")
	(net 4 "+5V")
	(net 5 "+12V")
	(net 6 "unconnected-(J1-Pin_1-Pad1)")
	(net 7 "unconnected-(J1-Pin_2-Pad2)")
	(net 8 "unconnected-(J1-Pin_3-Pad3)")
	(net 9 "Net-(J1-Pin_9)")
	(net 10 "Flow Pin2")
	(net 11 "Net-(J1-Pin_12)")
	(net 12 "unconnected-(J1-Pin_10-Pad10)")
	(net 13 "unconnected-(J1-Pin_11-Pad11)")
	(net 14 "unconnected-(J1-Pin_13-Pad13)")
	(net 15 "unconnected-(J1-Pin_14-Pad14)")
	(net 16 "unconnected-(J1-Pin_15-Pad15)")
	(net 17 "unconnected-(J2-Pin_1-Pad1)")
	(net 18 "unconnected-(J2-Pin_3-Pad3)")
	(net 19 "unconnected-(J2-Pin_5-Pad5)")
	(net 20 "unconnected-(J2-Pin_6-Pad6)")
	(net 21 "Net-(J2-Pin_7)")
	(net 22 "Net-(J2-Pin_8)")
	(net 23 "unconnected-(J2-Pin_9-Pad9)")
	(net 24 "unconnected-(J2-Pin_10-Pad10)")
	(net 25 "Flow Pin1")
	(net 26 "unconnected-(J2-Pin_13-Pad13)")
	(net 27 "unconnected-(J2-Pin_14-Pad14)")
	(net 28 "unconnected-(J2-Pin_15-Pad15)")
	(net 29 "WorkSwitch")
	(net 30 "Flow Sensor1")
	(net 31 "Flow Sensor2")
	(net 32 "Net-(R2-Pad2)")
	(net 33 "Net-(D1-A)")
	(net 34 "Net-(D3-A)")
	(net 35 "Net-(R7-Pad2)")
	(net 36 "Net-(D4-A)")
	(net 37 "Net-(D2-K)")
	(net 38 "Net-(J7-Pin_3)")
	(net 39 "Net-(J7-Pin_4)")
	(net 40 "Net-(J7-Pin_5)")
	(net 41 "Net-(J7-Pin_6)")
	(net 42 "Net-(J7-Pin_7)")
	(net 43 "Net-(J7-Pin_8)")
	(net 44 "Net-(J7-Pin_9)")
	(net 45 "Net-(J7-Pin_10)")
	(net 46 "Net-(J7-Pin_11)")
	(net 47 "Net-(J7-Pin_12)")
	(net 48 "Net-(J7-Pin_13)")
	(net 49 "Net-(J7-Pin_14)")
	(net 50 "Net-(J7-Pin_15)")
	(net 51 "Net-(J7-Pin_16)")
	(net 52 "Net-(J7-Pin_17)")
	(net 53 "Net-(J7-Pin_18)")
	(net 54 "Net-(U4-~{RESET})")
	(net 55 "unconnected-(U4-NC-Pad11)")
	(net 56 "unconnected-(U4-NC-Pad14)")
	(net 57 "unconnected-(U4-INTB-Pad19)")
	(net 58 "unconnected-(U4-INTA-Pad20)")
	(net 59 "PressurePin")
	(net 60 "WorkSwitchPin")
	(net 61 "Net-(R5-Pad2)")
	(net 62 "Net-(D5-A)")
	(net 63 "PressureSensor")
	(net 64 "Net-(J3-Pin_1)")
	(net 65 "unconnected-(J4-Red-Pad3)")
	(net 66 "unconnected-(J5-Red-Pad3)")
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 64.28 48.7 -90)
		(descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x15 2.54mm single row")
		(property "Reference" "J2"
			(at 0.25 -2.72 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Female"
			(at 0 38.33 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 17.78 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J2-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J2-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J2-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J2-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J2-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J2-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "WorkSwitchPin")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "PressurePin")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J2-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J2-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J2-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 86.2 58.65 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 5.075 0.175 360)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 6.675 0.275 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 33.8 73.72 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(R5-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 55.98 27.7 180)
		(descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-05A example for new part number: 22-27-2051, 5 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex KK-254 vertical")
		(property "Reference" "J9"
			(at 12.68 -3.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 5.08 1.99 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 -2.22 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.143678)
			(net 2 "Net-(J1-Pin_7)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_8)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_9)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_12)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.74 2.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-05A_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(at 38.66 79.7 90)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PC817"
			(at 3.81 4.87 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(R5-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "WorkSwitchPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MyFootprints:Grove"
		(layer "F.Cu")
		(at 37.4 27.52 180)
		(property "Reference" "J4"
			(at 6.6 -1.7 360)
			(layer "F.SilkS")
		)
		(property "Value" "Motor2 GRV"
			(at 0.1 -3.3 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "MyFootprints:Grove"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_9)")
			(pinfunction "Yellow")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_12)")
			(pinfunction "White")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 1 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(J4-Red-Pad3)")
			(pinfunction "Red")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at 3 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Black")
			(pintype "passive")
		)
		(model "${MYKICAD}/My3dShapes/110990030.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 64.23 33.49 -90)
		(descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x15 2.54mm single row")
		(property "Reference" "J1"
			(at 0.185 -2.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x15_Female"
			(at 0 38.33 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 17.78 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Flow Pin2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Flow Pin1")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J1-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J1-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 47.15 73.72 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(R7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 72.62 26.3 90)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "J7"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Relay"
			(at 1.27 25.19 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J7-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J7-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J7-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J7-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J7-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J7-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J7-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J7-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J7-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J7-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J7-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J7-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J7-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J7-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J7-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J7-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-14-5.0-H_1x14_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 108.1 116.2 90)
		(descr "Terminal Block Phoenix PT-1,5-14-5.0-H, 14 pins, pitch 5mm, size 70x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix PT-1,5-14-5.0-H pitch 5mm size 70x9mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J6"
			(at 68.9 1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x14"
			(at 32.5 6.06 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-14-5.0-H_1x14_P5.00mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 32.5 2.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "PressureSensor")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "WorkSwitch")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Flow Sensor1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Flow Sensor2")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+12V")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+12V")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+12V")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+12V")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 40 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 45 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 50 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 55 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 60 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 65 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-14-5.0-H_1x14_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 95.5 83.4 -90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 6.425 5.075 90)
			(layer "F.SilkS")
		)
		(property "Value" "1000uF"
			(at 10 2.6 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 80 48.4)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C6"
			(at -2.8 -0.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf"
			(at -3.6 0.8 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 41.6 99.8)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D5"
			(at 3.81 -2.12 360)
			(layer "F.SilkS")
		)
		(property "Value" "BAT42"
			(at 3.81 2.12 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "30V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 360)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 360)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-28_W7.62mm"
		(layer "F.Cu")
		(at 68.24 45.22 90)
		(descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "MCP23017_SP"
			(at 3.81 35.35 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, SPDIP-28"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J7-Pin_3)")
			(pinfunction "GPB0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J7-Pin_5)")
			(pinfunction "GPB1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J7-Pin_7)")
			(pinfunction "GPB2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J7-Pin_9)")
			(pinfunction "GPB3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J7-Pin_11)")
			(pinfunction "GPB4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J7-Pin_13)")
			(pinfunction "GPB5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J7-Pin_15)")
			(pinfunction "GPB6")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J7-Pin_17)")
			(pinfunction "GPB7")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(U4-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_7)")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_8)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(U4-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" thru_hole oval
			(at 7.62 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 7.62 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "17" thru_hole oval
			(at 7.62 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "18" thru_hole oval
			(at 7.62 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(U4-~{RESET})")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "19" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(U4-INTB-Pad19)")
			(pinfunction "INTB")
			(pintype "tri_state+no_connect")
		)
		(pad "20" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(U4-INTA-Pad20)")
			(pinfunction "INTA")
			(pintype "tri_state+no_connect")
		)
		(pad "21" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J7-Pin_18)")
			(pinfunction "GPA0")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J7-Pin_16)")
			(pinfunction "GPA1")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J7-Pin_14)")
			(pinfunction "GPA2")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J7-Pin_12)")
			(pinfunction "GPA3")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J7-Pin_10)")
			(pinfunction "GPA4")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J7-Pin_8)")
			(pinfunction "GPA5")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J7-Pin_6)")
			(pinfunction "GPA6")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J7-Pin_4)")
			(pinfunction "GPA7")
			(pintype "bidirectional")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(at 51.9425 79.7 90)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PC817"
			(at 3.81 4.87 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(R7-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Flow Pin1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MyFootprints:1N5408"
		(layer "F.Cu")
		(at 75.1 76.2)
		(descr "DO-201AD")
		(tags "Diode")
		(property "Reference" "D2"
			(at 15.225 5.9 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N5408"
			(at 9.2 -4.5 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "MyFootprints:1N5408"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 65.05 164.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 65.05 164.95 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6 4.1 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.25 2.25)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 22.6 0)
			(size 2.25 2.25)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+12V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_5W_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.8 1.8 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 103.9 26.8 -90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -3.932323 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1000uF"
			(at 3.967677 -6.2 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 79.88 89.55 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 5.08 -2.47 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 5.08 2.47 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Flow Sensor2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 31.45 68.2 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C9"
			(at 1.25 -2.5 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 2.5 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 60.5 73.72 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 48.88 54.8 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 360)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 5.08 2.37 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_7)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 89.3 48.4 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at -2.6 0.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at -3.5 -0.8 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 36.6 116.3)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 56.675 54.725 90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C5"
			(at 1.7 2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf"
			(at 0.1 3.6 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 93.5 116.4)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 79.88 96.3 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D3"
			(at 5.08 -2.47 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 5.08 2.47 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Flow Sensor1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 34.4 54.32 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "PressurePin")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 93.2 102.92)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J3"
			(at -0.2 7.58 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pressure"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "PressureSensor")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 41.6 107.9)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D6"
			(at 3.81 -2.12 360)
			(layer "F.SilkS")
		)
		(property "Value" "BAT42"
			(at 3.81 2.12 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/85660/bat42.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "30V 0.2A Small Signal Schottky Diode, DO-35"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 360)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 360)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 98.98 34.3 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 7.5 2.175 360)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.125 2.35 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(U4-~{RESET})")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 110.5 23.6)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MyFootprints:Grove"
		(layer "F.Cu")
		(at 64.4 27.52 180)
		(property "Reference" "J5"
			(at 5.5 -2.98 0)
			(layer "F.SilkS")
		)
		(property "Value" "Motor1 GRV"
			(at -0.3 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "MyFootprints:Grove"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_7)")
			(pinfunction "Yellow")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_8)")
			(pinfunction "White")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 1 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(J5-Red-Pad3)")
			(pinfunction "Red")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at 3 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Black")
			(pintype "passive")
		)
		(model "${MYKICAD}/My3dShapes/110990030.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 53.52 107.9)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 -2.37 360)
			(layer "F.SilkS")
		)
		(property "Value" "3K"
			(at 5.08 2.37 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 48.88 61 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.37 360)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 5.08 2.37 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pin_8)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MyFootprints:MD13S_Outline2"
		(layer "F.Cu")
		(at 26.6215 85.2985)
		(descr "13Amp DC Motor Driver (MD13S)<br><br><br>Created by: Wai Weng")
		(property "Reference" "REF**"
			(at 1.905 -35.052 0)
			(layer "F.SilkS")
		)
		(property "Value" "MDD10A"
			(at 7.7216 -59.4868 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "MyFootprints:MD13S_Outline2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "MDD3A"
			(at 7.19328 -22.10308 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "MD13S"
			(at 3.2004 -28.4734 0)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 2.88 -31.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.88 -3.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 58.88 -31.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 58.88 -3.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "MyFootprints:mEZD71201A"
		(layer "F.Cu")
		(at 99.405 60.205 180)
		(property "Reference" "RG1"
			(at 5.4864 -3.2004 0)
			(layer "F.SilkS")
		)
		(property "Value" "mEZD71201A"
			(at 5.1054 -1.4478 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "MyFootprints:mEZD71201A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/doc_url/L20vZS9tZXpkNzEyMDFhX3IxLjZfMS5wZGY/prod_id/NTUy/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at 5.0038 5.595238 90)
			(layer "F.SilkS")
		)
		(fp_text user "Vin"
			(at 2.4384 6 90)
			(layer "F.SilkS")
		)
		(fp_text user "Vout"
			(at 7.5184 5.5 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 2.3368 8.5 270)
			(size 1.59 1.59)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D2-K)")
			(pinfunction "Vin")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 4.8768 8.5 270)
			(size 1.59 1.59)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 7.4168 8.5 270)
			(size 1.59 1.59)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pinfunction "Vout")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 2.5 -8.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 63.68 99.8 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 5.08 -2.37 360)
			(layer "F.SilkS")
		)
		(property "Value" "2K"
			(at 5.08 2.37 360)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DIGIKEY-PURCHASE-URL" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D5-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MyFootprints:MD13S_Outline2"
		(layer "F.Cu")
		(at 26.52 120.26)
		(descr "13Amp DC Motor Driver (MD13S)<br><br><br>Created by: Wai Weng")
		(property "Reference" "REF**"
			(at 1.905 -35.052 0)
			(layer "F.SilkS")
		)
		(property "Value" "MDD10A"
			(at 7.7216 -59.4868 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "MyFootprints:MD13S_Outline2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "MDD3A"
			(at 7.19328 -22.10308 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(fp_text user "MD13S"
			(at 3.2004 -28.4734 0)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 2.88 -31.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.88 -3.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 58.88 -31.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 58.88 -3.06)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 79.88 103.05 180)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D4"
			(at 5.08 -2.47 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at 5.08 2.47 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1000V 1A General Purpose Rectifier Diode, DO-41"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 0)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "WorkSwitch")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "F.Cu")
		(at 65.225 79.7 90)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PC817"
			(at 3.81 4.87 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Flow Pin2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 28.4 23.5)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "RC12-3.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(gr_line
		(start 25 118)
		(end 25 22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 27 120)
		(mid 25.585786 119.414214)
		(end 25 118)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114 118)
		(mid 113.414214 119.414214)
		(end 112 120)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114 118)
		(end 114 22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 25 22)
		(mid 25.585786 20.585786)
		(end 27 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112 120)
		(end 27 120)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112 20)
		(end 27 20)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 112 20)
		(mid 113.414214 20.585786)
		(end 114 22)
		(layer "Edge.Cuts")
	)
	(gr_text "Nano"
		(at 45 40.7 0)
		(layer "F.SilkS")
	)
	(gr_text "PWM2\n"
		(at 38.35 22.095238 90)
		(layer "F.SilkS")
	)
	(gr_text "PWM2\n"
		(at 48.1 22.4 90)
		(layer "F.SilkS")
	)
	(gr_text "Flow1"
		(at 98.994047 106.933394 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 74.185 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 70.435 29.6 0)
		(layer "F.SilkS")
	)
	(gr_text "DIR2\n"
		(at 40.5 22.5 90)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 102.023809 81.415129 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 65.5 45.8 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 101.880952 76.431826 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 94.585 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 84.71 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 92.235 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "PWM1\n"
		(at 65.6 22.1 90)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 63.7 36.8 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 51.4 82.1 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 102.023809 86.398432 0)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 76.685 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "Pressure"
		(at 96.80357 116.9 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 88.5 103.5 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 94.56 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 89.76 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "PWM1\n"
		(at 53.2 22.4 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 101.880952 66.46522 0)
		(layer "F.SilkS")
	)
	(gr_text "WorkSwitch"
		(at 94.994047 111.916697 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 102.023809 91.381735 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 87.235 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 102.5 51.515311 0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 102.023809 96.365038 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 102.5 56.498614 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 79.235 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 64.8 82.1 0)
		(layer "F.SilkS")
	)
	(gr_text "Flow2"
		(at 64.2 84.6 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 76.735 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 87.185 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "Ethernet -->"
		(at 58.9 40.8 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 89.4 108.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Flow2"
		(at 98.994047 101.950091 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 64.05175 24.344047 90)
		(layer "F.SilkS")
	)
	(gr_text "Flow1"
		(at 51.1 84.6 0)
		(layer "F.SilkS")
	)
	(gr_text "WorkSwitch"
		(at 36 84.6 0)
		(layer "F.SilkS")
	)
	(gr_text "RC12-3\n14-Dec-2024"
		(at 74.6 116.8 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 101.880952 71.448523 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 92.31 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "DIR1\n"
		(at 55.75 22.804762 90)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 79.280833 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 61.3 22.695238 90)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 89.71 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "<-- USB"
		(at 31.2 40.7 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 82.135 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "DIR1\n"
		(at 67.75 22.504762 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 45.55 22.995238 90)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 81.826666 29.575 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 38.1 82.1 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 84.66 21.95 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 74.185 29.55 0)
		(layer "F.SilkS")
	)
	(gr_text "Pressure\nVoltage"
		(at 93.4 100.9 0)
		(layer "F.SilkS")
	)
	(gr_text "DIR2\n"
		(at 50.65 22.804762 90)
		(layer "F.SilkS")
	)
	(gr_text "I2C address 0x21"
		(at 72.5 36 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 36.80175 24.339285 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 101.880952 61.481917 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 34.05 22.690476 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 70.41 21.975 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.3 20.4) (xy 26.4 20.3) (xy 25.2 21.8) (xy 25.4 118.7) (xy 26.9 119.7) (xy 111.9 119.8) (xy 113.7 118.5)
				(xy 113.7 21.6)
			)
		)
	)
)
