<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<circle x="17.8944" y="17.8944" locked="yes" radius="1.905" width="0.1524" layer="20"/>
<circle x="58.3056" y="17.8944" locked="yes" radius="1.905" width="0.1524" layer="20"/>
<circle x="58.3056" y="58.3056" locked="yes" radius="1.905" width="0.1524" layer="20"/>
<circle x="17.8944" y="58.3056" locked="yes" radius="1.905" width="0.1524" layer="20"/>
<circle x="38.227" y="38.227" locked="yes" radius="38.354" width="0.1524" layer="20"/>
<circle x="38.227" y="38.227" radius="38.354" width="0.1524" layer="20"/>
<text>LED_DATAPIN</text>
<text>Arch Series LED Driver v2
Matt Richard 2021</text>
<wire x1="29.21" y1="55.753" x2="47.117" y2="55.753" width="0.254" layer="20"/>
<wire x1="47.117" y1="55.753" x2="47.117" y2="48.641" width="0.254" layer="20"/>
<wire x1="47.117" y1="48.641" x2="29.21" y2="48.641" width="0.254" layer="20"/>
<wire x1="29.21" y1="48.641" x2="29.21" y2="55.753" width="0.254" layer="20"/>
<text>6       5       7       8</text>
<text>GND    5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND  SEN  3.3</text>
</plain>
<libraries>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="WEMOS-D1-MINI_PRETTY">
<description>WeMos.cc
D1 mini
ESP8266 module</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_XTRA_BIG">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_OFFSET">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Long Pads w/ Offset Holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="74xx-eu" package="DIL14" value="74HCT125N">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="D1MINI" library="esp8266modules" package="WEMOS-D1-MINI_PRETTY" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="330">
<attribute name="PROD_ID" value="RES-8371"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="L10_D8" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L12_D8" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L11_D8" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L1_D5" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L3_D5" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L2_D5" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L4_D6" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L6_D6" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L5_D6" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L7_D7" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L9_D7" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="L8_D7" library="SparkFun-Connectors" package="2X3_OFFSET" value="AVR_SPI_PROG_3X2OFFSET_PADS">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02_XTRA_BIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="E5-10,5" value="">
<attribute name="VALUE"/>
</element>
<element name="SENSOR" library="SparkFun-Connectors" package="1X03_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D1MINI" pad="GND"/>
<contactref element="L12_D8" pad="2"/>
<contactref element="L11_D8" pad="2"/>
<contactref element="L12_D8" pad="1"/>
<contactref element="L10_D8" pad="2"/>
<contactref element="L11_D8" pad="1"/>
<contactref element="L10_D8" pad="1"/>
<contactref element="L1_D5" pad="1"/>
<contactref element="L9_D7" pad="2"/>
<contactref element="L8_D7" pad="2"/>
<contactref element="L9_D7" pad="1"/>
<contactref element="L7_D7" pad="2"/>
<contactref element="L8_D7" pad="1"/>
<contactref element="L7_D7" pad="1"/>
<contactref element="L4_D6" pad="1"/>
<contactref element="L5_D6" pad="2"/>
<contactref element="L6_D6" pad="1"/>
<contactref element="L4_D6" pad="2"/>
<contactref element="L5_D6" pad="1"/>
<contactref element="L6_D6" pad="2"/>
<contactref element="L3_D5" pad="2"/>
<contactref element="L2_D5" pad="2"/>
<contactref element="L3_D5" pad="1"/>
<contactref element="L1_D5" pad="2"/>
<contactref element="L2_D5" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="SENSOR" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="14"/>
<contactref element="D1MINI" pad="5V"/>
<contactref element="L10_D8" pad="6"/>
<contactref element="L11_D8" pad="5"/>
<contactref element="L11_D8" pad="6"/>
<contactref element="L12_D8" pad="5"/>
<contactref element="L10_D8" pad="5"/>
<contactref element="L12_D8" pad="6"/>
<contactref element="L9_D7" pad="6"/>
<contactref element="L8_D7" pad="6"/>
<contactref element="L9_D7" pad="5"/>
<contactref element="L7_D7" pad="6"/>
<contactref element="L8_D7" pad="5"/>
<contactref element="L7_D7" pad="5"/>
<contactref element="L4_D6" pad="5"/>
<contactref element="L4_D6" pad="6"/>
<contactref element="L5_D6" pad="5"/>
<contactref element="L5_D6" pad="6"/>
<contactref element="L6_D6" pad="5"/>
<contactref element="L6_D6" pad="6"/>
<contactref element="L3_D5" pad="6"/>
<contactref element="L2_D5" pad="6"/>
<contactref element="L3_D5" pad="5"/>
<contactref element="L2_D5" pad="5"/>
<contactref element="L1_D5" pad="6"/>
<contactref element="L1_D5" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="DIN3">
<contactref element="IC1" pad="9"/>
<contactref element="D1MINI" pad="D8"/>
</signal>
<signal name="DIN2">
<contactref element="IC1" pad="5"/>
<contactref element="D1MINI" pad="D6"/>
</signal>
<signal name="DIN1">
<contactref element="IC1" pad="2"/>
<contactref element="D1MINI" pad="D5"/>
</signal>
<signal name="DIN4">
<contactref element="IC1" pad="12"/>
<contactref element="D1MINI" pad="D7"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="8"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="11"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="DOUT1">
<contactref element="R1" pad="P$2"/>
<contactref element="L1_D5" pad="3"/>
</signal>
<signal name="DOUT2">
<contactref element="R2" pad="P$2"/>
<contactref element="L4_D6" pad="3"/>
</signal>
<signal name="DOUT3">
<contactref element="R3" pad="P$2"/>
<contactref element="L10_D8" pad="3"/>
</signal>
<signal name="DOUT4">
<contactref element="R4" pad="P$2"/>
<contactref element="L7_D7" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="L10_D8" pad="4"/>
<contactref element="L11_D8" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="L11_D8" pad="4"/>
<contactref element="L12_D8" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="L1_D5" pad="4"/>
<contactref element="L2_D5" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="L4_D6" pad="4"/>
<contactref element="L5_D6" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="L5_D6" pad="4"/>
<contactref element="L6_D6" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="L7_D7" pad="4"/>
<contactref element="L8_D7" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="L8_D7" pad="4"/>
<contactref element="L9_D7" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="L2_D5" pad="4"/>
<contactref element="L3_D5" pad="3"/>
</signal>
<signal name="N$8">
</signal>
<signal name="NOTGND">
</signal>
<signal name="3.3V">
<contactref element="SENSOR" pad="3"/>
<contactref element="D1MINI" pad="3V3"/>
</signal>
<signal name="SENSOR">
<contactref element="SENSOR" pad="2"/>
<contactref element="D1MINI" pad="A0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
