(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "SuperMEM Moel 1k")
		(date "2025-10-17")
		(rev "1.0")
		(company "kiwisincebirth")
		(comment 1 "Model 1k V2")
		(comment 2 "This is specifically for V2 of the Model 1k")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/A12")
	(net 2 "/A11")
	(net 3 "+5V")
	(net 4 "/A15")
	(net 5 "/A2")
	(net 6 "/D0")
	(net 7 "/D1")
	(net 8 "/D7")
	(net 9 "/D3")
	(net 10 "/A14")
	(net 11 "unconnected-(J1-NC-Pad1)")
	(net 12 "/D4")
	(net 13 "/A6")
	(net 14 "unconnected-(J1-A16-Pad2)")
	(net 15 "/D2")
	(net 16 "/D6")
	(net 17 "unconnected-(J1-CS2{slash}CE2-Pad30)")
	(net 18 "/A1")
	(net 19 "/A5")
	(net 20 "/A13")
	(net 21 "/D5")
	(net 22 "/A9")
	(net 23 "/A3")
	(net 24 "/A4")
	(net 25 "/A7")
	(net 26 "/A0")
	(net 27 "/A10")
	(net 28 "GND")
	(net 29 "/A8")
	(net 30 "/~{WR}")
	(net 31 "/~{CE}")
	(net 32 "/~{RD}")
	(net 33 "/RA16")
	(net 34 "/RA18")
	(net 35 "/RA17")
	(net 36 "/RA15")
	(net 37 "unconnected-(U3-Q5-Pad15)")
	(net 38 "unconnected-(U3-Q3-Pad10)")
	(net 39 "unconnected-(U2-CLK{slash}OD-Pad13)")
	(net 40 "~{RESET}")
	(net 41 "~{IN}")
	(net 42 "~{OUT}")
	(net 43 "~{LOAD}")
	(net 44 "/PA2")
	(net 45 "/PA3")
	(net 46 "/PA1")
	(net 47 "~{VIEW}")
	(net 48 "/PA0")
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 86.2 60.4 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C1"
			(at -1.35 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 1.25 2.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-32_W15.24mm"
		(layer "F.Cu")
		(at 101.65 42.6)
		(descr "32-lead though-hole mounted DIP package, row spacing 15.24mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "J1"
			(at 7.7 -2.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "SOCKET"
			(at 1.68 40.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C1008_Mar_2023V1.2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1-Mbit (128K X 8-bit) Low Power CMOS SRAM, single 2.7V ~ 5.5V power supply, 55ns, DIP-32"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(fp_text user "${REFERENCE}"
			(at 7.62 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 11 "unconnected-(J1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-A16-Pad2)")
			(pinfunction "A16")
			(pintype "input+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 15.24 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "18" thru_hole circle
			(at 15.24 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/D4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "19" thru_hole circle
			(at 15.24 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "20" thru_hole circle
			(at 15.24 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/D6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/~{CE}")
			(pinfunction "~{CS1}/~{CE1}")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "24" thru_hole circle
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "25" thru_hole circle
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "26" thru_hole circle
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "27" thru_hole circle
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "28" thru_hole circle
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/~{WR}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "30" thru_hole circle
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-CS2{slash}CE2-Pad30)")
			(pinfunction "CS2/CE2")
			(pintype "input+no_connect")
		)
		(pad "31" thru_hole circle
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/A15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-32_W15.24mm.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-32_W15.24mm_Socket.step"
			(hide yes)
			(offset
				(xyz 0 0 -4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 -1.5)
			)
			(scale
				(xyz 1 1 0.6)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.step"
			(offset
				(xyz 15.25 0 -1.5)
			)
			(scale
				(xyz 1 1 0.6)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 95.95 41.4)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 7.46 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "~{IN}")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "~{OUT}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "~{RESET}")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-24_W7.62mm_Socket"
		(layer "F.Cu")
		(at 93.08 33.95 90)
		(descr "24-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U2"
			(at 2.8 -2.83 180)
			(layer "F.SilkS")
		)
		(property "Value" "PAL24"
			(at 3.81 30.27 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "generic 24-pin Programmable Array Logic (PAL) device"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 13.97 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 26 "/A0")
			(pinfunction "OD/CLK")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A1")
			(pinfunction "I0")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/A2")
			(pinfunction "I1")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A3")
			(pinfunction "I2")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/A7")
			(pinfunction "I3")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/A6")
			(pinfunction "I4")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/A5")
			(pinfunction "I5")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/A4")
			(pinfunction "I6")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/A15")
			(pinfunction "I7")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "~{OUT}")
			(pinfunction "I8")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "~{IN}")
			(pinfunction "I9")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 7.62 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(U2-CLK{slash}OD-Pad13)")
			(pinfunction "CLK/OD")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole circle
			(at 7.62 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/PA0")
			(pinfunction "LR/O4")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PA2")
			(pinfunction "A0/O3")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PA3")
			(pinfunction "A1/O2")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/PA1")
			(pinfunction "A2/O1")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/RA15")
			(pinfunction "NC/O0")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/RA17")
			(pinfunction "O4/NC")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/RA18")
			(pinfunction "O3/A2")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/RA16")
			(pinfunction "O2/A1")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "~{VIEW}")
			(pinfunction "O1/A0")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "~{LOAD}")
			(pinfunction "O0/LR")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W7.62mm_Socket.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 88.88 57.98)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.82 -2.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HCT244"
			(at 3.81 25.19 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74ls244.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal Buffer and Line Driver With 3-State Output, active-low enables, non-inverting outputs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 47 "~{VIEW}")
			(pinfunction "OEa")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "I0a")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/D6")
			(pinfunction "O3b")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/PA0")
			(pinfunction "I1a")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D1")
			(pinfunction "O2b")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "I2a")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D2")
			(pinfunction "O1b")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PA3")
			(pinfunction "I3a")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/D4")
			(pinfunction "O0b")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 7.62 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "I0b")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at 7.62 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D3")
			(pinfunction "O3a")
			(pintype "tri_state")
		)
		(pad "13" thru_hole circle
			(at 7.62 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PA2")
			(pinfunction "I1b")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D5")
			(pinfunction "O2a")
			(pintype "tri_state")
		)
		(pad "15" thru_hole circle
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/PA1")
			(pinfunction "I2b")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D0")
			(pinfunction "O1a")
			(pintype "tri_state")
		)
		(pad "17" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "I3b")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D7")
			(pinfunction "O0a")
			(pintype "tri_state")
		)
		(pad "19" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "~{VIEW}")
			(pinfunction "OEb")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm"
		(layer "F.Cu")
		(at 75.88 63.02)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS174"
			(at 3.81 20.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS174"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Hex D-type Flip-Flop, reset"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 40 "~{RESET}")
			(pinfunction "~{Mr}")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/PA0")
			(pinfunction "Q0")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D0")
			(pinfunction "D0")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D1")
			(pinfunction "D1")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/PA1")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D3")
			(pinfunction "D2")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PA3")
			(pinfunction "Q2")
			(pintype "output")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 7.62 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "~{LOAD}")
			(pinfunction "Cp")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U3-Q3-Pad10)")
			(pinfunction "Q3")
			(pintype "output+no_connect")
		)
		(pad "11" thru_hole circle
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "D3")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PA2")
			(pinfunction "Q4")
			(pintype "output")
		)
		(pad "13" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D2")
			(pinfunction "D4")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "D5")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U3-Q5-Pad15)")
			(pinfunction "Q5")
			(pintype "output+no_connect")
		)
		(pad "16" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 89.9 26.35 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C3"
			(at -1.9 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 1.25 2.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 96.5 54.75 90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C2"
			(at 4.3 -0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 1.25 2.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 122.2 39.9 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C4"
			(at -2.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 1.25 2.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-32_W15.24mm"
		(layer "F.Cu")
		(at 104.35 40.05)
		(descr "32-lead though-hole mounted DIP package, row spacing 15.24mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U1"
			(at 7.62 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "AS6C4008-55PCN"
			(at 16.24 -2.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/AS6C4008.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "512K x 8 Low Power CMOS RAM, DIP-32"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "XMEM-M1K.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 34 "/RA18")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/RA16")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 15.24 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "18" thru_hole circle
			(at 15.24 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/D4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "19" thru_hole circle
			(at 15.24 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "20" thru_hole circle
			(at 15.24 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/D6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/~{CE}")
			(pinfunction "CE#")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "24" thru_hole circle
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/~{RD}")
			(pinfunction "OE#")
			(pintype "input")
		)
		(pad "25" thru_hole circle
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "26" thru_hole circle
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "27" thru_hole circle
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "28" thru_hole circle
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/~{WR}")
			(pinfunction "WE#")
			(pintype "input")
		)
		(pad "30" thru_hole circle
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/RA17")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "31" thru_hole circle
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/RA15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-32_W15.24mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 73.4875 83.2)
		(end 73.5125 45.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.55 83.2)
		(end 73.4875 83.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.55 22.65)
		(end 124.55 83.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.4 45.5)
		(end 87.4 22.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.4 22.65)
		(end 124.55 22.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.5125 45.5)
		(end 87.4 45.5)
		(layer "Edge.Cuts")
	)
	(image
		(at 101.888177 56.35)
		(layer "User.1")
		(scale 0.224089)
	)
	(image
		(at 93.206278 56.35)
		(layer "User.2")
		(scale 0.252219)
	)
	(gr_text "reset"
		(at 90 47.9 0)
		(layer "F.SilkS")
	)
	(gr_text "74HCT174"
		(at 79.15 63.8 270)
		(layer "F.SilkS")
	)
	(gr_text "in"
		(at 92.3 42.9 0)
		(layer "F.SilkS")
	)
	(gr_text "AS6C4008-55PCN"
		(at 111.3 41.05 270)
		(layer "F.SilkS")
	)
	(gr_text "SuperMem\n 512 KB"
		(at 81.85 53.15 0)
		(layer "F.SilkS")
	)
	(gr_text "74HCT244"
		(at 92.1 59.15 270)
		(layer "F.SilkS")
	)
	(gr_text "GAL22V10"
		(at 94.3 30.7 0)
		(layer "F.SilkS")
	)
	(gr_text "out"
		(at 91.4 45.4 0)
		(layer "F.SilkS")
	)
	(gr_text "512k Banked Ram\nTRS-80 Model-1K\n@kiwisincebirth\nV2 - 1/Oct/2025"
		(at 113.3 59.8 90)
		(layer "B.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.35 78.2) (xy 104.35 76.6) (xy 102.55 76.6) (xy 102.55 78.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 88.9 62.1) (xy 88.9 60.5) (xy 87.1 60.5) (xy 87.1 62.1)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 97.5 66.45) (xy 97.5 64.6) (xy 95.5 64.6) (xy 95.5 66.45)
			)
		)
	)
	(zone
		(net 28)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.35 23) (xy 124.35 82.85) (xy 73.85 82.85) (xy 73.85 45.85) (xy 87.8 45.85) (xy 87.8 23)
			)
		)
	)
	(embedded_fonts no)
)
