<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="10.668" x2="-0.254" y2="1.524" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="15.24" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="12.192" x2="15.24" y2="12.192" width="0" layer="20"/>
<text>5V</text>
<text>GND</text>
<text>SET</text>
<text>RX</text>
<text>TX</text>
<text>RST</text>
<wire x1="16.764" y1="10.668" x2="16.764" y2="1.524" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="-0.254" y2="1.524" width="0" layer="20" curve="-90"/>
<wire x1="16.764" y1="1.524" x2="15.24" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="15.24" y1="12.192" x2="16.764" y2="10.668" width="0" layer="20" curve="-90"/>
<wire x1="-0.254" y1="10.668" x2="1.27" y2="12.192" width="0" layer="20" curve="-90"/>
<text>PMSX003 Breakout</text>
<text>Designed by</text>
<text>Akram Ali</text>
<text>v0.1</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="molex">
<packages>
<package name="0532610871">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="adafruit" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="molex" package="0532610871" value="0532610871"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="SET">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="P$7"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="P$4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
