(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 58)
    (no_connects 0)
    (area 141.411405 102.32 158.907572 119.131171)
    (thickness 1.6)
    (drawings 20)
    (tracks 318)
    (zones 0)
    (modules 35)
    (nets 22)
  )
  (page A4)
  (title_block
    (title ampTPA2012D2)
    (date 2017-01-01)
    (rev 0.03)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 IN_L+)
  (net 4 "Net-(C5-Pad2)")
  (net 5 IN_L-)
  (net 6 "Net-(C6-Pad2)")
  (net 7 IN_R-)
  (net 8 "Net-(C7-Pad2)")
  (net 9 IN_R+)
  (net 10 "Net-(C8-Pad2)")
  (net 11 OUT_L-)
  (net 12 OUT_L+)
  (net 13 OUT_R-)
  (net 14 OUT_R+)
  (net 15 G0)
  (net 16 G1)
  (net 17 OUT_T_L-)
  (net 18 OUT_T_L+)
  (net 19 OUT_T_R-)
  (net 20 OUT_T_R+)
  (net 21 ON)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net G0)
    (add_net G1)
    (add_net IN_L+)
    (add_net IN_L-)
    (add_net IN_R+)
    (add_net IN_R-)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net ON)
    (add_net OUT_L+)
    (add_net OUT_L-)
    (add_net OUT_R+)
    (add_net OUT_R-)
    (add_net OUT_T_L+)
    (add_net OUT_T_L-)
    (add_net OUT_T_R+)
    (add_net OUT_T_R-)
  )
  (net_class PWR ""
    (clearance 0.15)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VDD)
  )
  (module qfn-20_mod0 (layer F.Cu) (tedit 58689A04)
    (at 151.4856 110.4138)
    (descr "Plastic QFP, Microchip QFN-20")
    (fp_text reference U1 (at 1.6764 1.6764) (layer F.SilkS) hide)
    (fp_text value TPA2012D2 (at 0 3.0988) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.00076 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 16 G1) (solder_mask_margin 0.07112))
    (pad 2 smd rect (at -0.50038 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 18 OUT_T_L+) (solder_mask_margin 0.07112))
    (pad 3 smd rect (at 0 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.07112))
    (pad 4 smd rect (at 0.50038 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112))
    (pad 6 smd rect (at 1.96596 1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07112))
    (pad 7 smd rect (at 1.96596 0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 21 ON) (solder_mask_margin 0.07112))
    (pad 8 smd rect (at 1.96596 0) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 21 ON) (solder_mask_margin 0.07112))
    (pad 9 smd rect (at 1.96596 -0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.07112))
    (pad 10 smd rect (at 1.96596 -1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07112))
    (pad 21 thru_hole rect (at 0.62484 0.62484) (size 1.24968 1.24968) (drill 0.5) (layers *.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at -0.62484 0.62484) (size 1.24968 1.24968) (drill 0.5) (layers *.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at -0.62484 -0.62484) (size 1.24968 1.24968) (drill 0.5) (layers *.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at 0.62484 -0.62484) (size 1.24968 1.24968) (drill 0.5) (layers *.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 11 smd rect (at 1.00076 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 19 OUT_T_R-) (solder_mask_margin 0.07112))
    (pad 12 smd rect (at 0.50038 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112))
    (pad 13 smd rect (at 0 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.07112))
    (pad 14 smd rect (at -0.50038 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 20 OUT_T_R+) (solder_mask_margin 0.07112))
    (pad 15 smd rect (at -1.00076 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 15 G0) (solder_mask_margin 0.07112))
    (pad 16 smd rect (at -1.96596 -1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad2)") (solder_mask_margin 0.07112))
    (pad 17 smd rect (at -1.96596 -0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)") (solder_mask_margin 0.07112))
    (pad 18 smd rect (at -1.96596 0) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07112))
    (pad 19 smd rect (at -1.96596 0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)") (solder_mask_margin 0.07112))
    (pad 20 smd rect (at -1.96596 1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad2)") (solder_mask_margin 0.07112))
    (pad 5 smd rect (at 1.00076 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT_T_L-) (solder_mask_margin 0.07112))
    (model walter/smd_qfn/qfn-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 5868994E)
    (at 150.7109 105.029 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C16 (at -0.6731 2.159 180) (layer F.SilkS) hide)
    (fp_text value 1n (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT_R+))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58689914)
    (at 155.956 112.268 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 1.4732 0.0508 360) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 21 ON))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897F4)
    (at 155.829 107.442)
    (fp_text reference P1 (at 2.1082 -0.2032 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897F6)
    (at 155.829 106.045)
    (fp_text reference P2 (at 2.2225 0.0635 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897D5)
    (at 145.542 111.125)
    (fp_text reference P3 (at -3.4925 0.3175) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 5 IN_L-))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897D7)
    (at 145.542 112.395)
    (fp_text reference P4 (at -3.429 0.4445) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 3 IN_L+))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897D3)
    (at 145.542 109.855)
    (fp_text reference P5 (at -3.2385 0.0635) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 7 IN_R-))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897D0)
    (at 145.542 108.585)
    (fp_text reference P6 (at -3.3655 0.0635) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 9 IN_R+))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897E3)
    (at 154.813 111.252)
    (fp_text reference P7 (at 2.9083 0.0762 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 21 ON))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897DD)
    (at 155.0162 116.0526 270)
    (fp_text reference P8 (at 1.8034 -0.381 360) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 11 OUT_L-))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897DB)
    (at 149.2504 116.0526 270)
    (fp_text reference P9 (at 1.9812 0.2032 360) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 12 OUT_L+))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 586897FA)
    (at 154.82062 105.03154)
    (fp_text reference P10 (at 3.16738 -1.71704 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 13 OUT_R-))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58689801)
    (at 149.0218 105.029)
    (fp_text reference P11 (at -0.5218 -2.029) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 14 OUT_R+))
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 586898D8)
    (at 148.8694 114.2492 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at -0.0508 0.2286 180) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 G1))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 5868990E)
    (at 152.2476 114.5794 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C9 (at 0.1016 0.0254 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 5868990B)
    (at 152.019 113.538 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C10 (at 0.0254 -0.0254 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 586897EB)
    (at 155.2956 108.966 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C11 (at -2.57048 -0.1524 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689957)
    (at 155.0416 110.0328 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C12 (at 0.1143 2.5908 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 586898FC)
    (at 153.416 115.824)
    (descr "SMT capacitor, 0402")
    (fp_text reference C13 (at 0 0.9144) (layer F.SilkS) hide)
    (fp_text value 1n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT_L-))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689909)
    (at 151.003 115.824 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C14 (at 0.1143 2.5908 180) (layer F.SilkS) hide)
    (fp_text value 1n (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT_L+))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689917)
    (at 154.178 114.173 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference L3 (at 0.1143 2.5908 90) (layer F.SilkS) hide)
    (fp_text value INDUCTOR (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT_T_L-))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT_L-))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689910)
    (at 150.3045 114.1095 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference L4 (at 0.1143 2.5908 90) (layer F.SilkS) hide)
    (fp_text value INDUCTOR (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 OUT_T_L+))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT_L+))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 5868998C)
    (at 154.051 106.807 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference L5 (at 0.1143 2.5908 270) (layer F.SilkS) hide)
    (fp_text value INDUCTOR (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 OUT_T_R-))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 13 OUT_R-))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 586898C3)
    (at 147.447 109.855 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C7 (at -1.651 -0.127 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 7 IN_R-))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 586898CA)
    (at 147.447 111.252 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at -1.651 0 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 IN_L-))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 586898D1)
    (at 147.447 112.522 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C5 (at -1.905 0 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 IN_L+))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58689977)
    (at 147.574 107.2515)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 1.4732 0.0508 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 G0))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689953)
    (at 152.019 105.918 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at 0.0254 0.0254 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 586898B4)
    (at 147.447 108.585 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C8 (at -1.8034 0 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 IN_R+))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C8-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689974)
    (at 150.1648 106.6673 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference L6 (at 0.1143 2.5908 270) (layer F.SilkS) hide)
    (fp_text value INDUCTOR (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 OUT_T_R+))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT_R+))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58689971)
    (at 147.574 106.172 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at 1.4732 0.0508 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 G0))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 5868995A)
    (at 152.146 107.061 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C3 (at -1.8034 0 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58689955)
    (at 153.162 105.029)
    (descr "SMT capacitor, 0402")
    (fp_text reference C15 (at 0.1143 2.5908) (layer F.SilkS) hide)
    (fp_text value 1n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 13 OUT_R-))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5868998F)
    (at 147.8788 114.2492 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 1.4732 0.0508 360) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 G1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 144.018 117.348) (end 157.226 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.018 103.632) (end 157.226 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.018 103.632) (end 144.018 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.226 117.348) (end 157.226 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 156.8704 105.918 90) (layer F.SilkS))
  (gr_text VDD (at 156.8704 107.442 90) (layer F.SilkS))
  (gr_text ON (at 154.8384 112.4204 90) (layer F.SilkS))
  (gr_text R (at 144.5768 109.474) (layer F.SilkS))
  (gr_text L (at 144.5768 111.5568) (layer F.SilkS))
  (gr_text L (at 151.8412 116.8908) (layer F.SilkS))
  (gr_text R (at 151.892 104.14) (layer F.SilkS))
  (gr_text - (at 154.8384 103.9876) (layer F.SilkS))
  (gr_text - (at 155.0924 116.9416) (layer F.SilkS))
  (gr_text + (at 148.9964 103.9876) (layer F.SilkS))
  (gr_text + (at 149.2504 116.9416) (layer F.SilkS))
  (gr_text + (at 144.5768 112.522) (layer F.SilkS))
  (gr_text "-\n" (at 144.5768 110.6424) (layer F.SilkS))
  (gr_text "-\n" (at 144.5768 110.3376) (layer F.SilkS))
  (gr_text + (at 144.5768 108.458) (layer F.SilkS))
  (gr_text "ampTDA2012D2\nrev0.03\nrel/2017-01" (at 148.0312 106.6292 90) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.226 117.348) (xy 144.018 117.348) (xy 144.018 103.632) (xy 157.226 103.632)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.226 117.348) (xy 144.018 117.348) (xy 144.018 103.632) (xy 157.226 103.632)
      )
    )
  )
)
