(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 391)
    (zones 0)
    (modules 33)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J3-Pad1)")
  (net 5 "Net-(J4-Pad1)")
  (net 6 "Net-(J5-Pad1)")
  (net 7 "Net-(J6-Pad1)")
  (net 8 "Net-(J7-Pad40)")
  (net 9 "Net-(J7-Pad38)")
  (net 10 "Net-(J7-Pad37)")
  (net 11 "Net-(J7-Pad36)")
  (net 12 "Net-(J7-Pad35)")
  (net 13 "Net-(J7-Pad34)")
  (net 14 "Net-(J7-Pad33)")
  (net 15 "Net-(J7-Pad32)")
  (net 16 "Net-(J7-Pad31)")
  (net 17 "Net-(J7-Pad30)")
  (net 18 "Net-(J7-Pad29)")
  (net 19 "Net-(J7-Pad28)")
  (net 20 "Net-(J7-Pad27)")
  (net 21 "Net-(J7-Pad26)")
  (net 22 "Net-(J7-Pad25)")
  (net 23 "Net-(J7-Pad24)")
  (net 24 "Net-(J7-Pad23)")
  (net 25 "Net-(J7-Pad22)")
  (net 26 "Net-(J7-Pad21)")
  (net 27 "Net-(J7-Pad20)")
  (net 28 "Net-(J7-Pad19)")
  (net 29 "Net-(J7-Pad18)")
  (net 30 "Net-(J7-Pad17)")
  (net 31 "Net-(J7-Pad16)")
  (net 32 "Net-(J7-Pad15)")
  (net 33 "Net-(J7-Pad14)")
  (net 34 "Net-(J7-Pad13)")
  (net 35 "Net-(J7-Pad12)")
  (net 36 "Net-(J7-Pad11)")
  (net 37 "Net-(J7-Pad10)")
  (net 38 "Net-(J7-Pad9)")
  (net 39 "Net-(J7-Pad8)")
  (net 40 "Net-(J7-Pad7)")
  (net 41 "Net-(J7-Pad6)")
  (net 42 "Net-(J7-Pad5)")
  (net 43 "Net-(J7-Pad4)")
  (net 44 "Net-(J7-Pad3)")
  (net 45 "Net-(J7-Pad2)")
  (net 46 "Net-(J7-Pad1)")
  (net 47 "Net-(J8-Pad1)")
  (net 48 "Net-(J9-Pad1)")
  (net 49 "Net-(J10-Pad1)")
  (net 50 "Net-(J11-Pad1)")
  (net 51 "Net-(J12-Pad1)")
  (net 52 "Net-(K1-Pad4)")
  (net 53 "Net-(K2-Pad4)")
  (net 54 "Net-(K3-Pad4)")
  (net 55 "Net-(K4-Pad4)")
  (net 56 "Net-(K5-Pad4)")
  (net 57 "Net-(K6-Pad4)")
  (net 58 "Net-(K7-Pad4)")
  (net 59 "Net-(K8-Pad4)")
  (net 60 "Net-(K9-Pad4)")
  (net 61 "Net-(K10-Pad4)")
  (net 62 "Net-(J7-Pad39)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad10)")
    (add_net "Net-(J7-Pad11)")
    (add_net "Net-(J7-Pad12)")
    (add_net "Net-(J7-Pad13)")
    (add_net "Net-(J7-Pad14)")
    (add_net "Net-(J7-Pad15)")
    (add_net "Net-(J7-Pad16)")
    (add_net "Net-(J7-Pad17)")
    (add_net "Net-(J7-Pad18)")
    (add_net "Net-(J7-Pad19)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad20)")
    (add_net "Net-(J7-Pad21)")
    (add_net "Net-(J7-Pad22)")
    (add_net "Net-(J7-Pad23)")
    (add_net "Net-(J7-Pad24)")
    (add_net "Net-(J7-Pad25)")
    (add_net "Net-(J7-Pad26)")
    (add_net "Net-(J7-Pad27)")
    (add_net "Net-(J7-Pad28)")
    (add_net "Net-(J7-Pad29)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad30)")
    (add_net "Net-(J7-Pad31)")
    (add_net "Net-(J7-Pad32)")
    (add_net "Net-(J7-Pad33)")
    (add_net "Net-(J7-Pad34)")
    (add_net "Net-(J7-Pad35)")
    (add_net "Net-(J7-Pad36)")
    (add_net "Net-(J7-Pad37)")
    (add_net "Net-(J7-Pad38)")
    (add_net "Net-(J7-Pad39)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad40)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad8)")
    (add_net "Net-(J7-Pad9)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K10-Pad4)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(K3-Pad4)")
    (add_net "Net-(K4-Pad4)")
    (add_net "Net-(K5-Pad4)")
    (add_net "Net-(K6-Pad4)")
    (add_net "Net-(K7-Pad4)")
    (add_net "Net-(K8-Pad4)")
    (add_net "Net-(K9-Pad4)")
  )
  (net_class "AC power" ""
    (clearance 1)
    (trace_width 1)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J6-Pad1)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 59.69 128.27)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J7 (at -1.27 2.77) (layer B.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at -1.27 -51.03) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 -90) (layer B.Fab))
    (pad 40 thru_hole oval (at -2.54 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J7-Pad40)"))
    (pad 39 thru_hole oval (at 0 -48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 38 thru_hole oval (at -2.54 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J7-Pad38)"))
    (pad 37 thru_hole oval (at 0 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J7-Pad37)"))
    (pad 36 thru_hole oval (at -2.54 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad36)"))
    (pad 35 thru_hole oval (at 0 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad35)"))
    (pad 34 thru_hole oval (at -2.54 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J7-Pad34)"))
    (pad 33 thru_hole oval (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J7-Pad33)"))
    (pad 32 thru_hole oval (at -2.54 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J7-Pad32)"))
    (pad 31 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J7-Pad31)"))
    (pad 30 thru_hole oval (at -2.54 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J7-Pad30)"))
    (pad 29 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J7-Pad29)"))
    (pad 28 thru_hole oval (at -2.54 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J7-Pad28)"))
    (pad 27 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J7-Pad27)"))
    (pad 26 thru_hole oval (at -2.54 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J7-Pad26)"))
    (pad 25 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J7-Pad25)"))
    (pad 24 thru_hole oval (at -2.54 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J7-Pad24)"))
    (pad 23 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J7-Pad23)"))
    (pad 22 thru_hole oval (at -2.54 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J7-Pad22)"))
    (pad 21 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad21)"))
    (pad 20 thru_hole oval (at -2.54 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad20)"))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J7-Pad19)"))
    (pad 18 thru_hole oval (at -2.54 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J7-Pad18)"))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J7-Pad17)"))
    (pad 16 thru_hole oval (at -2.54 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J7-Pad16)"))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J7-Pad15)"))
    (pad 14 thru_hole oval (at -2.54 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J7-Pad14)"))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J7-Pad13)"))
    (pad 12 thru_hole oval (at -2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J7-Pad12)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J7-Pad11)"))
    (pad 10 thru_hole oval (at -2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J7-Pad10)"))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J7-Pad9)"))
    (pad 8 thru_hole oval (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J7-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J7-Pad7)"))
    (pad 6 thru_hole oval (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J7-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad5)"))
    (pad 4 thru_hole oval (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J7-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J7-Pad3)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 57.15 138.43)
    (fp_text reference K4 (at -2.575001 -2.115001) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(J4-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 55 "Net-(K4-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 72.39 81.28)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q6 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 57 "Net-(K6-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 44 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "relays:woodeye logo" (layer F.Cu) (tedit 0)
    (at 106.045 133.35 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 57.15 149.86)
    (fp_text reference K3 (at -2.575001 -2.115001) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J3-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 54 "Net-(K3-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 96.52 146.05 180)
    (fp_text reference K8 (at -2.575001 -2.115001) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 49 "Net-(J10-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 59 "Net-(K8-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 98.425 79.375 270)
    (fp_text reference K9 (at -2.575001 -2.115001 90) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 50 "Net-(J11-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 60 "Net-(K9-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 69.85 165.1)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J3 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 98.425 165.1)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J10 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 49 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 71.755 107.315)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q10 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 61 "Net-(K10-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 "Net-(J7-Pad31)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 64.77 106.045)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q9 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 60 "Net-(K9-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "Net-(J7-Pad29)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 72.39 93.98)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q8 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 59 "Net-(K8-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 40 "Net-(J7-Pad7)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 72.39 87.63)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q7 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 58 "Net-(K7-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad5)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 65.405 85.09)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q5 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 56 "Net-(K5-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 39 "Net-(J7-Pad8)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 65.405 92.71)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 55 "Net-(K4-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 37 "Net-(J7-Pad10)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 66.04 117.475)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 54 "Net-(K3-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad36)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 72.39 100.33)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 53 "Net-(K2-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 36 "Net-(J7-Pad11)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 65.405 99.695)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 62 "Net-(J7-Pad39)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 52 "Net-(K1-Pad4)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 35 "Net-(J7-Pad12)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 96.52 157.48 180)
    (fp_text reference K10 (at -2.575001 -2.115001) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 51 "Net-(J12-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 61 "Net-(K10-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 86.36 79.375 270)
    (fp_text reference K7 (at -2.575001 -2.115001 90) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 48 "Net-(J9-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 58 "Net-(K7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 83.82 113.03 270)
    (fp_text reference K6 (at -2.575001 -2.115001 90) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 47 "Net-(J8-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 57 "Net-(K6-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 78.74 101.6)
    (fp_text reference K5 (at -2.575001 -2.115001) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(J5-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 56 "Net-(K5-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 72.39 113.03 270)
    (fp_text reference K2 (at -2.575001 -2.115001 90) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(J2-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 53 "Net-(K2-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_Panasonic_ALQ305:Panasonic-ALQ305-Manufacturer_Recommended (layer F.Cu) (tedit 60F1F793)
    (at 95.885 113.03 270)
    (fp_text reference K1 (at -2.575001 -2.115001 90) (layer F.SilkS))
    (fp_text value ALQ305 (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 43 "Net-(J7-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 2 thru_hole circle (at 17.78 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J6-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 3 thru_hole circle (at 10.16 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(J1-Pad1)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.899999 1.899999) (drill 1.4) (layers *.Cu *.Paste *.Mask)
      (net 52 "Net-(K1-Pad4)") (solder_mask_margin 0.0254) (solder_paste_margin 0.0254) (clearance 0.0254))
    (model eec.models/Panasonic_-_ALQ305.step
      (offset (xyz -96.77399854660034 0 5.079999923706055))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 84.455 165.1)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J12 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 51 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 86.36 72.39 180)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J11 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 50 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 72.39 72.39 180)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J9 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 48 "Net-(J9-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 105.41 88.9 90)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J8 (at 3.175 -5.56 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06 90) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 47 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 59.69 163.83 270)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J6 (at 3.175 -5.56 90) (layer F.SilkS))
    (fp_text value "24VAC in" (at 3.175 9.06 90) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 100.33 72.39 180)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J5 (at 3.175 -5.56) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 105.41 156.21 90)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J4 (at 3.175 -5.56 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06 90) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 105.41 102.87 90)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J2 (at 3.175 -5.56 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06 90) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal (layer F.Cu) (tedit 5B294EA2)
    (at 105.41 116.84 90)
    (descr "terminal block Metz Connect Type701_RT11L02HGLU, 2 pins, pitch 6.35mm, size 12.7x12.5mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_317011_RT11LxxHGLU_OFF-022798U.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type701_RT11L02HGLU pitch 6.35mm size 12.7x12.5mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J1 (at 3.175 -5.56 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.175 9.06 90) (layer F.Fab))
    (fp_text user %R (at 3.175 5.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 6.35 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type701_RT11L02HGLU_1x02_P6.35mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 107.315 133.35) (end 108.585 133.35) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 107.315 74.93) (end 108.585 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 58.42 74.93) (end 59.69 74.93) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 58.42 133.35) (end 59.69 133.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 63.5) (end 114.3 173.99) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 63.5) (end 114.3 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 173.99) (end 50.8 63.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 173.99) (end 50.8 173.99) (layer Edge.Cuts) (width 0.1))
)
