<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="40.64" y1="57.15" x2="73.66" y2="57.15" width="0.1524" layer="20"/>
<wire x1="73.66" y1="57.15" x2="73.66" y2="29.21" width="0.1524" layer="20"/>
<wire x1="40.64" y1="29.21" x2="40.64" y2="57.15" width="0.1524" layer="20"/>
<wire x1="40.64" y1="29.21" x2="44.45" y2="25.4" width="0.1524" layer="20"/>
<wire x1="44.45" y1="25.4" x2="69.85" y2="25.4" width="0.1524" layer="20"/>
<wire x1="69.85" y1="25.4" x2="73.66" y2="29.21" width="0.1524" layer="20"/>
<text>SONIC Prototype</text>
<text>7 Nov 2018</text>
<text>v 1</text>
</plain>
<libraries>
<library name="Keystone">
<packages>
<package name="20MM_SM_COIN_CELL_CLIP">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0603_B">
</package>
</packages>
</library>
<library name="C&amp;K">
<packages>
<package name="JS202011SCQN">
</package>
</packages>
</library>
<library name="microchip">
<packages>
<package name="SOIC-14-N">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0603">
<description>From Stackpole datasheet: https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf</description>
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN02">
</package>
</packages>
</library>
<library name="TAG-CONNECT">
<packages>
<package name="PLUG-OF-NAILS">
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF-TIGHT">
<description>&lt;h3&gt;Standoff (#4 Screw) - Tight fit around screw body&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="VISHAY">
<packages>
<package name="TEMT6000X01">
<description>Ambient Light Sensor&lt;br&gt;
http://www.vishay.com/docs/81579/temt6000.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B1" library="Keystone" package="20MM_SM_COIN_CELL_CLIP" value="BATTERY20MM"/>
<element name="C1" library="KEMET" package="0603_B" value="0.1u"/>
<element name="S1" library="C&amp;K" package="JS202011SCQN" value="SLIDE_DPDT"/>
<element name="U$1" library="microchip" package="SOIC-14-N" value="PICF1615"/>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="Stackpole" package="0603" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="OST" package="OSTVN02" value="M02"/>
<element name="U$3" library="TAG-CONNECT" package="PLUG-OF-NAILS" value="PIC_ICPH"/>
<element name="U$5" library="SparkFun-Hardware" package="STAND-OFF-TIGHT" value="">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="SparkFun-Hardware" package="STAND-OFF-TIGHT" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="Stackpole" package="0603" value="10K"/>
<element name="U$8" library="VISHAY" package="TEMT6000X01" value="PHOTOTRANSISTOR"/>
<element name="R3" library="Stackpole" package="0603" value="20K"/>
<element name="C2" library="KEMET" package="0603_B" value="0.1u"/>
</elements>
<signals>
<signal name="GND">
<contactref element="B1" pad="2"/>
<contactref element="U$1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="+">
<contactref element="B1" pad="3" route="any" routetag="G$1.+"/>
<contactref element="B1" pad="1" route="any" routetag="G$1.+"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="LED">
<contactref element="U$1" pad="6"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="CC">
<contactref element="U$1" pad="7"/>
<contactref element="U$8" pad="C"/>
</signal>
<signal name="PWM">
<contactref element="U$1" pad="11"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="C1IN1-">
<contactref element="U$1" pad="9"/>
<contactref element="R3" pad="2"/>
<contactref element="U$8" pad="E2"/>
<contactref element="U$8" pad="E1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="ICSPDAT">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="MCLR">
<contactref element="U$1" pad="4"/>
<contactref element="U$3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ICSPCLK">
<contactref element="U$1" pad="12"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="VDD">
<contactref element="S1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
