<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="6.6" y1="0" x2="16.4" y2="0" width="0" layer="20"/>
<wire x1="23" y1="6.6" x2="23" y2="16.4" width="0" layer="20"/>
<wire x1="16.4" y1="23" x2="6.6" y2="23" width="0" layer="20"/>
<wire x1="0" y1="16.4" x2="0" y2="6.6" width="0" layer="20"/>
<wire x1="16.4" y1="23" x2="23" y2="16.4" width="0" layer="20" curve="-43.843557"/>
<wire x1="23" y1="6.6" x2="16.4" y2="0" width="0" layer="20" curve="-43.843557"/>
<wire x1="6.6" y1="0" x2="0" y2="6.6" width="0" layer="20" curve="-43.843557"/>
<wire x1="0" y1="16.4" x2="6.6" y2="23" width="0" layer="20" curve="-43.843557"/>
<text>9-LED</text>
<text>Cree XP</text>
<text>D1</text>
<text>B+</text>
<text>B+</text>
<text>CUT</text>
<text>David Fleener</text>
</plain>
<libraries>
<library name="C_0805">
<packages>
<package name="CAPC2013X94N">
</package>
</packages>
</library>
<library name="SOD-323">
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="Seeed-OPL-Resistor">
<packages>
<package name="R0805">
</package>
</packages>
</library>
<library name="AMC7135_CC_regulator">
<packages>
<package name="AMC7135_CC_REGULATOR">
</package>
</packages>
</library>
<library name="Cree_XP">
<packages>
<package name="XP">
</package>
</packages>
</library>
<library name="ATtiny25.ssh">
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="C_0805" package="CAPC2013X94N" value="10pF">
<attribute name="OC_FARNELL" value="499158"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="OC_NEWARK" value="96K4767"/>
<attribute name="MPN" value="08051A100JAT2A"/>
<attribute name="VOLTAGERATING" value="100V"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="SOD-323" package="SOD-323" value="SOD-323"/>
<element name="OTC" library="C_0805" package="CAPC2013X94N" value="10pF">
<attribute name="OC_FARNELL" value="499158"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="OC_NEWARK" value="96K4767"/>
<attribute name="MPN" value="08051A100JAT2A"/>
<attribute name="VOLTAGERATING" value="100V"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Seeed-OPL-Resistor" package="R0805" value="220k">
<attribute name="NAME"/>
</element>
<element name="R2" library="Seeed-OPL-Resistor" package="R0805" value="47k">
<attribute name="NAME"/>
</element>
<element name="U$1" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U$17" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U$2" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U$20" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U$21" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="XP3" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="U$3" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="XP4" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="U$5" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U$6" library="AMC7135_CC_regulator" package="AMC7135_CC_REGULATOR" value="AMC7135_CC_REGULATOR"/>
<element name="U1" library="ATtiny25.ssh" package="SOIC127P600X175-8N" value="ATTINY25-20SSU">
<attribute name="OC_FARNELL" value="1636951"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_NEWARK" value="68T3605"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="MPN" value="ATTINY25-20SSU"/>
</element>
<element name="XP1" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP2" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP5" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP6" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP7" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP8" library="Cree_XP" package="XP" value="CREE_XP"/>
<element name="XP9" library="Cree_XP" package="XP" value="CREE_XP"/>
</elements>
<signals>
<signal name="V_DIV">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PIN6">
<contactref element="U1" pad="6"/>
<contactref element="U$20" pad="VDD"/>
<contactref element="U$3" pad="VDD"/>
<contactref element="U$21" pad="VDD"/>
<contactref element="U$6" pad="VDD"/>
<contactref element="U$5" pad="VDD"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="U$2" pad="VDD"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="OTC" pad="1"/>
<contactref element="XP2" pad="THERMAL"/>
<contactref element="XP8" pad="THERMAL"/>
<contactref element="XP7" pad="THERMAL"/>
<contactref element="XP6" pad="THERMAL"/>
<contactref element="XP5" pad="THERMAL"/>
<contactref element="XP1" pad="THERMAL"/>
<contactref element="R2" pad="1"/>
<contactref element="XP4" pad="THERMAL"/>
<contactref element="XP3" pad="THERMAL"/>
<contactref element="U$21" pad="GND1"/>
<contactref element="U$21" pad="GND2"/>
<contactref element="U$21" pad="GND3"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND3"/>
<contactref element="U$2" pad="GND1"/>
<contactref element="U$2" pad="GND2"/>
<contactref element="U$2" pad="GND3"/>
<contactref element="U$5" pad="GND1"/>
<contactref element="U$5" pad="GND2"/>
<contactref element="U$5" pad="GND3"/>
<contactref element="U$6" pad="GND1"/>
<contactref element="U$6" pad="GND2"/>
<contactref element="U$6" pad="GND3"/>
<contactref element="U$3" pad="GND1"/>
<contactref element="U$3" pad="GND2"/>
<contactref element="U$3" pad="GND3"/>
<contactref element="U$17" pad="GND1"/>
<contactref element="U$17" pad="GND2"/>
<contactref element="U$17" pad="GND3"/>
<contactref element="U$20" pad="GND1"/>
<contactref element="U$20" pad="GND2"/>
<contactref element="U$20" pad="GND3"/>
<contactref element="XP9" pad="THERMAL"/>
</signal>
<signal name="PIN5">
<contactref element="U1" pad="5"/>
<contactref element="U$17" pad="VDD"/>
</signal>
<signal name="LVP">
<contactref element="U1" pad="2"/>
<contactref element="OTC" pad="2"/>
</signal>
<signal name="LED+">
<contactref element="D1" pad="P$1"/>
<contactref element="XP2" pad="POSITIVE"/>
<contactref element="XP2" pad="POSITIVE1"/>
<contactref element="XP8" pad="POSITIVE"/>
<contactref element="XP8" pad="POSITIVE1"/>
<contactref element="XP7" pad="POSITIVE"/>
<contactref element="XP7" pad="POSITIVE1"/>
<contactref element="XP6" pad="POSITIVE"/>
<contactref element="XP6" pad="POSITIVE1"/>
<contactref element="XP5" pad="POSITIVE"/>
<contactref element="XP5" pad="POSITIVE1"/>
<contactref element="XP1" pad="POSITIVE"/>
<contactref element="XP1" pad="POSITIVE1"/>
<contactref element="R1" pad="2"/>
<contactref element="XP4" pad="POSITIVE"/>
<contactref element="XP4" pad="POSITIVE1"/>
<contactref element="XP3" pad="POSITIVE"/>
<contactref element="XP3" pad="POSITIVE1"/>
<contactref element="XP9" pad="POSITIVE"/>
<contactref element="XP9" pad="POSITIVE1"/>
</signal>
<signal name="VIN+">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="OUT"/>
<contactref element="U$6" pad="OUT"/>
<contactref element="U$5" pad="OUT"/>
<contactref element="U$21" pad="OUT"/>
<contactref element="U$1" pad="OUT"/>
<contactref element="U$2" pad="OUT"/>
<contactref element="XP5" pad="NEGATIVE"/>
<contactref element="XP5" pad="NEGATIVE1"/>
<contactref element="XP6" pad="NEGATIVE"/>
<contactref element="XP6" pad="NEGATIVE1"/>
<contactref element="XP7" pad="NEGATIVE"/>
<contactref element="XP7" pad="NEGATIVE1"/>
<contactref element="XP8" pad="NEGATIVE"/>
<contactref element="XP8" pad="NEGATIVE1"/>
<contactref element="XP2" pad="NEGATIVE"/>
<contactref element="XP2" pad="NEGATIVE1"/>
<contactref element="XP1" pad="NEGATIVE"/>
<contactref element="XP1" pad="NEGATIVE1"/>
<contactref element="U$17" pad="OUT"/>
<contactref element="U$20" pad="OUT"/>
<contactref element="XP4" pad="NEGATIVE"/>
<contactref element="XP4" pad="NEGATIVE1"/>
<contactref element="XP3" pad="NEGATIVE"/>
<contactref element="XP3" pad="NEGATIVE1"/>
<contactref element="XP9" pad="NEGATIVE1"/>
<contactref element="XP9" pad="NEGATIVE"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$37">
</signal>
<signal name="N$38">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$79">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="N$83">
</signal>
<signal name="N$84">
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$91">
</signal>
<signal name="N$92">
</signal>
<signal name="N$93">
</signal>
<signal name="N$94">
</signal>
</signals>
</board>
</drawing>
</eagle>
