(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 192)
    (no_connects 0)
    (area 128.194999 125.654999 188.670001 145.490001)
    (thickness 1.6)
    (drawings 32)
    (tracks 820)
    (zones 0)
    (modules 100)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.153)
    (user_trace_width 0.22)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.153)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (grid_origin 163.068 131.572)
    (visible_elements 7FFEEC7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 I2C_SCL)
  (net 3 I2C_SDA)
  (net 4 GND)
  (net 5 +12V)
  (net 6 +5V)
  (net 7 SD_MISO)
  (net 8 SD_CLK)
  (net 9 SD_MOSI)
  (net 10 SD_CS)
  (net 11 SW1)
  (net 12 SW2)
  (net 13 SW3)
  (net 14 SW4)
  (net 15 I2S_TX)
  (net 16 I2S_LRCLK)
  (net 17 I2S_MCLK)
  (net 18 I2S_BCLK)
  (net 19 AUD_GAIN_SEL)
  (net 20 AUD_RESET)
  (net 21 AUD_PWRDN)
  (net 22 AUD_OVRSMP_SEL)
  (net 23 "Net-(C5-Pad1)")
  (net 24 "Net-(C6-Pad1)")
  (net 25 "Net-(C10-Pad2)")
  (net 26 "Net-(C10-Pad1)")
  (net 27 "Net-(C17-Pad1)")
  (net 28 "Net-(C17-Pad2)")
  (net 29 "Net-(L2-Pad2)")
  (net 30 "Net-(L4-Pad2)")
  (net 31 AUD_INT)
  (net 32 "Net-(D1-Pad2)")
  (net 33 "Net-(C5-Pad2)")
  (net 34 "Net-(C7-Pad1)")
  (net 35 "Net-(C11-Pad2)")
  (net 36 "Net-(C11-Pad1)")
  (net 37 "Net-(C18-Pad2)")
  (net 38 "Net-(C18-Pad1)")
  (net 39 "Net-(J8-Pad1)")
  (net 40 "Net-(J8-Pad2)")
  (net 41 "Net-(J9-Pad1)")
  (net 42 "Net-(J9-Pad2)")
  (net 43 "Net-(R1-Pad1)")
  (net 44 "Net-(R2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net AUD_GAIN_SEL)
    (add_net AUD_INT)
    (add_net AUD_OVRSMP_SEL)
    (add_net AUD_PWRDN)
    (add_net AUD_RESET)
    (add_net GND)
    (add_net I2C_SCL)
    (add_net I2C_SDA)
    (add_net I2S_BCLK)
    (add_net I2S_LRCLK)
    (add_net I2S_MCLK)
    (add_net I2S_TX)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(L4-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net SD_CLK)
    (add_net SD_CS)
    (add_net SD_MISO)
    (add_net SD_MOSI)
    (add_net SW1)
    (add_net SW2)
    (add_net SW3)
    (add_net SW4)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78F1)
    (at 160.401 134.747)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7900)
    (at 153.416 136.398)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7900)
    (at 148.082 136.398)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7847)
    (at 187.452 126.746)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 158.818 128.072 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.103 -0.195 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 SD_CS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 163.068 132.334 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.413 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 59FA997A)
    (at 131.953 143.764 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.7 0 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 14 SW4))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 59FA98A5)
    (at 161.552 141.8915)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference BREATH (at -0.008 -5.2395) (layer F.SilkS))
    (fp_text value I2C_CONN (at 0 4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.5 -1.9375) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0.5 -1.9375) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 I2C_SDA))
    (pad 4 smd rect (at 1.5 -1.9375) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 I2C_SCL))
    (pad "" smd rect (at -2.8 1.9375) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module custom:Teensy3.4_SMD (layer B.Cu) (tedit 59FA798D)
    (at 147.32 136.144)
    (fp_text reference U2 (at 18.8595 -7.112 90) (layer B.SilkS))
    (fp_text value Teensy3.2 (at -0.3 -10.1) (layer B.Fab))
    (pad 17 smd rect (at 16.51 0) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 19 smd rect (at 16.51 5.08) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 16.51 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 16.51 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 SD_MISO))
    (pad 21 smd rect (at 13.97 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 SD_CLK))
    (pad 22 smd rect (at 11.43 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 SW1))
    (pad 23 smd rect (at 8.89 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 SW2))
    (pad 24 smd rect (at 6.35 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 SW3))
    (pad 25 smd rect (at 3.81 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 I2C_SDA))
    (pad 26 smd rect (at 1.27 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 I2C_SCL))
    (pad 27 smd rect (at -1.27 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 14 SW4))
    (pad 28 smd rect (at -3.81 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 31 AUD_INT))
    (pad 29 smd rect (at -6.35 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 15 I2S_TX))
    (pad 30 smd rect (at -8.89 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 16 I2S_LRCLK))
    (pad 31 smd rect (at -11.43 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 32 smd rect (at -13.97 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 33 smd rect (at -16.51 7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +5V))
    (pad 13 smd rect (at 13.97 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 17 I2S_MCLK))
    (pad 12 smd rect (at 11.43 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 10 SD_CS))
    (pad 11 smd rect (at 8.89 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 18 I2S_BCLK))
    (pad 10 smd rect (at 6.35 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 AUD_GAIN_SEL))
    (pad 9 smd rect (at 3.81 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 9 SD_MOSI))
    (pad 8 smd rect (at 1.27 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 20 AUD_RESET))
    (pad 7 smd rect (at -1.27 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 21 AUD_PWRDN))
    (pad 6 smd rect (at -3.81 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -6.35 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -8.89 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 22 AUD_OVRSMP_SEL))
    (pad 3 smd rect (at -11.43 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -13.97 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -16.51 -7.62) (size 1.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
  )
  (module Housings_SSOP:ST_PowerSSO-36_SlugDown_ThermalVias (layer B.Cu) (tedit 59AEF9D5)
    (at 175.006 131.572 180)
    (descr "ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)")
    (tags "ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm")
    (attr smd)
    (fp_text reference U3 (at -6.858 -0.8255 270) (layer B.SilkS))
    (fp_text value STA333ML (at 0 -6.1 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -4.9325 4.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -4.9325 3.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -4.9325 3.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -4.9325 2.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (pad 5 smd rect (at -4.9325 2.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C11-Pad2)"))
    (pad 6 smd rect (at -4.9325 1.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(L4-Pad2)"))
    (pad 7 smd rect (at -4.9325 1.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 8 smd rect (at -4.9325 0.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 5 +12V))
    (pad 9 smd rect (at -4.9325 0.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (pad 10 smd rect (at -4.9325 -0.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(L2-Pad2)"))
    (pad 11 smd rect (at -4.9325 -0.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 5 +12V))
    (pad 12 smd rect (at -4.9325 -1.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 13 smd rect (at -4.9325 -1.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C17-Pad1)"))
    (pad 14 smd rect (at -4.9325 -2.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C10-Pad1)"))
    (pad 15 smd rect (at -4.9325 -2.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C10-Pad2)"))
    (pad 16 smd rect (at -4.9325 -3.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 17 smd rect (at -4.9325 -3.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 18 smd rect (at -4.9325 -4.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 19 smd rect (at 4.9325 -4.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 20 smd rect (at 4.9325 -3.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 21 smd rect (at 4.9325 -3.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 22 smd rect (at 4.9325 -2.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 23 smd rect (at 4.9325 -2.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 21 AUD_PWRDN))
    (pad 24 smd rect (at 4.9325 -1.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C5-Pad1)"))
    (pad 25 smd rect (at 4.9325 -1.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C7-Pad1)"))
    (pad 26 smd rect (at 4.9325 -0.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 27 smd rect (at 4.9325 -0.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 17 I2S_MCLK))
    (pad 28 smd rect (at 4.9325 0.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 18 I2S_BCLK))
    (pad 29 smd rect (at 4.9325 0.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 16 I2S_LRCLK))
    (pad 30 smd rect (at 4.9325 1.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 15 I2S_TX))
    (pad 31 smd rect (at 4.9325 1.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 20 AUD_RESET))
    (pad 32 smd rect (at 4.9325 2.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 31 AUD_INT))
    (pad 33 smd rect (at 4.9325 2.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 22 AUD_OVRSMP_SEL))
    (pad 34 smd rect (at 4.9325 3.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 19 AUD_GAIN_SEL))
    (pad 35 smd rect (at 4.9325 3.75 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 36 smd rect (at 4.9325 4.25 180) (size 1.7 0.35) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 37 smd rect (at 0 0 180) (size 5.2 7.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at -1.5 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 1.5 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at -1.5 0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0 0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 1.5 0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at -1.5 -0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0 -0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 1.5 -0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at -1.5 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 1.5 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 37 smd rect (at 0 0 180) (size 4.3 4.3) (layers F.Cu F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/ST_PowerSSO-36_SlugDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 186.309 140.462 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at -2.286 -0.127 360) (layer B.SilkS))
    (fp_text value Bead (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 161.036 130.048 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D12813)
    (at 164.592 132.346 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.401 0 270) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0.508 0.508 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D127F5)
    (at 166.116 132.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.401 -0.127 450) (layer F.SilkS))
    (fp_text value 680p (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 169.926 127.762 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 169.926 135.382)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59FA9631)
    (at 179.832 127)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 3.048 0.508) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 179.832 128.778)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 3.048 0.254) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D13809)
    (at 179.832 134.366)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 3.048 0.254) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 1.016 0.508) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 184.404 140.462 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L2 (at -2.3876 -0.3556 180) (layer B.SilkS))
    (fp_text value Bead (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J8-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 59D1261F)
    (at 186.69 132.146 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L3 (at -2.3216 -0.0508 180) (layer B.SilkS))
    (fp_text value Bead (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at -5.08 -0.635 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 184.785 132.146 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L4 (at -2.3724 -0.1778 180) (layer B.SilkS))
    (fp_text value Bead (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J9-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(L4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.348 142.24)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.524) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 I2C_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59D12BBE)
    (at 152.146 142.24 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 I2C_SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.048 131.572 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.425 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59D12C75)
    (at 161.048 133.096 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.425 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 165.366 130.302 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.139 1.397 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D12628)
    (at 180.086 136.906)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 2.8575 0.0635) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.445) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 184.404 137.287 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.0762 -1.4224 90) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 184.785 129.044 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -0.242 -1.397 270) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(L4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59FA9A0C)
    (at 136.382 138.938 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.905 -1.397 180) (layer F.SilkS))
    (fp_text value .33u (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0.111 -0.0635 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59FA9A20)
    (at 132.322 138.938)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.766 1.3335) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 19.558 3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x6.7 (layer B.Cu) (tedit 58AA8BB3)
    (at 172.21 141.732)
    (descr "SMT capacitor, aluminium electrolytic, 8x6.7")
    (attr smd)
    (fp_text reference C12 (at 5.2344 -3.1496 90) (layer B.SilkS))
    (fp_text value "47u 25V" (at 0 5.45) (layer B.Fab))
    (fp_text user + (at -1.96 0.08) (layer B.Fab))
    (fp_text user + (at -4.78 -3.91) (layer B.SilkS))
    (fp_text user %R (at 0 -5.45) (layer B.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 4 2.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 3.05 0 180) (size 4 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x6.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 179.832 130.556)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 3.1115 0.0635) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at -0.0635 0.0635) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 179.832 132.588)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 3.048 0.0635) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at -0.4445 -0.1905) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 186.309 137.16 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0 1.2954 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 186.69 129.02 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 2.02 -0.254 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 59FA9981)
    (at 143.51 143.764 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at -1.7 0 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 11 SW1))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 59FA997E)
    (at 139.7 143.764 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J5 (at -1.7 0 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 59FA997C)
    (at 135.89 143.764 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -1.778 -0.3175 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 13 SW3))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 59FA95F8)
    (at 185.42 142.875 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference CHEST (at -1.7145 -0.1905 360) (layer F.SilkS))
    (fp_text value TRANSDUCER_A (at -1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J8-Pad1)"))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J8-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 59FA95EA)
    (at 186.05 134.62 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference HEAD (at -1.7272 -0.1828 360) (layer F.SilkS))
    (fp_text value TRANSDUCER_B (at -1.8 0 360) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J9-Pad2)"))
  )
  (module Diodes_SMD:D_0805 (layer F.Cu) (tedit 590CE9A4)
    (at 168.495 138.43)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0 -1.6) (layer F.SilkS))
    (fp_text value D (at 0 1.7) (layer F.Fab))
    (fp_text user %R (at 2.7645 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59FA963A)
    (at 180.975 143.51 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference 12V (at -2.9718 4.572 180) (layer F.SilkS))
    (fp_text value "12V PWR" (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59FA9A19)
    (at 134.378 140.97)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.917 -0.4445) (layer F.SilkS))
    (fp_text value 2.18K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59FA99FB)
    (at 139.942 139.446)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.242 1.143) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:MURATA_OKL1 (layer F.Cu) (tedit 59F93D00)
    (at 141.732 125.349 180)
    (fp_text reference U1 (at 12.3825 -13.589 180) (layer F.SilkS))
    (fp_text value OKL-T/1-W12N-C (at 6.604 0.762 180) (layer F.Fab))
    (pad 9 smd rect (at 1.905 -1.905 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.191 -1.905 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 6.477 -1.905 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 12 smd rect (at 8.763 -1.905 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 11.049 -1.905 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R2-Pad1)"))
    (pad 10 smd rect (at 1.905 -4.191 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1.905 -6.477 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R1-Pad1)"))
    (pad 11 smd rect (at 11.049 -4.191 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd rect (at 11.049 -6.477 180) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 3.048 -11.049 180) (size 4.064 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 3 smd rect (at 7.62 -11.049 180) (size 4.064 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at 11.049 -9.906 270) (size 4.064 1.778) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 151.396 126.238)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.5788 0.254) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:SDCard_Molex_5031821852 (layer F.Cu) (tedit 59FA6E9B)
    (at 141.954 126.116)
    (fp_text reference J2 (at 18.574 0.503) (layer F.SilkS))
    (fp_text value Micro_SD_Card (at 6.985 -3.175) (layer F.Fab))
    (pad 9 connect rect (at 14.5 4.5) (size 1.16 1.25) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 6 connect rect (at 12.7 14.65) (size 1.5 1.15) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 6 connect rect (at 4.9 14.65) (size 1.5 1.15) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 6 connect rect (at 14.9 2.4) (size 1.15 2.2) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 6 connect rect (at 0.6 13.9) (size 1.15 2.2) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 5.2 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 6.3 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 10 SD_CS))
    (pad 3 smd rect (at 7.4 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 9 SD_MOSI))
    (pad 4 smd rect (at 8.5 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at 9.6 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 8 SD_CLK))
    (pad 6 smd rect (at 10.7 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at 11.8 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 7 SD_MISO))
    (pad 8 smd rect (at 12.9 1.9) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask))
    (pad 6 connect rect (at 0.5 2.55) (size 0.95 2.5) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 9 connect rect (at 14.5 13.5) (size 1.16 1.2) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78F1)
    (at 158.17088 135.77316)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78F6)
    (at 156.1592 134.79272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7900)
    (at 152.4 134.366)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78C0)
    (at 172.20184 141.63548)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78CF)
    (at 165.81628 144.21612)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78C8)
    (at 168.656 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78BC)
    (at 172.212 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78AA)
    (at 178.562 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78A7)
    (at 178.816 141.732)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78B0)
    (at 175.26 139.7)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78D2)
    (at 168.402 139.446)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78E3)
    (at 165.608 135.89)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78E0)
    (at 168.402 137.16)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78D5)
    (at 172.212 136.906)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78D9)
    (at 173.228 135.89)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7847)
    (at 184.912 126.746)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7840)
    (at 182.372 126.746)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA788F)
    (at 187.452 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7888)
    (at 187.706 140.462)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7881)
    (at 187.706 138.176)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7876)
    (at 187.706 136.144)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA788C)
    (at 187.452 142.494)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7870)
    (at 187.706 130.302)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7893)
    (at 182.88 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7899)
    (at 182.626 140.97)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA789F)
    (at 180.594 138.684)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78A3)
    (at 178.054 140.208)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78B5)
    (at 175.26 144.272)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78EB)
    (at 162.306 142.24)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78E8)
    (at 164.338 139.192)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7904)
    (at 148.59 140.716)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7942)
    (at 134.874 130.302)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7940)
    (at 134.874 132.588)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA793D)
    (at 134.874 134.366)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7935)
    (at 137.16 134.366)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7938)
    (at 137.16 132.588)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA793A)
    (at 137.16 130.302)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA792F)
    (at 139.446 134.62)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA792C)
    (at 139.7 133.35)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA790F)
    (at 142.748 135.636)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7907)
    (at 145.288 133.096)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA791B)
    (at 144.78 130.048)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7925)
    (at 141.478 130.556)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA790C)
    (at 144.018 134.366)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7915)
    (at 142.748 132.842)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7921)
    (at 141.478 126.492)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA791D)
    (at 149.352 126.492)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA783A)
    (at 178.054 129.54)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7829)
    (at 172.72 128.27)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA7834)
    (at 176.784 128.27)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module custom:Via-0.6mm-Tented (layer F.Cu) (tedit 59FA78DC)
    (at 172.72 134.62)
    (fp_text reference REF** (at 0.5 4) (layer F.SilkS) hide)
    (fp_text value Via-0.6mm-Tented (at 0 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (gr_text 5V (at 132.5245 133.604) (layer F.SilkS))
  (gr_text GND (at 134.1755 134.6835) (layer F.SilkS))
  (gr_text 12V (at 138.3665 134.62) (layer F.SilkS))
  (gr_text GND (at 142.24 141.986 270) (layer F.SilkS))
  (gr_text 3V3 (at 143.51 141.986 270) (layer F.SilkS))
  (gr_text SW1 (at 144.653 141.986 270) (layer F.SilkS))
  (gr_text SW2 (at 140.843 141.986 270) (layer F.SilkS))
  (gr_text 3V3 (at 139.7 141.986 270) (layer F.SilkS))
  (gr_text GND (at 138.43 141.986 270) (layer F.SilkS))
  (gr_text SW3 (at 137.033 141.986 270) (layer F.SilkS))
  (gr_text 3V3 (at 135.89 141.986 270) (layer F.SilkS))
  (gr_text GND (at 134.62 141.986 270) (layer F.SilkS))
  (gr_text SW4 (at 133.096 141.986 270) (layer F.SilkS))
  (gr_text 3V3 (at 131.953 141.986 270) (layer F.SilkS))
  (gr_text GND (at 130.556 141.986 270) (layer F.SilkS))
  (gr_text 3V3 (at 160.02 141.732 270) (layer F.SilkS))
  (gr_text GND (at 161.036 141.732 270) (layer F.SilkS))
  (gr_text SCL (at 163.068 141.732 270) (layer F.SilkS))
  (gr_text SDA (at 162.1028 141.732 270) (layer F.SilkS))
  (gr_text SENS (at 161.4932 137.9728) (layer F.SilkS))
  (gr_text + (at 181.5592 139.3444) (layer B.SilkS))
  (gr_text - (at 184.8104 144.1196) (layer F.SilkS))
  (gr_text + (at 186.1312 144.1196) (layer F.SilkS))
  (gr_text - (at 185.42 136.0932) (layer F.SilkS))
  (gr_text + (at 186.7408 136.0932) (layer F.SilkS))
  (gr_text + (at 178.8668 138.7348) (layer F.SilkS))
  (gr_text "Revit - 11/2017" (at 165.862 142.494) (layer F.SilkS))
  (gr_text "Purr Engine V2.0" (at 165.862 140.97) (layer F.SilkS))
  (gr_line (start 128.27 145.415) (end 128.27 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.595 125.73) (end 128.27 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.595 145.415) (end 188.595 125.73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 145.415) (end 188.595 145.415) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.135 155.575) (xy 126.365 155.575) (xy 125.73 125.095) (xy 191.135 123.825)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 155.575) (xy 191.135 155.575) (xy 191.77 123.825) (xy 125.73 124.46)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.704 135.382) (xy 171.704 127.635) (xy 179.324 127.635) (xy 179.324 135.509) (xy 171.704 135.636)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.069 136.779) (xy 171.196 126.492) (xy 179.705 126.492) (xy 179.832 136.906)
      )
    )
  )
)
