(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "1")
  (net 2 "2")
  (net 3 "3")
  (net 4 "4")
  (net 5 "5")
  (net 6 "6")
  (net 7 "7")
  (net 8 "8")
  (net 9 "9")
  (net 10 "10")
  (net 11 "11")
  (net 12 "12")
  (net 13 "13")
  (net 14 "23")
  (net 15 "24")
  (net 16 "25")
  (net 17 "17")
  (net 18 "18")
  (net 19 "19")
  (net 20 "20")
  (net 21 "21")
  (net 22 "22")
  (net 23 "14")
  (net 24 "15")
  (net 25 "16")
  (footprint "Connector_Dsub:DSUB-25_Female_EdgeMount_P2.77mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 138.9367 60.0075 90)
    (descr "25-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 47.1mm")
    (property "Sheetfile" "A1000PAR.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -20.543333 0 90) (layer "F.SilkS"))
    (fp_text value "DB25_Female (A1000)" (at 0 16.86 90) (layer "F.Fab"))
    (fp_text user "PCB edge" (at -21.55 1.323333 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 3.39 90) (layer "F.Fab"))
    (pad "1" smd rect (at 16.62 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "13") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 13.85 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "12") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 11.08 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "11") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 8.31 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "10") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at 5.54 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "9") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect (at 2.77 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "8") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect (at 0 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "7") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect (at -2.77 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "6") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect (at -5.54 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "5") (pinfunction "9") (pintype "passive"))
    (pad "10" smd rect (at -8.31 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "4") (pinfunction "10") (pintype "passive"))
    (pad "11" smd rect (at -11.08 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3") (pinfunction "11") (pintype "passive"))
    (pad "12" smd rect (at -13.85 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "2") (pinfunction "12") (pintype "passive"))
    (pad "13" smd rect (at -16.62 0 90) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1") (pinfunction "13") (pintype "passive"))
    (pad "14" smd rect (at 15.235 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "16") (pinfunction "P14") (pintype "passive"))
    (pad "15" smd rect (at 12.465 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "15") (pinfunction "P15") (pintype "passive"))
    (pad "16" smd rect (at 9.695 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "14") (pinfunction "P16") (pintype "passive"))
    (pad "17" smd rect (at 6.925 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "22") (pinfunction "P17") (pintype "passive"))
    (pad "18" smd rect (at 4.155 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "21") (pinfunction "P18") (pintype "passive"))
    (pad "19" smd rect (at 1.385 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "20") (pinfunction "P19") (pintype "passive"))
    (pad "20" smd rect (at -1.385 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "19") (pinfunction "P20") (pintype "passive"))
    (pad "21" smd rect (at -4.155 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "18") (pinfunction "P21") (pintype "passive"))
    (pad "22" smd rect (at -6.925 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "17") (pinfunction "P22") (pintype "passive"))
    (pad "23" smd rect (at -9.695 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "25") (pinfunction "P23") (pintype "passive"))
    (pad "24" smd rect (at -12.465 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "24") (pinfunction "P24") (pintype "passive"))
    (pad "25" smd rect (at -15.235 0 90) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "23") (pinfunction "P25") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Female_EdgeMount_P2.77mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-25_Female_EdgeMount_P2.77mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 128.3475 60.0075 -90)
    (descr "25-pin D-Sub connector, solder-cups edge-mounted, female, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector edge mount solder cup female x-pin-pitch 2.77mm mounting holes distance 47.1mm")
    (property "Sheetfile" "A1000PAR.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at -20.543333 0 90) (layer "F.SilkS"))
    (fp_text value "DB25_Female (Peripheral)" (at 0 16.86 90) (layer "F.Fab"))
    (fp_text user "PCB edge" (at -21.55 1.323333 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 3.39 90) (layer "F.Fab"))
    (pad "1" smd rect (at 16.62 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "1") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 13.85 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "2") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 11.08 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "3") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 8.31 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "4") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at 5.54 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "5") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect (at 2.77 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "6") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect (at 0 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "7") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect (at -2.77 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "8") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect (at -5.54 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "9") (pinfunction "9") (pintype "passive"))
    (pad "10" smd rect (at -8.31 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "10") (pinfunction "10") (pintype "passive"))
    (pad "11" smd rect (at -11.08 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "11") (pinfunction "11") (pintype "passive"))
    (pad "12" smd rect (at -13.85 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "12") (pinfunction "12") (pintype "passive"))
    (pad "13" smd rect (at -16.62 0 270) (size 1.846667 3.48) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "13") (pinfunction "13") (pintype "passive"))
    (pad "14" smd rect (at 15.235 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "14") (pinfunction "P14") (pintype "passive"))
    (pad "15" smd rect (at 12.465 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "15") (pinfunction "P15") (pintype "passive"))
    (pad "16" smd rect (at 9.695 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "16") (pinfunction "P16") (pintype "passive"))
    (pad "17" smd rect (at 6.925 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "17") (pinfunction "P17") (pintype "passive"))
    (pad "18" smd rect (at 4.155 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "18") (pinfunction "P18") (pintype "passive"))
    (pad "19" smd rect (at 1.385 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "19") (pinfunction "P19") (pintype "passive"))
    (pad "20" smd rect (at -1.385 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "20") (pinfunction "P20") (pintype "passive"))
    (pad "21" smd rect (at -4.155 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "21") (pinfunction "P21") (pintype "passive"))
    (pad "22" smd rect (at -6.925 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "22") (pinfunction "P22") (pintype "passive"))
    (pad "23" smd rect (at -9.695 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "23") (pinfunction "P23") (pintype "passive"))
    (pad "24" smd rect (at -12.465 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "24") (pinfunction "P24") (pintype "passive"))
    (pad "25" smd rect (at -15.235 0 270) (size 1.846667 3.48) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "25") (pinfunction "P25") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Female_EdgeMount_P2.77mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 126.3142 78.5749) (end 126.3142 41.4147) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 126.3396 41.4147) (end 140.9446 41.4147) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140.9446 41.4147) (end 140.97 78.5749) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140.97 78.5749) (end 126.3142 78.5749) (layer "Edge.Cuts") (width 0.1))
  (gr_text "A1000\n" (at 135.7884 44.1706 90) (layer "F.SilkS"))
  (gr_text "Peripheral" (at 131.4958 74.4474 90) (layer "F.SilkS"))
)
