(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 355)
    (zones 0)
    (modules 12)
    (nets 44)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4732 1.4732)
    (pad_drill 0.9652)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-PadP$7)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-PadP$1)")
  (net 4 "Net-(C1-Pad1)")
  (net 5 "Net-(C2-Pad1)")
  (net 6 "Net-(U1-PadPGM)")
  (net 7 "Net-(J1-PadP$30)")
  (net 8 "Net-(U1-PadAREF)")
  (net 9 "Net-(Q2-Pad2)")
  (net 10 "Net-(J1-PadP$13)")
  (net 11 "Net-(J1-PadP$9)")
  (net 12 "Net-(J1-PadP$5)")
  (net 13 "Net-(J1-PadP$18)")
  (net 14 "Net-(J1-PadP$14)")
  (net 15 "Net-(J1-PadP$10)")
  (net 16 "Net-(J1-PadP$6)")
  (net 17 "Net-(J1-PadP$2)")
  (net 18 "Net-(J1-PadP$22)")
  (net 19 "Net-(J1-PadP$26)")
  (net 20 "Net-(R5-Pad2)")
  (net 21 "Net-(J1-PadP$32)")
  (net 22 "Net-(J1-PadP$28)")
  (net 23 "Net-(J1-PadP$24)")
  (net 24 "Net-(J1-PadP$20)")
  (net 25 "Net-(J1-PadP$4)")
  (net 26 "Net-(J1-PadP$8)")
  (net 27 "Net-(J1-PadP$12)")
  (net 28 "Net-(J1-PadP$16)")
  (net 29 "Net-(J1-PadP$3)")
  (net 30 "Net-(J1-PadP$15)")
  (net 31 "Net-(J1-PadP$17)")
  (net 32 "Net-(Q1-Pad2)")
  (net 33 "Net-(J1-PadP$40)")
  (net 34 "Net-(J1-PadP$39)")
  (net 35 "Net-(J1-PadP$37)")
  (net 36 "Net-(J1-PadP$35)")
  (net 37 "Net-(J1-PadP$33)")
  (net 38 "Net-(J1-PadP$29)")
  (net 39 "Net-(J1-PadP$27)")
  (net 40 "Net-(J1-PadP$25)")
  (net 41 "Net-(J1-PadP$23)")
  (net 42 "Net-(J1-PadP$21)")
  (net 43 "Net-(J1-PadP$19)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-PadP$1)")
    (add_net "Net-(J1-PadP$10)")
    (add_net "Net-(J1-PadP$12)")
    (add_net "Net-(J1-PadP$13)")
    (add_net "Net-(J1-PadP$14)")
    (add_net "Net-(J1-PadP$15)")
    (add_net "Net-(J1-PadP$16)")
    (add_net "Net-(J1-PadP$17)")
    (add_net "Net-(J1-PadP$18)")
    (add_net "Net-(J1-PadP$19)")
    (add_net "Net-(J1-PadP$2)")
    (add_net "Net-(J1-PadP$20)")
    (add_net "Net-(J1-PadP$21)")
    (add_net "Net-(J1-PadP$22)")
    (add_net "Net-(J1-PadP$23)")
    (add_net "Net-(J1-PadP$24)")
    (add_net "Net-(J1-PadP$25)")
    (add_net "Net-(J1-PadP$26)")
    (add_net "Net-(J1-PadP$27)")
    (add_net "Net-(J1-PadP$28)")
    (add_net "Net-(J1-PadP$29)")
    (add_net "Net-(J1-PadP$3)")
    (add_net "Net-(J1-PadP$30)")
    (add_net "Net-(J1-PadP$32)")
    (add_net "Net-(J1-PadP$33)")
    (add_net "Net-(J1-PadP$35)")
    (add_net "Net-(J1-PadP$37)")
    (add_net "Net-(J1-PadP$39)")
    (add_net "Net-(J1-PadP$4)")
    (add_net "Net-(J1-PadP$40)")
    (add_net "Net-(J1-PadP$5)")
    (add_net "Net-(J1-PadP$6)")
    (add_net "Net-(J1-PadP$7)")
    (add_net "Net-(J1-PadP$8)")
    (add_net "Net-(J1-PadP$9)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U1-PadAREF)")
    (add_net "Net-(U1-PadPGM)")
  )
  (module TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm (layer Top) (tedit 5D6B480A)
    (at 137.795 111.999)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference PWR (at -5.157 -31.09876) (layer B.SilkS))
    (fp_text value TestPoint_THTPad_D1.5mm_Drill0.7mm (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.157 -29.62696) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-PadP$19)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 127.386 83.6794 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference C1 (at -0.5452 -0.92964 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 134.488 100.294 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference C2 (at -0.69088 -1.66116 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:WM6787CT-ND (layer Bottom) (tedit 0)
    (at 132.624 105.37 90)
    (fp_text reference J1 (at 8.509 1.1684) (layer B.SilkS) hide)
    (fp_text value WM6787CT-ND (at 7.493 1.651) (layer B.SilkS) hide)
    (fp_text user J1 (at -0.01016 -0.00508 180) (layer B.SilkS))
    (fp_text user >Value (at 7.493 1.651 180) (layer B.Fab))
    (pad P$1 smd rect (at -4.7 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(J1-PadP$1)") (solder_mask_margin 0.1016))
    (pad P$2 smd rect (at -4.7 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 17 "Net-(J1-PadP$2)") (solder_mask_margin 0.1016))
    (pad P$3 smd rect (at -4.2 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 29 "Net-(J1-PadP$3)") (solder_mask_margin 0.1016))
    (pad P$4 smd rect (at -4.2 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 25 "Net-(J1-PadP$4)") (solder_mask_margin 0.1016))
    (pad P$5 smd rect (at -3.7 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 12 "Net-(J1-PadP$5)") (solder_mask_margin 0.1016))
    (pad P$6 smd rect (at -3.7 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 16 "Net-(J1-PadP$6)") (solder_mask_margin 0.1016))
    (pad P$7 smd rect (at -3.2 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 1 "Net-(J1-PadP$7)") (solder_mask_margin 0.1016))
    (pad P$8 smd rect (at -3.2 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 26 "Net-(J1-PadP$8)") (solder_mask_margin 0.1016))
    (pad P$9 smd rect (at -2.7 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 11 "Net-(J1-PadP$9)") (solder_mask_margin 0.1016))
    (pad P$10 smd rect (at -2.7 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 15 "Net-(J1-PadP$10)") (solder_mask_margin 0.1016))
    (pad P$11 smd rect (at -2.2 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(J1-PadP$1)") (solder_mask_margin 0.1016))
    (pad P$12 smd rect (at -2.2 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 27 "Net-(J1-PadP$12)") (solder_mask_margin 0.1016))
    (pad P$13 smd rect (at -1.7 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 10 "Net-(J1-PadP$13)") (solder_mask_margin 0.1016))
    (pad P$14 smd rect (at -1.7 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 14 "Net-(J1-PadP$14)") (solder_mask_margin 0.1016))
    (pad P$15 smd rect (at -1.2 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 30 "Net-(J1-PadP$15)") (solder_mask_margin 0.1016))
    (pad P$16 smd rect (at -1.2 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 28 "Net-(J1-PadP$16)") (solder_mask_margin 0.1016))
    (pad P$17 smd rect (at -0.7 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 31 "Net-(J1-PadP$17)") (solder_mask_margin 0.1016))
    (pad P$18 smd rect (at -0.7 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(J1-PadP$18)") (solder_mask_margin 0.1016))
    (pad P$19 smd rect (at -0.2 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 43 "Net-(J1-PadP$19)") (solder_mask_margin 0.1016))
    (pad P$20 smd rect (at -0.2 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 24 "Net-(J1-PadP$20)") (solder_mask_margin 0.1016))
    (pad P$21 smd rect (at 0.3 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 42 "Net-(J1-PadP$21)") (solder_mask_margin 0.1016))
    (pad P$22 smd rect (at 0.3 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(J1-PadP$22)") (solder_mask_margin 0.1016))
    (pad P$23 smd rect (at 0.8 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 41 "Net-(J1-PadP$23)") (solder_mask_margin 0.1016))
    (pad P$24 smd rect (at 0.8 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 23 "Net-(J1-PadP$24)") (solder_mask_margin 0.1016))
    (pad P$25 smd rect (at 1.3 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 40 "Net-(J1-PadP$25)") (solder_mask_margin 0.1016))
    (pad P$26 smd rect (at 1.3 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 19 "Net-(J1-PadP$26)") (solder_mask_margin 0.1016))
    (pad P$27 smd rect (at 1.8 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 39 "Net-(J1-PadP$27)") (solder_mask_margin 0.1016))
    (pad P$28 smd rect (at 1.8 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 22 "Net-(J1-PadP$28)") (solder_mask_margin 0.1016))
    (pad P$29 smd rect (at 2.3 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 38 "Net-(J1-PadP$29)") (solder_mask_margin 0.1016))
    (pad P$30 smd rect (at 2.3 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(J1-PadP$30)") (solder_mask_margin 0.1016))
    (pad P$31 smd rect (at 2.8 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad P$32 smd rect (at 2.8 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 21 "Net-(J1-PadP$32)") (solder_mask_margin 0.1016))
    (pad P$33 smd rect (at 3.3 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 37 "Net-(J1-PadP$33)") (solder_mask_margin 0.1016))
    (pad P$34 smd rect (at 3.3 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad P$35 smd rect (at 3.8 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 36 "Net-(J1-PadP$35)") (solder_mask_margin 0.1016))
    (pad P$36 smd rect (at 3.8 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 24 "Net-(J1-PadP$20)") (solder_mask_margin 0.1016))
    (pad P$37 smd rect (at 4.3 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 35 "Net-(J1-PadP$37)") (solder_mask_margin 0.1016))
    (pad P$38 smd rect (at 4.3 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad P$39 smd rect (at 4.8 2.85) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 34 "Net-(J1-PadP$39)") (solder_mask_margin 0.1016))
    (pad P$40 smd rect (at 4.8 -2.65) (size 1.1 0.3) (layers Bottom B.Paste B.Mask)
      (net 33 "Net-(J1-PadP$40)") (solder_mask_margin 0.1016))
    (pad P$43 smd rect (at 6 2.74 180) (size 1.32 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad P$44 smd rect (at 6 -2.54) (size 1.32 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad P$41 smd rect (at -5.9 2.74) (size 1.32 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad P$42 smd rect (at -5.9 -2.54) (size 1.32 1.3) (layers Bottom B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:SOT23-3 (layer Top) (tedit 0)
    (at 132.298 94.2137 270)
    (descr SOT23-3)
    (fp_text reference Q1 (at -1.72156 0.5619) (layer F.SilkS))
    (fp_text value 220mA/50V/3.5Ω (at 1.651 0) (layer F.Fab))
    (pad 3 smd rect (at 0 -1.1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 34 "Net-(J1-PadP$39)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.95 1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.95 1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:SOT23-3 (layer Top) (tedit 0)
    (at 132.395 89.2505 270)
    (descr SOT23-3)
    (fp_text reference Q2 (at -1.651 0) (layer F.SilkS))
    (fp_text value 220mA/50V/3.5Ω (at 1.651 0) (layer F.Fab))
    (pad 3 smd rect (at 0 -1.1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 35 "Net-(J1-PadP$37)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.95 1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.95 1 270) (size 0.8 0.9) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 128.113 93.4584 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R1 (at -0.58904 -0.83258 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 135.362 92.0988 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R2 (at -0.77008 -0.86046 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 34 "Net-(J1-PadP$39)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 135.606 87.1356 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R3 (at -0.6056 -0.96874 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 35 "Net-(J1-PadP$37)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:0603 (layer Top) (tedit 0)
    (at 127.869 88.5241 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R4 (at -0.64008 -0.8382 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers Top F.Paste F.Mask)
      (net 9 "Net-(Q2-Pad2)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:TEENSY_LC (layer Top) (tedit 0)
    (at 132.558 97.9018 270)
    (fp_text reference U1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value TEENSY_LC (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user "TEENSY LC" (at 0 5.08) (layer F.SilkS))
    (pad 25 thru_hole circle (at -3.81 -5.08 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-PadP$7)") (solder_mask_margin 0.1016))
    (pad GND3 thru_hole circle (at 16.51 0 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at -6.35 -5.08 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadP$1)") (solder_mask_margin 0.1016))
    (pad 3V2 thru_hole circle (at 16.51 2.54 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad VIN thru_hole circle (at 16.51 5.08 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad VUSB thru_hole circle (at -13.97 -5.08 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad PGM thru_hole circle (at 16.51 -2.54 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-PadPGM)") (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 16.51 -5.08 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-PadP$30)") (solder_mask_margin 0.1016))
    (pad AREF thru_hole circle (at -8.89 -5.08 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-PadAREF)") (solder_mask_margin 0.1016))
    (pad 5V thru_hole circle (at -16.51 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad GND1 thru_hole circle (at -16.51 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad GND2 thru_hole circle (at -13.97 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 3V1 thru_hole circle (at -11.43 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 0 thru_hole circle (at -13.97 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 "Net-(Q2-Pad2)") (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at -8.89 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-PadP$13)") (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at -6.35 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-PadP$9)") (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at -3.81 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-PadP$5)") (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at -1.27 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadP$18)") (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 1.27 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-PadP$14)") (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 3.81 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-PadP$10)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 6.35 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-PadP$6)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 8.89 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-PadP$2)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 11.43 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-PadP$22)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 13.97 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-PadP$26)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 16.51 -7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 20 "Net-(R5-Pad2)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 16.51 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-PadP$32)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 13.97 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-PadP$28)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 11.43 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-PadP$24)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 8.89 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-PadP$20)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 6.35 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-PadP$4)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 3.81 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-PadP$8)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.27 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-PadP$12)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -1.27 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-PadP$16)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -3.81 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-PadP$3)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -6.35 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-PadP$15)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -8.89 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-PadP$17)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -11.43 7.62 270) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 "Net-(Q1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module T61_LC_Scanner:SOT95P237X112-3N (layer Top) (tedit 0)
    (at 128.753 100.919)
    (fp_text reference U2 (at -0.53414 -1.77854) (layer F.SilkS))
    (fp_text value TLV810SDBZT (at 0 0) (layer F.SilkS) hide)
    (fp_text user TLV810 (at -1.5546 2.41969) (layer F.Fab))
    (pad 3 smd rect (at 1.0922 0) (size 1.3208 0.508) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -1.0922 0.9398) (size 1.3208 0.5588) (layers Top F.Paste F.Mask)
      (net 33 "Net-(J1-PadP$40)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.0922 -0.9398) (size 1.3208 0.5588) (layers Top F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
  )
  (gr_text 2 (at 128.48844 109.65208 180) (layer B.SilkS))
  (gr_line (start 123.66752 115.6716) (end 123.66752 80.1036) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.66752 115.6716) (end 141.44244 115.6716) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.66752 80.1036) (end 141.44244 80.1036) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.44244 115.6716) (end 141.44244 80.1036) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 136.91108 109.65208 180) (layer B.SilkS))
  (gr_text 39 (at 136.23544 100.0966 180) (layer B.SilkS))
  (gr_text 40 (at 127.24892 100.0966 180) (layer B.SilkS))
  (gr_text "Lenovo T61 Controller" (at 127.54356 80.63605 90) (layer B.SilkS))
  (gr_text "Version 2.1 HDR" (at 129.10312 80.8736 90) (layer B.SilkS))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.675 80.125) (xy 141.45 80.125) (xy 141.45 115.675) (xy 123.675 115.675)
      )
    )
  )
)
