(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 930)
    (zones 0)
    (modules 5)
    (nets 100)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.16)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 121.9 92.54)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-PadB60)")
  (net 2 "Net-(J1-PadB59)")
  (net 3 "Net-(J1-PadB19)")
  (net 4 "Net-(J1-PadB14)")
  (net 5 "Net-(J1-PadB11)")
  (net 6 "Net-(J1-PadB10)")
  (net 7 "Net-(J1-PadB2)")
  (net 8 "Net-(J1-PadB1)")
  (net 9 "Net-(J1-PadA60)")
  (net 10 "Net-(J1-PadA59)")
  (net 11 "Net-(J1-PadA41)")
  (net 12 "Net-(J1-PadA40)")
  (net 13 "Net-(J1-PadA19)")
  (net 14 "Net-(J1-PadA16)")
  (net 15 "Net-(J1-PadA14)")
  (net 16 "Net-(J1-PadA11)")
  (net 17 "Net-(J1-PadA9)")
  (net 18 "Net-(J1-PadA3)")
  (net 19 "Net-(J1-PadA2)")
  (net 20 "Net-(J1-PadA1)")
  (net 21 "Net-(J2-Pad1)")
  (net 22 "Net-(J2-Pad3)")
  (net 23 "Net-(J3-Pad28)")
  (net 24 "Net-(J3-Pad26)")
  (net 25 "Net-(J3-Pad25)")
  (net 26 "Net-(J3-Pad24)")
  (net 27 "Net-(J3-Pad23)")
  (net 28 "Net-(J3-Pad22)")
  (net 29 "Net-(J3-Pad21)")
  (net 30 "Net-(J3-Pad20)")
  (net 31 "Net-(J3-Pad19)")
  (net 32 "Net-(J3-Pad18)")
  (net 33 "Net-(J3-Pad17)")
  (net 34 "Net-(J3-Pad16)")
  (net 35 "Net-(J3-Pad14)")
  (net 36 "Net-(J3-Pad3)")
  (net 37 "Net-(J3-Pad1)")
  (net 38 JTAG)
  (net 39 +5V)
  (net 40 INTA#)
  (net 41 INTC#)
  (net 42 +3V3)
  (net 43 RST#)
  (net 44 GNT#)
  (net 45 GND)
  (net 46 AD[30])
  (net 47 AD[28])
  (net 48 AD[26])
  (net 49 AD[24])
  (net 50 IDSEL)
  (net 51 AD[22])
  (net 52 AD[20])
  (net 53 AD[18])
  (net 54 AD[16])
  (net 55 FRAME#)
  (net 56 TRDY#)
  (net 57 STOP#)
  (net 58 PAR)
  (net 59 AD[15])
  (net 60 AD[13])
  (net 61 AD[11])
  (net 62 AD[09])
  (net 63 C\BE#[0])
  (net 64 AD[06])
  (net 65 AD[04])
  (net 66 AD[02])
  (net 67 AD[00])
  (net 68 INTB#)
  (net 69 INTD#)
  (net 70 CLK)
  (net 71 REQ#)
  (net 72 AD[31])
  (net 73 AD[29])
  (net 74 AD[27])
  (net 75 AD[25])
  (net 76 C\BE#[3])
  (net 77 AD[23])
  (net 78 AD[21])
  (net 79 AD[19])
  (net 80 AD[17])
  (net 81 C\BE#[2])
  (net 82 IRDY#)
  (net 83 DEVSEL#)
  (net 84 LOCK#)
  (net 85 PERR#)
  (net 86 SERR#)
  (net 87 C\BE#[1])
  (net 88 AD[14])
  (net 89 AD[12])
  (net 90 AD[10])
  (net 91 AD[08])
  (net 92 AD[07])
  (net 93 AD[05])
  (net 94 AD[03])
  (net 95 AD[01])
  (net 96 +5VP)
  (net 97 +3.3VA)
  (net 98 "Net-(J1-PadA10)")
  (net 99 M66EN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5V)
    (add_net +5VP)
    (add_net AD[00])
    (add_net AD[01])
    (add_net AD[02])
    (add_net AD[03])
    (add_net AD[04])
    (add_net AD[05])
    (add_net AD[06])
    (add_net AD[07])
    (add_net AD[08])
    (add_net AD[09])
    (add_net AD[10])
    (add_net AD[11])
    (add_net AD[12])
    (add_net AD[13])
    (add_net AD[14])
    (add_net AD[15])
    (add_net AD[16])
    (add_net AD[17])
    (add_net AD[18])
    (add_net AD[19])
    (add_net AD[20])
    (add_net AD[21])
    (add_net AD[22])
    (add_net AD[23])
    (add_net AD[24])
    (add_net AD[25])
    (add_net AD[26])
    (add_net AD[27])
    (add_net AD[28])
    (add_net AD[29])
    (add_net AD[30])
    (add_net AD[31])
    (add_net CLK)
    (add_net C\BE#[0])
    (add_net C\BE#[1])
    (add_net C\BE#[2])
    (add_net C\BE#[3])
    (add_net DEVSEL#)
    (add_net FRAME#)
    (add_net GND)
    (add_net GNT#)
    (add_net IDSEL)
    (add_net INTA#)
    (add_net INTB#)
    (add_net INTC#)
    (add_net INTD#)
    (add_net IRDY#)
    (add_net JTAG)
    (add_net LOCK#)
    (add_net M66EN)
    (add_net "Net-(J1-PadA1)")
    (add_net "Net-(J1-PadA10)")
    (add_net "Net-(J1-PadA11)")
    (add_net "Net-(J1-PadA14)")
    (add_net "Net-(J1-PadA16)")
    (add_net "Net-(J1-PadA19)")
    (add_net "Net-(J1-PadA2)")
    (add_net "Net-(J1-PadA3)")
    (add_net "Net-(J1-PadA40)")
    (add_net "Net-(J1-PadA41)")
    (add_net "Net-(J1-PadA59)")
    (add_net "Net-(J1-PadA60)")
    (add_net "Net-(J1-PadA9)")
    (add_net "Net-(J1-PadB1)")
    (add_net "Net-(J1-PadB10)")
    (add_net "Net-(J1-PadB11)")
    (add_net "Net-(J1-PadB14)")
    (add_net "Net-(J1-PadB19)")
    (add_net "Net-(J1-PadB2)")
    (add_net "Net-(J1-PadB59)")
    (add_net "Net-(J1-PadB60)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad20)")
    (add_net "Net-(J3-Pad21)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad23)")
    (add_net "Net-(J3-Pad24)")
    (add_net "Net-(J3-Pad25)")
    (add_net "Net-(J3-Pad26)")
    (add_net "Net-(J3-Pad28)")
    (add_net "Net-(J3-Pad3)")
    (add_net PAR)
    (add_net PERR#)
    (add_net REQ#)
    (add_net RST#)
    (add_net SERR#)
    (add_net STOP#)
    (add_net TRDY#)
  )
  (net_class Oshpark ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical locked (layer B.Cu) (tedit 5D8E321F)
    (at 170.16 51.9 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value Conn_02x20_Odd_Even (at 1.27 -50.59 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -24.13 180) (layer B.Fab))
    (pad 40 thru_hole oval (at 2.54 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 INTA#))
    (pad 39 thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 INTB#))
    (pad 38 thru_hole oval (at 2.54 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 INTC#))
    (pad 37 thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 INTD#))
    (pad 36 thru_hole oval (at 2.54 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 RST#))
    (pad 35 thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 CLK))
    (pad 34 thru_hole oval (at 2.54 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 GNT#))
    (pad 33 thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 REQ#))
    (pad 32 thru_hole oval (at 2.54 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 AD[30]))
    (pad 31 thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 AD[31]))
    (pad 30 thru_hole oval (at 2.54 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 GND))
    (pad 29 thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 +3.3VA))
    (pad 28 thru_hole oval (at 2.54 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad28)"))
    (pad 27 thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 AD[29]))
    (pad 26 thru_hole oval (at 2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad26)"))
    (pad 25 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad25)"))
    (pad 24 thru_hole oval (at 2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad24)"))
    (pad 23 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad22)"))
    (pad 21 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad20)"))
    (pad 19 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad18)"))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad16)"))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 AD[08]))
    (pad 14 thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad14)"))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 AD[07]))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 GND))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 +5VP))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 C\BE#[0]))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 AD[05]))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 AD[06]))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 AD[03]))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 AD[04]))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 AD[01]))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 AD[02]))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 AD[00]))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical locked (layer B.Cu) (tedit 5D8E31E3)
    (at 121.9 92.54 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at 1.27 2.33 90) (layer B.SilkS) hide)
    (fp_text value Conn_02x20_Odd_Even (at 1.27 -50.59 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -24.13) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 AD[27]))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 AD[25]))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 AD[28]))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 C\BE#[3]))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 AD[26]))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 AD[23]))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 AD[24]))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 AD[21]))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 +5VP))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 GND))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 IDSEL))
    (pad 14 thru_hole oval (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 AD[19]))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 AD[22]))
    (pad 16 thru_hole oval (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 AD[17]))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 AD[20]))
    (pad 18 thru_hole oval (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 C\BE#[2]))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 AD[18]))
    (pad 20 thru_hole oval (at 2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 IRDY#))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 AD[16]))
    (pad 22 thru_hole oval (at 2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 DEVSEL#))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 FRAME#))
    (pad 24 thru_hole oval (at 2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 LOCK#))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 TRDY#))
    (pad 26 thru_hole oval (at 2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 PERR#))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 STOP#))
    (pad 28 thru_hole oval (at 2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 SERR#))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 +3.3VA))
    (pad 30 thru_hole oval (at 2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 PAR))
    (pad 32 thru_hole oval (at 2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 C\BE#[1]))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 AD[15]))
    (pad 34 thru_hole oval (at 2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 AD[14]))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 AD[13]))
    (pad 36 thru_hole oval (at 2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 AD[12]))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 AD[11]))
    (pad 38 thru_hole oval (at 2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 AD[10]))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 AD[09]))
    (pad 40 thru_hole oval (at 2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 M66EN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 134.594 72.718 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 97 +3.3VA))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5A3EABFC)
    (at 141.96 72.21 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8 270) (layer B.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 96 +5VP))
  )
  (module Connector_PCBEdge:BUS_PCI_UNIVERSAL_edgecuts locked (layer F.Cu) (tedit 5D8D5EDD)
    (at 146.02 112.66)
    (descr "PCI bus Edge Connector")
    (tags "PCI bus Edge Connector")
    (attr virtual)
    (fp_text reference J1 (at 11.81 -5.78) (layer F.SilkS) hide)
    (fp_text value Bus_PCI_32bit_Universal (at -18.29 -5.78) (layer F.Fab))
    (fp_arc (start -25.401 2.989) (end -25.401 3.37) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 22.864 2.989) (end 22.864 3.37) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 39.247 2.989) (end 39.247 3.37) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 25.401 2.989) (end 25.02 2.989) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start -22.859 2.989) (end -23.24 2.989) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start -39.239 2.989) (end -39.62 2.989) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 24.13 -4) (end 25.02 -4) (angle -180) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start -24.13 -4) (end -23.24 -4) (angle -180) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 39.247 3.37) (end 25.401 3.37) (layer Edge.Cuts) (width 0.1))
    (fp_text user %R (at 0 -0.76) (layer F.Fab))
    (fp_line (start 39.628 -4.89) (end 39.628 2.989) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 22.864 3.37) (end -22.859 3.37) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -23.24 2.989) (end -23.24 -4) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -25.02 -4) (end -25.02 2.989) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -25.401 3.37) (end -39.239 3.37) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -39.62 2.989) (end -39.62 -4.89) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 23.245 2.989) (end 23.24 -4) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 25.02 -4) (end 25.02 2.989) (layer Edge.Cuts) (width 0.1))
    (pad B62 connect rect (at 38.73 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B61 connect rect (at 37.46 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B60 connect rect (at 36.2 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-PadB60)"))
    (pad B59 connect rect (at 34.92 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-PadB59)"))
    (pad B58 connect rect (at 33.65 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 95 AD[01]))
    (pad B57 connect rect (at 32.38 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B56 connect rect (at 31.11 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 94 AD[03]))
    (pad B55 connect rect (at 29.84 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 93 AD[05]))
    (pad B54 connect rect (at 28.57 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B53 connect rect (at 27.3 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 92 AD[07]))
    (pad B52 connect rect (at 26.03 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 91 AD[08]))
    (pad B49 connect rect (at 22.22 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 99 M66EN))
    (pad B48 connect rect (at 20.95 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 90 AD[10]))
    (pad B47 connect rect (at 19.68 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 89 AD[12]))
    (pad B46 connect rect (at 18.41 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B45 connect rect (at 17.14 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 88 AD[14]))
    (pad B44 connect rect (at 15.88 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 87 C\BE#[1]))
    (pad B43 connect rect (at 14.6 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B42 connect rect (at 13.34 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 86 SERR#))
    (pad B41 connect rect (at 12.06 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B40 connect rect (at 10.79 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 85 PERR#))
    (pad B39 connect rect (at 9.52 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 84 LOCK#))
    (pad B38 connect rect (at 8.25 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B37 connect rect (at 6.98 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 83 DEVSEL#))
    (pad B36 connect rect (at 5.71 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B35 connect rect (at 4.44 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 82 IRDY#))
    (pad B34 connect rect (at 3.17 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B33 connect rect (at 1.9 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 81 C\BE#[2]))
    (pad B32 connect rect (at 0.63 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 80 AD[17]))
    (pad B31 connect rect (at -0.64 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B30 connect rect (at -1.91 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 79 AD[19]))
    (pad B29 connect rect (at -3.18 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 78 AD[21]))
    (pad B28 connect rect (at -4.45 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B27 connect rect (at -5.72 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 77 AD[23]))
    (pad B26 connect rect (at -6.99 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 76 C\BE#[3]))
    (pad B25 connect rect (at -8.26 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B24 connect rect (at -9.53 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 75 AD[25]))
    (pad B23 connect rect (at -10.8 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 74 AD[27]))
    (pad B22 connect rect (at -12.07 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B21 connect rect (at -13.34 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 73 AD[29]))
    (pad B20 connect rect (at -14.61 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 72 AD[31]))
    (pad B19 connect rect (at -15.88 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-PadB19)"))
    (pad B18 connect rect (at -17.15 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 71 REQ#))
    (pad B17 connect rect (at -18.42 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B16 connect rect (at -19.69 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 70 CLK))
    (pad B15 connect rect (at -20.96 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B14 connect rect (at -22.23 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-PadB14)"))
    (pad B11 connect rect (at -26.04 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 5 "Net-(J1-PadB11)"))
    (pad B10 connect rect (at -27.31 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 6 "Net-(J1-PadB10)"))
    (pad B9 connect rect (at -28.58 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B8 connect rect (at -29.85 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 69 INTD#))
    (pad B7 connect rect (at -31.12 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 68 INTB#))
    (pad B6 connect rect (at -32.39 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B5 connect rect (at -33.66 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B4 connect rect (at -34.93 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 38 JTAG))
    (pad B3 connect rect (at -36.2 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B2 connect rect (at -37.47 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 7 "Net-(J1-PadB2)"))
    (pad B1 connect rect (at -38.73 -1.33) (size 1.02 4.57) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-PadB1)"))
    (pad A62 connect rect (at 38.73 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A61 connect rect (at 37.46 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A60 connect rect (at 36.2 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 9 "Net-(J1-PadA60)"))
    (pad A59 connect rect (at 34.92 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-PadA59)"))
    (pad A58 connect rect (at 33.65 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 67 AD[00]))
    (pad A57 connect rect (at 32.38 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 66 AD[02]))
    (pad A56 connect rect (at 31.11 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A55 connect rect (at 29.84 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 65 AD[04]))
    (pad A54 connect rect (at 28.57 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 64 AD[06]))
    (pad A53 connect rect (at 27.3 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A52 connect rect (at 26.03 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 63 C\BE#[0]))
    (pad A49 connect rect (at 22.22 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 62 AD[09]))
    (pad A48 connect rect (at 20.95 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A47 connect rect (at 19.68 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 61 AD[11]))
    (pad A46 connect rect (at 18.41 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 60 AD[13]))
    (pad A45 connect rect (at 17.14 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A44 connect rect (at 15.88 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 59 AD[15]))
    (pad A43 connect rect (at 14.6 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 58 PAR))
    (pad A42 connect rect (at 13.34 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A41 connect rect (at 12.06 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 11 "Net-(J1-PadA41)"))
    (pad A40 connect rect (at 10.79 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 12 "Net-(J1-PadA40)"))
    (pad A39 connect rect (at 9.52 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A38 connect rect (at 8.25 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 57 STOP#))
    (pad A37 connect rect (at 6.98 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A36 connect rect (at 5.71 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 56 TRDY#))
    (pad A35 connect rect (at 4.44 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A34 connect rect (at 3.17 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 55 FRAME#))
    (pad A33 connect rect (at 1.9 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A32 connect rect (at 0.63 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 54 AD[16]))
    (pad A31 connect rect (at -0.64 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 53 AD[18]))
    (pad A30 connect rect (at -1.91 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A29 connect rect (at -3.18 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 52 AD[20]))
    (pad A28 connect rect (at -4.45 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 51 AD[22]))
    (pad A27 connect rect (at -5.72 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A26 connect rect (at -6.99 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 50 IDSEL))
    (pad A25 connect rect (at -8.26 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 49 AD[24]))
    (pad A24 connect rect (at -9.53 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A23 connect rect (at -10.8 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 48 AD[26]))
    (pad A22 connect rect (at -12.07 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 47 AD[28]))
    (pad A21 connect rect (at -13.34 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A20 connect rect (at -14.61 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 46 AD[30]))
    (pad A19 connect rect (at -15.88 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 13 "Net-(J1-PadA19)"))
    (pad A18 connect rect (at -17.15 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A17 connect rect (at -18.42 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 44 GNT#))
    (pad A16 connect rect (at -19.69 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 14 "Net-(J1-PadA16)"))
    (pad A15 connect rect (at -20.96 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 43 RST#))
    (pad A14 connect rect (at -22.23 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 15 "Net-(J1-PadA14)"))
    (pad A11 connect rect (at -26.04 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 16 "Net-(J1-PadA11)"))
    (pad A10 connect rect (at -27.31 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 98 "Net-(J1-PadA10)"))
    (pad A9 connect rect (at -28.58 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 17 "Net-(J1-PadA9)"))
    (pad A8 connect rect (at -29.85 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A7 connect rect (at -31.12 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 41 INTC#))
    (pad A6 connect rect (at -32.39 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 40 INTA#))
    (pad A5 connect rect (at -33.66 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A4 connect rect (at -34.93 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 38 JTAG))
    (pad A3 connect rect (at -36.2 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 18 "Net-(J1-PadA3)"))
    (pad A2 connect rect (at -37.47 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 19 "Net-(J1-PadA2)"))
    (pad A1 connect rect (at -38.73 -1.33) (size 1.02 4.57) (layers B.Cu B.Mask)
      (net 20 "Net-(J1-PadA1)"))
    (pad B62 connect rect (at 38.73 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B61 connect rect (at 37.46 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B60 connect rect (at 36.2 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-PadB60)"))
    (pad B59 connect rect (at 34.92 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 2 "Net-(J1-PadB59)"))
    (pad B58 connect rect (at 33.65 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 95 AD[01]))
    (pad B57 connect rect (at 32.38 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B56 connect rect (at 31.11 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 94 AD[03]))
    (pad B55 connect rect (at 29.84 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 93 AD[05]))
    (pad B54 connect rect (at 28.57 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B53 connect rect (at 27.3 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 92 AD[07]))
    (pad B52 connect rect (at 26.03 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 91 AD[08]))
    (pad B49 connect rect (at 22.22 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 99 M66EN))
    (pad B48 connect rect (at 20.95 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 90 AD[10]))
    (pad B47 connect rect (at 19.68 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 89 AD[12]))
    (pad B46 connect rect (at 18.41 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B45 connect rect (at 17.14 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 88 AD[14]))
    (pad B44 connect rect (at 15.88 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 87 C\BE#[1]))
    (pad B43 connect rect (at 14.6 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B42 connect rect (at 13.34 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 86 SERR#))
    (pad B41 connect rect (at 12.06 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B40 connect rect (at 10.79 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 85 PERR#))
    (pad B39 connect rect (at 9.52 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 84 LOCK#))
    (pad B38 connect rect (at 8.25 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B37 connect rect (at 6.98 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 83 DEVSEL#))
    (pad B36 connect rect (at 5.71 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B35 connect rect (at 4.44 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 82 IRDY#))
    (pad B34 connect rect (at 3.17 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B33 connect rect (at 1.9 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 81 C\BE#[2]))
    (pad B32 connect rect (at 0.63 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 80 AD[17]))
    (pad B31 connect rect (at -0.64 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B30 connect rect (at -1.91 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 79 AD[19]))
    (pad B29 connect rect (at -3.18 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 78 AD[21]))
    (pad B28 connect rect (at -4.45 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B27 connect rect (at -5.72 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 77 AD[23]))
    (pad B26 connect rect (at -6.99 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 76 C\BE#[3]))
    (pad B25 connect rect (at -8.26 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 42 +3V3))
    (pad B24 connect rect (at -9.53 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 75 AD[25]))
    (pad B23 connect rect (at -10.8 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 74 AD[27]))
    (pad B22 connect rect (at -12.07 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B21 connect rect (at -13.34 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 73 AD[29]))
    (pad B20 connect rect (at -14.61 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 72 AD[31]))
    (pad B19 connect rect (at -15.88 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-PadB19)"))
    (pad B18 connect rect (at -17.15 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 71 REQ#))
    (pad B17 connect rect (at -18.42 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B16 connect rect (at -19.69 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 70 CLK))
    (pad B15 connect rect (at -20.96 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B14 connect rect (at -22.23 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-PadB14)"))
    (pad B11 connect rect (at -26.04 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 5 "Net-(J1-PadB11)"))
    (pad B10 connect rect (at -27.31 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 6 "Net-(J1-PadB10)"))
    (pad B9 connect rect (at -28.58 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B8 connect rect (at -29.85 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 69 INTD#))
    (pad B7 connect rect (at -31.12 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 68 INTB#))
    (pad B6 connect rect (at -32.39 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B5 connect rect (at -33.66 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 39 +5V))
    (pad B4 connect rect (at -34.93 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 38 JTAG))
    (pad B3 connect rect (at -36.2 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 45 GND))
    (pad B2 connect rect (at -37.47 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 7 "Net-(J1-PadB2)"))
    (pad B1 connect rect (at -38.73 1.33) (size 0.51 0.76) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-PadB1)"))
    (pad A62 connect rect (at 38.73 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A61 connect rect (at 37.46 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A60 connect rect (at 36.2 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 9 "Net-(J1-PadA60)"))
    (pad A59 connect rect (at 34.92 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-PadA59)"))
    (pad A58 connect rect (at 33.65 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 67 AD[00]))
    (pad A57 connect rect (at 32.38 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 66 AD[02]))
    (pad A56 connect rect (at 31.11 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A55 connect rect (at 29.84 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 65 AD[04]))
    (pad A54 connect rect (at 28.57 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 64 AD[06]))
    (pad A53 connect rect (at 27.3 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A52 connect rect (at 26.03 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 63 C\BE#[0]))
    (pad A49 connect rect (at 22.22 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 62 AD[09]))
    (pad A48 connect rect (at 20.95 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A47 connect rect (at 19.68 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 61 AD[11]))
    (pad A46 connect rect (at 18.41 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 60 AD[13]))
    (pad A45 connect rect (at 17.14 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A44 connect rect (at 15.88 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 59 AD[15]))
    (pad A43 connect rect (at 14.6 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 58 PAR))
    (pad A42 connect rect (at 13.34 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A41 connect rect (at 12.06 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 11 "Net-(J1-PadA41)"))
    (pad A40 connect rect (at 10.79 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 12 "Net-(J1-PadA40)"))
    (pad A39 connect rect (at 9.52 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A38 connect rect (at 8.25 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 57 STOP#))
    (pad A37 connect rect (at 6.98 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A36 connect rect (at 5.71 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 56 TRDY#))
    (pad A35 connect rect (at 4.44 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A34 connect rect (at 3.17 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 55 FRAME#))
    (pad A33 connect rect (at 1.9 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A32 connect rect (at 0.63 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 54 AD[16]))
    (pad A31 connect rect (at -0.64 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 53 AD[18]))
    (pad A30 connect rect (at -1.91 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A29 connect rect (at -3.18 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 52 AD[20]))
    (pad A28 connect rect (at -4.45 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 51 AD[22]))
    (pad A27 connect rect (at -5.72 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A26 connect rect (at -6.99 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 50 IDSEL))
    (pad A25 connect rect (at -8.26 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 49 AD[24]))
    (pad A24 connect rect (at -9.53 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A23 connect rect (at -10.8 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 48 AD[26]))
    (pad A22 connect rect (at -12.07 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 47 AD[28]))
    (pad A21 connect rect (at -13.34 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 42 +3V3))
    (pad A20 connect rect (at -14.61 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 46 AD[30]))
    (pad A19 connect rect (at -15.88 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 13 "Net-(J1-PadA19)"))
    (pad A18 connect rect (at -17.15 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 45 GND))
    (pad A17 connect rect (at -18.42 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 44 GNT#))
    (pad A16 connect rect (at -19.69 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 14 "Net-(J1-PadA16)"))
    (pad A15 connect rect (at -20.96 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 43 RST#))
    (pad A14 connect rect (at -22.23 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 15 "Net-(J1-PadA14)"))
    (pad A11 connect rect (at -26.04 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 16 "Net-(J1-PadA11)"))
    (pad A10 connect rect (at -27.31 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 98 "Net-(J1-PadA10)"))
    (pad A9 connect rect (at -28.58 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 17 "Net-(J1-PadA9)"))
    (pad A8 connect rect (at -29.85 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A7 connect rect (at -31.12 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 41 INTC#))
    (pad A6 connect rect (at -32.39 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 40 INTA#))
    (pad A5 connect rect (at -33.66 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 39 +5V))
    (pad A4 connect rect (at -34.93 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 38 JTAG))
    (pad A3 connect rect (at -36.2 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 18 "Net-(J1-PadA3)"))
    (pad A2 connect rect (at -37.47 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 19 "Net-(J1-PadA2)"))
    (pad A1 connect rect (at -38.73 1.33) (size 0.51 0.76) (layers B.Cu B.Mask)
      (net 20 "Net-(J1-PadA1)"))
  )
  (gr_text "defparam 2019" (at 143.998 66.378) (layer F.SilkS))
  (gr_text "Nano Face Down\nUSB Points ---->" (at 158.73 79.84) (layer F.SilkS))
  (gr_text PCI-2-Nano (at 151.11 63.33) (layer F.SilkS))
  (gr_text 3.3Vb (at 131.26 72.885) (layer F.SilkS))
  (gr_text 5Vb (at 144.71 71.025) (layer B.SilkS))
  (gr_arc (start 184.378 98.753) (end 185.648 98.753) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 176.3135 96.213) (end 175.0435 96.213) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 173.7735 48.0927) (end 175.0435 48.0927) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 117.8935 48.08) (end 117.8935 46.81) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 115.3535 96.213) (end 115.3535 97.483) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 107.67 98.753) (end 107.67 97.483) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 184.378 97.483) (end 176.3135 97.483) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.3535 97.483) (end 107.67 97.483) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.0435 96.213) (end 175.0435 48.0927) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.6235 96.213) (end 116.6235 48.08) (layer Edge.Cuts) (width 0.05))
  (gr_text "(A Side) Chassis-->" (at 115.7 100.91) (layer B.SilkS))
  (gr_text "<--Chassis (B Side)" (at 115.77 100.91) (layer F.SilkS))
  (gr_line (start 173.7735 46.8227) (end 117.8935 46.81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185.648 107.77) (end 185.648 98.753) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.4 107.77) (end 106.4 98.753) (layer Edge.Cuts) (width 0.05))
  (zone (net 45) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.4 108.913) (xy 185.394 108.913) (xy 185.394 46.937) (xy 185.394 45.921) (xy 106.4 45.921)
        (xy 106.4 108.786)
      )
    )
  )
  (zone (net 45) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.4 108.913) (xy 185.648 108.913) (xy 185.648 45.921) (xy 106.4 45.921) (xy 106.4 108.278)
      )
    )
  )
)
