(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 46)
    (no_connects 0)
    (area 12.401549 17.652999 46.912784 38.03396)
    (thickness 1.6002)
    (drawings 6)
    (tracks 198)
    (zones 0)
    (modules 25)
    (nets 16)
  )
  (page A4)
  (title_block
    (date "29 aug 2014")
  )
  (layers
    (0 Front signal)
    (31 Back signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.24892)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.127)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 0.39878 1.5494)
    (pad_drill 0)
    (pad_to_mask_clearance 0.00762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 /Bat+)
  (net 2 GND)
  (net 3 N-000002)
  (net 4 N-000004)
  (net 5 N-000005)
  (net 6 N-000006)
  (net 7 N-000009)
  (net 8 N-000010)
  (net 9 N-000011)
  (net 10 N-000012)
  (net 11 N-000013)
  (net 12 N-000014)
  (net 13 N-000015)
  (net 14 N-000017)
  (net 15 N-000018)
  (net_class Default "This is the default net class."
    (clearance 0.24892)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /Bat+)
    (add_net GND)
    (add_net N-000002)
    (add_net N-000004)
    (add_net N-000005)
    (add_net N-000006)
    (add_net N-000009)
    (add_net N-000010)
    (add_net N-000011)
    (add_net N-000012)
    (add_net N-000013)
    (add_net N-000014)
    (add_net N-000015)
    (add_net N-000017)
    (add_net N-000018)
  )
  (module SOT-23-5 (layer Front) (tedit 537AC0AD)
    (at 23.368 26.416 270)
    (descr SOT23-5)
    (tags "SOT-23-5,5 lead, SOT-23")
    (fp_text reference U1 (at 0 0 270) (layer F.SilkS))
    (fp_text value LP5907 (at 0 0.508 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.94996 1.19888 270) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 1 /Bat+))
    (pad 4 smd rect (at 0.94996 -1.19888 270) (size 0.59944 1.24968) (layers Front F.Paste F.Mask))
    (pad 3 smd rect (at 0.94996 1.19888 270) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 8 N-000010))
    (pad 2 smd rect (at 0 1.19888 270) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -0.94996 -1.19888 270) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 13 N-000015))
    (model smd/smd_transistors/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PMBT2907 (layer Front) (tedit 537AC608)
    (at 23.368 30.226 90)
    (descr SOT23)
    (tags PMBT2907,PMBT2907A)
    (fp_text reference Q1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2N2907 (at 0 0.508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.9525 1.05664 90) (size 0.59944 1.00076) (layers Front F.Paste F.Mask)
      (net 9 N-000011))
    (pad 3 smd rect (at 0 -1.05664 90) (size 0.59944 1.00076) (layers Front F.Paste F.Mask)
      (net 8 N-000010))
    (pad 1 smd rect (at 0.9525 1.05664 90) (size 0.59944 1.00076) (layers Front F.Paste F.Mask)
      (net 1 /Bat+))
    (model smd/smd_transistors/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_JST_2 (layer Front) (tedit 53E52BF6)
    (at 15.24 26.67 270)
    (descr "JST Connectorm 2 Pin")
    (tags JST,Connector,2,pin)
    (fp_text reference P3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value Bat (at -3.81 -3.556 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /Bat+))
    (pad 2 thru_hole circle (at 1.27 -3.81 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Conn_1 (layer Front) (tedit 53E52A22)
    (at 30.734 35.814)
    (descr "Connector 1 pin")
    (tags Connector,1,pin)
    (fp_text reference P4 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value 9V (at 0 -1.778) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 N-000017))
  )
  (module R_1206 (layer Front) (tedit 53919B83)
    (at 23.368 33.528)
    (descr "SMD, Resistor, 1206")
    (fp_text reference R1 (at 0 -0.0508 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.50114) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 9 N-000011))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 10 N-000012))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 53E4FF72)
    (at 23.622 22.606 180)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10µ (at 0 1.50114 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 1 /Bat+))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 27.432 29.718 90)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C2 (at 0 -0.0508 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 1.50114 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 13 N-000015))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 39.116 27.432)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C4 (at 0 -0.0508 90) (layer F.SilkS))
    (fp_text value 10µ (at 0 1.50114) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 4 N-000004))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 30.226 29.718 90)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C3 (at 0 -0.0508 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.50114 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 13 N-000015))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_6 (layer Front) (tedit 53E52C5E)
    (at 36.322 22.352 270)
    (descr WE_Transformer)
    (tags SMD_6,WE,Transformer,6,pin)
    (fp_text reference T1 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value 1:1.7 (at 0 1.016 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 11 N-000013))
    (pad 2 smd rect (at 0 4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 13 N-000015))
    (pad 3 smd rect (at 2.54 4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 12 N-000014))
    (pad 4 smd rect (at 2.54 -4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 6 N-000006))
    (pad 5 smd rect (at 0 -4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask))
    (pad 6 smd rect (at -2.54 -4.56946 270) (size 1.27 1.27) (layers Front F.Paste F.Mask)
      (net 5 N-000005))
    (model smd/smd_dil/so-14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_1206 (layer Front) (tedit 53E511F6)
    (at 34.798 33.528 180)
    (descr "SMD, Resistor, 1206")
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.50114 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 14 N-000017))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 15 N-000018))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_1206 (layer Front) (tedit 53919B83)
    (at 43.942 36.068)
    (descr "SMD, Resistor, 1206")
    (fp_text reference R3 (at 0 -0.0508 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.50114) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 7 N-000009))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module R_1206 (layer Front) (tedit 53919B83)
    (at 40.894 33.528 180)
    (descr "SMD, Resistor, 1206")
    (fp_text reference R4 (at 0 -0.0508 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.50114 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 15 N-000018))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 7 N-000009))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 43.942 30.734 180)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C5 (at 0 -0.0508 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.50114 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 3 N-000002))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 37.846 36.068)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C6 (at 0 -0.0508 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.50114) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 15 N-000018))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C_1206 (layer Front) (tedit 537AC487)
    (at 33.274 28.702 270)
    (descr "SMD, Capacitor, 1206")
    (fp_text reference C7 (at 0 -0.0508 360) (layer F.SilkS))
    (fp_text value 22µ (at 0 1.50114 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 270) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 14 N-000017))
    (pad 2 smd rect (at -1.397 0 270) (size 1.6002 1.8034) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/capacitors/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_1_Round (layer Front) (tedit 53E52A3D)
    (at 19.05 35.814 180)
    (descr "Connector 1 pin round")
    (tags Connector,1,pin,Round)
    (fp_text reference P1 (at 0 1.016 180) (layer F.SilkS) hide)
    (fp_text value Ring (at 0 2.032 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 N-000012))
  )
  (module Conn_2 (layer Front) (tedit 53E52A54)
    (at 20.32 19.304)
    (descr "Connector 2 pins")
    (tags Connector,2,pin)
    (fp_text reference P2 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value Charger (at 4.826 -0.254) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /Bat+))
    (pad 2 thru_hole circle (at 1.27 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module SOT-23-5 (layer Front) (tedit 537AC0AD)
    (at 28.194 23.876)
    (descr SOT23-5)
    (tags "SOT-23-5,5 lead, SOT-23")
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value SN6501 (at 0 0.508) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.94996 1.19888) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 12 N-000014))
    (pad 4 smd rect (at 0.94996 -1.19888) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.94996 1.19888) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 11 N-000013))
    (pad 2 smd rect (at 0 1.19888) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 13 N-000015))
    (pad 5 smd rect (at -0.94996 -1.19888) (size 0.59944 1.24968) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/smd_transistors/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD_123 (layer Front) (tedit 53E5361F)
    (at 43.18 21.336 90)
    (descr SOD_123)
    (tags "SMT, SMD, SOD23, Diode")
    (fp_text reference D4 (at 0.1524 0.0508 90) (layer F.SilkS))
    (fp_text value MBR0520L (at 0 1.143 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.63576 0 90) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 5 N-000005))
    (pad 2 smd rect (at -1.63576 0 90) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 4 N-000004))
    (model smd/resistors/r_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD_123 (layer Front) (tedit 53E535F4)
    (at 45.466 21.336 270)
    (descr SOD_123)
    (tags "SMT, SMD, SOD23, Diode")
    (fp_text reference D3 (at -0.0762 -0.8636 270) (layer F.SilkS))
    (fp_text value MBR0520L (at 0 1.143 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.63576 0 270) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.63576 0 270) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 5 N-000005))
    (model smd/resistors/r_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD_123 (layer Front) (tedit 53E5360C)
    (at 43.18 26.67 90)
    (descr SOD_123)
    (tags "SMT, SMD, SOD23, Diode")
    (fp_text reference D2 (at -0.1778 0.8382 90) (layer F.SilkS))
    (fp_text value MBR0520L (at 0 1.143 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.63576 0 90) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 6 N-000006))
    (pad 2 smd rect (at -1.63576 0 90) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 4 N-000004))
    (model smd/resistors/r_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOD_123 (layer Front) (tedit 53E53602)
    (at 45.466 26.67 270)
    (descr SOD_123)
    (tags "SMT, SMD, SOD23, Diode")
    (fp_text reference D1 (at -0.0762 -0.8636 270) (layer F.SilkS))
    (fp_text value MBR0520L (at 0 1.143 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.63576 0 270) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.63576 0 270) (size 1.24968 1.24968) (layers Front F.Paste F.Mask)
      (net 6 N-000006))
    (model smd/resistors/r_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSOP-8 (layer Front) (tedit 53E53B7D)
    (at 38.1 30.48 270)
    (descr MSOP-8)
    (tags MSOP,8,PowerPad)
    (fp_text reference U3 (at -1.7526 2.0066 360) (layer F.SilkS))
    (fp_text value TPS7A4901 (at 1.397 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.97536 2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 14 N-000017))
    (pad 2 smd rect (at -0.32512 2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 15 N-000018))
    (pad 3 smd rect (at 0.32512 2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask))
    (pad 4 smd rect (at 0.97536 2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.97536 -2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 4 N-000004))
    (pad 6 smd rect (at 0.32512 -2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 3 N-000002))
    (pad 7 smd rect (at -0.32512 -2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask))
    (pad 8 smd rect (at -0.97536 -2.10058 270) (size 0.39878 1.5494) (layers Front F.Paste F.Mask)
      (net 4 N-000004))
    (pad 9 smd rect (at 0 0 270) (size 1.88976 1.56972) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model smd/smd_dil/msoic-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_1_Round (layer Front) (tedit 51D18C65)
    (at 27.686 35.814)
    (descr "Connector 1 pin round")
    (tags Connector,1,pin,Round)
    (fp_text reference P5 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -1.778) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text "Music Unfolding\nLiPo Battery \n9V Boost" (at 36.322 24.13) (layer F.SilkS))
  (gr_line (start 17.526 37.338) (end 17.526 17.78) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 46.736 37.338) (end 17.526 37.338) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 46.736 17.78) (end 46.736 37.338) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 17.526 17.78) (end 46.736 17.78) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_text "MusicUnfolding.com\nLiPo Battery Boost" (at 26.67 18.796) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.762) (thermal_bridge_width 1.524) (smoothing chamfer))
    (polygon
      (pts
        (xy 46.736 37.338) (xy 46.736 18.034) (xy 17.526 18.034) (xy 17.526 37.338)
      )
    )
  )
)
