(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 52)
    (zones 0)
    (modules 9)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 155.448 62.23)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B1-Pad1)")
  (net 2 "Net-(B1-Pad2)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 GNDPWR)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDPWR)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.715 61.595 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 152.4 53.38 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C1 (at -1.945 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.3 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 146.725 53.34)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C2 (at 1.27 2.54) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.25 2.3) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module km-kicad-library:GDL75V (layer F.Cu) (tedit 5F5D1FBB)
    (at 164.592 60.9092 270)
    (fp_text reference GD1 (at 0 4.699 270) (layer F.SilkS))
    (fp_text value GDT (at 0 -5.715 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
  )
  (module Diode_THT:D_T-1_P2.54mm_Vertical_KathodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 149.352 59.69 270)
    (descr "Diode, T-1 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Vertical pin pitch 2.54mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at -5.08 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.609214 90) (layer F.Fab) hide)
    (fp_text user K (at -2 0 90) (layer F.Fab))
    (fp_text user K (at -2 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P2.54mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 155.448 62.23 90)
    (descr "Diode, T-1 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Vertical pin pitch 2.54mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at -5.08 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.609214 90) (layer F.Fab))
    (fp_text user A (at 4.54 0 90) (layer F.Fab))
    (fp_text user A (at 4.54 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module km-kicad-library:A32265-ND (layer F.Cu) (tedit 5F5D5DA2)
    (at 177.8 57.15 90)
    (fp_text reference J1 (at -6.35 -8.636 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0.635 -9.525 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.08 5.08 90) (size 3.556 3.556) (drill 2.0828) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 3.556 3.556) (drill 2.0828) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.286 2.286) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad1)"))
  )
  (module km-kicad-library:A32265-ND (layer F.Cu) (tedit 5F5D5DA2)
    (at 137.16 57.15 90)
    (fp_text reference J2 (at -6.858 8.636 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0.635 -9.525 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.286 2.286) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.778 1.778) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 3.556 3.556) (drill 2.0828) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole circle (at -5.08 5.08 90) (size 3.556 3.556) (drill 2.0828) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
  )
  (module TestPoint:TestPoint_2Pads_Pitch5.08mm_Drill1.3mm (layer F.Cu) (tedit 5BD71EB4)
    (at 161.925 53.34 180)
    (descr "Test point with 2 pads, pitch 5.08mm, hole diameter 1.3mm, wire diameter 1.0mm")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference B1 (at 2.54 -2.5) (layer F.SilkS))
    (fp_text value Bulb (at 2.54 3) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(B1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
  )
  (gr_text "another fine product by" (at 176.3395 61.5315) (layer B.SilkS))
  (gr_text W8VOS (at 175.895 63.3095) (layer B.SilkS))
  (gr_text GUARD (at 176.5935 58.2295) (layer B.SilkS))
  (gr_text R (at 167.0685 57.5945) (layer B.SilkS))
  (gr_text Reciever (at 176.5935 55.8165) (layer B.SilkS))
  (gr_text BULB (at 159.4612 59.0804) (layer B.SilkS))
  (gr_text RIG (at 146.05 57.15) (layer F.SilkS))
  (gr_text ANT (at 168.402 57.15) (layer F.SilkS))
  (gr_text <ANT (at 183.515 57.15) (layer B.SilkS))
  (gr_line (start 186.69 52.07) (end 186.69 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 182.88 62.23) (end 182.88 66.04) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 182.88 52.07) (end 186.69 52.07) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text RIG> (at 131.445 57.15) (layer B.SilkS))
  (gr_text 20/09/20 (at 180.34 50.8) (layer B.SilkS))
  (gr_text W8VOS (at 165.1 49.53) (layer F.SilkS))
  (gr_text "Reciever Guard v1.0" (at 153.67 49.53) (layer F.SilkS))
  (gr_line (start 132.08 48.26) (end 182.88 48.26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.88 66.04) (end 132.08 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 52.07) (end 128.27 62.23) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132.08 52.07) (end 132.08 48.26) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132.08 62.23) (end 128.27 62.23) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4572))
    (polygon
      (pts
        (xy 186.756916 66.04) (xy 128.336916 66.04) (xy 128.336916 48.26) (xy 186.756916 48.26)
      )
    )
  )
  (zone (net 5) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4572))
    (polygon
      (pts
        (xy 186.69 66.04) (xy 128.27 66.04) (xy 128.27 48.26) (xy 186.69 48.26)
      )
    )
  )
)
