(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 20)
    (no_connects 0)
    (area 137.768329 101.649529 201.270871 139.752071)
    (thickness 1.6)
    (drawings 6)
    (tracks 36)
    (zones 0)
    (modules 13)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 137.7696 139.7508)
    (grid_origin 137.7696 139.7508)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory production/))
  )
  (net 0 "")
  (net 1 gnd)
  (net 2 VDD)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(JP1-Pad1)")
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(R2-Pad1)")
  (net 8 /BOUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BOUT)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net VDD)
    (add_net gnd)
  )
  (net_class test ""
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 placed (layer F.Cu) (tedit 57C8F7AB)
    (at 187.3 128.321 180)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 0.5084 -1.5238 180) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 1.778 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 placed (layer F.Cu) (tedit 57C8F8DB)
    (at 164.44 106.731)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 0.5076 -1.5242) (layer F.SilkS))
    (fp_text value "1uF (optional)" (at 1.25 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /BOUT))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_pth_diodes:diode_do41 placed (layer F.Cu) (tedit 57C8F729)
    (at 191.11 113.081 180)
    (descr "Diode, DO-41 package")
    (fp_text reference D1 (at -0.2536 0.0002 180) (layer F.SilkS))
    (fp_text value 1N5817 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (model walter/pth_diodes/diode_do41.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM placed (layer F.Cu) (tedit 57C905DE)
    (at 166.98 133.401 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at 1.2704 1.7782 180) (layer F.SilkS))
    (fp_text value CHARGING (at -6.3496 -1.9048 180) (layer F.SilkS))
    (fp_text user K (at 0.762 -1.778 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 57C8F816)
    (at 189.84 106.731 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -2.54 3.175 180) (layer F.SilkS) hide)
    (fp_text value "FAST CHARGE" (at 2.9212 1.3966 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-3-3,5-h (layer F.Cu) (tedit 57C8F890)
    (at 196.19 120.701 90)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at 1.3972 1.3966 90) (layer F.SilkS))
    (fp_text value "B  G +5" (at 0.0002 -5.0804 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (pad 1 thru_hole rect (at 3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at -3.5 -0.7 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 8 /BOUT))
    (model walter/conn_pt-1_5/pt_1,5-3-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57C8F769)
    (at 175.87 128.321 180)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 470R (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R1-Pad2)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57C8F71A)
    (at 175.87 113.081)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 0) (layer F.SilkS))
    (fp_text value 10K (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_resistors:RC03 (layer F.Cu) (tedit 57C8F711)
    (at 175.87 106.731)
    (descr "Resistor, RC03")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 0 0) (layer F.SilkS))
    (fp_text value 10K (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(JP1-Pad1)"))
    (model walter/pth_resistors/rc03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_capacitors:cnp_3mm_disc (layer F.Cu) (tedit 57C8F8AE)
    (at 184.76 120.701 270)
    (descr "Small ceramic capacitor")
    (tags C)
    (fp_text reference C2 (at -0.0002 0.7624 270) (layer F.SilkS))
    (fp_text value 100n (at 0 -2.286 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 VDD))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (model walter/capacitors/cnp_3mm_disc.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gama:LOGO2 (layer F.Cu) (tedit 0)
    (at 191.7446 134.0358)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (module w_battery_holders:keystone_103 (layer F.Cu) (tedit 57C90604)
    (at 153.01 120.701)
    (descr "Keystone type 103 battery holder")
    (fp_text reference BAT1 (at -0.0004 -8.8902) (layer F.SilkS))
    (fp_text value LIR2032 (at -9.5254 -11.4302) (layer F.SilkS))
    (pad 2 thru_hole circle (at -5.2832 0) (size 2.99974 2.99974) (drill 1.4986) (layers *.Cu *.Mask F.SilkS)
      (net 1 gnd))
    (pad 1 thru_hole rect (at 15.2146 0) (size 2.9972 2.9972) (drill 1.4986) (layers *.Cu *.Mask F.SilkS)
      (net 8 /BOUT))
    (model walter/battery_holders/keystone_103.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gama:TSOT-23 (layer F.Cu) (tedit 57C8FFB5)
    (at 175.87 120.701)
    (solder_mask_margin 0.0762)
    (clearance 0.1524)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value LTC4054L-4.2 (at -1.27 3.81) (layer F.Fab) hide)
    (pad 5 smd rect (at -0.95 -1.31) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R2-Pad1)") (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -0.95 1.31) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)") (solder_mask_margin 0.0762))
    (pad 2 smd rect (at 0 1.31) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 1 gnd) (solder_mask_margin 0.0762))
    (pad 4 smd rect (at 0.95 -1.31) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD) (solder_mask_margin 0.0762))
    (pad 3 smd rect (at 0.95 1.31) (size 0.62 1.22) (layers F.Cu F.Paste F.Mask)
      (net 8 /BOUT) (solder_mask_margin 0.0762))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text "© 2016 REV A" (at 193.6496 137.8458) (layer F.Mask))
  (target plus (at 137.7696 139.7508) (size 5) (width 0.1) (layer Edge.Cuts))
  (gr_line (start 137.7696 101.6508) (end 137.7696 139.7508) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 201.2696 101.6508) (end 137.7696 101.6508) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 201.2696 139.7508) (end 201.2696 101.6508) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 137.7696 139.7508) (end 201.2696 139.7508) (layer Edge.Cuts) (width 0.00254))
  (zone (net 1) (net_name gnd) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.2696 139.7508) (xy 137.7696 139.7508) (xy 137.7696 101.6508) (xy 201.2696 101.6508)
      )
    )
  )
  (zone (net 1) (net_name gnd) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.2696 139.7508) (xy 137.7696 139.7508) (xy 137.7696 101.6508) (xy 201.2696 101.6508)
      )
    )
  )
)
