<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="-1.27" x2="52.54" y2="-1.27" width="0" layer="20"/>
<wire x1="52.54" y1="-1.27" x2="52.54" y2="51.27" width="0" layer="20"/>
<wire x1="52.54" y1="51.27" x2="-1.27" y2="51.27" width="0" layer="20"/>
<wire x1="-1.27" y1="51.27" x2="-1.27" y2="-1.27" width="0" layer="20"/>
<text>Mt. Brighton Avalanche Oscillator v4
www.northcoastmodularcollective.com
January, 2020</text>
<hole x="24.365" y="44.665" drill="3.18"/>
<text>Built By:</text>
<text>RED</text>
<text>BLACK</text>
<text>Mt. Brighton Avalanche Oscillator</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="thonkiconn">
<packages>
<package name="WQP-PJ301M-12_JACK">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EVUFXL">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="DECADE-libraries20151104">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_2MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK"/>
<element name="FREQ" library="pot" package="EVUFXL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0204/7" value="330">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204/7" value="22k">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="E2,5-5" value="2.2uF">
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="+" library="DECADE-libraries20151104" package="1X01_2MM" value="M01PTH_2MM"/>
<element name="-" library="DECADE-libraries20151104" package="1X01_2MM" value="M01PTH_2MM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="P$3"/>
<contactref element="LED1" pad="K"/>
<contactref element="C1" pad="-"/>
<contactref element="-" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="C1" pad="+"/>
<contactref element="FREQ" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="FREQ" pad="1"/>
<contactref element="FREQ" pad="2"/>
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
<signal name="S$5">
</signal>
<signal name="S$6">
</signal>
<signal name="N$1">
<contactref element="+" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
