<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="14.732" y1="3.048" x2="70.231" y2="3.048" width="0" layer="20"/>
<wire x1="70.231" y1="3.048" x2="70.231" y2="46.101" width="0" layer="20"/>
<wire x1="70.231" y1="46.101" x2="14.732" y2="46.101" width="0" layer="20"/>
<wire x1="14.732" y1="46.101" x2="14.732" y2="3.048" width="0" layer="20"/>
<hole x="66.294" y="7.112" drill="2.794"/>
<hole x="19.05" y="7.112" drill="2.794"/>
<hole x="66.294" y="42.164" drill="2.794"/>
<text>GND</text>
<text>GND</text>
<text>+5VDC</text>
<text>+5VDC</text>
<text>SDA</text>
<text>SDA</text>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>SCL</text>
<text>SCL</text>
<text>SCL</text>
<hole x="19.05" y="42.164" drill="2.794"/>
<text>IGN+</text>
<text>IGN+</text>
</plain>
<libraries>
<library name="Seeed-Capacitor">
<packages>
<package name="C1206">
</package>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Diode">
<packages>
<package name="DO-214AC">
<description>http://www.sycelectronica.com.ar/semiconductores/1N4007-SMD.pdf</description>
</package>
</packages>
</library>
<library name="Seeed-Resistor">
<packages>
<package name="R0805">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2041">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
</packages>
</library>
<library name="x27_168">
<packages>
<package name="DEFAULT">
<description>x27.168 Stepper Motor</description>
</package>
</packages>
</library>
<library name="GaugeLibrary">
<packages>
<package name="1210SMD">
</package>
<package name="NEEDLE_ILLUMINATION_BOARD">
</package>
<package name="HTSSOP28">
</package>
</packages>
</library>
<library name="ON Semiconductor_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:34:29</description>
<packages>
<package name="SOIC127P1021X265-20N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Seeed-Capacitor" package="C0805" value="200nF">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
</element>
<element name="C2" library="Seeed-Capacitor" package="C0805" value="200nF">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
</element>
<element name="C3" library="Seeed-Capacitor" package="C0805" value="100nF">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
</element>
<element name="C4" library="Seeed-Capacitor" package="C0805" value="100nF">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
</element>
<element name="C5" library="Seeed-Capacitor" package="C0805" value="100nF">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
</element>
<element name="C6" library="Seeed-Capacitor" package="C1206" value="100uf">
<attribute name="MPN" value="GRM31CR60J107ME39L"/>
</element>
<element name="D1" library="Seeed-Diode" package="DO-214AC" value="1N4007">
<attribute name="MPN" value="1N4007"/>
</element>
<element name="R1" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R2" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R27" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R28" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R3" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R4" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R5" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R6" library="Seeed-Resistor" package="R0805" value="1K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="SYSTEM_BUS" library="con-molex" package="22-23-2041" value="22-23-2041">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="OC_FARNELL" value="1462920"/>
<attribute name="OC_NEWARK" value="38C0355"/>
</element>
<element name="U$1" library="x27_168" package="DEFAULT" value="X27.168"/>
<element name="U$2" library="GaugeLibrary" package="1210SMD" value="IN-S128TATRGB"/>
<element name="U$3" library="GaugeLibrary" package="1210SMD" value="IN-S128TATRGB"/>
<element name="U$4" library="GaugeLibrary" package="1210SMD" value="IN-S128TATRGB"/>
<element name="U1" library="ON Semiconductor_By_element14_Batch_1" package="SOIC127P1021X265-20N" value="AMIS30624C6244RG">
<attribute name="MPN" value="AMIS30624C6244RG"/>
<attribute name="OC_FARNELL" value="1641410"/>
<attribute name="OC_NEWARK" value="03P0834"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="ON SEMICONDUCTOR"/>
</element>
<element name="ILLUMINATION" library="GaugeLibrary" package="NEEDLE_ILLUMINATION_BOARD" value="NEEDLE_ILLUMINATION"/>
<element name="U$6" library="GaugeLibrary" package="HTSSOP28" value="PCA9955BTWJ"/>
<element name="R7" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="R8" library="Seeed-Resistor" package="R0805" value="4k">
<attribute name="MPN" value="RC0805JR-071KL"/>
</element>
<element name="U$5" library="GaugeLibrary" package="1210SMD" value="IN-S128TATRGB"/>
<element name="IGNITION_VOLTAGE" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="A2"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="A1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="15"/>
<contactref element="U$1" pad="B2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="13"/>
<contactref element="U$1" pad="B1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="2"/>
<contactref element="U$6" pad="SCL"/>
<contactref element="SYSTEM_BUS" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="1"/>
<contactref element="U$6" pad="SDA"/>
<contactref element="SYSTEM_BUS" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="SYSTEM_BUS" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U$6" pad="VDD"/>
<contactref element="R7" pad="2"/>
<contactref element="U$2" pad="COMMON"/>
<contactref element="ILLUMINATION" pad="ANODE"/>
<contactref element="U$4" pad="COMMON"/>
<contactref element="U$5" pad="COMMON"/>
<contactref element="U$3" pad="COMMON"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$6" pad="AD2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U$6" pad="AD1"/>
</signal>
<signal name="N$40">
<contactref element="U1" pad="9"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$42">
<contactref element="U1" pad="11"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="12"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="U1" pad="8"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="U1" pad="20"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U$6" pad="AD0"/>
</signal>
<signal name="N$27">
<contactref element="U$6" pad="RESET#"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U$6" pad="REXT"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="B-GND"/>
<contactref element="U$6" pad="LED15"/>
</signal>
<signal name="N$14">
<contactref element="U$2" pad="G-GND"/>
<contactref element="U$6" pad="LED14"/>
</signal>
<signal name="N$15">
<contactref element="U$2" pad="R-GND"/>
<contactref element="U$6" pad="LED13"/>
</signal>
<signal name="N$16">
<contactref element="U$3" pad="B-GND"/>
<contactref element="U$6" pad="LED12"/>
</signal>
<signal name="N$17">
<contactref element="U$3" pad="G-GND"/>
<contactref element="U$6" pad="LED11"/>
</signal>
<signal name="N$18">
<contactref element="U$3" pad="R-GND"/>
<contactref element="U$6" pad="LED10"/>
</signal>
<signal name="N$19">
<contactref element="U$5" pad="B-GND"/>
<contactref element="U$6" pad="LED9"/>
</signal>
<signal name="N$20">
<contactref element="U$5" pad="G-GND"/>
<contactref element="U$6" pad="LED8"/>
</signal>
<signal name="N$21">
<contactref element="U$5" pad="R-GND"/>
<contactref element="U$6" pad="LED7"/>
</signal>
<signal name="N$22">
<contactref element="U$4" pad="B-GND"/>
<contactref element="U$6" pad="LED6"/>
</signal>
<signal name="N$23">
<contactref element="U$4" pad="G-GND"/>
<contactref element="U$6" pad="LED5"/>
</signal>
<signal name="N$24">
<contactref element="U$4" pad="R-GND"/>
<contactref element="U$6" pad="LED4"/>
</signal>
<signal name="N$25">
<contactref element="ILLUMINATION" pad="B"/>
<contactref element="U$6" pad="LED3"/>
</signal>
<signal name="N$26">
<contactref element="ILLUMINATION" pad="G"/>
<contactref element="U$6" pad="LED1"/>
</signal>
<signal name="N$28">
<contactref element="ILLUMINATION" pad="R"/>
<contactref element="U$6" pad="LED0"/>
</signal>
<signal name="N$9">
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="IGNITION_VOLTAGE" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="SYSTEM_BUS" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="17"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="U$6" pad="VSS_2"/>
<contactref element="U$6" pad="VSS_1"/>
<contactref element="U$6" pad="VSS_0"/>
<contactref element="U$6" pad="OE#"/>
<contactref element="R8" pad="2"/>
<contactref element="IGNITION_VOLTAGE" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
