(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 43)
    (no_connects 2)
    (area 100.504028 67.749928 156.917163 117.8874)
    (thickness 1.6)
    (drawings 5)
    (tracks 146)
    (zones 0)
    (modules 12)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 XTAL)
  (net 3 RESET)
  (net 4 "PIN0(RX)")
  (net 5 "PIN1(TX)")
  (net 6 PIN2)
  (net 7 "PIN3(PWM)")
  (net 8 PIN4)
  (net 9 VCC)
  (net 10 PIN5)
  (net 11 "PIN6(PWM)")
  (net 12 PIN7)
  (net 13 PIN8)
  (net 14 PIN9)
  (net 15 PIN10)
  (net 16 PIN11)
  (net 17 PIN12)
  (net 18 PIN13)
  (net 19 AREF)
  (net 20 A0)
  (net 21 A1)
  (net 22 A2)
  (net 23 A3)
  (net 24 A4)
  (net 25 A5)
  (net 26 "Net-(P1-Pad2)")
  (net 27 "Net-(P1-Pad3)")
  (net 28 "Net-(P2-Pad3)")
  (net 29 "Net-(P2-Pad7)")
  (net 30 "Net-(P2-Pad8)")
  (net 31 "Net-(P2-Pad9)")
  (net 32 "Net-(P2-Pad10)")
  (net 33 +3V3)
  (net 34 "Net-(P3-Pad4)")
  (net 35 "Net-(R2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net AREF)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "PIN0(RX)")
    (add_net "PIN1(TX)")
    (add_net PIN10)
    (add_net PIN11)
    (add_net PIN12)
    (add_net PIN13)
    (add_net PIN2)
    (add_net "PIN3(PWM)")
    (add_net PIN4)
    (add_net PIN5)
    (add_net "PIN6(PWM)")
    (add_net PIN7)
    (add_net PIN8)
    (add_net PIN9)
    (add_net RESET)
    (add_net VCC)
    (add_net XTAL)
  )
  (module Connect:USB_B (layer F.Cu) (tedit 58B9A434)
    (at 142.24 99.695 270)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference P1 (at 11.049 1.27 360) (layer F.SilkS))
    (fp_text value USB_B (at 4.699 1.27 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 4 thru_hole circle (at 1.99898 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.99898 2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P1-Pad3)"))
    (pad 5 thru_hole circle (at 4.699 7.26948 180) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 4.699 -4.72948 180) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Connect.3dshapes/USB_B.wrl
      (at (xyz 0.185 -0.05 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 116.84 101.6)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 XTAL))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 116.84 93.98)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.25 -2.5) (layer F.SilkS))
    (fp_text value 22pF (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 XTAL))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Atmel_By_element14_Batch_1-00:DIP254P762X457-28 (layer F.Cu) (tedit 0)
    (at 132.08 106.68)
    (fp_text reference IC1 (at -8.7376 5.8166) (layer F.SilkS))
    (fp_text value ATMEGA328P-P (at -7.2644 -36.195) (layer F.SilkS))
    (fp_text user * (at -8.2042 -34.1376) (layer F.SilkS))
    (fp_text user * (at -8.2042 -34.1376) (layer Dwgs.User))
    (pad 1 thru_hole rect (at -7.62 -33.02) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 2 thru_hole circle (at -7.62 -30.48) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 4 "PIN0(RX)"))
    (pad 3 thru_hole circle (at -7.62 -27.94) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 5 "PIN1(TX)"))
    (pad 4 thru_hole circle (at -7.62 -25.4) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 6 PIN2))
    (pad 5 thru_hole circle (at -7.62 -22.86) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 7 "PIN3(PWM)"))
    (pad 6 thru_hole circle (at -7.62 -20.32) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 8 PIN4))
    (pad 7 thru_hole circle (at -7.62 -17.78) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 8 thru_hole circle (at -7.62 -15.24) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -7.62 -12.7) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 2 XTAL))
    (pad 10 thru_hole circle (at -7.62 -10.16) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 2 XTAL))
    (pad 11 thru_hole circle (at -7.62 -7.62) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 10 PIN5))
    (pad 12 thru_hole circle (at -7.62 -5.08) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 11 "PIN6(PWM)"))
    (pad 13 thru_hole circle (at -7.62 -2.54) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 12 PIN7))
    (pad 14 thru_hole circle (at -7.62 0) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 13 PIN8))
    (pad 15 thru_hole circle (at 0 0) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 14 PIN9))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 PIN10))
    (pad 17 thru_hole circle (at 0 -5.08) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 16 PIN11))
    (pad 18 thru_hole circle (at 0 -7.62) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 17 PIN12))
    (pad 19 thru_hole circle (at 0 -10.16) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 18 PIN13))
    (pad 20 thru_hole circle (at 0 -12.7) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 21 thru_hole circle (at 0 -15.24) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 19 AREF))
    (pad 22 thru_hole circle (at 0 -17.78) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole circle (at 0 -20.32) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 20 A0))
    (pad 24 thru_hole circle (at 0 -22.86) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 21 A1))
    (pad 25 thru_hole circle (at 0 -25.4) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 22 A2))
    (pad 26 thru_hole circle (at 0 -27.94) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 23 A3))
    (pad 27 thru_hole circle (at 0 -30.48) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 24 A4))
    (pad 28 thru_hole circle (at 0 -33.02) (size 1.6764 1.6764) (drill 1.1176) (layers *.Cu *.Mask)
      (net 25 A5))
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 58C040E8)
    (at 149.86 111.76 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value "CONN_01X16(LCD)" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 PIN4))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 A1))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 A2))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 A3))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 A4))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 A5))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 108.585 91.44)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS))
    (fp_text value "CONN_01X08(RC522)" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 PIN9))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 PIN11))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 PIN12))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 PIN13))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 PIN10))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 121.285 101.6 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012 90) (layer F.SilkS))
    (fp_text value 1M (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 XTAL))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 XTAL))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 144.145 91.44 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.05892 -3.50012 180) (layer F.SilkS))
    (fp_text value 1M (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module Potentiometers:Potentiometer_WirePads_Small (layer F.Cu) (tedit 5446FD75)
    (at 136.525 78.105 90)
    (descr "Potentiometer, Wire Pads only, small, RevA, 02 Aug 2010,")
    (tags "Potentiometer, Wire Pads only, small, RevA, 02 Aug 2010,")
    (fp_text reference RV1 (at 0.0508 -5.95884 90) (layer F.SilkS))
    (fp_text value POT (at -1.34874 10.78992 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.99898 1.99898) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P2-Pad3)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.99898 1.99898) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 0)
    (at 139.7 85.725)
    (fp_text reference SW1 (at 0 -0.762) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 PIN5))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 PIN5))
  )
  (module Regulators:LM3940IT-3.3 (layer F.Cu) (tedit 58B74972)
    (at 112.395 79.375 270)
    (fp_text reference U2 (at 0 0.5 270) (layer F.SilkS))
    (fp_text value LD1117S33TR (at 0 -0.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 12.192 -7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 12.192 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 3 thru_hole circle (at 12.192 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 +3V3))
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 0)
    (at 113.665 98.425 90)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value 16MHz (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (gr_line (start 151.13 72.39) (end 151.13 113.665) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 72.39) (end 151.13 72.39) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 73.025) (end 107.315 72.39) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.315 113.665) (end 107.315 73.025) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.13 113.665) (end 107.315 113.665) (angle 90) (layer Edge.Cuts) (width 0.1))
)
