(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6002)
    (drawings 7)
    (tracks 67)
    (zones 0)
    (modules 6)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Din)
  (net 4 /HV6)
  (net 5 /HV5)
  (net 6 /HV4)
  (net 7 /HV9)
  (net 8 /HV3)
  (net 9 /HV8)
  (net 10 /HV2)
  (net 11 /HV7)
  (net 12 /HV1)
  (net 13 "Net-(LED1-Pad1-DOUT)")
  (net 14 "Net-(NX1-PadP$A)")
  (net 15 "Net-(J1-Pad13)")
  (net 16 "Net-(J1-Pad15)")
  (net 17 /HV0)
  (net 18 "Net-(J1-Pad17)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Din)
    (add_net /HV0)
    (add_net /HV1)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(LED1-Pad1-DOUT)")
    (add_net "Net-(NX1-PadP$A)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 167.02 112.13 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module mynixies:mynixies-CD28 (layer F.Cu) (tedit 200000)
    (at 160.081321 119.539963)
    (attr virtual)
    (fp_text reference NX1 (at -0.49784 -11.99896) (layer F.Fab))
    (fp_text value CD28 (at 0 9.590037) (layer F.SilkS))
    (pad P$A thru_hole circle (at -1.76276 2.4257) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 14 "Net-(NX1-PadP$A)"))
    (pad P$9 thru_hole circle (at -5.93852 -0.8509) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 7 /HV9))
    (pad P$8 thru_hole circle (at -4.5339 -3.92684) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 9 /HV8))
    (pad P$7 thru_hole circle (at -1.69164 -5.75564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 11 /HV7))
    (pad P$6 thru_hole circle (at 1.68656 -5.75564) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 4 /HV6))
    (pad P$5 thru_hole circle (at 4.53136 -3.92938) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 5 /HV5))
    (pad P$4 thru_hole circle (at 5.93852 -0.85344) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 6 /HV4))
    (pad P$3 thru_hole circle (at 5.45592 2.49174) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 8 /HV3))
    (pad P$2 thru_hole circle (at 3.24358 5.04698) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 10 /HV2))
    (pad P$1 thru_hole circle (at 0 5.99948) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 12 /HV1))
    (pad P$0 thru_hole circle (at -5.45592 2.49428) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Mask)
      (net 17 /HV0))
  )
  (module kicad_mpa:Recessed_3535_LED_Cutout (layer F.Cu) (tedit 60398527)
    (at 160.52 118.88 135)
    (fp_text reference LED1 (at -0.085786 2.914213 135) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0 -5.25 135) (layer F.Fab))
    (fp_line (start -2 -2) (end 2 -2) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2 -2) (end 2 2) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2 2) (end -2 2) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -2 2) (end -2 -2) (layer Edge.Cuts) (width 0.15))
    (pad 4-VDD smd rect (at -2.75 1 135) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1-DOUT smd rect (at 2.75 1 135) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(LED1-Pad1-DOUT)"))
    (pad 2-GND smd rect (at 2.75 -1 135) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3-DIN smd rect (at -2.75 -1 135) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /Din))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.02 124.13 225)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43 225) (layer B.Fab))
    (fp_text value 20k (at 0.176777 -1.59099 225) (layer B.SilkS))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad17)"))
    (pad 1 smd roundrect (at -0.7875 0 225) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(NX1-PadP$A)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.52 116.88 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.43 315) (layer B.Fab))
    (fp_text value 0.1uF (at 0 2.096 315) (layer B.Fab))
    (fp_text user %R (at 0 0 315) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x09_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 149.86 136.144 270)
    (descr "Through hole angled pin header, 2x09, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 5.655 2.27 270) (layer B.Fab))
    (fp_text value Clock (at -2.032 -10.16) (layer B.SilkS))
    (fp_text user %R (at 5.31 -10.16) (layer B.Fab))
    (pad 18 thru_hole oval (at 2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad17)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV6))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV5))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV4))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /HV0))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV3))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV9))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV2))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV8))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV1))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV7))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x09_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 160.02 119.38) (end 172.019999 112.268001) (angle -118.6923821) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us CD28,\nGR-707, GR-772" (at 164.52 110.88) (layer B.Mask))
  (gr_line (start 148.02 134.38) (end 148.02 112.268) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 141.38) (end 148.02 134.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.02 134.38) (end 172.02 112.268) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.02 141.38) (end 172.02 134.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 141.38) (end 172.02 141.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 173.355 101.58) (xy 146.685 101.38) (xy 146.02 142.38) (xy 173.62 142.58)
      )
    )
  )
)
