(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 120)
    (no_connects 1)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 5)
    (tracks 487)
    (zones 0)
    (modules 50)
    (nets 75)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 +5V)
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D5-Pad1)")
  (net 5 "Net-(D6-Pad1)")
  (net 6 "Net-(D11-Pad2)")
  (net 7 "Net-(D10-Pad1)")
  (net 8 "Net-(D13-Pad1)")
  (net 9 "Net-(D14-Pad1)")
  (net 10 IN1)
  (net 11 IN8)
  (net 12 IN2)
  (net 13 IN7)
  (net 14 IN3)
  (net 15 IN6)
  (net 16 IN4)
  (net 17 IN5)
  (net 18 NC01)
  (net 19 NC02)
  (net 20 CM01)
  (net 21 CM02)
  (net 22 NO01)
  (net 23 NO02)
  (net 24 NC03)
  (net 25 NC04)
  (net 26 CM03)
  (net 27 CM04)
  (net 28 NO03)
  (net 29 NO04)
  (net 30 NC05)
  (net 31 NC06)
  (net 32 CM05)
  (net 33 CM06)
  (net 34 NO05)
  (net 35 NO06)
  (net 36 NC07)
  (net 37 NC08)
  (net 38 CM07)
  (net 39 CM08)
  (net 40 NO07)
  (net 41 NO08)
  (net 42 NC09)
  (net 43 NC10)
  (net 44 CM09)
  (net 45 CM10)
  (net 46 NO09)
  (net 47 NO10)
  (net 48 NC11)
  (net 49 NC12)
  (net 50 CM11)
  (net 51 CM12)
  (net 52 NO11)
  (net 53 NO12)
  (net 54 NC13)
  (net 55 NC14)
  (net 56 CM13)
  (net 57 CM14)
  (net 58 NO13)
  (net 59 NO14)
  (net 60 NC15)
  (net 61 NC16)
  (net 62 CM15)
  (net 63 CM16)
  (net 64 NO15)
  (net 65 NO16)
  (net 66 "Net-(Q1-Pad1)")
  (net 67 GND)
  (net 68 "Net-(Q2-Pad1)")
  (net 69 "Net-(Q3-Pad1)")
  (net 70 "Net-(Q4-Pad1)")
  (net 71 "Net-(Q5-Pad1)")
  (net 72 "Net-(Q6-Pad1)")
  (net 73 "Net-(Q7-Pad1)")
  (net 74 "Net-(Q8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CM01)
    (add_net CM02)
    (add_net CM03)
    (add_net CM04)
    (add_net CM05)
    (add_net CM06)
    (add_net CM07)
    (add_net CM08)
    (add_net CM09)
    (add_net CM10)
    (add_net CM11)
    (add_net CM12)
    (add_net CM13)
    (add_net CM14)
    (add_net CM15)
    (add_net CM16)
    (add_net IN1)
    (add_net IN2)
    (add_net IN3)
    (add_net IN4)
    (add_net IN5)
    (add_net IN6)
    (add_net IN7)
    (add_net IN8)
    (add_net NC01)
    (add_net NC02)
    (add_net NC03)
    (add_net NC04)
    (add_net NC05)
    (add_net NC06)
    (add_net NC07)
    (add_net NC08)
    (add_net NC09)
    (add_net NC10)
    (add_net NC11)
    (add_net NC12)
    (add_net NC13)
    (add_net NC14)
    (add_net NC15)
    (add_net NC16)
    (add_net NO01)
    (add_net NO02)
    (add_net NO03)
    (add_net NO04)
    (add_net NO05)
    (add_net NO06)
    (add_net NO07)
    (add_net NO08)
    (add_net NO09)
    (add_net NO10)
    (add_net NO11)
    (add_net NO12)
    (add_net NO13)
    (add_net NO14)
    (add_net NO15)
    (add_net NO16)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(Q8-Pad1)")
  )
  (net_class +5V ""
    (clearance 0.5)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class GND ""
    (clearance 0.5)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59658F8D)
    (at 107.75 86.25 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5965BFD9)
    (at 100.25 125.5 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59658F8A)
    (at 105.25 90.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D5-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5965BFDF)
    (at 102.75 121 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59658F90)
    (at 102.75 86.25 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D11-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5965BFDD)
    (at 105 125.5 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 100.25 90.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D13-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5965BFE2)
    (at 107.75 121 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q8-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D14-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965AB3B)
    (at 114.25 100.75 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 1.75 450) (layer F.SilkS))
    (fp_text value GenericGreen (at -6.1 1.7 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965963F)
    (at 142.75 135 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 3 0.25 270) (layer F.SilkS))
    (fp_text value GenericGreen (at -6.25 2 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965AB45)
    (at 114.25 93 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at -0.25 -1.75 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.2 -1.7 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965963B)
    (at 142.75 127 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at -3 -0.75 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.5 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59659D7E)
    (at 114.9 84.1 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at 0.15 2.4 270) (layer F.SilkS))
    (fp_text value GenericGreen (at -7 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965BB02)
    (at 142.85 117.95 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at 0.2 1.8 270) (layer F.SilkS))
    (fp_text value GenericGreen (at -4.25 -0.25 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 59659D7B)
    (at 114.9 75.7 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at 0.7 -2.4 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D5-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965BAEB)
    (at 142.85 110.15 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at -0.2 -1.8 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 5 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965A422)
    (at 142.75 100.75 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D9 (at 0.5 3.75 270) (layer F.SilkS))
    (fp_text value GenericGreen (at 0 1.75 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D11-Pad2)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965AE6B)
    (at 114.375 134.625 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D10 (at 0 1.75 270) (layer F.SilkS))
    (fp_text value GenericGreen (at 0 1.75 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965A3E8)
    (at 142.75 92.75 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D11-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965AE57)
    (at 114.375 127.125 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965A04E)
    (at 143 84.25 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D13 (at 0.25 2.5 270) (layer F.SilkS))
    (fp_text value GenericGreen (at 0 1.75 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5965AB35)
    (at 114.625 118.375 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D14 (at 0.125 1.875 270) (layer F.SilkS))
    (fp_text value GenericGreen (at 7.5 3.25 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965A17C)
    (at 143 76 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D15 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D13-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 5965AADC)
    (at 114.625 110.375 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D16 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D14-Pad1)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x04 (layer F.Cu) (tedit 59658E86)
    (at 104 105.75 180)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P1 (at 6.5 0.25 270) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 0.1 -6.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.81 3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 10 IN1))
    (pad 3 smd rect (at -1.27 3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 12 IN2))
    (pad 5 smd rect (at 1.27 3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 14 IN3))
    (pad 7 smd rect (at 3.81 3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 16 IN4))
    (pad 8 smd rect (at 3.81 -3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 17 IN5))
    (pad 6 smd rect (at 1.27 -3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 15 IN6))
    (pad 4 smd rect (at -1.27 -3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 13 IN7))
    (pad 2 smd rect (at -3.81 -3.2 180) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 11 IN8))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 59649C48)
    (at 133.5 97)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P2 (at 5.2 0.1 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 22 NO01))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 20 CM01))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 18 NC01))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 19 NC02))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 21 CM02))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 23 NO02))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 59659D5D)
    (at 134.25 80)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P3 (at 5.25 0.5 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 28 NO03))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 26 CM03))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 24 NC03))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 25 NC04))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 27 CM04))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 29 NO04))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 5965A1B2)
    (at 161.75 96.75)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P4 (at 5.25 0 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 34 NO05))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 32 CM05))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 30 NC05))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 31 NC06))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 33 CM06))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 35 NO06))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 59659936)
    (at 162.25 80)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P5 (at 5.25 -0.25 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 40 NO07))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 38 CM07))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 36 NC07))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 37 NC08))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 39 CM08))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 41 NO08))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 5965BCF2)
    (at 161.75 131)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P6 (at 5.25 0.25 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 46 NO09))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 44 CM09))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 42 NC09))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 43 NC10))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 45 CM10))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 47 NO10))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 59659786)
    (at 162 114.25)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P7 (at 5.25 -0.25 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 52 NO11))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 50 CM11))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 48 NC11))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 49 NC12))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 51 CM12))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 53 NO12))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 5965BCFA)
    (at 133.875 131.125)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P8 (at 5.125 0.375 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 58 NO13))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 56 CM13))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 54 NC13))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 55 NC14))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 57 CM14))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 59 NO14))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_SMT_02x03 (layer F.Cu) (tedit 5965AA4B)
    (at 133.875 114.375)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference P9 (at 5.25 -0.25 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0.1 -6.55) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 64 NO15))
    (pad 3 smd rect (at 0 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 62 CM15))
    (pad 5 smd rect (at 2.54 3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 60 NC15))
    (pad 6 smd rect (at 2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 61 NC16))
    (pad 4 smd rect (at 0 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 63 CM16))
    (pad 2 smd rect (at -2.54 -3.2) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 65 NO16))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59658F1A)
    (at 107.75 96 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.5 -1.25 360) (layer F.SilkS))
    (fp_text value 22k (at 2.25 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 IN1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5965BFF8)
    (at 100.25 115.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 IN5))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59658F2E)
    (at 105.25 96 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.5 -1.25 540) (layer F.SilkS))
    (fp_text value 22k (at 2.25 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 IN2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5965BFF4)
    (at 102.75 115.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 IN6))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59658FA8)
    (at 102.75 96 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.5 -1.25 360) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 IN3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5965BFEF)
    (at 105.25 115.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 IN7))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59658FA2)
    (at 100.25 96 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.5 -1.25 360) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 IN4))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5965BFE7)
    (at 107.75 115.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 22k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(Q8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 IN8))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD locked (layer F.Cu) (tedit 59659B3B)
    (at 122.125 97.125 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL1 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at -0.125 7.625 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 18 NC01))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 23 NO02))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 20 CM01))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 21 CM02))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 22 NO01))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 19 NC02))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965BCE2)
    (at 150.5 131 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL2 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 42 NC09))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 47 NO10))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 44 CM09))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 45 CM10))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 46 NO09))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 43 NC10))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 59659D39)
    (at 122.855 79.974999 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL3 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 24 NC03))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 29 NO04))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 26 CM03))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 27 CM04))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 28 NO03))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 25 NC04))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 4 "Net-(D5-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965BACC)
    (at 150.75 114.25 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL4 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 48 NC11))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 53 NO12))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 50 CM11))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 51 CM12))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 52 NO11))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 49 NC12))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 5 "Net-(D6-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965A1A4)
    (at 150.5 96.75 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL5 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 30 NC05))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 35 NO06))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 32 CM05))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 33 CM06))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 34 NO05))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 31 NC06))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 6 "Net-(D11-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965AE77)
    (at 122.375 131.125 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL6 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 54 NC13))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 59 NO14))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 56 CM13))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 57 CM14))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 58 NO13))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 55 NC14))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965A052)
    (at 150.75 80 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL7 (at 0.25 -7.25 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 36 NC07))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 41 NO08))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 38 CM07))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 39 CM08))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 40 NO07))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 37 NC08))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 8 "Net-(D13-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-10_W9.53mm_SMD (layer F.Cu) (tedit 5965AA44)
    (at 122.525 114.325 90)
    (descr "10-lead dip package, row spacing 9.53 mm (375 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 9.53mm 375mil SMD")
    (attr smd)
    (fp_text reference RL8 (at 0 -7.47 90) (layer F.SilkS))
    (fp_text value G6H-2 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 60 NC15))
    (pad 7 smd rect (at 4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 65 NO16))
    (pad 3 smd rect (at -4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 62 CM15))
    (pad 8 smd rect (at 4.765 0 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 63 CM16))
    (pad 4 smd rect (at -4.765 2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 64 NO15))
    (pad 9 smd rect (at 4.765 -2.54 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 61 NC16))
    (pad 5 smd rect (at -4.765 5.08 90) (size 2 1.78) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 4.765 -5.08 90) (size 2 1.78) (layers F.Cu F.Mask)
      (net 9 "Net-(D14-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-10_W9.53mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5965AE41)
    (at 100.25 73.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 2.75 1.5 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 95.5 142) (end 95.5 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5 142) (end 95.5 142) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5 140) (end 169.5 142) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5 70) (end 169.5 140) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.5 70) (end 169.5 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 67) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110 80.25) (xy 110 128) (xy 97 128) (xy 97 75.25) (xy 105 75.25)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166 137.5) (xy 111.75 137.5) (xy 111.75 80.25) (xy 106 74.75) (xy 97 74.75)
        (xy 97 71.25) (xy 166 71.25)
      )
    )
  )
)
