(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 87)
    (no_connects 0)
    (area 149.911999 61.951799 185.622001 135.761801)
    (thickness 1.6)
    (drawings 97)
    (tracks 337)
    (zones 0)
    (modules 49)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 /sig4)
  (net 2 GND)
  (net 3 /sig2)
  (net 4 /sig1)
  (net 5 /sig3)
  (net 6 /sig8)
  (net 7 /sig6)
  (net 8 /sig5)
  (net 9 /sig7)
  (net 10 +5V)
  (net 11 /sig3_isolated)
  (net 12 /bec_esc_1)
  (net 13 /sig4_isolated)
  (net 14 /sig2_isolated)
  (net 15 /sig1_isolated)
  (net 16 /bec_gnd_1)
  (net 17 /sig7_isolated)
  (net 18 /bec_esc_2)
  (net 19 /sig8_isolated)
  (net 20 /sig6_isolated)
  (net 21 /sig5_isolated)
  (net 22 /bec_gnd_2)
  (net 23 /t1)
  (net 24 /t2)
  (net 25 /t3)
  (net 26 /t4)
  (net 27 /sig1_in)
  (net 28 /sig2_in)
  (net 29 /sig3_in)
  (net 30 /sig4_in)
  (net 31 /sig5_in)
  (net 32 /sig6_in)
  (net 33 /sig7_in)
  (net 34 /sig8_in)
  (net 35 "Net-(P1-Pad3)")
  (net 36 "Net-(P1-Pad4)")
  (net 37 "Net-(P1-Pad5)")
  (net 38 "Net-(P1-Pad6)")
  (net 39 "Net-(P1-Pad7)")
  (net 40 "Net-(U1-Pad6)")
  (net 41 "Net-(U1-Pad7)")
  (net 42 "Net-(U1-Pad10)")
  (net 43 "Net-(U1-Pad11)")
  (net 44 "Net-(U2-Pad6)")
  (net 45 "Net-(U2-Pad7)")
  (net 46 "Net-(U2-Pad10)")
  (net 47 "Net-(U2-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /bec_esc_1)
    (add_net /bec_esc_2)
    (add_net /bec_gnd_1)
    (add_net /bec_gnd_2)
    (add_net /sig1)
    (add_net /sig1_in)
    (add_net /sig1_isolated)
    (add_net /sig2)
    (add_net /sig2_in)
    (add_net /sig2_isolated)
    (add_net /sig3)
    (add_net /sig3_in)
    (add_net /sig3_isolated)
    (add_net /sig4)
    (add_net /sig4_in)
    (add_net /sig4_isolated)
    (add_net /sig5)
    (add_net /sig5_in)
    (add_net /sig5_isolated)
    (add_net /sig6)
    (add_net /sig6_in)
    (add_net /sig6_isolated)
    (add_net /sig7)
    (add_net /sig7_in)
    (add_net /sig7_isolated)
    (add_net /sig8)
    (add_net /sig8_in)
    (add_net /sig8_isolated)
    (add_net /t1)
    (add_net /t2)
    (add_net /t3)
    (add_net /t4)
    (add_net GND)
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 58C1AE33)
    (at 153.162 111.5568)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module robosub_footprints:robosub_logo-medium (layer F.Cu) (tedit 0)
    (at 175.8442 117.983)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 58222436)
    (at 153.57602 91.567)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P1-Pad7)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223DF)
    (at 173.15602 92.532 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /t1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223DD)
    (at 173.15602 95.072 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /t2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223DA)
    (at 173.15602 100.152 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /t3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223F7)
    (at 173.15602 107.772 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /sig7))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223F5)
    (at 173.15602 105.232 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /sig8))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223E9)
    (at 173.15602 84.912 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /sig2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223ED)
    (at 173.15602 82.372 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /sig1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223F1)
    (at 173.15602 102.692 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /t4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223E6)
    (at 173.15602 87.452 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P10 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /sig3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223E2)
    (at 173.15602 89.992 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /sig4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223FD)
    (at 173.15602 112.852 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P12 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /sig5))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5822240B)
    (at 173.15602 110.312 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P13 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /sig6))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer B.Cu) (tedit 574D979F)
    (at 161.73704 88.1634 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 6 90) (layer B.SilkS))
    (fp_text value Si866x (at 0 -6 90) (layer B.Fab))
    (pad 1 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /sig4_in))
    (pad 3 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /sig3_in))
    (pad 4 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /sig2_in))
    (pad 5 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 /sig1_in))
    (pad 6 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /bec_gnd_1))
    (pad 10 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 /sig1_isolated))
    (pad 13 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 /sig2_isolated))
    (pad 14 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /sig3_isolated))
    (pad 15 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /sig4_isolated))
    (pad 16 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /bec_esc_1))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer B.Cu) (tedit 574D979F)
    (at 162.98418 108.20402 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 6 270) (layer B.SilkS))
    (fp_text value Si866x (at 0 -6 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 /sig5_in))
    (pad 3 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 32 /sig6_in))
    (pad 4 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 /sig7_in))
    (pad 5 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 /sig8_in))
    (pad 6 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 22 /bec_gnd_2))
    (pad 10 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /sig8_isolated))
    (pad 13 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /sig7_isolated))
    (pad 14 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 /sig6_isolated))
    (pad 15 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /sig5_isolated))
    (pad 16 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /bec_esc_2))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 582223D7)
    (at 173.15602 97.612 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P16 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222433)
    (at 157.48 84.201 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /sig1_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /sig1))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222430)
    (at 160.528 84.201 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /sig2_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /sig2))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5822242D)
    (at 163.322 84.201 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /sig3_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /sig3))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5822242B)
    (at 165.989 84.244 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /sig4_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /sig4))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222411)
    (at 158.623 111.082 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /sig5_in))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /sig5))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5822240E)
    (at 161.544 111.082 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /sig6_in))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /sig6))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222408)
    (at 164.592 111.082 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /sig7_in))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /sig7))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222404)
    (at 167.259 111.082 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /sig8_in))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /sig8))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222427)
    (at 157.48 92.118 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /t1))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /sig1_in))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222422)
    (at 160.528 92.075 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /t2))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /sig2_in))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222424)
    (at 163.322 92.075 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /t3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /sig3_in))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222452)
    (at 165.989 92.075 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 16.299 -3.302 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /t4))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /sig4_in))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5822241D)
    (at 158.623 104.183 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /sig5_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /t1))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5822241B)
    (at 161.544 104.183 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /sig6_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /t2))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222418)
    (at 164.592 104.14 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /sig7_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /t3))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58222416)
    (at 167.259 104.14 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /sig8_in))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /t4))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222461)
    (at 152.6032 64.4652)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W1 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /sig1_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5822245E)
    (at 155.6512 64.4652)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /sig2_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5822245B)
    (at 158.8262 64.4652)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W3 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /sig3_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222459)
    (at 161.8742 64.4652)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W4 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /sig4_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222470)
    (at 152.781 132.08)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W5 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /sig5_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5822246E)
    (at 155.829 132.08)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W6 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /sig6_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5822246C)
    (at 158.623 132.08)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W7 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /sig7_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5822246A)
    (at 161.544 132.08)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W8 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /sig8_isolated))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222463)
    (at 152.7302 71.2216)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W9 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /bec_esc_1))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222472)
    (at 152.781 124.968)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W10 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /bec_esc_2))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222466)
    (at 152.6794 75.5142)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W11 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /bec_gnd_1))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 58222474)
    (at 152.781 118.872)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference W12 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /bec_gnd_2))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 58C1AE35)
    (at 153.162 86.1568)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MaestroJSTConnector:JST_PUD (layer F.Cu) (tedit 5AF299EF)
    (at 176.657 73.533 180)
    (fp_text reference P14 (at 2.5 3 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at -3.5 3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -3 1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 /bec_gnd_1))
    (pad 3 thru_hole circle (at -1 1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 /bec_esc_1))
    (pad 5 thru_hole circle (at 1 1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 /sig4_isolated))
    (pad 7 thru_hole circle (at 3 1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -3 -1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 /sig2_isolated))
    (pad 4 thru_hole circle (at -1 -1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 /sig1_isolated))
    (pad 6 thru_hole circle (at 1 -1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 /sig3_isolated))
    (pad 8 thru_hole circle (at 3 -1 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module MaestroJSTConnector:JST_PUD (layer F.Cu) (tedit 5AF299EF)
    (at 176.53 123.19)
    (fp_text reference P15 (at 2.5 3) (layer F.SilkS))
    (fp_text value CONN_01X06 (at -3.5 3) (layer F.Fab))
    (pad 1 thru_hole rect (at -3 1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 22 /bec_gnd_2))
    (pad 3 thru_hole circle (at -1 1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 18 /bec_esc_2))
    (pad 5 thru_hole circle (at 1 1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 /sig5_isolated))
    (pad 7 thru_hole circle (at 3 1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -3 -1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 /sig6_isolated))
    (pad 4 thru_hole circle (at -1 -1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 /sig8_isolated))
    (pad 6 thru_hole circle (at 1 -1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 /sig7_isolated))
    (pad 8 thru_hole circle (at 3 -1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 149.987 135.6868) (end 185.547 135.6868) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.547 135.6868) (end 185.547 62.0268) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.547 62.0268) (end 149.987 62.0268) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.987 62.0268) (end 149.987 135.6868) (layer Edge.Cuts) (width 0.15))
  (gr_text 4 (at 161.8742 66.2432 90) (layer F.SilkS))
  (gr_text 3 (at 158.8262 66.2432 90) (layer F.SilkS))
  (gr_text 2 (at 155.6512 66.2432 90) (layer F.SilkS))
  (gr_text 1 (at 152.6032 66.2432 90) (layer F.SilkS))
  (gr_text "Iso TP" (at 153.8732 68.0212) (layer F.SilkS))
  (gr_text "Iso TP" (at 155.448 128.27) (layer F.SilkS))
  (gr_text 8 (at 161.544 130.429 90) (layer F.SilkS))
  (gr_text 7 (at 158.623 130.429 90) (layer F.SilkS))
  (gr_text 6 (at 155.829 130.302 90) (layer F.SilkS))
  (gr_text 5 (at 152.781 130.302 90) (layer F.SilkS))
  (gr_text "BEC PWR 1" (at 158.369 124.968) (layer F.SilkS))
  (gr_text "BEC PWR 1" (at 158.3182 71.2216) (layer F.SilkS))
  (gr_text "BEC GND 1" (at 158.2674 75.6412) (layer F.SilkS))
  (gr_text "BEC GND 2" (at 158.242 118.872) (layer F.SilkS))
  (gr_text "Maestro Adapter\nBen Songras\nMay '18 - RevC" (at 183.4007 66.4718) (layer B.SilkS))
  (gr_text 11 (at 157.607 114.7064) (layer F.SilkS))
  (gr_text 10 (at 161.544 114.681) (layer F.SilkS))
  (gr_text 9 (at 164.5666 114.7318) (layer F.SilkS))
  (gr_text 8 (at 167.259 114.681) (layer F.SilkS))
  (gr_text 3 (at 166.116 80.645) (layer F.SilkS))
  (gr_text 2 (at 163.322 80.645) (layer F.SilkS))
  (gr_text 1 (at 160.528 80.645) (layer F.SilkS))
  (gr_text 0 (at 157.48 80.645) (layer F.SilkS))
  (gr_text 4 (at 158.496 100.838) (layer F.SilkS))
  (gr_text 4 (at 157.48 95.631) (layer F.SilkS))
  (gr_text 5 (at 160.528 95.631) (layer F.SilkS))
  (gr_text 5 (at 161.417 100.711) (layer F.SilkS))
  (gr_text 6 (at 164.592 100.711) (layer F.SilkS))
  (gr_text 6 (at 163.449 95.631) (layer F.SilkS))
  (gr_text 7 (at 165.989 95.631) (layer F.SilkS))
  (gr_text 7 (at 167.132 100.711) (layer F.SilkS))
  (gr_text sig8 (at 167.132 107.569 90) (layer F.SilkS))
  (gr_text sig7 (at 164.592 107.696 90) (layer F.SilkS))
  (gr_text sig6 (at 161.544 107.696 90) (layer F.SilkS))
  (gr_text sig5 (at 158.623 107.569 90) (layer F.SilkS))
  (gr_text sig4 (at 165.862 88.138 90) (layer F.SilkS))
  (gr_text sig3 (at 163.195 88.138 90) (layer F.SilkS))
  (gr_text sig1 (at 157.353 88.011 90) (layer F.SilkS))
  (gr_text sig2 (at 160.401 88.138 90) (layer F.SilkS))
  (gr_text 11 (at 181.61 112.776) (layer F.SilkS))
  (gr_text 10 (at 181.61 110.363) (layer F.SilkS))
  (gr_text 9 (at 181.61 107.823) (layer F.SilkS))
  (gr_text 8 (at 181.61 105.156) (layer F.SilkS))
  (gr_text 7 (at 181.61 102.743) (layer F.SilkS))
  (gr_text 6 (at 181.61 100.203) (layer F.SilkS))
  (gr_text 5V (at 181.61 97.663) (layer F.SilkS))
  (gr_text 5 (at 181.61 94.996) (layer F.SilkS))
  (gr_text 4 (at 181.61 92.456) (layer F.SilkS))
  (gr_text 3 (at 181.61 89.916) (layer F.SilkS))
  (gr_text 2 (at 181.61 87.376) (layer F.SilkS))
  (gr_text 1 (at 181.61 84.963) (layer F.SilkS))
  (gr_text 0 (at 181.483 82.55) (layer F.SilkS))
)
