(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 10)
    (area 101.524999 63.424999 157.555001 129.615001)
    (thickness 1.6)
    (drawings 45)
    (tracks 697)
    (zones 0)
    (modules 89)
    (nets 68)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2286)
    (user_trace_width 0.2286)
    (user_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.254)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFDE79)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 +12V)
  (net 9 +5V)
  (net 10 "Net-(C11-Pad1)")
  (net 11 +1V5)
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(D6-Pad2)")
  (net 18 "Net-(D6-Pad1)")
  (net 19 /3_SCL)
  (net 20 /PS0_3V)
  (net 21 /PS1_3V)
  (net 22 /2_SDA)
  (net 23 "Net-(G1-Pad7)")
  (net 24 "Net-(G1-Pad8)")
  (net 25 /INT_3V)
  (net 26 /I2CADDR_3V)
  (net 27 "Net-(J1-Pad9)")
  (net 28 "Net-(J1-Pad8)")
  (net 29 "Net-(J1-Pad1)")
  (net 30 /5)
  (net 31 /MOSI)
  (net 32 /SCK)
  (net 33 /MISO)
  (net 34 "Net-(J1-Pad10)")
  (net 35 /INT1)
  (net 36 /KillSW_Batt_12V)
  (net 37 /12)
  (net 38 /1)
  (net 39 /0)
  (net 40 /A5)
  (net 41 /A4)
  (net 42 /A3)
  (net 43 /A2)
  (net 44 /A1)
  (net 45 /A0)
  (net 46 /AREF)
  (net 47 /RST)
  (net 48 /6)
  (net 49 /11)
  (net 50 /10)
  (net 51 /13)
  (net 52 VBAT)
  (net 53 /9_UART_RXD)
  (net 54 "Net-(Q1-Pad1)")
  (net 55 "Net-(Q3-Pad1)")
  (net 56 "Net-(U1-Pad1)")
  (net 57 "Net-(U1-Pad2)")
  (net 58 "Net-(C14-Pad2)")
  (net 59 "Net-(C15-Pad2)")
  (net 60 "Net-(C16-Pad2)")
  (net 61 "Net-(C17-Pad2)")
  (net 62 /RightMotorHi)
  (net 63 /RightMotorLow)
  (net 64 /LeftMotorHi)
  (net 65 /LeftMotorLow)
  (net 66 /EN)
  (net 67 "Net-(J6-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.254)
    (uvia_drill 0)
    (add_net +12V)
    (add_net +1V5)
    (add_net +3V3)
    (add_net +5V)
    (add_net /0)
    (add_net /1)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /2_SDA)
    (add_net /3_SCL)
    (add_net /5)
    (add_net /6)
    (add_net /9_UART_RXD)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /EN)
    (add_net /I2CADDR_3V)
    (add_net /INT1)
    (add_net /INT_3V)
    (add_net /KillSW_Batt_12V)
    (add_net /LeftMotorHi)
    (add_net /LeftMotorLow)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PS0_3V)
    (add_net /PS1_3V)
    (add_net /RST)
    (add_net /RightMotorHi)
    (add_net /RightMotorLow)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(G1-Pad7)")
    (add_net "Net-(G1-Pad8)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net VBAT)
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A8B79F8)
    (at 142.494 107.696 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 0 1.65 90) (layer B.Fab))
    (fp_text value 4.7k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C16-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 44 /A1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_3001_1x12mm-CoinCell (layer F.Cu) (tedit 5A88A837)
    (at 124.46 71.12 180)
    (descr http://www.keyelco.com/product-pdf.cfm?p=778)
    (tags "Keystone type 3001 coin cell retainer")
    (fp_text reference BT1 (at 0 -8 180) (layer F.Fab))
    (fp_text value CR1220 (at 0 7.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.6 0 180) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 6.6 0 180) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 4 4) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Battery_Holders.3dshapes/Keystone_3001_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0.11))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A88A7D8)
    (at 123.825 109.855 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 7pF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A88A7D4)
    (at 123.825 111.125 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 7pF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A88A811)
    (at 117.602 98.552 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A88A81D)
    (at 117.602 91.694 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5A88A823)
    (at 128.016 84.836)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.5) (layer B.Fab))
    (fp_text value 0.33uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A88A9EE)
    (at 130.302 88.138 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 4.7uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 +12V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A88A9F1)
    (at 130.302 90.424 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 4.7uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A88AA0B)
    (at 129.54 94.742)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5) (layer F.Fab))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A88AA07)
    (at 132.334 97.536 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.5 270) (layer F.Fab))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A88A9FD)
    (at 129.54 99.822)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.5) (layer F.Fab))
    (fp_text value 4.7uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A88A84B)
    (at 153.67 83.185 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 180) (layer F.Fab))
    (fp_text value 12V_LED (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A88A850)
    (at 153.67 85.09 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 180) (layer F.Fab))
    (fp_text value 5V_LED (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A88A856)
    (at 153.67 86.995 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 180) (layer F.Fab))
    (fp_text value 3V3_LED (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A88A85A)
    (at 153.67 88.9 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 180) (layer F.Fab))
    (fp_text value 1V5_LED (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A88A85D)
    (at 153.67 90.805 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.45 180) (layer F.Fab))
    (fp_text value SD_LED (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_LGA:LGA-28_5.2x3.8mm_Pitch0.5mm (layer F.Cu) (tedit 5A88A7CF)
    (at 123.19 106.68 180)
    (descr "LGA 28 5.2x3.8mm Pitch 0.5mm")
    (tags "LGA 28 5.2x3.8mm Pitch 0.5mm")
    (attr smd)
    (fp_text reference G1 (at 0 -3.25 180) (layer F.Fab))
    (fp_text value BNO055 (at 0 3.3 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 19 smd rect (at 2.3875 -0.75 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 19 /3_SCL))
    (pad 6 smd rect (at -2.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 20 /PS0_3V))
    (pad 2 smd rect (at -2.3875 -0.75 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.3875 -0.25 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -2.3875 0.25 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -2.3875 0.75 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 21 /PS1_3V))
    (pad 28 smd rect (at -1.75 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 27 smd rect (at -1.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 26 smd rect (at -0.75 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 25 smd rect (at -0.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 0.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 0.75 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.75 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.25 -1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 22 /2_SDA))
    (pad 7 smd rect (at -1.75 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(G1-Pad7)"))
    (pad 8 smd rect (at -1.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(G1-Pad8)"))
    (pad 9 smd rect (at -0.75 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 10 smd rect (at -0.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 0.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 12 smd rect (at 0.75 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.75 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 25 /INT_3V))
    (pad 15 smd rect (at 2.25 1.6625 180) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 2.3875 -0.25 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.3875 0.25 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 26 /I2CADDR_3V))
    (pad 16 smd rect (at 2.3875 0.75 270) (size 0.254 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_LGA.3dshapes/BNO055.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Card:Hirose_DM3AT-SF-PEJM5 (layer F.Cu) (tedit 5A88A7C7)
    (at 126.365 113.884)
    (descr "Micro SD, SMD, right-angle, push-pull (https://www.hirose.com/product/en/download_file/key_name/DM3AT-SF-PEJM5/category/Drawing%20(2D)/doc_file_id/44099/?file_category_id=6&item_id=06090031000&is_series=)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J1 (at -2.85 -2.4) (layer F.Fab))
    (fp_text value Micro_SD_Card_Det_Hirose_DM3AT (at -2.85 16.7) (layer F.Fab))
    (fp_text user KEEPOUT (at -3.85 5.2) (layer Cmts.User))
    (fp_text user %R (at -2.85 7.5) (layer F.Fab))
    (fp_text user KEEPOUT (at 1.425 14.775) (layer Cmts.User))
    (fp_text user KEEPOUT (at -9.625 3.875 90) (layer Cmts.User))
    (fp_text user KEEPOUT (at -8.55 9.5 90) (layer Cmts.User))
    (pad 9 smd rect (at -8.65 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at -7.7 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad8)"))
    (pad 1 smd rect (at 0 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.1 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /5))
    (pad 3 smd rect (at -2.2 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /MOSI))
    (pad 4 smd rect (at -3.3 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -4.4 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /SCK))
    (pad 6 smd rect (at -5.5 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -6.6 -0.6) (size 0.7 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /MISO))
    (pad 11 smd rect (at 1.55 -0.6) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -9.6 3.7) (size 1 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -9.6 9.9) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at -9.6 14.05) (size 1 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 3.9 14.5) (size 1.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Card.3dshapes/Hirose_DM3AT-SF-PEJM5.wrl
      (at (xyz -6.7125 -6.4375 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5ABD2C50)
    (at 125.476 98.806)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value INT1 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /INT1))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x16_Pitch2.54mm locked (layer F.Cu) (tedit 5A88A7C1)
    (at 114.3 111.76 180)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer F.Fab))
    (fp_text value Conn_01x16 (at 0 40.43 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /12))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /0))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /MISO))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SCK))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /A5))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /A4))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /A3))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /A2))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /A1))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /A0))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /AREF))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /RST))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5A88A78E)
    (at 106.68 81.915 180)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 4.385 -2.27 180) (layer F.Fab))
    (fp_text value stairSensor (at 4.385 9.89 180) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /A3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J6-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A88A77D)
    (at 106.68 109.22 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 4.385 -2.27 180) (layer F.Fab))
    (fp_text value NeoPixel (at 4.385 7.35 180) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /A5))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5A88A785)
    (at 106.68 97.79 180)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 4.385 -2.27 180) (layer F.Fab))
    (fp_text value Relay (at 4.385 9.89 180) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /A4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /A4))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12_Pitch2.54mm locked (layer F.Cu) (tedit 5A88A82D)
    (at 134.62 83.82)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.Fab))
    (fp_text value Conn_01x12 (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 VBAT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /EN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /13))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /12))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /11))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /10))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /9_UART_RXD))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /3_SCL))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /2_SDA))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A88A7DF)
    (at 119.126 105.41)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference JP1 (at 0 -1.35) (layer F.Fab))
    (fp_text value Addr (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I2CADDR_3V))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A88A9E1)
    (at 141.224 83.82)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5) (layer B.Fab))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5A88A9D8)
    (at 141.224 86.995)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 2.5) (layer B.Fab))
    (fp_text value Q_NPN_BEC (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A818)
    (at 117.602 95.25 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 270) (layer F.Fab))
    (fp_text value 1k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A7FC)
    (at 127.508 102.616 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 180) (layer F.Fab))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /PS0_3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A7F7)
    (at 127.508 104.394 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 180) (layer F.Fab))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /PS1_3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A7E4)
    (at 119.126 107.696 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.Fab))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /I2CADDR_3V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9EA)
    (at 151.13 83.185 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 500 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A8A7)
    (at 131.445 106.045)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.Fab))
    (fp_text value 4.7k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /3_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A8AB)
    (at 131.445 107.95)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65) (layer F.Fab))
    (fp_text value 4.7k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /2_SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9E4)
    (at 151.13 85.09 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A949)
    (at 143.764 103.378)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.65) (layer B.Fab))
    (fp_text value 49.9k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 64 /LeftMotorHi))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A8EA)
    (at 143.764 110.49)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.65) (layer B.Fab))
    (fp_text value 49.9k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C16-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 62 /RightMotorHi))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9DD)
    (at 151.13 86.995 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 65 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A8E6)
    (at 143.764 98.044 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 49.9k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 65 /LeftMotorLow))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A8D4)
    (at 143.764 105.156 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 49.9k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 63 /RightMotorLow))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A8AF)
    (at 131.445 111.76)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.65) (layer F.Fab))
    (fp_text value 910k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /A2))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /KillSW_Batt_12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5ABD2EB6)
    (at 138.684 83.82 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value 1k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A88A8C4)
    (at 131.445 109.855)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.65) (layer F.Fab))
    (fp_text value 200k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /A2))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A934)
    (at 142.494 100.711 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 1.65 90) (layer B.Fab))
    (fp_text value 4.7k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A8D9)
    (at 140.462 98.044)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.65) (layer B.Fab))
    (fp_text value 4.7k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9D4)
    (at 151.13 88.9 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9C5)
    (at 138.684 86.995 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 1.65 270) (layer B.Fab))
    (fp_text value 1k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 /SCK))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A88A9CC)
    (at 151.13 90.805 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 0 1.65 180) (layer B.Fab))
    (fp_text value 150 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A88A815)
    (at 121.412 96.52 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5 90) (layer F.Fab))
    (fp_text value PCF8523 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /2_SDA))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /3_SCL))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /INT1))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353_SC-70-5 (layer B.Cu) (tedit 5A8B81C0)
    (at 139.954 100.711)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (attr smd)
    (fp_text reference U2 (at 0 2) (layer B.Fab))
    (fp_text value LMV321LICT (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(C15-Pad2)"))
    (pad 3 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 45 /A0))
    (pad 5 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353_SC-70-5 (layer B.Cu) (tedit 5A88A8F0)
    (at 139.954 107.696)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (attr smd)
    (fp_text reference U3 (at 0 2) (layer B.Fab))
    (fp_text value LMV321LICT (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C17-Pad2)"))
    (pad 3 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C16-Pad2)"))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 44 /A1))
    (pad 5 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2_Rectifier (layer F.Cu) (tedit 5A88A829)
    (at 123.698 82.55 180)
    (descr TO-252-2)
    (tags "TO-252-2 Rectifier")
    (attr smd)
    (fp_text reference U4 (at -0.575 -4.55 180) (layer F.Fab))
    (fp_text value L7805 (at -0.625 4.8 180) (layer F.Fab))
    (fp_text user %R (at -0.05 0 180) (layer F.Fab))
    (pad 1 smd rect (at -4.575 -2.3 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +12V))
    (pad 3 smd rect (at -4.575 2.28 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 2.825 0 90) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A88A9C0)
    (at 129.54 97.028 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U6 (at 0 -2.9 180) (layer F.Fab))
    (fp_text value LP2985LV (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +1V5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_SeikoEpson_MC146-4pin_6.7x1.5mm (layer F.Cu) (tedit 5A88A7CB)
    (at 122.555 110.49 180)
    (descr "SMD Crystal Seiko Epson MC-146 https://support.epson.biz/td/api/doc_check.php?dl=brief_MC-156_en.pdf, 6.7x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -1.95 180) (layer F.Fab))
    (fp_text value 32.768kHz (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.15 0.45 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 3.15 0.45 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3.15 -0.45 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -3.15 -0.45 180) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_SeikoEpson_MC146-4pin_6.7x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_SeikoEpson_MC146-4pin_6.7x1.5mm (layer F.Cu) (tedit 5ABD2E9F)
    (at 121.666 101.346)
    (descr "SMD Crystal Seiko Epson MC-146 https://support.epson.biz/td/api/doc_check.php?dl=brief_MC-156_en.pdf, 6.7x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y2 (at 0 -1.95) (layer F.SilkS) hide)
    (fp_text value 32.768kHz (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.15 0.45) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 3.15 0.45) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 3.15 -0.45) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -3.15 -0.45) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_SeikoEpson_MC146-4pin_6.7x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A8B7A10)
    (at 144.399 100.711 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 1.5 270) (layer B.Fab))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 45 /A0))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A8B7A92)
    (at 140.462 103.378 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 0.1uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A8B81BB)
    (at 144.399 107.696 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 1.5 270) (layer B.Fab))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 44 /A1))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(C16-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5A8B81B3)
    (at 140.208 110.49 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 1.5 180) (layer B.Fab))
    (fp_text value 0.1uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5ABD2ED4)
    (at 140.462 105.156)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 0 1.65) (layer B.SilkS) hide)
    (fp_text value 4.7k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 +1V5))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5A8DD45E)
    (at 106.68 68.58)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference W1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mount1 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5A8DD469)
    (at 106.68 124.46)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference W2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mount2 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5A8DD45A)
    (at 152.4 68.58)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference W3 (at 0 -4.2) (layer F.Fab) hide)
    (fp_text value Mount4 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5A8DD464)
    (at 152.4 124.46)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference W4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mount3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A8C49E3)
    (at 127.254 107.442 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A8C49DB)
    (at 122.428 103.378 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5ABD2EC5)
    (at 128.27 80.264)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module phoenix_push_term_block:1862071_5pos_term_block (layer F.Cu) (tedit 5ABBECA6)
    (at 147.32 104.775 90)
    (fp_text reference J3 (at 0 11.684 90) (layer F.Fab))
    (fp_text value Analog_IN (at 0 10 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -7 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 /KillSW_Batt_12V))
    (pad 2 thru_hole circle (at -3.5 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 /RightMotorHi))
    (pad 3 thru_hole circle (at 0 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 /RightMotorLow))
    (pad 4 thru_hole circle (at 3.5 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 /LeftMotorHi))
    (pad 5 thru_hole circle (at 7 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 /LeftMotorLow))
    (pad "" np_thru_hole circle (at -7 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.5 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module phoenix_push_term_block:1862042_2pos_term_block (layer F.Cu) (tedit 5ABBED8F)
    (at 147.32 76.835 90)
    (fp_text reference J4 (at 0 11.684 90) (layer F.Fab))
    (fp_text value "Batt. Conn" (at 0 10 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.75 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.75 5 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 +12V))
    (pad "" np_thru_hole circle (at -1.75 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.75 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B0C)
    (at 154.94 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP1 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value LML (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 65 /LeftMotorLow))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B06)
    (at 153.035 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP2 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value LMH (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 64 /LeftMotorHi))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2AFD)
    (at 151.13 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP3 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value RML (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 63 /RightMotorLow))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2AEB)
    (at 149.225 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP4 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value RMH (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 62 /RightMotorHi))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2AE4)
    (at 147.32 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP5 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value KillSW (at 0 3.175 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 36 /KillSW_Batt_12V))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B1B)
    (at 145.415 83.185)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP6 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value +12v (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2BED)
    (at 111.76 86.36)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP7 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value RightMotor (at -5.715 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 44 /A1))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2BE9)
    (at 111.76 83.82)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP8 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value LeftMotor (at -5.08 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 45 /A0))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B20)
    (at 145.415 85.09)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP9 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value +5v (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2BEF)
    (at 111.76 88.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP10 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value KS_Batt (at -4.445 -0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 43 /A2))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B24)
    (at 145.415 86.995)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP11 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value +3v (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST placed (layer F.Cu) (tedit 5ABD2B2C)
    (at 145.415 88.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP12 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value +1V5 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 11 +1V5))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5ABD2E90)
    (at 128.27 90.424 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at 0 -4.5 180) (layer F.SilkS) hide)
    (fp_text value ZLDO1117G33TA (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +12V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5ABD2ADC)
    (at 145.415 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP13 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value SCL (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 19 /3_SCL))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 5ABD2ACA)
    (at 143.51 115.57)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference TP14 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value SDA (at 0 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 22 /2_SDA))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5ABD2EB2)
    (at 139.2022 90.5764 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value 49.9k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 51 /13))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5ABD2EAF)
    (at 141.4678 95.6056 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value 49.9k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 50 /10))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x2_W7.62mm_Slide_Copal_CHS-B (layer F.Cu) (tedit 5ABD2B30)
    (at 142.875 92.71)
    (descr "2x-dip-switch, Slide, row spacing 7.62 mm (300 mils), Copal_CHS-B")
    (tags "DIP Switch Slide 7.62mm 300mil Copal_CHS-B")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.965) (layer F.SilkS) hide)
    (fp_text value ModeSel (at 0 2.965) (layer F.Fab))
    (fp_text user %R (at 2.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 -0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 51 /13))
    (pad 3 smd rect (at 3.81 0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.81 0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 50 /10))
    (pad 4 smd rect (at 3.81 -0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_DIP_x2_W7.62mm_Slide_Copal_CHS-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer B.Cu) (tedit 0)
    (at 141.605 123.825 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "For use with Adafruit Feather products" (at 125.095 116.205 360) (layer B.SilkS))
  (gr_text "Rev 1.1 - Mar 2018" (at 130.175 75.565) (layer B.SilkS))
  (gr_text "Layout by Patrick Smith" (at 129.54 78.105 360) (layer B.SilkS))
  (gr_text "Mizzou Go Baby Go" (at 129.54 66.675) (layer B.SilkS))
  (gr_text Battery (at 138.43 76.835) (layer F.SilkS))
  (gr_text GND (at 141.605 79.375) (layer F.SilkS))
  (gr_text +12V (at 140.97 74.295) (layer F.SilkS))
  (gr_text RightMotor (at 139.954 106.299) (layer F.SilkS))
  (gr_text LeftMotor (at 140.335 99.314) (layer F.SilkS))
  (gr_text High (at 142.24 101.219) (layer F.SilkS))
  (gr_text High (at 142.24 107.95) (layer F.SilkS))
  (gr_text NC (at 109.855 74.295) (layer F.SilkS))
  (gr_text A3 (at 109.855 76.835) (layer F.SilkS))
  (gr_text D22/A4 (at 109.855 93.98) (layer F.SilkS))
  (gr_text StairSensor (at 112.395 78.74 270) (layer F.SilkS))
  (gr_text Relay (at 106.045 100.33 360) (layer F.SilkS))
  (gr_text "RGB LED" (at 106.045 112.395) (layer F.SilkS))
  (gr_text D23/A5 (at 110.49 104.14) (layer F.SilkS))
  (gr_text +5V (at 109.22 90.805) (layer F.SilkS))
  (gr_text +5V (at 109.855 106.68) (layer F.SilkS))
  (gr_text +3V3 (at 109.855 79.375) (layer F.SilkS))
  (gr_text GND (at 109.855 109.22) (layer F.SilkS))
  (gr_text GND (at 109.22 97.155) (layer F.SilkS))
  (gr_text GND (at 109.855 81.915) (layer F.SilkS))
  (gr_text 12V (at 148.59 83.185) (layer F.SilkS))
  (gr_text 5V (at 148.59 85.09) (layer F.SilkS))
  (gr_text 3.3V (at 148.59 86.995) (layer F.SilkS))
  (gr_text 1.5V (at 148.59 88.9) (layer F.SilkS))
  (gr_text SD (at 148.59 90.805) (layer F.SilkS))
  (gr_text Low (at 142.24 97.663) (layer F.SilkS))
  (gr_text Low (at 142.24 104.775) (layer F.SilkS))
  (gr_text "Kill Switch" (at 140.335 111.76) (layer F.SilkS))
  (gr_line (start 101.6 68.58) (end 101.6 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 63.5) (end 106.68 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 124.46) (end 157.48 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.68 129.54) (end 152.4 129.54) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 106.68 68.58) (end 101.6 68.58) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 68.58) (end 152.4 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 124.46) (end 157.48 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 106.68 124.46) (end 106.68 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 129.54) (xy 101.6 129.54) (xy 101.6 63.5) (xy 157.48 63.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 129.54) (xy 101.6 129.54) (xy 101.6 63.5) (xy 157.48 63.5)
      )
    )
  )
)
