(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g0214c9d)")
  (general
    (thickness 1.6)
    (drawings 97)
    (tracks 269)
    (zones 0)
    (modules 19)
    (nets 19)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 3.3v)
  (net 3 /A0)
  (net 4 /A1)
  (net 5 /A2)
  (net 6 /A3)
  (net 7 /A4)
  (net 8 /A5)
  (net 9 /LiPo_V+)
  (net 10 /SCL)
  (net 11 /SDA)
  (net 12 /D5)
  (net 13 /D4)
  (net 14 /D3)
  (net 15 /D0)
  (net 16 /D1)
  (net 17 /D2)
  (net 18 /PWR_BUTTON)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /LiPo_V+)
    (add_net /PWR_BUTTON)
    (add_net /SCL)
    (add_net /SDA)
    (add_net 3.3v)
    (add_net GND)
  )
  (net_class Thick ""
    (clearance 0.1778)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module belamini_cape_B2:1X10_analog (layer Top) (tedit 5C7FCC54)
    (at 153.5811 90.297 180)
    (fp_text reference J1 (at -1.3462 -1.8288 90) (layer F.SilkS))
    (fp_text value M10SILK_FEMALE_PTH (at -1.27 3.175) (layer F.Fab))
    (pad 10 thru_hole circle (at 22.86 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A0) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A1) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /A2) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /A3) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /A4) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /A5) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module belamini_cape_B2:2X18_P1 (layer Top) (tedit 5C893D1E)
    (at 152.3111 111.8489)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference P1 (at 24.2189 0.8001 90) (layer F.SilkS))
    (fp_text value PINHD-2X18 (at -22.86 4.445) (layer F.Fab))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 3.3v) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module belamini_cape_B2:2X18_P2 (layer Top) (tedit 5C893D19)
    (at 152.3111 86.4489)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference P2 (at 24.2189 0.8001 90) (layer F.SilkS))
    (fp_text value PINHD-2X18 (at -22.86 4.445) (layer F.Fab))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 3.3v) (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /LiPo_V+) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /PWR_BUTTON) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /SDA) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /D5) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /SCL) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /D4) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /D3) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /D2) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /D1) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /D0) (solder_mask_margin 0.1016))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965 (layer Top) (tedit 5BDC4BB5)
    (at 129 80.8)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965 (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965 (layer Top) (tedit 5BDC4BB5)
    (at 129 117.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965 (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965 (layer Top) (tedit 5BDC4C1C)
    (at 175 117.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965 (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 137.6807 82.7786)
    (fp_text reference "" (at 152.3111 86.4489) (layer F.SilkS))
    (fp_text value "" (at 152.3111 86.4489) (layer F.SilkS))
    (fp_text user J5 (at 152.5524 86.9823) (layer F.SilkS))
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 5BE0611B)
    (at 165.735 103.346 90)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at -3.0226 -2.4257 90) (layer B.SilkS) hide)
    (fp_text value Grove_4x2mm (at 3 -7.25 90) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 90) (layer B.Fab))
    (pad 4 thru_hole oval (at 6 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 3.3v))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /SDA))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB821A)
    (at 174 79.6 270)
    (fp_text reference J5 (at 0.1941 1.1403 270) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 270) (layer F.Fab))
    (pad 1 thru_hole custom (at 0.508 3.556 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 12 /D5) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 4 thru_hole custom (at 0.508 12.7 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 8 /A5) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB8203)
    (at 160 79.6 270)
    (fp_text reference J6 (at 0.2068 0.6404 270) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 270) (layer F.Fab))
    (pad 4 thru_hole custom (at 0.508 12.7 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 7 /A4) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 13 /D4) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 1 thru_hole custom (at 0.508 3.556 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB80AE)
    (at 146 79.6 270)
    (fp_text reference J7 (at 0.1687 0.5596 270) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 270) (layer F.Fab))
    (pad 1 thru_hole custom (at 0.508 3.556 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 14 /D3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 4 thru_hole custom (at 0.508 12.7 270) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 6 /A3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB8085)
    (at 130 118.7 90)
    (fp_text reference J8 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 90) (layer F.Fab))
    (pad 4 thru_hole custom (at 0.508 12.7 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 3 /A0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 15 /D0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 1 thru_hole custom (at 0.508 3.556 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB808A)
    (at 144 118.7 90)
    (fp_text reference J9 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole custom (at 0.508 3.556 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 16 /D1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 4 thru_hole custom (at 0.508 12.7 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 4 /A1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module belamini_cape_B2:1x4_edge_sew_big (layer Top) (tedit 5BDB808D)
    (at 158 118.7 90)
    (fp_text reference J10 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value Connector_4x2mm (at 0 -0.5 90) (layer F.Fab))
    (pad 4 thru_hole custom (at 0.508 12.7 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 5 /A2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 3 thru_hole custom (at 0.508 9.652 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 17 /D2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 2 thru_hole custom (at 0.508 6.604 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
    (pad 1 thru_hole custom (at 0.508 3.556 90) (size 2 2) (drill oval 2 1.5) (layers *.Cu *.Mask)
      (net 2 3.3v) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.9812 -0.9398) (xy -1.9812 0.9398) (xy 1.1176 0.9398) (xy 1.1176 -0.9398)) (width 0.15))
      ))
  )
  (module Connectors_JST:JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled (layer Bottom) (tedit 58D404C7)
    (at 130.9751 104.1019 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB, side entry type, surface mount, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (attr smd)
    (fp_text reference J2 (at 0 5.625 90) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -5.375 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer B.Fab))
    (pad "" smd rect (at 3.35 -2.875 90) (size 1.5 3.4) (layers Bottom B.Paste B.Mask))
    (pad "" smd rect (at -3.35 -2.875 90) (size 1.5 3.4) (layers Bottom B.Paste B.Mask))
    (pad 2 smd rect (at 1 2.875 90) (size 1 3.5) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 2.875 90) (size 1 3.5) (layers Bottom B.Paste B.Mask)
      (net 9 /LiPo_V+))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module belamini_cape_B2:TACTILE_SWITCH_SMD-4 (layer Bottom) (tedit 0)
    (at 127.6858 86.487 90)
    (fp_text reference SW1 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value SW_Push_Dual (at 0 0 90) (layer B.SilkS) hide)
    (pad 4 smd rect (at 2.075 -1.075) (size 0.65 1.05) (layers Bottom B.Paste B.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -2.075 -1.075) (size 0.65 1.05) (layers Bottom B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 2.075 1.075) (size 0.65 1.05) (layers Bottom B.Paste B.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -2.075 1.075) (size 0.65 1.05) (layers Bottom B.Paste B.Mask)
      (net 18 /PWR_BUTTON) (solder_mask_margin 0.1016))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_DIN965 (layer Top) (tedit 5BDC4BB5)
    (at 175 80.8)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.35) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_DIN965 (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module belamini_cape_B2:bela_logo_sm (layer Top) (tedit 0)
    (at 139.7508 105.9942 90)
    (fp_text reference LOGO (at 0 5 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0 90) (layer F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Top) (tedit 5C893888)
    (at 137.033 105.283 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /LiPo_V+))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SDA (at 168.529 101.346) (layer F.SilkS))
  (gr_text SCL (at 168.529 103.378) (layer F.SilkS))
  (gr_text G (at 167.513 99.441) (layer F.SilkS))
  (gr_text V+ (at 168.275 97.409) (layer F.SilkS))
  (gr_text SDA (at 168.529 101.346) (layer B.SilkS))
  (gr_text SCL (at 168.529 103.378) (layer B.SilkS))
  (gr_text V+ (at 170.8277 115.8 180) (layer B.SilkS))
  (gr_text V+ (at 161.671 115.824 180) (layer B.SilkS))
  (gr_text D2 (at 167.64 115.824 180) (layer B.SilkS))
  (gr_text "A0\n" (at 170.688 115.824 180) (layer B.SilkS))
  (gr_text G (at 164.5285 115.824 180) (layer B.SilkS))
  (gr_text "A1\n" (at 156.718 115.824 180) (layer B.SilkS))
  (gr_text D1 (at 153.67 115.824 180) (layer B.SilkS))
  (gr_text V+ (at 147.701 115.824 180) (layer B.SilkS))
  (gr_text G (at 150.5585 115.824 180) (layer B.SilkS))
  (gr_text "A0\n" (at 142.6845 115.824 180) (layer B.SilkS))
  (gr_text D0 (at 139.6365 115.824 180) (layer B.SilkS))
  (gr_text V+ (at 161.3535 115.824 180) (layer F.SilkS))
  (gr_text G (at 164.6555 115.824 180) (layer F.SilkS))
  (gr_text G (at 150.6855 115.824 180) (layer F.SilkS))
  (gr_text V+ (at 147.3835 115.824 180) (layer F.SilkS))
  (gr_text G (at 136.652 115.824 180) (layer F.SilkS))
  (gr_text V+ (at 133.35 115.824 180) (layer F.SilkS))
  (gr_text "A0\n" (at 170.6245 115.8 180) (layer F.SilkS))
  (gr_text D2 (at 167.64 115.824 180) (layer F.SilkS))
  (gr_text "A1\n" (at 156.6545 115.8 180) (layer F.SilkS))
  (gr_text D1 (at 153.67 115.824 180) (layer F.SilkS))
  (gr_text D0 (at 139.6365 115.824 180) (layer F.SilkS))
  (gr_text "A0\n" (at 142.621 115.8 180) (layer F.SilkS))
  (gr_text V+ (at 167.894 97.409) (layer B.SilkS))
  (gr_text G (at 167.64 99.441) (layer B.SilkS))
  (gr_text 3 (at 131.1783 79.9973) (layer B.SilkS))
  (gr_text 4 (at 145.4785 79.9846) (layer B.SilkS))
  (gr_text 5 (at 159.385 79.9973) (layer B.SilkS))
  (gr_text 2 (at 159.5755 118.4021) (layer B.SilkS))
  (gr_text 1 (at 145.5674 118.4021) (layer B.SilkS))
  (gr_text 0 (at 131.5212 118.3894) (layer B.SilkS))
  (gr_text V+ (at 170.567396 82.502283) (layer F.SilkS))
  (gr_text V+ (at 170.110196 82.502283) (layer B.SilkS))
  (gr_text V+ (at 156.686296 82.502283) (layer F.SilkS))
  (gr_text V+ (at 156.229096 82.502283) (layer B.SilkS))
  (gr_text V+ (at 142.601996 82.502283) (layer F.SilkS))
  (gr_text V+ (at 142.144796 82.502283) (layer B.SilkS))
  (gr_text G (at 153.447796 82.502283) (layer B.SilkS))
  (gr_text G (at 167.443196 82.502283) (layer B.SilkS))
  (gr_text G (at 139.401596 82.502283) (layer B.SilkS))
  (gr_text G (at 139.401596 82.5) (layer F.SilkS))
  (gr_text G (at 153.447796 82.502283) (layer F.SilkS))
  (gr_text G (at 167.443196 82.502283) (layer F.SilkS))
  (gr_text G (at 136.525 115.824 180) (layer B.SilkS))
  (gr_text V+ (at 133.6675 115.824 180) (layer B.SilkS))
  (gr_text LiPo (at 127.5461 104.0257 270) (layer F.SilkS))
  (gr_text "12/18\n" (at 143.973 100.508 90) (layer B.SilkS))
  (gr_text bela.io (at 141.273 100.508 90) (layer B.SilkS))
  (gr_text D5 (at 164.348 82.5111) (layer B.SilkS))
  (gr_text A3 (at 133.3 82.5) (layer B.SilkS))
  (gr_text "A4\n" (at 147.3 82.5111) (layer B.SilkS))
  (gr_text A5 (at 161.3 82.5111) (layer B.SilkS))
  (gr_text D4 (at 150.348 82.5111) (layer B.SilkS))
  (gr_text D3 (at 136.348 82.5111) (layer B.SilkS))
  (gr_text 3 (at 131.2799 80) (layer F.SilkS))
  (gr_text 4 (at 145.4277 79.9846) (layer F.SilkS))
  (gr_text A5 (at 161.3 82.5) (layer F.SilkS))
  (gr_text D5 (at 164.348 82.5) (layer F.SilkS))
  (gr_text "A4\n" (at 147.3 82.5) (layer F.SilkS))
  (gr_text D4 (at 150.348 82.5) (layer F.SilkS))
  (gr_text D3 (at 136.348 82.5) (layer F.SilkS))
  (gr_text A3 (at 133.3 82.5) (layer F.SilkS))
  (gr_text bela.io (at 160.4 100.508 90) (layer F.SilkS))
  (gr_arc (start 146.6 106.4) (end 145.6 106.4) (angle -93) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.6 94.4) (end 145.6 106.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.6 94.4) (end 158.6 106.4) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.6 106.4) (end 157.6 107.4) (angle -93) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.6 107.4) (end 157.6 107.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.6 93.4) (end 146.6 93.4) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.6 94.4) (end 158.6 94.4) (angle -93) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.6 94.4) (end 146.6 93.4) (angle -93) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175 117.3) (end 178 117.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173 107.3) (end 173 108.3) (angle 93) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175 120.3) (end 129 120.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 108.3) (end 173 108.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 117.3) (end 178 108.3) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129 117.3) (end 129 120.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129 81) (end 129 78) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173 91) (end 173 90) (angle -93) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175 81) (end 178 81) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "11/18\n" (at 163.2 100.508 90) (layer F.SilkS))
  (gr_text 5 (at 159.4358 80) (layer F.SilkS))
  (gr_text 0 (at 131.5212 118.4) (layer F.SilkS))
  (gr_text 2 (at 159.6263 118.4) (layer F.SilkS))
  (gr_text 1 (at 145.5674 118.4) (layer F.SilkS))
  (gr_text I2C (at 161.5821 99.8728 90) (layer B.SilkS))
  (gr_line (start 175 78) (end 129 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172 91) (end 172 107.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 81) (end 178 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 90) (end 173 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 117.3) (end 126 81) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.095 77.47) (xy 125.095 120.65) (xy 178.435 120.65) (xy 178.435 77.47)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.381)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.205816 109.22) (xy 174.205816 114.427) (xy 130.517816 114.427) (xy 130.517816 109.22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.381)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.235031 83.82) (xy 174.371 89.027) (xy 130.683 89.027) (xy 130.547031 83.82)
      )
    )
  )
)
