<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="27.46" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="27.96" y2="0" width="0" layer="20"/>
<wire x1="27.96" y1="0" x2="30.5" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="30.5" y1="2.54" x2="30.5" y2="27.46" width="0" layer="20"/>
<wire x1="30.5" y1="27.46" x2="27.96" y2="30" width="0" layer="20" curve="90"/>
<wire x1="27.96" y1="30" x2="2.54" y2="30" width="0" layer="20"/>
<wire x1="2.54" y1="30" x2="0" y2="27.46" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ESP8266-ESP12E">
<packages>
<package name="ESP8266-ESP12E">
<description>
&lt;b&gt;ESP8266-12E with additional I/O and GPIO04/05 corrected&lt;/b&gt;&lt;p&gt;
The author cannot warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by PuceBaboon.com. Komagane, Nagano, JAPAN&lt;/author&gt;
</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SW_TACT_3X6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="100nF"/>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="10uF"/>
<element name="IC1" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
</element>
<element name="JP1" library="pinhead" package="1X08" value=""/>
<element name="JP2" library="pinhead" package="1X08" value=""/>
<element name="JP3" library="pinhead" package="1X02" value=""/>
<element name="MDL1" library="ESP8266-ESP12E" package="ESP8266-ESP12E" value=""/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="10K"/>
<element name="SW1" library="dp_devices" package="SW_TACT_3X6" value="SW_TACT_2P-3X6"/>
<element name="SW2" library="dp_devices" package="SW_TACT_3X6" value="SW_TACT_2P-3X6"/>
</elements>
<signals>
<signal name="GPIO2">
<contactref element="R1" pad="1"/>
<contactref element="MDL1" pad="11"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="GND">
<contactref element="MDL1" pad="9"/>
<contactref element="R3" pad="1"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="RESET">
<contactref element="MDL1" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="MDL1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="CH_PD">
<contactref element="MDL1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GPIO16">
<contactref element="MDL1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="GPIO14">
<contactref element="MDL1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="GPIO12">
<contactref element="MDL1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="GPIO13">
<contactref element="MDL1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="MDL1" pad="16"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RX">
<contactref element="MDL1" pad="15"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GPIO5">
<contactref element="MDL1" pad="14"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="GPIO4">
<contactref element="MDL1" pad="13"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="GPIO0">
<contactref element="MDL1" pad="12"/>
<contactref element="SW1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="GPIO15">
<contactref element="MDL1" pad="10"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="CS">
<contactref element="MDL1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="MDL1" pad="18"/>
</signal>
<signal name="GPIO9">
<contactref element="MDL1" pad="19"/>
</signal>
<signal name="GPIO10">
<contactref element="MDL1" pad="20"/>
</signal>
<signal name="MOSI">
<contactref element="MDL1" pad="21"/>
</signal>
<signal name="CLK">
<contactref element="MDL1" pad="22"/>
</signal>
<signal name="VCC3V">
<contactref element="MDL1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
