(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VBUS")
  (net 3 "Net-(J1-PadA5)")
  (net 4 "Net-(J1-PadA6)")
  (net 5 "Net-(J1-PadA7)")
  (net 6 "unconnected-(J1-PadA8)")
  (net 7 "Net-(J1-PadB5)")
  (net 8 "unconnected-(J1-PadB8)")
  (net 9 "Net-(J1-PadS1)")
  (net 10 "+3.3VP")
  (net 11 "/GPIO0")
  (net 12 "/GPIO1")
  (net 13 "/GPIO2")
  (net 14 "/GPIO3")
  (net 15 "/GPIO4")
  (net 16 "/GPIO5")
  (net 17 "/GPIO6")
  (net 18 "/GPIO7")
  (net 19 "/QSPI_SS")
  (net 20 "/QSPI_SD1")
  (net 21 "/QSPI_SD2")
  (net 22 "/QSPI_SD0")
  (net 23 "/QSPI_SCLK")
  (net 24 "/QSPI_SD3")
  (net 25 "+3.3V")
  (net 26 "Net-(R6-Pad2)")
  (net 27 "unconnected-(U2-Pad4)")
  (net 28 "+3.3VA")
  (net 29 "unconnected-(U3-Pad8)")
  (net 30 "unconnected-(U4-Pad11)")
  (net 31 "unconnected-(U4-Pad12)")
  (net 32 "unconnected-(U4-Pad13)")
  (net 33 "unconnected-(U4-Pad14)")
  (net 34 "unconnected-(U4-Pad16)")
  (net 35 "unconnected-(U4-Pad17)")
  (net 36 "unconnected-(U4-Pad18)")
  (net 37 "Net-(C5-Pad2)")
  (net 38 "Net-(R10-Pad2)")
  (net 39 "+1V1")
  (net 40 "Net-(R9-Pad2)")
  (net 41 "unconnected-(U4-Pad27)")
  (net 42 "unconnected-(U4-Pad28)")
  (net 43 "unconnected-(U4-Pad29)")
  (net 44 "unconnected-(U4-Pad30)")
  (net 45 "unconnected-(U4-Pad31)")
  (net 46 "unconnected-(U4-Pad32)")
  (net 47 "unconnected-(U4-Pad34)")
  (net 48 "unconnected-(U4-Pad35)")
  (net 49 "Net-(SW2-Pad1)")
  (net 50 "Net-(R11-Pad2)")
  (net 51 "/USB_D_N")
  (net 52 "/USB_D_P")
  (net 53 "Net-(C6-Pad2)")
  (net 54 "Net-(D1-Pad2)")
  (net 55 "Net-(R2-Pad1)")
  (net 56 "/SWCLK")
  (net 57 "/SWD")
  (net 58 "/ADC0")
  (net 59 "/ADC1")
  (net 60 "/ADC2")
  (net 61 "/ADC3")
  (net 62 "Net-(U4-Pad15)")
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.6418 84.963 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -0.4826 1.143 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -0.1778 1.4648 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.075 95.925)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.764 94.869 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0.127 3.3274 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.5204 93.0656 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.6164 86.995 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "+3.3VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12" (layer "F.Cu")
    (tedit 5D3C0721)
    (at 130.9612 91.44 -90)
    (descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
    (tags "usb usb-c 2.0 pd")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 4.3942 -5.0292 90) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle_USB2.0" (at 0 5.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "A1" smd rect (at -3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" smd rect (at -2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_HRO_TYPE-C-31-M-12.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.0446 97.1246 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -0.127 1.2954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.9324 94.8716 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0.1296 3.4798 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.45 84.5)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U4-Pad15)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3.3VP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.3256 86.106 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.903 0.0508 90) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 159.45 85.09)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 5.655 -2.27) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x06_Odd_Even" (at 9.58 5.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 6.35 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "+3.3VP") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "+3.3VP") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/GPIO7") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/GPIO6") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/GPIO5") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/GPIO4") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/GPIO3") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GPIO2") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/GPIO1") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/GPIO0") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.8976 94.869 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -0.3556 3.8608 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.5 95.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/QSPI_SS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 130.792 83.6422)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at 0.15 -2.6) (layer "F.SilkS") hide)
    (fp_text value "RESET" (at -0.0254 2.6162) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R9-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(R9-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 142.15 99.75 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "/ADC0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "/ADC1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "/ADC2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/ADC3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "+3.3V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.8242 94.869 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0.508 -2.286 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.3 93 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at -0.48 -1.143 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.5966 82.8548 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "27pF" (at -0.089 1.4266 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 138.075 94.975)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 1.4478 1.2208) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.4752 84.3604 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -2.286 -0.0254 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.415 84.3534 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -0.4248 0.0508 90) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3112 87.122)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0.0254) (layer "F.SilkS") hide)
    (fp_text value "1M" (at 0.0254 1.0922) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J1-PadS1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.1046 85.8774)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -0.1016 1.8484) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3112 90.17)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.8542 0) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.5 96.675 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/QSPI_SS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.5364 87.2744 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0.6884 1.2716 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.8684 88.7984)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at -2.4384 -0.0254) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 136.159 83.185 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.330007 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/SWCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/SWD") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 154.1018 87.3252)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "AP2112K-3.3" (at -0.6858 3.4992) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(R6-Pad2)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "unconnected-(U2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "+3.3VA") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "rp2040-pmod:USON-8_2x3" (layer "F.Cu")
    (tedit 632A3751)
    (at 149.795 96.625 180)
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -3.005 -0.875 180) (layer "F.SilkS") hide)
    (fp_text value "W25Q16JVUXIQ" (at 10.935 2.135 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.75 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/QSPI_SS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd rect (at -1.2 -0.25 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/QSPI_SD1") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd rect (at -1.2 0.25 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/QSPI_SD2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd rect (at -1.2 0.75 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 1.2 0.75 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/QSPI_SD0") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd rect (at 1.2 0.25 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/QSPI_SCLK") (pinfunction "CLK") (pintype "input"))
    (pad "7" smd rect (at 1.2 -0.25 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/QSPI_SD3") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "8" smd rect (at 1.2 -0.75 180) (size 0.3 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect (at 0 0 180) (size 0.2 1.6) (layers "F.Cu" "F.Mask"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.6418 83.1342 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3.3VP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3124 91.2114)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.8542 0.016) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-PadA7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/USB_D_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm" (layer "F.Cu")
    (tedit 627AC11D)
    (at 145.923 89.8144 180)
    (descr "QFN, 56 Pin (https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf#page=634), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -4.82) (layer "F.SilkS") hide)
    (fp_text value "RP2040" (at -0.889 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at 0.8 -0.8 180) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
    (pad "" smd roundrect locked (at 0.8 0.8 180) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
    (pad "" smd roundrect locked (at -0.8 -0.8 180) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
    (pad "" smd roundrect locked (at -0.8 0.8 180) (size 1.29 1.29) (layers "F.Paste") (roundrect_rratio 0.193798))
    (pad "1" smd roundrect locked (at -3.4375 -2.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -3.4375 -2.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/GPIO0") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -3.4375 -1.8 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/GPIO1") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -3.4375 -1.4 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GPIO2") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -3.4375 -1 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/GPIO3") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -3.4375 -0.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/GPIO4") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -3.4375 -0.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/GPIO5") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -3.4375 0.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/GPIO6") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at -3.4375 0.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/GPIO7") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -3.4375 1 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "11" smd roundrect locked (at -3.4375 1.4 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "unconnected-(U4-Pad11)") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at -3.4375 1.8 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "unconnected-(U4-Pad12)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -3.4375 2.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "unconnected-(U4-Pad13)") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at -3.4375 2.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(U4-Pad14)") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at -2.6 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U4-Pad15)") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at -2.2 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "unconnected-(U4-Pad16)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at -1.8 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "unconnected-(U4-Pad17)") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at -1.4 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(U4-Pad18)") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at -1 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "TESTEN") (pintype "input"))
    (pad "20" smd roundrect locked (at -0.6 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C5-Pad2)") (pinfunction "XIN") (pintype "input"))
    (pad "21" smd roundrect locked (at -0.2 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R10-Pad2)") (pinfunction "XOUT") (pintype "passive"))
    (pad "22" smd roundrect locked (at 0.2 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "23" smd roundrect locked (at 0.6 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd roundrect locked (at 1 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/SWCLK") (pinfunction "SWCLK") (pintype "output"))
    (pad "25" smd roundrect locked (at 1.4 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/SWD") (pinfunction "SWD") (pintype "bidirectional"))
    (pad "26" smd roundrect locked (at 1.8 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R9-Pad2)") (pinfunction "RUN") (pintype "input"))
    (pad "27" smd roundrect locked (at 2.2 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "unconnected-(U4-Pad27)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "28" smd roundrect locked (at 2.6 3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "unconnected-(U4-Pad28)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "29" smd roundrect locked (at 3.4375 2.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "unconnected-(U4-Pad29)") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "30" smd roundrect locked (at 3.4375 2.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "unconnected-(U4-Pad30)") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "31" smd roundrect locked (at 3.4375 1.8 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "unconnected-(U4-Pad31)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "32" smd roundrect locked (at 3.4375 1.4 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "unconnected-(U4-Pad32)") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "33" smd roundrect locked (at 3.4375 1 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "34" smd roundrect locked (at 3.4375 0.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "unconnected-(U4-Pad34)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd roundrect locked (at 3.4375 0.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U4-Pad35)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd roundrect locked (at 3.4375 -0.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(SW2-Pad1)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd roundrect locked (at 3.4375 -0.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R11-Pad2)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd roundrect locked (at 3.4375 -1 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/ADC0") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "39" smd roundrect locked (at 3.4375 -1.4 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/ADC1") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "40" smd roundrect locked (at 3.4375 -1.8 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/ADC2") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "41" smd roundrect locked (at 3.4375 -2.2 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/ADC3") (pinfunction "GPIO29_ADC3") (pintype "bidirectional"))
    (pad "42" smd roundrect locked (at 3.4375 -2.6 180) (size 0.875 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "43" smd roundrect locked (at 2.6 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd roundrect locked (at 2.2 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "VREG_IN") (pintype "power_in"))
    (pad "45" smd roundrect locked (at 1.8 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pinfunction "VREG_VOUT") (pintype "power_out"))
    (pad "46" smd roundrect locked (at 1.4 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/USB_D_N") (pinfunction "USB_DM") (pintype "bidirectional"))
    (pad "47" smd roundrect locked (at 1 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/USB_D_P") (pinfunction "USB_DP") (pintype "bidirectional"))
    (pad "48" smd roundrect locked (at 0.6 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd roundrect locked (at 0.2 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pinfunction "IOVDD") (pintype "passive"))
    (pad "50" smd roundrect locked (at -0.2 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pinfunction "DVDD") (pintype "passive"))
    (pad "51" smd roundrect locked (at -0.6 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/QSPI_SD3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd roundrect locked (at -1 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/QSPI_SCLK") (pinfunction "QSPI_SCLK") (pintype "output"))
    (pad "53" smd roundrect locked (at -1.4 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/QSPI_SD0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd roundrect locked (at -1.8 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/QSPI_SD2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd roundrect locked (at -2.2 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/QSPI_SD1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd roundrect locked (at -2.6 -3.4375 180) (size 0.2 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/QSPI_SS") (pinfunction "QSPI_SS") (pintype "bidirectional"))
    (pad "57" smd rect locked (at 0 0 180) (size 3.2 3.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3124 92.1766)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.8542 0.0668) (layer "F.SilkS") hide)
    (fp_text value "27" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-PadA6)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/USB_D_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.859 94.869 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0.635 -2.5908 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.125 82.825 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0.089 0.8934 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "+3.3VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.4404 82.469 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -1.7662 0 90) (layer "F.SilkS") hide)
    (fp_text value "27pF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "rp2040-pmod:SOT-5x3" (layer "F.Cu")
    (tedit 6373DCE3)
    (at 154.1 83.64 180)
    (descr "SOT563")
    (tags "SOT-563")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -1.7 180) (layer "F.SilkS") hide)
    (fp_text value "LM66200" (at 0 1.75 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 -0.76 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -0.75 -0.26 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "+3.3V") (pinfunction "VOUT") (pintype "power_out"))
    (pad "3" smd rect (at -0.75 0.24 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3.3VP") (pinfunction "VIN1") (pintype "input"))
    (pad "4" smd rect (at -0.75 0.74 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "/ON") (pintype "input"))
    (pad "5" smd rect (at 0.75 0.74 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd rect (at 0.75 0.24 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "+3.3VA") (pinfunction "VIN2") (pintype "input"))
    (pad "7" smd rect (at 0.75 -0.26 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "+3.3V") (pinfunction "VOUT") (pintype "power_out"))
    (pad "8" smd rect (at 0.75 -0.76 180) (size 0.7 0.34) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U3-Pad8)") (pinfunction "ST") (pintype "output+no_connect"))
  )
  (footprint "Crystal:Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 148.0058 83.7692)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM8G http://www.abracon.com/Resonators/ABM8G.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2.45) (layer "F.SilkS") hide)
    (fp_text value "12Mhz" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(C6-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C5-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 143.51 84.3604 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -1.8288 -0.2032 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+1V1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3112 93.218)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.8288 0) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 136.9822 99.06 180)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at 0 -0.0508) (layer "F.SilkS") hide)
    (fp_text value "USER1" (at -0.4826 -3.4544) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(SW2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(SW2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 130.9612 99.06)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0.0254 0.0508) (layer "F.SilkS") hide)
    (fp_text value "USB Boot" (at -0.1512 3.429) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at -2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(R2-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(R2-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.5204 88.2142 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "rp2040-pmod.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.16 -270) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -0.4826 1.4812 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-6385637E" (layer "F.Cu")
    (tedit 6385637E)
    (at 154.675 92.45)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-6385637E" (at 0 -1.12808) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 1.12808) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-6385637E" (layer "B.Cu")
    (tedit 6385637E)
    (at 149.55 89.825 180)
    (descr "Converted using: scripting")
    (tags "svg2mod")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-6385637E" (at 0 1.12808) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -1.12808) (layer "B.SilkS") hide)
  )
  (gr_rect (start 127 81.28) (end 166.37 101.6) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "1" (at 144.625 97.825) (layer "B.SilkS"))
  (gr_text "0" (at 164.3634 97.9932) (layer "B.SilkS"))
  (gr_text "ANALOG" (at 137.922 99.8982) (layer "B.SilkS"))
  (gr_text "5" (at 157.1244 92.71) (layer "B.SilkS"))
  (gr_text "+3.3" (at 164.775 85.1) (layer "B.SilkS"))
  (gr_text "7" (at 157.0482 90.2716) (layer "B.SilkS"))
  (gr_text "1" (at 156.9974 97.79) (layer "B.SilkS"))
  (gr_text "SWCLK" (at 137.4902 86.106 315) (layer "B.SilkS"))
  (gr_text "DEBUG" (at 132.5118 83.2358) (layer "B.SilkS"))
  (gr_text "+3.3" (at 156.5 85.025) (layer "B.SilkS"))
  (gr_text "  (\\__/)\n  ( . _ .)\n / >   " (at 152.725 88.025) (layer "B.SilkS"))
  (gr_text "0" (at 142.125 97.775) (layer "B.SilkS"))
  (gr_text "2" (at 164.2872 95.377) (layer "B.SilkS"))
  (gr_text "GND" (at 164.425 87.65) (layer "B.SilkS"))
  (gr_text "SWD" (at 142.4178 85.7504 315) (layer "B.SilkS"))
  (gr_text "GND" (at 156.8 87.575) (layer "B.SilkS"))
  (gr_text "2" (at 147.2 97.85) (layer "B.SilkS"))
  (gr_text "VREF" (at 151.525 97.175 315) (layer "B.SilkS"))
  (gr_text "GND" (at 154.075 97.1 315) (layer "B.SilkS"))
  (gr_text "3" (at 149.725 97.775) (layer "B.SilkS"))
  (gr_text "GND" (at 140.1064 86.0806 315) (layer "B.SilkS"))
  (gr_text "3" (at 157.2006 95.25) (layer "B.SilkS"))
  (gr_text "4" (at 164.2872 92.9386) (layer "B.SilkS"))
  (gr_text "PMOD" (at 160.949996 82.574994) (layer "B.SilkS"))
  (gr_text "ADC" (at 145.2118 95.2246 315) (layer "B.SilkS"))
  (gr_text "6" (at 164.2872 90.2462) (layer "B.SilkS"))
  (gr_text "BOOT" (at 130.9878 96.8502) (layer "F.SilkS"))
  (gr_text ":0" (at 164.7 92.7 315) (layer "F.SilkS"))
  (gr_text "USR" (at 137 96.85) (layer "F.SilkS"))
  (gr_text "DEBUG" (at 138.3284 85.5218) (layer "F.SilkS"))
  (gr_text "RST" (at 130.6068 86.0044) (layer "F.SilkS"))
  (gr_text " /\\_/\\\n ( o.o )\n > ^ <" (at 164.55 85.2) (layer "F.SilkS"))
  (gr_text "PMOD" (at 160.775 82.775) (layer "F.SilkS"))
  (gr_text "m_w" (at 164.719 97.7138 45) (layer "F.SilkS"))
  (gr_text "  (\\__/)\n  ( . _ .)\n / > $" (at 164.4 90.05) (layer "F.SilkS"))
  (gr_text "ANALOG" (at 143 97.525) (layer "F.SilkS"))
  (gr_text "  (\\__/)\n  ( . _ .)\n / >   " (at 151.7 90.725) (layer "F.SilkS"))
  (gr_text "B^)" (at 164.825 87.65 315) (layer "F.SilkS"))
  (gr_text " (\\/) \n(oo)\n(__)\n" (at 164.7 95.275) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 101.6)
        (xy 127 101.6)
        (xy 127 81.28)
        (xy 166.37 81.28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161 86.95)
        (xy 160.725 87.95)
        (xy 160.425 86.925)
        (xy 159.75 86.45)
        (xy 161.675 86.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.457699 88.358367)
        (xy 160.732699 87.358367)
        (xy 161.032699 88.383367)
        (xy 161.707699 88.858367)
        (xy 159.782699 88.858367)
      )
    )
  )
)
