(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (title_block
    (title "XBT Autolauncher 3.0")
    (date "2024-06-20")
    (rev "3")
    (company "NOAA/AOML")
    (comment 1 "Christian Saiz")
  )
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" mixed)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 52 186)
    (grid_origin 52 186)
    (pcbplotparams
      (layerselection 0x00010e8_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "V3_GERBERS/")
    )
  )
  (net 0 "")
  (net 1 "/+19.5V")
  (net 2 "GND")
  (net 3 "+12V")
  (net 4 "+5V")
  (net 5 "+3.3V")
  (net 6 "Net-(SW1-A)")
  (net 7 "Net-(U4-C1+)")
  (net 8 "Net-(U4-C1-)")
  (net 9 "Net-(U6-PD0)")
  (net 10 "Net-(U4-C2+)")
  (net 11 "Net-(U4-C2-)")
  (net 12 "Net-(U6-PD1)")
  (net 13 "Net-(U4-VS-)")
  (net 14 "Net-(U4-VS+)")
  (net 15 "Vmotor_out")
  (net 16 "Net-(IC3-VCP)")
  (net 17 "Net-(IC3-CP2)")
  (net 18 "Net-(IC3-CP1)")
  (net 19 "Net-(J7-Pin_1)")
  (net 20 "Net-(IC4-VCP)")
  (net 21 "Net-(IC4-CP2)")
  (net 22 "Net-(IC4-CP1)")
  (net 23 "Net-(IC5-VCP)")
  (net 24 "Net-(IC5-CP2)")
  (net 25 "Net-(IC5-CP1)")
  (net 26 "Net-(IC6-VCP)")
  (net 27 "Net-(IC6-CP2)")
  (net 28 "Net-(IC6-CP1)")
  (net 29 "Net-(IC7-VCP)")
  (net 30 "Net-(IC7-CP2)")
  (net 31 "Net-(IC7-CP1)")
  (net 32 "Net-(IC8-VCP)")
  (net 33 "Net-(IC8-CP2)")
  (net 34 "Net-(IC8-CP1)")
  (net 35 "Net-(IC9-VCP)")
  (net 36 "Net-(IC9-CP2)")
  (net 37 "Net-(IC9-CP1)")
  (net 38 "Net-(IC10-VCP)")
  (net 39 "Net-(IC10-CP2)")
  (net 40 "Net-(IC10-CP1)")
  (net 41 "Net-(U18-+)")
  (net 42 "/+19.5V_raw")
  (net 43 "Net-(U6-PC1)")
  (net 44 "Net-(IC1-Q4)")
  (net 45 "Net-(IC1-Q1)")
  (net 46 "/RelayControl/Reset1")
  (net 47 "SSR_xbt1")
  (net 48 "SSR_xbt4")
  (net 49 "Net-(IC1-Q2)")
  (net 50 "Net-(IC1-Q3)")
  (net 51 "SSR_xbt3")
  (net 52 "unconnected-(IC1-NC-Pad13)")
  (net 53 "SSR_xbt2")
  (net 54 "Net-(IC2-Q4)")
  (net 55 "Net-(IC2-Q1)")
  (net 56 "/RelayControl/Reset2")
  (net 57 "SSR_xbt5")
  (net 58 "SSR_xbt8")
  (net 59 "Net-(IC2-Q2)")
  (net 60 "Net-(IC2-Q3)")
  (net 61 "SSR_xbt7")
  (net 62 "unconnected-(IC2-NC-Pad13)")
  (net 63 "SSR_xbt6")
  (net 64 "Net-(IC3-AOUT1)")
  (net 65 "Net-(IC3-ISENA)")
  (net 66 "Net-(IC3-AOUT2)")
  (net 67 "Net-(IC3-BOUT2)")
  (net 68 "Net-(IC3-ISENB)")
  (net 69 "Net-(IC3-BOUT1)")
  (net 70 "/MotorControl/Vref")
  (net 71 "unconnected-(IC3-NFAULT-Pad18)")
  (net 72 "unconnected-(IC3-DECAY-Pad19)")
  (net 73 "DIR")
  (net 74 "Enable_M1")
  (net 75 "STEP")
  (net 76 "unconnected-(IC3-NC-Pad23)")
  (net 77 "/MotorControl/Mode_0")
  (net 78 "/MotorControl/Mode_1")
  (net 79 "/MotorControl/Mode_2")
  (net 80 "unconnected-(IC3-NHOME-Pad27)")
  (net 81 "Net-(IC4-AOUT1)")
  (net 82 "Net-(IC4-ISENA)")
  (net 83 "Net-(IC4-AOUT2)")
  (net 84 "Net-(IC4-BOUT2)")
  (net 85 "Net-(IC4-ISENB)")
  (net 86 "Net-(IC4-BOUT1)")
  (net 87 "unconnected-(IC4-NFAULT-Pad18)")
  (net 88 "unconnected-(IC4-DECAY-Pad19)")
  (net 89 "Enable_M2")
  (net 90 "unconnected-(IC4-NC-Pad23)")
  (net 91 "unconnected-(IC4-NHOME-Pad27)")
  (net 92 "Net-(IC5-AOUT1)")
  (net 93 "Net-(IC5-ISENA)")
  (net 94 "Net-(IC5-AOUT2)")
  (net 95 "Net-(IC5-BOUT2)")
  (net 96 "Net-(IC5-ISENB)")
  (net 97 "Net-(IC5-BOUT1)")
  (net 98 "unconnected-(IC5-NFAULT-Pad18)")
  (net 99 "unconnected-(IC5-DECAY-Pad19)")
  (net 100 "Enable_M3")
  (net 101 "unconnected-(IC5-NC-Pad23)")
  (net 102 "unconnected-(IC5-NHOME-Pad27)")
  (net 103 "Net-(IC6-AOUT1)")
  (net 104 "Net-(IC6-ISENA)")
  (net 105 "Net-(IC6-AOUT2)")
  (net 106 "Net-(IC6-BOUT2)")
  (net 107 "Net-(IC6-ISENB)")
  (net 108 "Net-(IC6-BOUT1)")
  (net 109 "unconnected-(IC6-NFAULT-Pad18)")
  (net 110 "unconnected-(IC6-DECAY-Pad19)")
  (net 111 "Enable_M4")
  (net 112 "unconnected-(IC6-NC-Pad23)")
  (net 113 "unconnected-(IC6-NHOME-Pad27)")
  (net 114 "Net-(IC7-AOUT1)")
  (net 115 "Net-(IC7-ISENA)")
  (net 116 "Net-(IC7-AOUT2)")
  (net 117 "Net-(IC7-BOUT2)")
  (net 118 "Net-(IC7-ISENB)")
  (net 119 "Net-(IC7-BOUT1)")
  (net 120 "unconnected-(IC7-NFAULT-Pad18)")
  (net 121 "unconnected-(IC7-DECAY-Pad19)")
  (net 122 "Enable_M5")
  (net 123 "unconnected-(IC7-NC-Pad23)")
  (net 124 "unconnected-(IC7-NHOME-Pad27)")
  (net 125 "Net-(IC8-AOUT1)")
  (net 126 "Net-(IC8-ISENA)")
  (net 127 "Net-(IC8-AOUT2)")
  (net 128 "Net-(IC8-BOUT2)")
  (net 129 "Net-(IC8-ISENB)")
  (net 130 "Net-(IC8-BOUT1)")
  (net 131 "unconnected-(IC8-NFAULT-Pad18)")
  (net 132 "unconnected-(IC8-DECAY-Pad19)")
  (net 133 "Enable_M6")
  (net 134 "unconnected-(IC8-NC-Pad23)")
  (net 135 "unconnected-(IC8-NHOME-Pad27)")
  (net 136 "Net-(IC9-AOUT1)")
  (net 137 "Net-(IC9-ISENA)")
  (net 138 "Net-(IC9-AOUT2)")
  (net 139 "Net-(IC9-BOUT2)")
  (net 140 "Net-(IC9-ISENB)")
  (net 141 "Net-(IC9-BOUT1)")
  (net 142 "unconnected-(IC9-NFAULT-Pad18)")
  (net 143 "unconnected-(IC9-DECAY-Pad19)")
  (net 144 "Enable_M7")
  (net 145 "unconnected-(IC9-NC-Pad23)")
  (net 146 "unconnected-(IC9-NHOME-Pad27)")
  (net 147 "Net-(IC10-AOUT1)")
  (net 148 "Net-(IC10-ISENA)")
  (net 149 "Net-(IC10-AOUT2)")
  (net 150 "Net-(IC10-BOUT2)")
  (net 151 "Net-(IC10-ISENB)")
  (net 152 "Net-(IC10-BOUT1)")
  (net 153 "unconnected-(IC10-NFAULT-Pad18)")
  (net 154 "unconnected-(IC10-DECAY-Pad19)")
  (net 155 "Enable_M8")
  (net 156 "unconnected-(IC10-NC-Pad23)")
  (net 157 "unconnected-(IC10-NHOME-Pad27)")
  (net 158 "xbt_B")
  (net 159 "/Dout_toComputer")
  (net 160 "xbt_C")
  (net 161 "/Din_fromComputer")
  (net 162 "xbt_A")
  (net 163 "/SWDIO")
  (net 164 "/SWCLK")
  (net 165 "Net-(JP13-A)")
  (net 166 "/UART3_TX")
  (net 167 "/RelayControl/XBT1_A")
  (net 168 "/RelayControl/XBT1_B")
  (net 169 "/RelayControl/XBT1_C")
  (net 170 "/RelayControl/XBT2_A")
  (net 171 "/RelayControl/XBT2_B")
  (net 172 "/RelayControl/XBT2_C")
  (net 173 "/RelayControl/XBT3_A")
  (net 174 "/RelayControl/XBT3_B")
  (net 175 "/RelayControl/XBT3_C")
  (net 176 "/RelayControl/XBT4_A")
  (net 177 "/RelayControl/XBT4_B")
  (net 178 "/RelayControl/XBT4_C")
  (net 179 "/RelayControl/XBT5_A")
  (net 180 "/RelayControl/XBT5_B")
  (net 181 "/RelayControl/XBT5_C")
  (net 182 "/RelayControl/XBT6_A")
  (net 183 "/RelayControl/XBT6_B")
  (net 184 "/RelayControl/XBT6_C")
  (net 185 "/RelayControl/XBT7_A")
  (net 186 "/RelayControl/XBT7_B")
  (net 187 "/RelayControl/XBT7_C")
  (net 188 "/RelayControl/XBT8_A")
  (net 189 "/RelayControl/XBT8_B")
  (net 190 "/RelayControl/XBT8_C")
  (net 191 "/I2C1_SDA")
  (net 192 "/I2C1_SCL")
  (net 193 "/MUX_output")
  (net 194 "Net-(JP2-B)")
  (net 195 "unconnected-(J16-Pin_2-Pad2)")
  (net 196 "unconnected-(J16-Pin_4-Pad4)")
  (net 197 "unconnected-(J17-Pin_2-Pad2)")
  (net 198 "unconnected-(J17-Pin_4-Pad4)")
  (net 199 "unconnected-(J19-Pin_2-Pad2)")
  (net 200 "unconnected-(J19-Pin_4-Pad4)")
  (net 201 "unconnected-(J20-Pin_2-Pad2)")
  (net 202 "unconnected-(J20-Pin_4-Pad4)")
  (net 203 "unconnected-(J22-Pin_2-Pad2)")
  (net 204 "unconnected-(J22-Pin_4-Pad4)")
  (net 205 "unconnected-(J23-Pin_2-Pad2)")
  (net 206 "unconnected-(J23-Pin_4-Pad4)")
  (net 207 "/MUX_select")
  (net 208 "/Din_fromGPS")
  (net 209 "Net-(U18--)")
  (net 210 "Net-(J3-Pin_2)")
  (net 211 "Net-(JP6-B)")
  (net 212 "Net-(JP7-B)")
  (net 213 "Net-(JP8-A)")
  (net 214 "Net-(JP8-B)")
  (net 215 "Net-(JP4-B)")
  (net 216 "Net-(JP5-B)")
  (net 217 "Net-(JP6-A)")
  (net 218 "Net-(JP7-A)")
  (net 219 "unconnected-(K1-NC_1-Pad3)")
  (net 220 "Net-(K1--_1)")
  (net 221 "unconnected-(K1-NC_2-Pad10)")
  (net 222 "unconnected-(K2-NC_1-Pad3)")
  (net 223 "Net-(K2--_1)")
  (net 224 "unconnected-(K2-NC_2-Pad10)")
  (net 225 "unconnected-(K3-NC_1-Pad3)")
  (net 226 "Net-(K3--_1)")
  (net 227 "unconnected-(K3-NC_2-Pad10)")
  (net 228 "unconnected-(K4-NC_1-Pad3)")
  (net 229 "Net-(K4--_1)")
  (net 230 "unconnected-(K4-NC_2-Pad10)")
  (net 231 "Net-(K12--_1)")
  (net 232 "/RelayControl/Reset3")
  (net 233 "unconnected-(K6-NC_1-Pad3)")
  (net 234 "unconnected-(K5-NC_1-Pad3)")
  (net 235 "Net-(K6--_1)")
  (net 236 "unconnected-(K6-NC_2-Pad10)")
  (net 237 "unconnected-(K7-NC_1-Pad3)")
  (net 238 "Net-(K5--_1)")
  (net 239 "Net-(K7--_1)")
  (net 240 "unconnected-(K5-NC_2-Pad10)")
  (net 241 "unconnected-(K10-COM_1-Pad4)")
  (net 242 "unconnected-(K7-NC_2-Pad10)")
  (net 243 "unconnected-(K8-NC_1-Pad3)")
  (net 244 "Net-(K8--_1)")
  (net 245 "unconnected-(K8-NC_2-Pad10)")
  (net 246 "unconnected-(K10-NO_1-Pad5)")
  (net 247 "Net-(K11-NO_1)")
  (net 248 "Net-(K12-NO_1)")
  (net 249 "unconnected-(K10-NC_1-Pad3)")
  (net 250 "Net-(K10--_1)")
  (net 251 "unconnected-(K12-NO_2-Pad8)")
  (net 252 "unconnected-(K11-NC_1-Pad3)")
  (net 253 "Net-(K11--_1)")
  (net 254 "unconnected-(K11-NC_2-Pad10)")
  (net 255 "unconnected-(K12-NC_1-Pad3)")
  (net 256 "unconnected-(K12-COM_2-Pad9)")
  (net 257 "unconnected-(K12-NC_2-Pad10)")
  (net 258 "Net-(U6-BOOT0)")
  (net 259 "/UART3_RX")
  (net 260 "relay_xbt8")
  (net 261 "relay_xbt7")
  (net 262 "relay_xbt6")
  (net 263 "relay_xbt5")
  (net 264 "relay_xbt4")
  (net 265 "relay_xbt3")
  (net 266 "relay_xbt2")
  (net 267 "relay_xbt1")
  (net 268 "Net-(J25-Pin_2)")
  (net 269 "relay_reset3")
  (net 270 "relay_reset2")
  (net 271 "relay_reset1")
  (net 272 "relay_cal_res")
  (net 273 "relay_cal_cont")
  (net 274 "relay_gnd_cond")
  (net 275 "unconnected-(U4-T2OUT-Pad7)")
  (net 276 "unconnected-(U4-R2IN-Pad8)")
  (net 277 "/UART1_TX")
  (net 278 "/UART1_RX")
  (net 279 "unconnected-(U6-PB12-Pad33)")
  (net 280 "Net-(D4-K)")
  (net 281 "Net-(D5-K)")
  (net 282 "Net-(D6-K)")
  (net 283 "Net-(Q1-G)")
  (net 284 "/VDDA")
  (net 285 "Net-(R36-Pad1)")
  (net 286 "Net-(R37-Pad1)")
  (net 287 "Net-(R38-Pad1)")
  (net 288 "Net-(R39-Pad1)")
  (net 289 "Net-(R40-Pad1)")
  (net 290 "Net-(R41-Pad1)")
  (net 291 "Net-(R42-Pad1)")
  (net 292 "Net-(R43-Pad1)")
  (net 293 "unconnected-(U6-PB2-Pad28)")
  (net 294 "Net-(D7-K)")
  (net 295 "unconnected-(U6-PC5-Pad25)")
  (net 296 "unconnected-(RN1-Pad9)")
  (net 297 "unconnected-(J18-Pin_2-Pad2)")
  (net 298 "unconnected-(J18-Pin_4-Pad4)")
  (net 299 "unconnected-(J21-Pin_2-Pad2)")
  (net 300 "unconnected-(J21-Pin_4-Pad4)")
  (net 301 "Net-(D7-A)")
  (net 302 "Net-(JP14-A)")
  (net 303 "Net-(JP12-A)")
  (net 304 "Net-(J4-Pin_1)")
  (net 305 "Net-(J4-Pin_2)")
  (net 306 "Net-(J4-Pin_3)")
  (net 307 "Net-(J4-Pin_6)")
  (net 308 "unconnected-(U4-R2OUT-Pad9)")
  (net 309 "unconnected-(U4-T2IN-Pad10)")
  (net 310 "unconnected-(U6-PA3-Pad17)")
  (net 311 "unconnected-(RN3-Pad9)")
  (net 312 "Net-(J3-Pin_1)")
  (net 313 "/VDD")
  (net 314 "unconnected-(IC3-V3P3OUT-Pad15)")
  (net 315 "unconnected-(IC3-NENBL-Pad21)")
  (net 316 "unconnected-(IC4-V3P3OUT-Pad15)")
  (net 317 "unconnected-(IC4-NENBL-Pad21)")
  (net 318 "unconnected-(IC5-V3P3OUT-Pad15)")
  (net 319 "unconnected-(IC5-NENBL-Pad21)")
  (net 320 "unconnected-(IC6-V3P3OUT-Pad15)")
  (net 321 "unconnected-(IC6-NENBL-Pad21)")
  (net 322 "unconnected-(IC7-V3P3OUT-Pad15)")
  (net 323 "unconnected-(IC7-NENBL-Pad21)")
  (net 324 "unconnected-(IC8-V3P3OUT-Pad15)")
  (net 325 "unconnected-(IC8-NENBL-Pad21)")
  (net 326 "unconnected-(IC9-V3P3OUT-Pad15)")
  (net 327 "unconnected-(IC9-NENBL-Pad21)")
  (net 328 "unconnected-(IC10-V3P3OUT-Pad15)")
  (net 329 "unconnected-(IC10-NENBL-Pad21)")
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 102.8273 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at 3.6727 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 169 "/RelayControl/XBT1_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 168 "/RelayControl/XBT1_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 167 "/RelayControl/XBT1_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/MALE_TBP02P1-381-03BE.step"
      (offset (xyz 7.5 -6.5 18.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 180 90))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 295.05 125.4 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K11" (at 2 -3 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 252 "unconnected-(K11-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 160 "xbt_C") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(K11-NO_1)") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 253 "Net-(K11--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 232 "/RelayControl/Reset3") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(K11-NO_1)") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 254 "unconnected-(K11-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Header_screw_7x1_TB001-500-07BE:CUI_TB001-500-07BE" (layer "F.Cu")
    (at 351 114 -90)
    (property "Cost" "0.96")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TB001-500-07BE/10064063")
    (property "Part" "TB001-500-07BE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J7" (at 31.25 6.75 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x07" (at 12.502 5.361 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J7-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 10 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 15 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 5 "+3.3V") (pinfunction "Pin_4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 20 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 191 "/I2C1_SDA") (pinfunction "Pin_5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 25 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 192 "/I2C1_SCL") (pinfunction "Pin_6") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 30 0 270) (size 1.95 1.95) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive") (solder_mask_margin 0.102))
    (model ":KICAD7_3DMODEL_DIR:TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-7_1x07_P5.00mm_Horizontal.step"
      (offset (xyz 30 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -180))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 74.8978 145)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.96 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 74.4486 144.4258)
          (xy 75.347 144.4258)
          (xy 75.347 145.5742)
          (xy 74.4486 145.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 277.8003 122)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R36" (at 3.1997 0 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "Net-(R36-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 277.5082 121.4412)
          (xy 278.0924 121.4412)
          (xy 278.0924 122.5588)
          (xy 277.5082 122.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 150.9278 164.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C69" (at 0.0722 2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 150.4786 163.9258)
          (xy 151.377 163.9258)
          (xy 151.377 165.0742)
          (xy 150.4786 165.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Images_logos:AOML_logo" (layer "F.Cu")
    (at 118.9 117.7)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 317.0842 153.5)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C62" (at -0.0842 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(IC8-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(IC8-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 316.635 152.9258)
          (xy 317.5334 152.9258)
          (xy 317.5334 154.0742)
          (xy 316.635 154.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 255.8003 127)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U15" (at -0.8003 -3) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(IC2-Q4)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "Net-(R38-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "/RelayControl/XBT6_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 58 178)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 7.1 -0.1) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 125.5 155.725)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C51" (at 0 -2.225 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 125.0508 155.1508)
          (xy 125.9492 155.1508)
          (xy 125.9492 156.2992)
          (xy 125.0508 156.2992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mosfet_BSS138PW:SC-70_SOT323_NEX-M" (layer "F.Cu")
    (at 340.2 157.7)
    (tags "BSS138PW_115 ")
    (property "Cost" "0.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/nexperia-usa-inc/BSS138PW-115/2779826?utm_adgroup=&utm_source=google&utm_medium=cpc&utm_campaign=PMax%20Supplier_Focus%20Supplier&utm_term=&utm_content=&utm_id=go_cmp-20243063242_adg-_ad-__dev-c_ext-_prd-_sig-CjwKCAjw65-zBhBkEiwAjrqRMF4G4BwjgMNveDGP77wLVM4s0FI1kyH44MSKZHqjQpmjM5HI8YLAxhoCdiYQAvD_BwE&gad_source=1&gclid=CjwKCAjw65-zBhBkEiwAjrqRMF4G4BwjgMNveDGP77wLVM4s0FI1kyH44MSKZHqjQpmjM5HI8YLAxhoCdiYQAvD_BwE")
    (property "Part" "BSS138PW,115")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "50V Vds, 0.22A Id, N-Channel MOSFET, SOT-23")
    (property "ki_keywords" "N-Channel MOSFET")
    (attr smd)
    (fp_text reference "Q1" (at 3 -0.6 unlocked) (layer "F.SilkS"))
    (fp_text value "BSS138" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.649999 0.9271) (size 0.508 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "Net-(Q1-G)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.649999 0.9271) (size 0.508 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 0 -0.9271) (size 0.508 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "/Din_fromGPS") (pinfunction "D") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/BSS138PW_115/SC-70_SOT323_NEX.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Current_sense_amp_INA213AIDCKR:DCK0006A_L" (layer "F.Cu")
    (at 76.7 163.3)
    (tags "INA213AIDCKR ")
    (property "Cost" "0.97")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/INA213AIDCKR/1898607")
    (property "Part" "INA213AIDCKR")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Bidirectional, Low- and High-Side Voltage Output, Current-Sense Amplifier, SOT-23-6")
    (property "ki_keywords" "current monitor shunt sensor bidirectional")
    (attr smd)
    (fp_text reference "U5" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "INA213AIDCKR" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "Designator60" (at -1.2192 -2.4892 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.024999 -0.650001 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "REF") (pintype "input"))
    (pad "2" smd rect (at -1.024999 0 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.024999 0.649999 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "V+") (pintype "power_in"))
    (pad "4" smd rect (at 1.025002 0.649999 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "Net-(JP4-B)") (pinfunction "+") (pintype "input"))
    (pad "5" smd rect (at 1.025002 0 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "Net-(JP5-B)") (pinfunction "-") (pintype "input"))
    (pad "6" smd rect (at 1.025002 -0.650001 90) (size 0.399999 0.650001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U6-PC1)") (pintype "output"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/CurrentSense_DCK0006A.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 275.25638 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K7" (at 5 -3.25638 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -3.76 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -3.76 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 237 "unconnected-(K7-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 185 "/RelayControl/XBT7_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 239 "Net-(K7--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/RelayControl/Reset2") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 186 "/RelayControl/XBT7_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 242 "unconnected-(K7-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 307.05 131.48)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP6" (at -1.8 -2.48) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 217 "Net-(JP6-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 211 "Net-(JP6-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 201.5472 141.75 180)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 3.2972 1 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 201.9964 142.3242)
          (xy 201.098 142.3242)
          (xy 201.098 141.1758)
          (xy 201.9964 141.1758)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_20pF-lowESR:CAPC220145_88N_KEM" (layer "F.Cu")
    (at 195 132 180)
    (tags "C0805C200J5GACTU ")
    (property "Cost" "0.27")
    (property "Digikey" "https://www.digikey.com/en/products/detail/kemet/C0805C200J5GAC7800/2212144")
    (property "Part" "C0805C200J5GAC7800")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0.25 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "20p" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.802799 0 180) (size 1.305598 1.449997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U6-PD1)") (pintype "passive"))
    (pad "2" smd rect (at 0.802799 0 180) (size 1.305598 1.449997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 195.0992 132.674199)
          (xy 194.9008 132.674199)
          (xy 194.9008 131.325801)
          (xy 195.0992 131.325801)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 100.3 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K1" (at 5.5 -2.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.16 -4 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0.16 -4 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 219 "unconnected-(K1-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 167 "/RelayControl/XBT1_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 220 "Net-(K1--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "/RelayControl/Reset1") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 168 "/RelayControl/XBT1_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 221 "unconnected-(K1-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 129.5 153.725 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 1.975 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(IC6-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 129.7921 154.2838)
          (xy 129.2079 154.2838)
          (xy 129.2079 153.1662)
          (xy 129.7921 153.1662)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 254.4142 153.425 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R35" (at -0.0858 1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(IC10-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 254.7063 153.9838)
          (xy 254.1221 153.9838)
          (xy 254.1221 152.8662)
          (xy 254.7063 152.8662)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 85.2978 148.04)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at -2.9 -0.7) (layer "F.SilkS"))
    (fp_text value "12V" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "+12V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 236.7443 120)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Cost" "0.16")
    (property "Digikey" "https://www.digikey.com/en/products/detail/microchip-technology/AT24C01D-STUM-T/4914368")
    (property "Part" "AT24C01D-STUM-T")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, SOT-23-5")
    (property "ki_keywords" "I2C Serial EEPROM Nonvolatile Memory")
    (attr smd)
    (fp_text reference "U7" (at -2.9943 -2.4) (layer "F.SilkS"))
    (fp_text value "AT24C01D-STUM-T" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 192 "/I2C1_SCL") (pinfunction "SCL") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "/I2C1_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "WP") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 342 107)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE076K8L/1079385")
    (property "Part" "RT0805FRE076K8L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 3.25 0.75 unlocked) (layer "F.SilkS"))
    (fp_text value "6.8k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "/UART3_RX") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 341.7079 106.4412)
          (xy 342.2921 106.4412)
          (xy 342.2921 107.5588)
          (xy 341.7079 107.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 198.9142 150.425)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C31" (at 1.7526 -1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 180.4473 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 3.5527 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 178 "/RelayControl/XBT4_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 177 "/RelayControl/XBT4_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 176 "/RelayControl/XBT4_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 76 108.5)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP12" (at -4 0) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 303 "Net-(JP12-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 162 "xbt_A") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (at 75.5 95.5)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Cost" "1.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/LM7805MPX-NOPB/6110583")
    (property "Part" "LM7805MPX/NOPB")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1A Low Dropout regulator, positive, 5.0V fixed output, SOT-223")
    (property "ki_keywords" "linear regulator ldo fixed positive")
    (attr smd)
    (fp_text reference "U2" (at -7.1 0.1) (layer "F.SilkS"))
    (fp_text value "LM7805MPX" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pinfunction "VI") (pintype "power_in") (zone_connect 1) (thermal_bridge_width 1))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_width 1))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_width 1.5))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 329.3 98.75 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP16" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 305 "Net-(J4-Pin_2)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 158 "xbt_B") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 103.5722 154.5)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C42" (at -0.0722 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(IC3-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(IC3-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 103.123 153.9258)
          (xy 104.0214 153.9258)
          (xy 104.0214 155.0742)
          (xy 103.123 155.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 340.2 166.1 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE075K1L/1079334")
    (property "Part" "RT0805FRE075K1L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R48" (at -0.0903 -1.8588 unlocked) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "Net-(Q1-G)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 340.4921 166.6588)
          (xy 339.9079 166.6588)
          (xy 339.9079 165.5412)
          (xy 340.4921 165.5412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 277.78368 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J14" (at 3.71632 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 187 "/RelayControl/XBT7_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 186 "/RelayControl/XBT7_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 185 "/RelayControl/XBT7_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 81.4978 152.2348 -90)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at 4.9652 -4.8022 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 3 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_8x1_216550:CONN_216550-1_TEC" (layer "F.Cu")
    (at 68.229001 125.6599 -90)
    (tags "216550-1 ")
    (property "Cost" "1.68")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216550-1/1920152")
    (property "Part" "216550-1")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "216550-1")
    (attr through_hole)
    (fp_text reference "J2" (at 4.445 3.229001 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "216550-1" (at 4.445 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.445 0 -90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.27 6.36 270) (size 3.3274 3.3274) (drill 3.3274) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 10.16 6.36 270) (size 3.3274 3.3274) (drill 3.3274) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 303 "Net-(JP12-A)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 165 "Net-(JP13-A)") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 161 "/Din_fromComputer") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 3.81 -2.54 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 42 "/+19.5V_raw") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 42 "/+19.5V_raw") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 6.35 -2.54 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 159 "/Dout_toComputer") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at 7.62 0 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 302 "Net-(JP14-A)") (pinfunction "7") (pintype "unspecified"))
    (pad "8" thru_hole circle (at 8.89 -2.54 270) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "unspecified"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/ul_216550-1/c-216550-1-k-3d.stp"
      (offset (xyz 4.5 -3.5 16.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 246 131)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP16" (at -0.25 -1.75) (layer "F.SilkS"))
    (fp_text value "3V3" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 5 "+3.3V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 125.4278 160.8426)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R21" (at -0.1778 -2.0926 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "Net-(IC6-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 125.1357 160.2838)
          (xy 125.7199 160.2838)
          (xy 125.7199 161.4014)
          (xy 125.1357 161.4014)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 154.9278 161)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R30" (at -3.6778 -1.25 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(IC9-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 154.6357 160.4412)
          (xy 155.2199 160.4412)
          (xy 155.2199 161.5588)
          (xy 154.6357 161.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 148.5 138)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "Vin-adc" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 209 "Net-(U18--)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (at 328.4 93.475 90)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (property "Cost" "0.6")
    (property "Digikey" "https://www.digikey.com/en/products/detail/sullins-connector-solutions/PPTC071LFBN-RC/810146")
    (property "Part" "PPTC071LFBN-RC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x07" (at 0 18.01 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 304 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 305 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 306 "Net-(J4-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 166 "/UART3_TX") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 307 "Net-(J4-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 235 131)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at -3.5 -1.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(U4-VS+)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 234.5508 130.4258)
          (xy 235.4492 130.4258)
          (xy 235.4492 131.5742)
          (xy 234.5508 131.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 293.97615 149.425)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C32" (at 1.77385 -1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 284.562 152.275 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 2.025 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(IC5-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 284.8541 152.8338)
          (xy 284.2699 152.8338)
          (xy 284.2699 151.7162)
          (xy 284.8541 151.7162)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 223.923048 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K5" (at 5.75 -2.923048 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 234 "unconnected-(K5-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 179 "/RelayControl/XBT5_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 238 "Net-(K5--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/RelayControl/Reset2") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 180 "/RelayControl/XBT5_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 240 "unconnected-(K5-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 333.6 98.75 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP17" (at 0.05 -2 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 306 "Net-(J4-Pin_3)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 160 "xbt_C") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 313.5842 153.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(IC8-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 313.8763 154.0588)
          (xy 313.2921 154.0588)
          (xy 313.2921 152.9412)
          (xy 313.8763 152.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 96 161)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R12" (at -3.25 0 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(IC3-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 95.7079 160.4412)
          (xy 96.2921 160.4412)
          (xy 96.2921 161.5588)
          (xy 95.7079 161.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 242 120)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 3 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 241.5508 119.4258)
          (xy 242.4492 119.4258)
          (xy 242.4492 120.5742)
          (xy 241.5508 120.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 200.475 124.25)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0.025 -1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 200.0258 123.6758)
          (xy 200.9242 123.6758)
          (xy 200.9242 124.8242)
          (xy 200.0258 124.8242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 88.5 133.9)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "Vin" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "/+19.5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_022uF:CAPC2012X135N" (layer "F.Cu")
    (at 69.75 102)
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B224KBFNNNE/3886751")
    (property "Part" "CL21B224KBFNNNE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 3.5 0) (layer "F.SilkS"))
    (fp_text value "0.22u" (at 1.59 1.27) (layer "F.Fab"))
    (pad "1" smd rect (at -0.863 0) (size 1.1 1.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 0.863 0) (size 1.1 1.38) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 223.843 155.55)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C58" (at -0.093 2.2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(IC7-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 223.3938 154.9758)
          (xy 224.2922 154.9758)
          (xy 224.2922 156.1242)
          (xy 223.3938 156.1242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Header_male_4x1:CONN_61300411121_WRE" (layer "F.Cu")
    (at 226 117 180)
    (tags "61300411121 ")
    (property "Cost" "0.19")
    (property "Digikey" "https://www.digikey.com/en/products/detail/w%C3%BCrth-elektronik/61300411121/4846827")
    (property "Part" "61300411121")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 10.75 -0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 313 "/VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 163 "/SWDIO") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 164 "/SWCLK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 1.651 1.651) (drill 1.143) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 57.46 108 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Cost" "0.34")
    (property "Digikey" "https://www.digikey.com/en/products/detail/sullins-connector-solutions/PPPC021LFBN-RC/810174")
    (property "Part" "PPPC021LFBN-RC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J24" (at 0.2 5.94) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/+19.5V_raw") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 178.15 130.5 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 313 "/VDD") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 5 "+3.3V") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 284.562 154.275)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C41" (at -0.312 2.225 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(IC5-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 284.1128 153.7008)
          (xy 285.0112 153.7008)
          (xy 285.0112 154.8492)
          (xy 284.1128 154.8492)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 152.288 122)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R40" (at -3.538 -0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "Net-(R40-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 151.9959 121.4412)
          (xy 152.5801 121.4412)
          (xy 152.5801 122.5588)
          (xy 151.9959 122.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Polyfuse_1A_1812:0ZCG_BEL" (layer "F.Cu")
    (at 349.5 151.5 180)
    (tags "0ZCG0050FF2C ")
    (property "Cost" "0.11")
    (property "Digikey" "https://www.digikey.com/en/products/detail/bel-fuse-inc/0ZCG0050FF2C/4156296")
    (property "Part" "0ZCG0050FF2C")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at -5.7 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "1A" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.6162 0 180) (size 1.778 3.5052) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd rect (at 2.6162 0 180) (size 1.778 3.5052) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "Net-(J3-Pin_1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 351.1764 153.2018)
          (xy 347.8236 153.2018)
          (xy 347.8236 149.7982)
          (xy 351.1764 149.7982)
        )
      )
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/0ZCG0050FF2C/0ZCG_BEL.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 218.6491 160.55)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R22" (at -1.6491 -2.3 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "Net-(IC7-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 218.357 159.9912)
          (xy 218.9412 159.9912)
          (xy 218.9412 161.1088)
          (xy 218.357 161.1088)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_driver_ULN2003ADR:D0016A_L" (layer "F.Cu")
    (at 212.5 108.5)
    (tags "ULN2003ADR ")
    (property "Cost" "0.46")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/ULN2003ADR/277011?s=N4IgTCBcDa4JwDYC0BGAzAgHKpA5AIiALoC%2BQA")
    (property "Part" "ULN2003ADR")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16")
    (property "ki_keywords" "darlington transistor array")
    (attr smd)
    (fp_text reference "U9" (at -4.111002 -6.5 unlocked) (layer "F.SilkS"))
    (fp_text value "ULN2003ADR" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "Designator9" (at -3.2004 -6.1468 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd oval (at -2.625001 -4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "relay_xbt7") (pinfunction "I1") (pintype "input"))
    (pad "2" smd oval (at -2.625001 -3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "relay_xbt8") (pinfunction "I2") (pintype "input"))
    (pad "3" smd oval (at -2.625001 -1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "relay_gnd_cond") (pinfunction "I3") (pintype "input"))
    (pad "4" smd oval (at -2.625001 -0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "relay_cal_cont") (pinfunction "I4") (pintype "input"))
    (pad "5" smd oval (at -2.625001 0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "relay_cal_res") (pinfunction "I5") (pintype "input"))
    (pad "6" smd oval (at -2.625001 1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "I6") (pintype "input"))
    (pad "7" smd oval (at -2.625001 3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "relay_reset3") (pinfunction "I7") (pintype "input"))
    (pad "8" smd oval (at -2.625001 4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "EN") (pintype "input"))
    (pad "9" smd oval (at 2.624999 4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "COM") (pintype "passive"))
    (pad "10" smd oval (at 2.624999 3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "/RelayControl/Reset3") (pinfunction "O7") (pintype "open_collector"))
    (pad "11" smd oval (at 2.624999 1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/RelayControl/Reset2") (pinfunction "O6") (pintype "open_collector"))
    (pad "12" smd oval (at 2.624999 0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "Net-(K12--_1)") (pinfunction "O5") (pintype "open_collector"))
    (pad "13" smd oval (at 2.624999 -0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "Net-(K11--_1)") (pinfunction "O4") (pintype "open_collector"))
    (pad "14" smd oval (at 2.624999 -1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "Net-(K10--_1)") (pinfunction "O3") (pintype "open_collector"))
    (pad "15" smd oval (at 2.624999 -3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "Net-(K8--_1)") (pinfunction "O2") (pintype "open_collector"))
    (pad "16" smd oval (at 2.624999 -4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(K7--_1)") (pinfunction "O1") (pintype "open_collector"))
    (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 184.9278 160.925)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R13" (at -1.1778 -2.175 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(IC4-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 184.6357 160.3662)
          (xy 185.2199 160.3662)
          (xy 185.2199 161.4838)
          (xy 184.6357 161.4838)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_047uF:CAP_CL_21_SAM" (layer "F.Cu")
    (at 241 131)
    (tags "CL21B474KBFNNNG ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B474KBFNNNG/3894539")
    (property "Part" "CL21B474KBFNNNG")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "0.47u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8763 0) (size 1.0668 1.3462) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.8763 0) (size 1.0668 1.3462) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 240.7079 130.3777)
          (xy 241.2921 130.3777)
          (xy 241.2921 131.6223)
          (xy 240.7079 131.6223)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Latch_CD4043BDR:SOIC127P600X175-16N" (layer "F.Cu")
    (at 141.288 124)
    (descr "D (R-PDSO-G16)")
    (tags "Integrated Circuit")
    (property "Cost" "0.49")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/CD4043BDR/1691049?s=N4IgTCBcDa4JwDYC0BmAjAFkUtSByAIiALoC%2BQA")
    (property "Part" "CD4043BDR")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "CMOS Quad NOR R/S Latch with 3-State Outputs")
    (attr smd)
    (fp_text reference "IC1" (at -2.038 7.25) (layer "F.SilkS"))
    (fp_text value "CD4043BDR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.712 -4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(IC1-Q4)") (pinfunction "Q4") (pintype "passive"))
    (pad "2" smd rect (at -2.712 -3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(IC1-Q1)") (pinfunction "Q1") (pintype "passive"))
    (pad "3" smd rect (at -2.712 -1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "R1") (pintype "passive"))
    (pad "4" smd rect (at -2.712 -0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "SSR_xbt1") (pinfunction "S1") (pintype "passive"))
    (pad "5" smd rect (at -2.712 0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "ENABLE") (pintype "passive"))
    (pad "6" smd rect (at -2.712 1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "SSR_xbt4") (pinfunction "S2") (pintype "passive"))
    (pad "7" smd rect (at -2.712 3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "R2") (pintype "passive"))
    (pad "8" smd rect (at -2.712 4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "9" smd rect (at 2.712 4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(IC1-Q2)") (pinfunction "Q2") (pintype "passive"))
    (pad "10" smd rect (at 2.712 3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(IC1-Q3)") (pinfunction "Q3") (pintype "passive"))
    (pad "11" smd rect (at 2.712 1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "R3") (pintype "passive"))
    (pad "12" smd rect (at 2.712 0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "SSR_xbt3") (pinfunction "S3") (pintype "passive"))
    (pad "13" smd rect (at 2.712 -0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(IC1-NC-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd rect (at 2.712 -1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "SSR_xbt2") (pinfunction "S4") (pintype "passive"))
    (pad "15" smd rect (at 2.712 -3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "R4") (pintype "passive"))
    (pad "16" smd rect (at 2.712 -4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "VDD") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 180.3694 115.8322)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at 3.1306 -0.0822 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(SW1-A)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 179.9202 115.258)
          (xy 180.8186 115.258)
          (xy 180.8186 116.4064)
          (xy 179.9202 116.4064)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 342 104)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE073K3L/1079226")
    (property "Part" "RT0805FRE073K3L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at 3.5 -0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "/UART3_RX") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "Net-(J4-Pin_6)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 341.7079 103.4412)
          (xy 342.2921 103.4412)
          (xy 342.2921 104.5588)
          (xy 341.7079 104.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 186 116)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 2.5 -0.25) (layer "F.SilkS"))
    (fp_text value "D3V3" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 313 "/VDD") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 305.4278 164)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C56" (at 0.0722 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 304.9786 163.4258)
          (xy 305.877 163.4258)
          (xy 305.877 164.5742)
          (xy 304.9786 164.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 155 156)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C68" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 154.5508 155.4258)
          (xy 155.4492 155.4258)
          (xy 155.4492 156.5742)
          (xy 154.5508 156.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 250.4142 155.425)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C70" (at 0 -2.425 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 249.965 154.8508)
          (xy 250.8634 154.8508)
          (xy 250.8634 155.9992)
          (xy 249.965 155.9992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 162.9278 129.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 3.3222 -1.25) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 58 92)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -6.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 356 178)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -6.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 96 164.5)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(IC3-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 95.7079 163.9412)
          (xy 96.2921 163.9412)
          (xy 96.2921 165.0588)
          (xy 95.7079 165.0588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 309.4278 160.6)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R23" (at -1.9278 -2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(IC8-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 309.1357 160.0412)
          (xy 309.7199 160.0412)
          (xy 309.7199 161.1588)
          (xy 309.1357 161.1588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 179 151.25)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP17" (at 3 -1.25) (layer "F.SilkS"))
    (fp_text value "DIR" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 73 "DIR") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 295.05 141.48 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K9" (at 2.54 -3 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 217 "Net-(JP6-A)") (pinfunction "NC_1") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 211 "Net-(JP6-B)") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 250 "Net-(K10--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 232 "/RelayControl/Reset3") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 212 "Net-(JP7-B)") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 218 "Net-(JP7-A)") (pinfunction "NC_2") (pintype "passive"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 130.576 127)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U10" (at -2.288 -3) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(IC1-Q1)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "Net-(R43-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "/RelayControl/XBT1_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Shunt_PE2512FKE070R1L:RESC6331X89N" (layer "F.Cu")
    (at 64.7 165.4 90)
    (property "Cost" "0.6")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/PE2512FKE070R1L/5138678")
    (property "Part" "PE2512FKE070R1L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -0.176 0 90) (layer "F.SilkS"))
    (fp_text value "0.1" (at -0.91 2.31 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.926 0 90) (size 1.46 3.44) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "Net-(JP2-B)") (pintype "passive") (solder_mask_margin 0.102) (zone_connect 1) (thermal_bridge_width 2.5))
    (pad "2" smd rect (at 2.926 0 90) (size 1.46 3.44) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pintype "passive") (solder_mask_margin 0.102) (zone_connect 1) (thermal_bridge_width 2.5))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/Resistor_current_PE2512FKE070R1L.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 322.2014 131.48)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP8" (at -4.2014 0.02) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 213 "Net-(JP8-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 214 "Net-(JP8-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Zener_3V3_BZT52C3V3-7-F:SOD3715X135N" (layer "F.Cu")
    (at 82.955 167.8 180)
    (property "Cost" "0.21")
    (property "Digikey" "https://www.digikey.com/en/products/detail/diodes-incorporated/BZT52C3V3-7-F/717734")
    (property "Part" "BZT52C3V3-7-F")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at 0.155 2.1) (layer "F.SilkS"))
    (fp_text value "3.3V" (at 5.08 1.905) (layer "F.Fab"))
    (pad "A" smd rect (at 1.68 0 180) (size 1.21 0.73) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.102))
    (pad "K" smd rect (at -1.68 0 180) (size 1.21 0.73) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U6-PC1)") (pinfunction "K") (pintype "passive") (solder_mask_margin 0.102))
    (model ":KICAD7_3DMODEL_DIR:Diode_SMD.3dshapes/D_SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 288.062 152.275)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C44" (at 0 -2.025 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(IC5-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(IC5-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 287.6128 151.7008)
          (xy 288.5112 151.7008)
          (xy 288.5112 152.8492)
          (xy 287.6128 152.8492)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "STM32F103RBT6TR:LQFP64-10x10mm" (layer "F.Cu")
    (at 206 133)
    (tags "STM32F103RBT6TR ")
    (property "Cost" "7.5")
    (property "Digikey" "https://www.digikey.com/en/products/detail/stmicroelectronics/STM32F103RBT6TR/2122443")
    (property "Part" "STM32F103RBT6TR")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64")
    (property "ki_keywords" "Arm Cortex-M3 STM32F1 STM32F103")
    (attr smd)
    (fp_text reference "U6" (at 0 0 unlocked) (layer "F.SilkS"))
    (fp_text value "STM32F103RBTx" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -5.749999 -3.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pinfunction "VBAT") (pintype "power_in"))
    (pad "2" smd rect (at -5.749999 -3.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "SSR_xbt3") (pinfunction "PC13") (pintype "bidirectional"))
    (pad "3" smd rect (at -5.749999 -2.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "SSR_xbt2") (pinfunction "PC14") (pintype "bidirectional"))
    (pad "4" smd rect (at -5.749999 -2.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "SSR_xbt1") (pinfunction "PC15") (pintype "bidirectional"))
    (pad "5" smd rect (at -5.749999 -1.749999) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U6-PD0)") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "6" smd rect (at -5.749999 -1.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U6-PD1)") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "7" smd rect (at -5.749999 -0.750001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(SW1-A)") (pinfunction "NRST") (pintype "input"))
    (pad "8" smd rect (at -5.749999 -0.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "Net-(U18--)") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "9" smd rect (at -5.749999 0.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U6-PC1)") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "10" smd rect (at -5.749999 0.750001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Enable_M1") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "11" smd rect (at -5.749999 1.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Enable_M2") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "12" smd rect (at -5.749999 1.749999) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSSA") (pintype "power_in"))
    (pad "13" smd rect (at -5.749999 2.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "/VDDA") (pinfunction "VDDA") (pintype "power_in"))
    (pad "14" smd rect (at -5.749999 2.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "Enable_M3") (pinfunction "PA0") (pintype "bidirectional"))
    (pad "15" smd rect (at -5.749999 3.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Enable_M4") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "16" smd rect (at -5.749999 3.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "/MUX_select") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "17" smd rect (at -3.75 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "unconnected-(U6-PA3-Pad17)") (pinfunction "PA3") (pintype "bidirectional+no_connect"))
    (pad "18" smd rect (at -3.250001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "19" smd rect (at -2.75 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "20" smd rect (at -2.250001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Enable_M5") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "21" smd rect (at -1.749999 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Enable_M6") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "22" smd rect (at -1.25 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "Enable_M7") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "23" smd rect (at -0.750001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Enable_M8") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "24" smd rect (at -0.25 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "25" smd rect (at 0.25 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "unconnected-(U6-PC5-Pad25)") (pinfunction "PC5") (pintype "bidirectional+no_connect"))
    (pad "26" smd rect (at 0.750001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "27" smd rect (at 1.25 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "Net-(D7-A)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "28" smd rect (at 1.749999 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "unconnected-(U6-PB2-Pad28)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "29" smd rect (at 2.250001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/UART3_TX") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "30" smd rect (at 2.75 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "/UART3_RX") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "31" smd rect (at 3.250001 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "32" smd rect (at 3.75 5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "33" smd rect (at 5.749999 3.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "unconnected-(U6-PB12-Pad33)") (pinfunction "PB12") (pintype "bidirectional+no_connect"))
    (pad "34" smd rect (at 5.749999 3.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J7-Pin_1)") (pinfunction "PB13") (pintype "bidirectional"))
    (pad "35" smd rect (at 5.749999 2.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "SSR_xbt8") (pinfunction "PB14") (pintype "bidirectional"))
    (pad "36" smd rect (at 5.749999 2.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "SSR_xbt7") (pinfunction "PB15") (pintype "bidirectional"))
    (pad "37" smd rect (at 5.749999 1.749999) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "SSR_xbt6") (pinfunction "PC6") (pintype "bidirectional"))
    (pad "38" smd rect (at 5.749999 1.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "SSR_xbt5") (pinfunction "PC7") (pintype "bidirectional"))
    (pad "39" smd rect (at 5.749999 0.750001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "relay_reset3") (pinfunction "PC8") (pintype "bidirectional"))
    (pad "40" smd rect (at 5.749999 0.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "PC9") (pintype "bidirectional"))
    (pad "41" smd rect (at 5.749999 -0.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "relay_cal_res") (pinfunction "PA8") (pintype "bidirectional"))
    (pad "42" smd rect (at 5.749999 -0.750001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "/UART1_TX") (pinfunction "PA9") (pintype "bidirectional"))
    (pad "43" smd rect (at 5.749999 -1.25) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "/UART1_RX") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "44" smd rect (at 5.749999 -1.749999) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "relay_cal_cont") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "45" smd rect (at 5.749999 -2.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "relay_gnd_cond") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "46" smd rect (at 5.749999 -2.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/SWDIO") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "47" smd rect (at 5.749999 -3.250001) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "48" smd rect (at 5.749999 -3.75) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "49" smd rect (at 3.75 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "/SWCLK") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "50" smd rect (at 3.250001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "relay_xbt8") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "51" smd rect (at 2.75 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "relay_xbt7") (pinfunction "PC10") (pintype "bidirectional"))
    (pad "52" smd rect (at 2.250001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "relay_xbt1") (pinfunction "PC11") (pintype "bidirectional"))
    (pad "53" smd rect (at 1.749999 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "relay_xbt2") (pinfunction "PC12") (pintype "bidirectional"))
    (pad "54" smd rect (at 1.25 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "relay_xbt3") (pinfunction "PD2") (pintype "bidirectional"))
    (pad "55" smd rect (at 0.750001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "relay_xbt4") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "56" smd rect (at 0.25 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "relay_xbt5") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "57" smd rect (at -0.25 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "relay_xbt6") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "58" smd rect (at -0.750001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "/I2C1_SCL") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "59" smd rect (at -1.25 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "/I2C1_SDA") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "60" smd rect (at -1.749999 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "Net-(U6-BOOT0)") (pinfunction "BOOT0") (pintype "input"))
    (pad "61" smd rect (at -2.250001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "PB8") (pintype "bidirectional"))
    (pad "62" smd rect (at -2.75 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "SSR_xbt4") (pinfunction "PB9") (pintype "bidirectional"))
    (pad "63" smd rect (at -3.250001 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "64" smd rect (at -3.75 -5.749999 90) (size 1.1938 0.3048) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pinfunction "VDD") (pintype "power_in"))
    (model ":KICAD7_3DMODEL_DIR:Package_QFP.3dshapes/HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 193.57225 153.925)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C43" (at 0 -1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(IC4-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(IC4-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 193.12305 153.3508)
          (xy 194.02145 153.3508)
          (xy 194.02145 154.4992)
          (xy 193.12305 154.4992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal_8mhz_small:XTAL_ABM3-8.000MHZ-D2Y-T_ABR-M" (layer "F.Cu")
    (at 185.5 130.5 180)
    (tags "ABM3-8.000MHZ-D2Y-T ")
    (property "Cost" "0.57")
    (property "Digikey" "https://www.digikey.com/en/products/detail/abracon-llc/ABM3-8-000MHZ-D2Y-T/2344570")
    (property "Part" "ABM3-8.000MHZ-D2Y-T")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Two pin crystal")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y1" (at 4.2 2.4 unlocked) (layer "F.SilkS"))
    (fp_text value "8MHz" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.7018 0 270) (size 2.0066 2.3114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U6-PD0)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.7018 0 270) (size 2.0066 2.3114) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U6-PD1)") (pinfunction "2") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 185.9953 131.5541)
          (xy 185.0047 131.5541)
          (xy 185.0047 129.4459)
          (xy 185.9953 129.4459)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 188.0527 129.4459)
          (xy 182.9473 129.4459)
          (xy 182.9473 128.849)
          (xy 188.0527 128.849)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 188.0527 132.151)
          (xy 182.9473 132.151)
          (xy 182.9473 131.5541)
          (xy 188.0527 131.5541)
        )
      )
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/ABM3_8_000MHZ_D2Y_T/XTAL_ABM3-8_000MHZ-D2Y-T_ABR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 219.843 155.55)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C53" (at -0.093 -2.05 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 219.3938 154.9758)
          (xy 220.2922 154.9758)
          (xy 220.2922 156.1242)
          (xy 219.3938 156.1242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 356 92)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -6.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 152.288 118)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U13" (at -2.038 -3.25) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(IC1-Q2)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "Net-(R40-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "/RelayControl/XBT4_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 207 92)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -6.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 193.4028 136 180)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 4.6528 0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "/VDDA") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 193.852 136.5742)
          (xy 192.9536 136.5742)
          (xy 192.9536 135.4258)
          (xy 193.852 135.4258)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 277.795 118)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U17" (at -2 -3) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(IC2-Q2)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "Net-(R36-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "/RelayControl/XBT8_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 252.117014 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J13" (at 3.882986 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 184 "/RelayControl/XBT6_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 183 "/RelayControl/XBT6_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 182 "/RelayControl/XBT6_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 129.5 155.725)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C57" (at 0 2.025 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(IC6-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 129.0508 155.1508)
          (xy 129.9492 155.1508)
          (xy 129.9492 156.2992)
          (xy 129.0508 156.2992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 238 141)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 4 0 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(U4-VS-)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 237.5508 140.4258)
          (xy 238.4492 140.4258)
          (xy 238.4492 141.5742)
          (xy 237.5508 141.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 300.923048 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K8" (at 5 -3.423048 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 243 "unconnected-(K8-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 188 "/RelayControl/XBT8_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 244 "Net-(K8--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/RelayControl/Reset2") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 189 "/RelayControl/XBT8_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 245 "unconnected-(K8-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 230 137)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(U4-C2+)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(U4-C2-)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 229.5508 136.4258)
          (xy 230.4492 136.4258)
          (xy 230.4492 137.5742)
          (xy 229.5508 137.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 121.4278 164.225)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C52" (at 0 2.275 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 120.9786 163.6508)
          (xy 121.877 163.6508)
          (xy 121.877 164.7992)
          (xy 120.9786 164.7992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 255.795 118)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U14" (at -1.045 -3.25) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(IC2-Q1)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "/RelayControl/XBT5_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 257.9864 153.425)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C75" (at 0 -1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(IC10-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(IC10-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 257.5372 152.8508)
          (xy 258.4356 152.8508)
          (xy 258.4356 153.9992)
          (xy 257.5372 153.9992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 62.48 103.4 -90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Cost" "0.38")
    (property "Digikey" "https://www.digikey.com/en/products/detail/sullins-connector-solutions/PPPC031LFBN-RC/810175")
    (property "Part" "PPPC031LFBN-RC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.32 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 159 "/Dout_toComputer") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 161 "/Din_fromComputer") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 126.173333 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K2" (at 5.5 -2.673333 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0.54 -3.84 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0.54 -3.84 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 222 "unconnected-(K2-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 170 "/RelayControl/XBT2_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 223 "Net-(K2--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "/RelayControl/Reset1") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 171 "/RelayControl/XBT2_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 224 "unconnected-(K2-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_driver_ULN2003ADR:D0016A_L" (layer "F.Cu")
    (at 201.375001 108.595)
    (tags "ULN2003ADR ")
    (property "Cost" "0.46")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/ULN2003ADR/277011?s=N4IgTCBcDa4JwDYC0BGAzAgHKpA5AIiALoC%2BQA")
    (property "Part" "ULN2003ADR")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16")
    (property "ki_keywords" "darlington transistor array")
    (attr smd)
    (fp_text reference "U8" (at 3.374999 -6.595 unlocked) (layer "F.SilkS"))
    (fp_text value "ULN2003ADR" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "Designator9" (at -3.2004 -6.1468 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd oval (at -2.625001 -4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "relay_xbt1") (pinfunction "I1") (pintype "input"))
    (pad "2" smd oval (at -2.625001 -3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "relay_xbt2") (pinfunction "I2") (pintype "input"))
    (pad "3" smd oval (at -2.625001 -1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "relay_xbt3") (pinfunction "I3") (pintype "input"))
    (pad "4" smd oval (at -2.625001 -0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "relay_xbt4") (pinfunction "I4") (pintype "input"))
    (pad "5" smd oval (at -2.625001 0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "relay_xbt5") (pinfunction "I5") (pintype "input"))
    (pad "6" smd oval (at -2.625001 1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "relay_xbt6") (pinfunction "I6") (pintype "input"))
    (pad "7" smd oval (at -2.625001 3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "I7") (pintype "input"))
    (pad "8" smd oval (at -2.625001 4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "EN") (pintype "input"))
    (pad "9" smd oval (at 2.624999 4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "COM") (pintype "passive"))
    (pad "10" smd oval (at 2.624999 3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/RelayControl/Reset1") (pinfunction "O7") (pintype "open_collector"))
    (pad "11" smd oval (at 2.624999 1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "Net-(K6--_1)") (pinfunction "O6") (pintype "open_collector"))
    (pad "12" smd oval (at 2.624999 0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "Net-(K5--_1)") (pinfunction "O5") (pintype "open_collector"))
    (pad "13" smd oval (at 2.624999 -0.635 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "Net-(K4--_1)") (pinfunction "O4") (pintype "open_collector"))
    (pad "14" smd oval (at 2.624999 -1.905 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "Net-(K3--_1)") (pinfunction "O3") (pintype "open_collector"))
    (pad "15" smd oval (at 2.624999 -3.175 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "Net-(K2--_1)") (pinfunction "O2") (pintype "open_collector"))
    (pad "16" smd oval (at 2.624999 -4.445 90) (size 0.549999 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "Net-(K1--_1)") (pinfunction "O1") (pintype "open_collector"))
    (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_green_0603:LED_B1911PG--20D000514U1930_HVK" (layer "F.Cu")
    (at 80.0382 145 180)
    (tags "B1911PG--20D000514U1930 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/harvatek-corporation/B1911PG-20D000514U1930/15519992")
    (property "Part" "B1911PG--20D000514U1930")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D4" (at 0 1.96 unlocked) (layer "F.SilkS"))
    (fp_text value "led" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pinfunction "A") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 219.5722 164.05)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R25" (at -0.0722 2.2 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(IC7-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 219.2801 163.4912)
          (xy 219.8643 163.4912)
          (xy 219.8643 164.6088)
          (xy 219.2801 164.6088)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 190.00005 153.925 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R19" (at 0.00005 1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(IC4-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 190.29215 154.4838)
          (xy 189.70795 154.4838)
          (xy 189.70795 153.3662)
          (xy 190.29215 153.3662)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 280.562 154.275)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C37" (at 0.188 -2.275 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 280.1128 153.7008)
          (xy 281.0112 153.7008)
          (xy 281.0112 154.8492)
          (xy 280.1128 154.8492)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 314.5014 141.48 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K10" (at 2.54 -2.4514 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 249 "unconnected-(K10-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 241 "unconnected-(K10-COM_1-Pad4)") (pinfunction "COM_1") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 246 "unconnected-(K10-NO_1-Pad5)") (pinfunction "NO_1") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 250 "Net-(K10--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 232 "/RelayControl/Reset3") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 214 "Net-(JP8-B)") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 160 "xbt_C") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 213 "Net-(JP8-A)") (pinfunction "NC_2") (pintype "passive"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 121.5 134.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP15" (at -0.75 -2) (layer "F.SilkS"))
    (fp_text value "Vref" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 167.91415 150.5)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C66" (at 1.83585 -2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 152.288 131)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R41" (at -3.538 0 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "Net-(R41-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 151.9959 130.4412)
          (xy 152.5801 130.4412)
          (xy 152.5801 131.5588)
          (xy 151.9959 131.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 189 142)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at -0.25 -2) (layer "F.SilkS"))
    (fp_text value "A3V3" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 284 "/VDDA") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_20pF-lowESR:CAPC220145_88N_KEM" (layer "F.Cu")
    (at 195 129 180)
    (tags "C0805C200J5GACTU ")
    (property "Cost" "0.27")
    (property "Digikey" "https://www.digikey.com/en/products/detail/kemet/C0805C200J5GAC7800/2212144")
    (property "Part" "C0805C200J5GAC7800")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0.25 2 unlocked) (layer "F.SilkS"))
    (fp_text value "20p" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.802799 0 180) (size 1.305598 1.449997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U6-PD0)") (pintype "passive"))
    (pad "2" smd rect (at 0.802799 0 180) (size 1.305598 1.449997) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 195.0992 129.674199)
          (xy 194.9008 129.674199)
          (xy 194.9008 128.325801)
          (xy 195.0992 128.325801)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 177.92 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K4" (at 5 -2.92 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 228 "unconnected-(K4-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 176 "/RelayControl/XBT4_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 229 "Net-(K4--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "/RelayControl/Reset1") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 177 "/RelayControl/XBT4_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 230 "unconnected-(K4-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_6.4mm_M6_ISO7380_Pad" (layer "F.Cu")
    (at 207 178)
    (descr "Mounting Hole 6.4mm, M6, ISO7380")
    (tags "mounting hole 6.4mm m6 iso7380")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (clearance 1)
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -6.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.5 8.5) (drill 6.35) (layers "F&B.Cu" "*.Mask")
      (clearance 0.5))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 85.3176 145 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-072K4L/727690")
    (property "Part" "RC0805FR-072K4L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R44" (at 0.0698 2.46 unlocked) (layer "F.SilkS"))
    (fp_text value "2.4k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "Net-(D4-K)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 85.6097 145.5588)
          (xy 85.0255 145.5588)
          (xy 85.0255 144.4412)
          (xy 85.6097 144.4412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 309.5842 155.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C55" (at 0 -2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 309.135 154.9258)
          (xy 310.0334 154.9258)
          (xy 310.0334 156.0742)
          (xy 309.135 156.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 162.9278 125.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at 3.0722 -0.25) (layer "F.SilkS"))
    (fp_text value "3V3" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 5 "+3.3V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 185.5722 164.425)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 2.325 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(IC4-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 185.2801 163.8662)
          (xy 185.8643 163.8662)
          (xy 185.8643 164.9838)
          (xy 185.2801 164.9838)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 262.5 161)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC10" (at 6.75 -5) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(IC10-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(IC10-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(IC10-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "Net-(IC10-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(IC10-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(IC10-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(IC10-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(IC10-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(IC10-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "unconnected-(IC10-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Enable_M6") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Enable_M6") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "unconnected-(IC10-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "unconnected-(IC10-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "unconnected-(IC10-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "unconnected-(IC10-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "unconnected-(IC10-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 85.4 162.3)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0.1 2.1) (layer "F.SilkS"))
    (fp_text value "MotorCurrent-adc" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 43 "Net-(U6-PC1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 298.24 115.4)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/CFR-25JR-52-15K/12002")
    (property "Part" "CFR-25JR-52-15K")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R11" (at -3.74 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(K11-NO_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 99.9278 156.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C39" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(IC3-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 99.4786 155.9258)
          (xy 100.377 155.9258)
          (xy 100.377 157.0742)
          (xy 99.4786 157.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_1uF-ceramic:CAP_CL21_SAM" (layer "F.Cu")
    (at 193.4028 138.25 180)
    (tags "CL21B105KBFNNNE ")
    (property "Cost" "0.11")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B105KBFNNNE/3886687")
    (property "Part" "CL21B105KBFNNNE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 4.9028 0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "/VDDA") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 193.852 138.8242)
          (xy 192.9536 138.8242)
          (xy 192.9536 137.6758)
          (xy 193.852 137.6758)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 94.5 101.5)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 0 2) (layer "F.SilkS"))
    (fp_text value "5V" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 4 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 229.9278 134 180)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at -0.0722 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U4-C1+)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U4-C1-)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 230.377 134.5742)
          (xy 229.4786 134.5742)
          (xy 229.4786 133.4258)
          (xy 230.377 133.4258)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "OpAmp_LMV321B-TR:S5TSOT23-5-A_TPK-M" (layer "F.Cu")
    (at 141.7105 137.049999)
    (tags "LMV321B-TR ")
    (property "Cost" "0.34")
    (property "Digikey" "https://www.digikey.com/en/products/detail/3peak/LMV321B-TR/22228606")
    (property "Part" "LMV321B-TR")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low Power Single Operational Amplifier, SOT-23-5")
    (property "ki_keywords" "single opamp")
    (attr smd)
    (fp_text reference "U18" (at 3.2895 -2.299999 unlocked) (layer "F.SilkS"))
    (fp_text value "LMV321B-TR" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.7145 -2.601) (layer "F.SilkS"))
    (fp_text user "*" (at -1.7145 -2.601 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.6096 -1.5088 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -0.6096 -1.5088) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4605 -0.950001) (size 1.1938 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U18-+)") (pinfunction "+") (pintype "input"))
    (pad "2" smd rect (at -1.4605 0) (size 1.1938 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd rect (at -1.4605 0.950001) (size 1.1938 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "Net-(U18--)") (pinfunction "-") (pintype "input"))
    (pad "4" smd rect (at 1.4605 0.950001) (size 1.1938 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "Net-(U18--)") (pintype "output"))
    (pad "5" smd rect (at 1.4605 -0.950001) (size 1.1938 0.508) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "V+") (pintype "power_in"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/LMV321B_TR/S5T_SOT23-5-A__TPK.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Network_resistor_10k_bussed:746X101103JP-3" (layer "F.Cu")
    (at 201.374999 100.22 -90)
    (descr "746X101103JP-3")
    (tags "Resistor Network (8-Pin)")
    (property "Cost" "0.22")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cts-resistor-products/746X101103JP/1118444")
    (property "Part" "746X101103JP")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor Networks & Arrays 10Kohms 25V 5%")
    (attr smd)
    (fp_text reference "RN1" (at -0.02 3.374999 90) (layer "F.SilkS"))
    (fp_text value "746X101103JP" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.28 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "relay_xbt4") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -0.64 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "relay_xbt3") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "relay_xbt2") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 0.64 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "relay_xbt1") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at 1.28 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect (at 1.28 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "relay_xbt5") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect (at 0 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "relay_reset1") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect (at 0.64 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "relay_xbt6") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect (at -0.64 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "unconnected-(RN1-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" smd rect (at -1.28 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "10") (pintype "passive"))
    (model "746X101103JP.stp"
      (offset (xyz -1.769999954 -1.070000036 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 246.3509 163.925)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C71" (at -0.1009 2.075 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 245.9017 163.3508)
          (xy 246.8001 163.3508)
          (xy 246.8001 164.4992)
          (xy 245.9017 164.4992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_033uF:CAP_CL21_SAM" (layer "F.Cu")
    (at 69.5978 142.84)
    (tags "CL21B334KBFNNNE ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B334KBFNNNE/3886781")
    (property "Part" "CL21B334KBFNNNE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.6978 0 unlocked) (layer "F.SilkS"))
    (fp_text value "0.33u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/+19.5V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 69.1486 142.2658)
          (xy 70.047 142.2658)
          (xy 70.047 143.4142)
          (xy 69.1486 143.4142)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 159.0722 156)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C72" (at 0.1778 2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(IC9-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 158.623 155.4258)
          (xy 159.5214 155.4258)
          (xy 159.5214 156.5742)
          (xy 158.623 156.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT1000uF:CAP_PK&slash_PZ_10X16_LOW_RUB" (layer "F.Cu")
    (at 89 123 90)
    (tags "25PX1000MEFCT810X16 ")
    (property "Cost" "0.67")
    (property "Digikey" "https://www.digikey.com/en/products/detail/rubycon/25PX1000MEFCT810X16/3134863")
    (property "Part" "25PX1000MEFCT810X16")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1000u" (at 2.5 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 1 "/+19.5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/25PX1000MEFCT810X16/CAP_PKPZ_10X16_LOW_RUB.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 85.66415 95.5)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at 1.58585 5.25 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D10.0mm_H20.0mm_P5.00mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 96 156.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C33" (at -3.5 0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 95.5508 155.9258)
          (xy 96.4492 155.9258)
          (xy 96.4492 157.0742)
          (xy 95.5508 157.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 108 162)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC3" (at 7 -6) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(IC3-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(IC3-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(IC3-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(IC3-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(IC3-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(IC3-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(IC3-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(IC3-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(IC3-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "unconnected-(IC3-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Enable_M1") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Enable_M1") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "unconnected-(IC3-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "unconnected-(IC3-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "unconnected-(IC3-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "unconnected-(IC3-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "unconnected-(IC3-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Shottky_B340AE_13:CR_SMA_320-340AE_DIO" (layer "F.Cu")
    (at 80 133 180)
    (tags "B340AE-13 ")
    (property "Cost" "0.37")
    (property "Digikey" "https://www.digikey.com/en/products/detail/diodes-incorporated/B340AE-13/7352831")
    (property "Part" "B340AE-13")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "30V 3A Schottky Barrier Rectifier Diode, DO-201AD")
    (property "ki_keywords" "diode Schottky")
    (zone_connect 1)
    (attr smd)
    (fp_text reference "D1" (at 0 -3 unlocked) (layer "F.SilkS"))
    (fp_text value "B340AE-13" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.8542 0 270) (size 1.6256 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/+19.5V") (pinfunction "K") (pintype "passive") (thermal_bridge_width 1.5))
    (pad "2" smd rect (at 1.8542 0 270) (size 1.6256 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/+19.5V_raw") (pinfunction "A") (pintype "passive") (zone_connect 1) (thermal_bridge_width 1.5))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 80.7112 133.8636)
          (xy 79.2888 133.8636)
          (xy 79.2888 132.1364)
          (xy 80.7112 132.1364)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 82.7432 132.1364)
          (xy 77.2568 132.1364)
          (xy 77.2568 131.5903)
          (xy 82.7432 131.5903)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 82.7432 134.4097)
          (xy 77.2568 134.4097)
          (xy 77.2568 133.8636)
          (xy 82.7432 133.8636)
        )
      )
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/Diode_B340AE-13.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 314.5014 125.48 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K12" (at 2.08 -2.4514 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 255 "unconnected-(K12-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 248 "Net-(K12-NO_1)") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 231 "Net-(K12--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 232 "/RelayControl/Reset3") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 251 "unconnected-(K12-NO_2-Pad8)") (pinfunction "NO_2") (pintype "passive+no_connect"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 256 "unconnected-(K12-COM_2-Pad9)") (pinfunction "COM_2") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 257 "unconnected-(K12-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 255.795 122)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R39" (at 3.205 0 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 255.5029 121.4412)
          (xy 256.0871 121.4412)
          (xy 256.0871 122.5588)
          (xy 255.5029 122.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 76 114.5)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP14" (at -4 0) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 302 "Net-(JP14-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 160 "xbt_C") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 128.700633 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 3.299367 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 172 "/RelayControl/XBT2_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 171 "/RelayControl/XBT2_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 170 "/RelayControl/XBT2_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 213.975 126.25)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0.025 -2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 213.5258 125.6758)
          (xy 214.4242 125.6758)
          (xy 214.4242 126.8242)
          (xy 213.5258 126.8242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (at 167.4278 138.25)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Cost" "0.69")
    (property "Digikey" "https://www.digikey.com/en/products/detail/microchip-technology/MCP1825ST-3302E-DB/1635518")
    (property "Part" "MCP1825ST-3302E/DB")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "800mA Fixed Low Drop Positive Voltage Regulator, Fixed Output 1.2V, SOT-223")
    (property "ki_keywords" "REGULATOR LDO 1.2V")
    (attr smd)
    (fp_text reference "U3" (at 3.2722 -4.85) (layer "F.SilkS"))
    (fp_text value "MCP1825ST-3302E/DB" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (zone_connect 1) (thermal_bridge_width 1.5))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 250.3509 163.925)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R33" (at -0.1009 2.075 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(IC10-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 250.0588 163.3662)
          (xy 250.643 163.3662)
          (xy 250.643 164.4838)
          (xy 250.0588 164.4838)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Images_logos:xbt" (layer "F.Cu")
    (at 353.850235 102.25945 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Dip_switch_DS01C-254-L-03BE:SW_DS01C-254-L-03BE" (layer "F.Cu")
    (at 104 133 180)
    (property "Cost" "0.57")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/DS01C-254-L-03BE/11310858")
    (property "Part" "DS01C-254-L-03BE")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
    (property "ki_keywords" "dip switch")
    (attr through_hole)
    (fp_text reference "SW2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "SW_DIP_x03" (at 11.891 7.111) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.54 -3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 0 -3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 2.54 -3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at 2.54 3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "+3.3V") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at 0 3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "+3.3V") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole rect (at -2.54 3.81 180) (size 1.58 1.58) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "+3.3V") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/switch_x3_CUI_DEVICES_DS01C-254-L-03BE.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Latch_CD4043BDR:SOIC127P600X175-16N" (layer "F.Cu")
    (at 266.795 124)
    (descr "D (R-PDSO-G16)")
    (tags "Integrated Circuit")
    (property "Cost" "0.49")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/CD4043BDR/1691049?s=N4IgTCBcDa4JwDYC0BmAjAFkUtSByAIiALoC%2BQA")
    (property "Part" "CD4043BDR")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "CMOS Quad NOR R/S Latch with 3-State Outputs")
    (attr smd)
    (fp_text reference "IC2" (at 0.205 7) (layer "F.SilkS"))
    (fp_text value "CD4043BDR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.712 -4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(IC2-Q4)") (pinfunction "Q4") (pintype "passive"))
    (pad "2" smd rect (at -2.712 -3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(IC2-Q1)") (pinfunction "Q1") (pintype "passive"))
    (pad "3" smd rect (at -2.712 -1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "R1") (pintype "passive"))
    (pad "4" smd rect (at -2.712 -0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "SSR_xbt5") (pinfunction "S1") (pintype "passive"))
    (pad "5" smd rect (at -2.712 0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "ENABLE") (pintype "passive"))
    (pad "6" smd rect (at -2.712 1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "SSR_xbt8") (pinfunction "S2") (pintype "passive"))
    (pad "7" smd rect (at -2.712 3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "R2") (pintype "passive"))
    (pad "8" smd rect (at -2.712 4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "9" smd rect (at 2.712 4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(IC2-Q2)") (pinfunction "Q2") (pintype "passive"))
    (pad "10" smd rect (at 2.712 3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(IC2-Q3)") (pinfunction "Q3") (pintype "passive"))
    (pad "11" smd rect (at 2.712 1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "R3") (pintype "passive"))
    (pad "12" smd rect (at 2.712 0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "SSR_xbt7") (pinfunction "S3") (pintype "passive"))
    (pad "13" smd rect (at 2.712 -0.635 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "unconnected-(IC2-NC-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd rect (at 2.712 -1.905 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "SSR_xbt6") (pinfunction "S4") (pintype "passive"))
    (pad "15" smd rect (at 2.712 -3.175 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "R4") (pintype "passive"))
    (pad "16" smd rect (at 2.712 -4.445 90) (size 0.65 1.525) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "VDD") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 130.576 131)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R43" (at -3.326 0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "Net-(R43-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 130.2839 130.4412)
          (xy 130.8681 130.4412)
          (xy 130.8681 131.5588)
          (xy 130.2839 131.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 231.938 161.125)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC7" (at 6.312 -4.875) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(IC7-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(IC7-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(IC7-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(IC7-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "Net-(IC7-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "Net-(IC7-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "Net-(IC7-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "Net-(IC7-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(IC7-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "unconnected-(IC7-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Enable_M5") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "Enable_M5") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "unconnected-(IC7-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "unconnected-(IC7-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "unconnected-(IC7-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "unconnected-(IC7-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "unconnected-(IC7-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 159.0722 154 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R34" (at 0.0722 2 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(IC9-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 159.3643 154.5588)
          (xy 158.7801 154.5588)
          (xy 158.7801 153.4412)
          (xy 159.3643 153.4412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 137.91415 150.275)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C48" (at 1.7526 -2.025 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Linear_regulator_L7812ABD2T_TR:DPAK_BD2T-TR_STM" (layer "F.Cu")
    (at 63.0213 151.54 90)
    (tags "L7812ABD2T-TR ")
    (property "Cost" "1.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/stmicroelectronics/L7812ABD2T-TR/1038261")
    (property "Part" "L7812ABD2T-TR")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1A Low Dropout regulator, positive, 5.0V fixed output, SOT-223")
    (property "ki_keywords" "linear regulator ldo fixed positive")
    (attr smd)
    (fp_text reference "U1" (at 5 6.453 90 unlocked) (layer "F.SilkS"))
    (fp_text value "L7812ABD2T-TR" (at 0 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -4.25 6.953 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.54 4.2418 90) (layer "F.Fab"))
    (fp_text user "*" (at -2.54 4.2418 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.54 9.8552 90) (size 0.9398 3.2004) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/+19.5V") (pinfunction "VI") (pintype "power_in") (zone_connect 1) (thermal_bridge_width 1))
    (pad "2" smd rect (at 0 -2.5781 90) (size 10.5918 8.2042) (property pad_prop_heatsink) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_width 4))
    (pad "3" smd rect (at 2.54 9.8552 90) (size 0.9398 3.2004) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12V") (pinfunction "VO") (pintype "power_out") (thermal_bridge_width 1))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/VoltageRegulator_12V_DPAK_BD2T-TR_STM.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 227.343 153.55)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C61" (at -0.093 -2.3 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(IC7-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(IC7-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 226.8938 152.9758)
          (xy 227.7922 152.9758)
          (xy 227.7922 154.1242)
          (xy 226.8938 154.1242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Multiplexer_SN74LVC1G3157:SOT65P210X110-6N" (layer "F.Cu")
    (at 252.95 139.1)
    (descr "DCK (R-PDSO-G6)")
    (tags "Integrated Circuit")
    (property "Cost" "0.34")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/SN74LVC1G3157DCKR/562895")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "SN74LVC1G3157DCKR, Analogue Switch Single SPDT, 3, 5V, 6-Pin, SC-70")
    (attr smd)
    (fp_text reference "IC11" (at -0.2 -2.6) (layer "F.SilkS"))
    (fp_text value "SN74LVC1G3157DCKR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -0.65 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "/UART1_TX") (pinfunction "B2") (pintype "passive"))
    (pad "2" smd rect (at -0.95 0 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -0.95 0.65 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "/Din_fromGPS") (pinfunction "B1") (pintype "passive"))
    (pad "4" smd rect (at 0.95 0.65 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "/MUX_output") (pinfunction "A") (pintype "passive"))
    (pad "5" smd rect (at 0.95 0 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "VCC") (pintype "passive"))
    (pad "6" smd rect (at 0.95 -0.65 90) (size 0.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "/MUX_select") (pinfunction "S") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/LIB_SN74LVC1G3157DCKR/SN74LVC1G3157DCKR/3D/SN74LVC1G3157DCKR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_network_x4_10k-1204:RESCAXS80P320X160X70-8N" (layer "F.Cu")
    (at 141.608 115.555)
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/YC164-JR-1310KL/17023153?s=N4IgTCBcDaIJ4GMCMA2ALAWgFYCcNIGYkAGAawBsQBdAXyA")
    (property "Part" "YC164-JR-1310KL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "4 resistor network, parallel topology")
    (property "ki_keywords" "R network parallel topology isolated")
    (attr smd)
    (fp_text reference "RN4" (at -3.858 -0.055) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.4254 2.4048) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.885 -1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 2 "GND") (pinfunction "R1.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd roundrect (at -0.885 -0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 2 "GND") (pinfunction "R2.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd roundrect (at -0.885 0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 2 "GND") (pinfunction "R3.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd roundrect (at -0.885 1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 2 "GND") (pinfunction "R4.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" smd roundrect (at 0.885 1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 51 "SSR_xbt3") (pinfunction "R4.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" smd roundrect (at 0.885 0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 53 "SSR_xbt2") (pinfunction "R3.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" smd roundrect (at 0.885 -0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 48 "SSR_xbt4") (pinfunction "R2.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" smd roundrect (at 0.885 -1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 47 "SSR_xbt1") (pinfunction "R1.2") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "LED_green_0603:LED_B1911PG--20D000514U1930_HVK" (layer "F.Cu")
    (at 167.9278 123)
    (tags "B1911PG--20D000514U1930 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/harvatek-corporation/B1911PG-20D000514U1930/15519992")
    (property "Part" "B1911PG--20D000514U1930")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D6" (at 2.5722 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "led" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.5715 0) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.5715 0) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "A") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 108.9328 150.975)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C30" (at 1.8172 -2.475 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 342 129)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE0710KL/1078908")
    (property "Part" "RT0805FRE0710KL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J7-Pin_1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 341.7079 128.4412)
          (xy 342.2921 128.4412)
          (xy 342.2921 129.5588)
          (xy 341.7079 129.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 277.795 131)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R37" (at 3.205 0 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "Net-(R37-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 277.5029 130.4412)
          (xy 278.0871 130.4412)
          (xy 278.0871 131.5588)
          (xy 277.5029 131.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 92 164.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C34" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 91.5508 163.9258)
          (xy 92.4492 163.9258)
          (xy 92.4492 165.0742)
          (xy 91.5508 165.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 130.5 139.75 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE075K1L/1079334")
    (property "Part" "RT0805FRE075K1L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U18-+)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 130.7921 140.3088)
          (xy 130.2079 140.3088)
          (xy 130.2079 139.1912)
          (xy 130.7921 139.1912)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 226.450348 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 4.049652 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 181 "/RelayControl/XBT5_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 180 "/RelayControl/XBT5_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 179 "/RelayControl/XBT5_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 210.975 141.75 180)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at -3.025 1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 211.4242 142.3242)
          (xy 210.5258 142.3242)
          (xy 210.5258 141.1758)
          (xy 211.4242 141.1758)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (at 67 183)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID1" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 130.576 122)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R42" (at -3.326 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "Net-(R42-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 130.2839 121.4412)
          (xy 130.8681 121.4412)
          (xy 130.8681 122.5588)
          (xy 130.2839 122.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 279.5 160)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R14" (at -1.25 -2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(IC5-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 279.2079 159.4412)
          (xy 279.7921 159.4412)
          (xy 279.7921 160.5588)
          (xy 279.2079 160.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 255.795 131)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-10330RL/13694160")
    (property "Part" "RC0805FR-10330RL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R38" (at 3.205 0 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "Net-(R38-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 255.5029 130.4412)
          (xy 256.0871 130.4412)
          (xy 256.0871 131.5588)
          (xy 255.5029 131.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 190.00005 155.925)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C40" (at -0.00005 2.075 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(IC4-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 189.55085 155.3508)
          (xy 190.44925 155.3508)
          (xy 190.44925 156.4992)
          (xy 189.55085 156.4992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_network_x4_10k-1204:RESCAXS80P320X160X70-8N" (layer "F.Cu")
    (at 267.115 115.76)
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/YC164-JR-1310KL/17023153?s=N4IgTCBcDaIJ4GMCMA2ALAWgFYCcNIGYkAGAawBsQBdAXyA")
    (property "Part" "YC164-JR-1310KL")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "4 resistor network, parallel topology")
    (property "ki_keywords" "R network parallel topology isolated")
    (attr smd)
    (fp_text reference "RN2" (at -3.615 -0.01) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.4254 2.4048) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.885 -1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 2 "GND") (pinfunction "R1.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd roundrect (at -0.885 -0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 2 "GND") (pinfunction "R2.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd roundrect (at -0.885 0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 2 "GND") (pinfunction "R3.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd roundrect (at -0.885 1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 2 "GND") (pinfunction "R4.1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" smd roundrect (at 0.885 1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 61 "SSR_xbt7") (pinfunction "R4.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" smd roundrect (at 0.885 0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 63 "SSR_xbt6") (pinfunction "R3.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" smd roundrect (at 0.885 -0.4) (size 0.9 0.53) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.13)
      (net 58 "SSR_xbt8") (pinfunction "R2.2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" smd roundrect (at 0.885 -1.24) (size 0.9 0.61) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 57 "SSR_xbt5") (pinfunction "R1.2") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 94.0842 91.2)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-07750RL/728134")
    (property "Part" "RC0805FR-07750RL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R45" (at -3.8342 -0.45 unlocked) (layer "F.SilkS"))
    (fp_text value "750" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "Net-(D5-K)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 93.7921 90.6412)
          (xy 94.3763 90.6412)
          (xy 94.3763 91.7588)
          (xy 93.7921 91.7588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 170 126)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 2.75 -0.25 90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 169.5508 125.4258)
          (xy 170.4492 125.4258)
          (xy 170.4492 126.5742)
          (xy 169.5508 126.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_green_0603:LED_B1911PG--20D000514U1930_HVK" (layer "F.Cu")
    (at 210 145.5 180)
    (tags "B1911PG--20D000514U1930 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/harvatek-corporation/B1911PG-20D000514U1930/15519992")
    (property "Part" "B1911PG--20D000514U1930")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "led" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 351.25 158.09 -90)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 8.81 4.75 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 312 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 210 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0 270) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 232.75715 150.05)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C49" (at 1.49285 -2.05 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Precision_resistor_5k:Y1453_VIS" (layer "F.Cu")
    (at 319.0815 115.4)
    (tags "Y14535K00000V9L ")
    (property "Cost" "38.87")
    (property "Digikey" "https://www.digikey.com/en/products/detail/vpg-foil-resistors/Y14535K00000V9L/2609897")
    (property "Part" "Y14535K00000V9L")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr through_hole)
    (fp_text reference "R10" (at -4.0315 0 unlocked) (layer "F.SilkS"))
    (fp_text value "5k" (at 1.9685 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9685 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(K11-NO_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.937 0) (size 1.397 1.397) (drill 0.889) (layers "*.Cu" "*.Mask")
      (net 248 "Net-(K12-NO_1)") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/Precision_resistor_Y14535K00000V9L.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 250 160.60925)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R31" (at -1.75 -2.35925 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(IC10-ISENA)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 249.7079 160.05045)
          (xy 250.2921 160.05045)
          (xy 250.2921 161.16805)
          (xy 249.7079 161.16805)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_10k_smt:POT_TC33_3X3P8_BRN" (layer "F.Cu")
    (at 114.5 133 -90)
    (tags "TC33X-2-103E ")
    (property "Cost" "0.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/bourns-inc/TC33X-2-103E/612858")
    (property "Part" "TC33X-2-103E")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr smd)
    (fp_text reference "RV1" (at -3.5 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.3843 270) (size 0.9398 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 -1.0922 270) (size 1.4986 2.1336) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0.95 1.3843 270) (size 0.9398 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/potentiometer_TC-33X-2.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 167.438 161.8731)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC9" (at 6.062 -5.6231) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(IC9-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(IC9-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(IC9-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "Net-(IC9-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(IC9-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(IC9-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(IC9-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "Net-(IC9-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(IC9-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "unconnected-(IC9-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "Enable_M3") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "Enable_M3") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "unconnected-(IC9-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "unconnected-(IC9-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "unconnected-(IC9-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "unconnected-(IC9-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "unconnected-(IC9-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 100 154.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(IC3-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 100.2921 155.0588)
          (xy 99.7079 155.0588)
          (xy 99.7079 153.9412)
          (xy 100.2921 153.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 200.8509 119.5588)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE0710KL/1078908")
    (property "Part" "RT0805FRE0710KL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.8991 0.1912 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "Net-(J25-Pin_2)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "Net-(U6-BOOT0)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 200.5588 119)
          (xy 201.143 119)
          (xy 201.143 120.1176)
          (xy 200.5588 120.1176)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 130.576 118)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U11" (at -2 -3.25) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(IC1-Q4)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "Net-(R42-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "/RelayControl/XBT2_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 76 111.5)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP13" (at -4 0) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 165 "Net-(JP13-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 158 "xbt_B") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 195.9 117.075)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/adam-tech/PH1-03-UA/9830289")
    (property "Part" "PH1-03-UA")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J25" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 313 "/VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 268 "Net-(J25-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 154.9278 164.5)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "Net-(IC9-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 154.6357 163.9412)
          (xy 155.2199 163.9412)
          (xy 155.2199 165.0588)
          (xy 154.6357 165.0588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 313.5842 155.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C59" (at 0 2.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(IC8-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 313.135 154.9258)
          (xy 314.0334 154.9258)
          (xy 314.0334 156.0742)
          (xy 313.135 156.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 214 145.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805JR-07330RL/728311")
    (property "Part" "RC0805JR-07330RL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R47" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "Net-(D7-K)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 214.2921 146.0588)
          (xy 213.7079 146.0588)
          (xy 213.7079 144.9412)
          (xy 214.2921 144.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 121.5 140)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP18" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 137.438 161.5)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC6" (at 6.062 -5.5) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(IC6-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(IC6-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(IC6-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "Net-(IC6-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "Net-(IC6-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "Net-(IC6-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "Net-(IC6-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(IC6-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "Net-(IC6-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "unconnected-(IC6-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Enable_M2") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Enable_M2") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "unconnected-(IC6-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "unconnected-(IC6-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "unconnected-(IC6-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "unconnected-(IC6-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "unconnected-(IC6-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 181.5722 164.425)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C36" (at -0.3222 2.325 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 181.123 163.8508)
          (xy 182.0214 163.8508)
          (xy 182.0214 164.9992)
          (xy 181.123 164.9992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (at 67 89)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID2" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Capacitor_1uF-ceramic:CAP_CL21_SAM" (layer "F.Cu")
    (at 170 129)
    (tags "CL21B105KBFNNNE ")
    (property "Cost" "0.11")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B105KBFNNNE/3886687")
    (property "Part" "CL21B105KBFNNNE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 3 0.25 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 169.5508 128.4258)
          (xy 170.4492 128.4258)
          (xy 170.4492 129.5742)
          (xy 169.5508 129.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 215.5722 164.05)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C54" (at 0 2.2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 215.123 163.4758)
          (xy 216.0214 163.4758)
          (xy 216.0214 164.6242)
          (xy 215.123 164.6242)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_switch_smt:SMT_FS" (layer "F.Cu")
    (at 180 121)
    (tags "PTS526 SK15 SMTR2 LFS ")
    (property "Cost" "0.14")
    (property "Digikey" "https://www.digikey.com/en/products/detail/c-k/PTS526-SK15-SMTR2-LFS/10056626")
    (property "Part" "PTS526 SK15 SMTR2 LFS")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MEC 5E single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "SW1" (at 0 0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "TS02-66-70-BK-160-LCR-D" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -3.43535 -3.556 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -3.43535 -3.556) (layer "F.SilkS"))
    (fp_text user "*" (at -2.3241 -2.6289) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -2.3241 -2.6289 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -3.18135 -1.8542) (size 0.9525 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 3.18135 -1.8542) (size 0.9525 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -3.18135 1.8542) (size 0.9525 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(SW1-A)") (pinfunction "K") (pintype "passive"))
    (pad "4" smd rect (at 3.18135 1.8542) (size 0.9525 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(SW1-A)") (pinfunction "A") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/button_PTS526_SK15_SMTR2_LFS.stp"
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 292.5 160.5)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC5" (at 6.25 -4.75) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(IC5-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(IC5-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(IC5-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(IC5-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(IC5-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Net-(IC5-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Net-(IC5-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(IC5-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "Net-(IC5-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "unconnected-(IC5-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "Enable_M7") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "Enable_M7") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(IC5-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "unconnected-(IC5-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "unconnected-(IC5-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(IC5-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(IC5-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 125.4278 164.225)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R24" (at 0.0722 2.275 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "Net-(IC6-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 125.1357 163.6662)
          (xy 125.7199 163.6662)
          (xy 125.7199 164.7838)
          (xy 125.1357 164.7838)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite-bead-100:IND_25_0805_FRT" (layer "F.Cu")
    (at 193.475 140.75)
    (tags "2508051017Y0 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/fair-rite-products-corp/2508051017Y0/8594285")
    (property "Part" "2508051017Y0")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB1" (at 0.025 2 unlocked) (layer "F.SilkS"))
    (fp_text value "100" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8763 0) (size 1.1684 1.4478) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.8763 0) (size 1.1684 1.4478) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "/VDDA") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 193.2337 140.0769)
          (xy 193.7163 140.0769)
          (xy 193.7163 141.4231)
          (xy 193.2337 141.4231)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Inductor_SMD.3dshapes/L_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 77.5722 102)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 4.4278 0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 77.123 101.4258)
          (xy 78.0214 101.4258)
          (xy 78.0214 102.5742)
          (xy 77.123 102.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Images_logos:NOAA_logo" (layer "F.Cu")
    (at 105.2 117.8)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 340.2 153.2)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE0710KL/1078908")
    (property "Part" "RT0805FRE0710KL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R50" (at 0.1 -2.1 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "/Din_fromGPS") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 339.9079 152.6412)
          (xy 340.4921 152.6412)
          (xy 340.4921 153.7588)
          (xy 339.9079 153.7588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 279.5722 163.275)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R17" (at -0.0722 2.475 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Net-(IC5-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 279.2801 162.7162)
          (xy 279.8643 162.7162)
          (xy 279.8643 163.8338)
          (xy 279.2801 163.8338)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 263.82835 149.925)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C67" (at 1.67165 -2.175 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 254.4142 155.425)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C73" (at -0.1642 2.075 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(IC10-VCP)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 253.965 154.8508)
          (xy 254.8634 154.8508)
          (xy 254.8634 155.9992)
          (xy 253.965 155.9992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 135 135.5)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C78" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U18-+)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 134.5508 134.9258)
          (xy 135.4492 134.9258)
          (xy 135.4492 136.0742)
          (xy 134.5508 136.0742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 152.046666 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K3" (at 5.5 -3.046666 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -4.030133 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -4.030133 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 225 "unconnected-(K3-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 173 "/RelayControl/XBT3_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 226 "Net-(K3--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "/RelayControl/Reset1") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 174 "/RelayControl/XBT3_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 227 "unconnected-(K3-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 79.1 175.25 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (zone_connect 1)
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 194 "Net-(JP2-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_100uF:PCAP_8x112_PAN" (layer "F.Cu")
    (at 322.579 150.425)
    (tags "ECA-1HM101 ")
    (property "Cost" "0.39")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ECA-1HM101/245041")
    (property "Part" "ECA-1HM101")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C50" (at 1.921 -2.425 unlocked) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5052 0) (size 1.524 1.524) (drill 0.9652) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D8.0mm_H7.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 75.7 167.7 -90)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 -2.211 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 270) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 270) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 76.2742 167.2508)
          (xy 76.2742 168.1492)
          (xy 75.1258 168.1492)
          (xy 75.1258 167.2508)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 198 161.5)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC4" (at 6.25 -5) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(IC4-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(IC4-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(IC4-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(IC4-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(IC4-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(IC4-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(IC4-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(IC4-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(IC4-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "unconnected-(IC4-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Enable_M4") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Enable_M4") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "unconnected-(IC4-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "unconnected-(IC4-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "unconnected-(IC4-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "unconnected-(IC4-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "unconnected-(IC4-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Relay_TX-L2-5V:RELAY_TX2_L2_PAN" (layer "F.Cu")
    (at 249.589714 107 90)
    (tags "TX2-L2-5V ")
    (property "Cost" "3.61")
    (property "Digikey" "https://www.digikey.com/en/products/detail/panasonic-electric-works/TX2-L2-5V/570921")
    (property "Part" "TX2-L2-5V")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "DPDT PCB Mount Latching Relay 2 A, 5V dc For Use In Telecommunications Applications")
    (attr through_hole)
    (fp_text reference "K6" (at 5 -3.089714 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TX2-L2-5V" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -3.76 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -3.76 90 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at 0 -1.693333 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 6.3373 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at 0 -1.693333 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 233 "unconnected-(K6-NC_1-Pad3)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 162 "xbt_A") (pinfunction "COM_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 182 "/RelayControl/XBT6_A") (pinfunction "NO_1") (pintype "passive"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 235 "Net-(K6--_1)") (pinfunction "-_1") (pintype "passive"))
    (pad "7" thru_hole circle (at 5.08 12.7 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "/RelayControl/Reset2") (pinfunction "-_2") (pintype "passive"))
    (pad "8" thru_hole circle (at 5.08 10.16 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 183 "/RelayControl/XBT6_B") (pinfunction "NO_2") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.08 7.62 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 158 "xbt_B") (pinfunction "COM_2") (pintype "passive"))
    (pad "10" thru_hole circle (at 5.08 5.08 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 236 "unconnected-(K6-NC_2-Pad10)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "+_2") (pintype "passive"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/RELAY_TX2_L2_PAN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 70.45 163.2)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at -0.05 -2.1) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 3 "+12V") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 215 "Net-(JP4-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 236.8818 124.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE074K7L/1079294")
    (property "Part" "RT0805FRE074K7L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at 3.1318 0 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "/I2C1_SDA") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 237.1739 125.0588)
          (xy 236.5897 125.0588)
          (xy 236.5897 123.9412)
          (xy 237.1739 123.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 133 153.725)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C60" (at 0 -1.975 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(IC6-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(IC6-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 132.5508 153.1508)
          (xy 133.4492 153.1508)
          (xy 133.4492 154.2992)
          (xy 132.5508 154.2992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Network_resistor_10k_bussed:746X101103JP-3" (layer "F.Cu")
    (at 212.499998 100.22 -90)
    (descr "746X101103JP-3")
    (tags "Resistor Network (8-Pin)")
    (property "Cost" "0.22")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cts-resistor-products/746X101103JP/1118444")
    (property "Part" "746X101103JP")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Resistor Networks & Arrays 10Kohms 25V 5%")
    (attr smd)
    (fp_text reference "RN3" (at -0.42 -3.400002 90) (layer "F.SilkS"))
    (fp_text value "746X101103JP" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.28 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "relay_cal_cont") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -0.64 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "relay_gnd_cond") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "relay_xbt8") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 0.64 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "relay_xbt7") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at 1.28 0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect (at 1.28 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "relay_cal_res") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect (at 0 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "relay_reset3") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect (at 0.64 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "relay_reset2") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect (at -0.64 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "unconnected-(RN3-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" smd rect (at -1.28 -0.85 270) (size 0.35 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "10") (pintype "passive"))
    (model "746X101103JP.stp"
      (offset (xyz -1.769999954 -1.070000036 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Zener_3V3_BZT52C3V3-7-F:SOD3715X135N" (layer "F.Cu")
    (at 141.75 141.75 180)
    (property "Cost" "0.21")
    (property "Digikey" "https://www.digikey.com/en/products/detail/diodes-incorporated/BZT52C3V3-7-F/717734")
    (property "Part" "BZT52C3V3-7-F")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D2" (at 5.5 -0.25) (layer "F.SilkS"))
    (fp_text value "3.3V" (at 5.08 1.905) (layer "F.Fab"))
    (pad "A" smd rect (at 1.68 0 180) (size 1.21 0.73) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.102))
    (pad "K" smd rect (at -1.68 0 180) (size 1.21 0.73) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "Net-(U18--)") (pinfunction "K") (pintype "passive") (solder_mask_margin 0.102))
    (model ":KICAD7_3DMODEL_DIR:Diode_SMD.3dshapes/D_SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 342 132)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J7-Pin_1)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 341.5508 131.4258)
          (xy 342.4492 131.4258)
          (xy 342.4492 132.5742)
          (xy 341.5508 132.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_001uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 162.5722 154)
    (tags "CL21B103KBANNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B103KBANNNC/3886673")
    (property "Part" "CL21B103KBANNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C74" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(IC9-CP2)") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(IC9-CP1)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 162.123 153.4258)
          (xy 163.0214 153.4258)
          (xy 163.0214 154.5742)
          (xy 162.123 154.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 223.843 153.55 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805FR-131ML/14008312")
    (property "Part" "RC0805FR-131ML")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 2.05 unlocked) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(IC7-VCP)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 224.1351 154.1088)
          (xy 223.5509 154.1088)
          (xy 223.5509 152.9912)
          (xy 224.1351 152.9912)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 340.2 162.3)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE0710KL/1078908")
    (property "Part" "RT0805FRE0710KL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R49" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "Net-(Q1-G)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "Net-(J3-Pin_2)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 339.9079 161.7412)
          (xy 340.4921 161.7412)
          (xy 340.4921 162.8588)
          (xy 339.9079 162.8588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_1uF-ceramic:CAP_CL21_SAM" (layer "F.Cu")
    (at 165.25 133)
    (tags "CL21B105KBFNNNE ")
    (property "Cost" "0.11")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B105KBFNNNE/3886687")
    (property "Part" "CL21B105KBFNNNE")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -3.15 0 unlocked) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 164.8008 132.4258)
          (xy 165.6992 132.4258)
          (xy 165.6992 133.5742)
          (xy 164.8008 133.5742)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 277.795 127)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U16" (at -2 -3) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(IC2-Q3)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "Net-(R37-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "/RelayControl/XBT7_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 309.4278 164)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE071RL/5934333")
    (property "Part" "RT0805FRE071RL")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R26" (at -0.1778 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "1" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(IC8-ISENB)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 309.1357 163.4412)
          (xy 309.7199 163.4412)
          (xy 309.7199 164.5588)
          (xy 309.1357 164.5588)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 325 98.75 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP15" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 304 "Net-(J4-Pin_1)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 162 "xbt_A") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "LED_green_0603:LED_B1911PG--20D000514U1930_HVK" (layer "F.Cu")
    (at 94.0785 93.7 180)
    (tags "B1911PG--20D000514U1930 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/harvatek-corporation/B1911PG-20D000514U1930/15519992")
    (property "Part" "B1911PG--20D000514U1930")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D5" (at 0.0785 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "led" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.5715 0 180) (size 0.4572 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+5V") (pinfunction "A") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm" (layer "F.Cu")
    (at 152.288 127)
    (descr "https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html")
    (tags "MFSOP 4 pin SMD")
    (property "Cost" "1.28")
    (property "Digikey" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/TLP170AM-TPL-E/12698771")
    (property "Part" "TLP170AM(TPL,E")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "MOSFET Photorelay 1-Form-A, Voff 60V, Ion 100mA, SOP6")
    (property "ki_keywords" "MOSFET Output Photorelay 1-Form-A")
    (attr smd)
    (fp_text reference "U12" (at -0.538 -3) (layer "F.SilkS"))
    (fp_text value "TLP170AM" (at 0 2.921) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(IC1-Q3)") (pintype "passive"))
    (pad "3" smd rect (at -3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "Net-(R41-Pad1)") (pintype "passive"))
    (pad "4" smd rect (at 3.15 1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "/RelayControl/XBT3_C") (pintype "passive"))
    (pad "6" smd rect (at 3.15 -1.27) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "xbt_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MFSOP6-4_4.4x3.6mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 168.0769 120 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RC0805JR-07330RL/728311")
    (property "Part" "RC0805JR-07330RL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R46" (at 0 2 unlocked) (layer "F.SilkS"))
    (fp_text value "330" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "Net-(D6-K)") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 168.369 120.5588)
          (xy 167.7848 120.5588)
          (xy 167.7848 119.4412)
          (xy 168.369 119.4412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 186.00005 155.925)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C35" (at 0 -1.925 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 185.55085 155.3508)
          (xy 186.44925 155.3508)
          (xy 186.44925 156.4992)
          (xy 185.55085 156.4992)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Motor_controller_DRV8825PWPR:SOP65P640X120-29N" (layer "F.Cu")
    (at 322.0842 161)
    (descr "DRV8825PWPR")
    (tags "Integrated Circuit")
    (property "Cost" "5.65")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/drv8825pwpr/2695909")
    (property "Part" "DRV8825PWPR")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "2.5A Bipolar Stepper Motor Driver with On-Chip 1/32 Microstepping Indexer (Step/Dir Ctrl)")
    (attr smd)
    (fp_text reference "IC8" (at 6.1658 -4.75) (layer "F.SilkS"))
    (fp_text value "DRV8825PWPR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(IC8-CP1)") (pinfunction "CP1") (pintype "passive"))
    (pad "2" smd rect (at -2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(IC8-CP2)") (pinfunction "CP2") (pintype "passive"))
    (pad "3" smd rect (at -2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(IC8-VCP)") (pinfunction "VCP") (pintype "passive"))
    (pad "4" smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMA") (pintype "passive"))
    (pad "5" smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(IC8-AOUT1)") (pinfunction "AOUT1") (pintype "passive"))
    (pad "6" smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(IC8-ISENA)") (pinfunction "ISENA") (pintype "passive"))
    (pad "7" smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(IC8-AOUT2)") (pinfunction "AOUT2") (pintype "passive"))
    (pad "8" smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "Net-(IC8-BOUT2)") (pinfunction "BOUT2") (pintype "passive"))
    (pad "9" smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(IC8-ISENB)") (pinfunction "ISENB") (pintype "passive"))
    (pad "10" smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(IC8-BOUT1)") (pinfunction "BOUT1") (pintype "passive"))
    (pad "11" smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pinfunction "VMB") (pintype "passive"))
    (pad "12" smd rect (at -2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "AVREF") (pintype "passive"))
    (pad "13" smd rect (at -2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/MotorControl/Vref") (pinfunction "BVREF") (pintype "passive"))
    (pad "14" smd rect (at -2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "15" smd rect (at 2.938 4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "unconnected-(IC8-V3P3OUT-Pad15)") (pinfunction "V3P3OUT") (pintype "passive+no_connect"))
    (pad "16" smd rect (at 2.938 3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Enable_M8") (pinfunction "NRESET") (pintype "passive"))
    (pad "17" smd rect (at 2.938 2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Enable_M8") (pinfunction "NSLEEP") (pintype "passive"))
    (pad "18" smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(IC8-NFAULT-Pad18)") (pinfunction "NFAULT") (pintype "passive+no_connect"))
    (pad "19" smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(IC8-DECAY-Pad19)") (pinfunction "DECAY") (pintype "passive+no_connect"))
    (pad "20" smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "DIR") (pinfunction "DIR") (pintype "passive"))
    (pad "21" smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "unconnected-(IC8-NENBL-Pad21)") (pinfunction "NENBL") (pintype "passive+no_connect"))
    (pad "22" smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "STEP") (pinfunction "STEP") (pintype "passive"))
    (pad "23" smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "unconnected-(IC8-NC-Pad23)") (pinfunction "NC") (pintype "no_connect"))
    (pad "24" smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/MotorControl/Mode_0") (pinfunction "MODE0") (pintype "passive"))
    (pad "25" smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/MotorControl/Mode_1") (pinfunction "MODE1") (pintype "passive"))
    (pad "26" smd rect (at 2.938 -2.925 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/MotorControl/Mode_2") (pinfunction "MODE2") (pintype "passive"))
    (pad "27" smd rect (at 2.938 -3.575 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(IC8-NHOME-Pad27)") (pinfunction "NHOME") (pintype "passive+no_connect"))
    (pad "28" smd rect (at 2.938 -4.225 90) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "29" smd rect (at 0 0) (size 3.1 5.18) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive") (zone_connect 1) (thermal_bridge_width 2))
    (model "DRV8825PWPR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/DRV8825PWPR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 70.45 167.2)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP5" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 194 "Net-(JP2-B)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 216 "Net-(JP5-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 300.75 131.48)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Cost" "")
    (property "Part" "")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP7" (at -3 -2.23) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 218 "Net-(JP7-A)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 212 "Net-(JP7-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 225 121 180)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 4 -0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0 180) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 225.4492 121.5742)
          (xy 224.5508 121.5742)
          (xy 224.5508 120.4258)
          (xy 225.4492 120.4258)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 236.8818 115.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE074K7L/1079294")
    (property "Part" "RT0805FRE074K7L")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R7" (at 3.1375 0 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+3.3V") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "/I2C1_SCL") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 237.1739 116.0588)
          (xy 236.5897 116.0588)
          (xy 236.5897 114.9412)
          (xy 237.1739 114.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_0805:RC0805N_YAG" (layer "F.Cu")
    (at 130.5 135.5 180)
    (tags "RT0805FRE0747KL ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/yageo/RT0805FRE0747KL/1079274")
    (property "Part" "RT0805FRE0747KL")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -2 unlocked) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(U18-+)") (pintype "passive"))
    (pad "2" smd rect (at 0.8509 0 180) (size 1.016 1.2192) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/+19.5V") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 130.7921 136.0588)
          (xy 130.2079 136.0588)
          (xy 130.2079 134.9412)
          (xy 130.7921 134.9412)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Resistor_SMD.3dshapes/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 154.573966 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 3.676034 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 175 "/RelayControl/XBT3_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 174 "/RelayControl/XBT3_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 173 "/RelayControl/XBT3_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm" (layer "F.Cu")
    (at 347 183)
    (descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
    (tags "fiducial")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID3" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 0.75 0.75) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.375) (clearance 0.375))
  )
  (footprint "Capacitor_01uF-0805:CAP_CL21_SAM" (layer "F.Cu")
    (at 275.5722 163.275)
    (tags "CL21B104KBCNNNC ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661")
    (property "Part" "CL21B104KBCNNNC")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C38" (at 0.1778 2.725 unlocked) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.9278 0) (size 0.8556 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Vmotor_out") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 275.123 162.7008)
          (xy 276.0214 162.7008)
          (xy 276.0214 163.8492)
          (xy 275.123 163.8492)
        )
      )
    )
    (model ":KICAD7_3DMODEL_DIR:Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 238 136)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Cost" "1.07")
    (property "Digikey" "https://www.digikey.com/en/products/detail/texas-instruments/MAX3232EIPWR/968150?s=N4IgTCBcDa4JwDYC0BGOAWAzMlSByAIiALoC%2BQA")
    (property "Part" "MAX3232EIPWR")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3.0V to 5.5V, Low-Power, up to 1Mbps, True RS-232 Transceivers Using Four 0.1μF External Capacitors")
    (property "ki_keywords" "rs232 uart transceiver line-driver")
    (attr smd)
    (fp_text reference "U4" (at 0.25 -3.75) (layer "F.SilkS"))
    (fp_text value "MAX3232" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(U4-C1+)") (pinfunction "C1+") (pintype "passive"))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(U4-VS+)") (pinfunction "VS+") (pintype "power_out"))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U4-C1-)") (pinfunction "C1-") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U4-C2+)") (pinfunction "C2+") (pintype "passive"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U4-C2-)") (pinfunction "C2-") (pintype "passive"))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(U4-VS-)") (pinfunction "VS-") (pintype "power_out"))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 275 "unconnected-(U4-T2OUT-Pad7)") (pinfunction "T2OUT") (pintype "output+no_connect"))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 276 "unconnected-(U4-R2IN-Pad8)") (pinfunction "R2IN") (pintype "input+no_connect"))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 308 "unconnected-(U4-R2OUT-Pad9)") (pinfunction "R2OUT") (pintype "output+no_connect"))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 309 "unconnected-(U4-T2IN-Pad10)") (pinfunction "T2IN") (pintype "input+no_connect"))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 193 "/MUX_output") (pinfunction "T1IN") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 278 "/UART1_RX") (pinfunction "R1OUT") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "/Din_fromComputer") (pinfunction "R1IN") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "/Dout_toComputer") (pinfunction "T1OUT") (pintype "output"))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_10uF:CAP_WCAP-ATG5_05.0X11.0_WRE" (layer "F.Cu")
    (at 188 120)
    (tags "860020572003 ")
    (property "Cost" "0.1")
    (property "Digikey" "https://www.digikey.com/en/products/detail/w%C3%BCrth-elektronik/860020572003/5727172")
    (property "Part" "860020572003")
    (property "Sheetfile" "AOML_AB_3.0_reorganized-v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at -2.5 2.5 unlocked) (layer "F.SilkS"))
    (fp_text value "10u" (at 1 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 313 "/VDD") (pintype "passive"))
    (pad "2" thru_hole circle (at 2 0) (size 1.3208 1.3208) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model ":KICAD7_3DMODEL_DIR:Capacitor_THT.3dshapes/C_Radial_D5.0mm_H11.0mm_P2.00mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CUI_3x1_connector:CUI_TBP02R2-381-03BE" (layer "F.Cu")
    (at 303.450348 93.75)
    (property "Cost" "0.58")
    (property "Digikey" "https://www.digikey.com/en/products/detail/cui-devices/TBP02R2-381-03BE/10238470")
    (property "Part" "TBP02R2-381-03BE")
    (property "Sheetfile" "RelayControl.kicad_sch")
    (property "Sheetname" "RelayControl")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at 3.549652 -2.75) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 14.48 4.361) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 190 "/RelayControl/XBT8_C") (pinfunction "Pin_1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at 3.81 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 189 "/RelayControl/XBT8_B") (pinfunction "Pin_2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at 7.62 0) (size 2.1 2.1) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 188 "/RelayControl/XBT8_A") (pinfunction "Pin_3") (pintype "passive") (solder_mask_margin 0.102))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/TBP02R2_381_03BE-digikey/TBP02R2-381-03BE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 186.96 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J17" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -2.76 0.64 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0.44 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 8.025 2.7919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.725 1.2919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(IC4-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 197 "unconnected-(J17-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(IC4-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 198 "unconnected-(J17-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(IC4-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(IC4-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 97.46 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J16" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.575 1.0419 180 unlocked) (layer "B.SilkS") hide)
    (fp_text user "6" (at 7.925 2.7919 180 unlocked) (layer "B.SilkS") hide)
    (fp_text user "6" (at 7.94 2.44 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.66 0.44 180 unlocked) (layer "F.SilkS"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(IC3-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 195 "unconnected-(J16-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(IC3-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 196 "unconnected-(J16-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(IC3-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(IC3-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 156.71 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J22" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5083 1.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -2.31 1.04 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0.44 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 8.2417 2.7919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 136 "Net-(IC9-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 203 "unconnected-(J22-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 138 "Net-(IC9-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 204 "unconnected-(J22-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 139 "Net-(IC9-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 141 "Net-(IC9-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 126.96 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J19" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8.84 1.04 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "1" (at -1.524 1.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "6" (at 7.9583 3.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.96 0.44 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 103 "Net-(IC6-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 199 "unconnected-(J19-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 105 "Net-(IC6-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 200 "unconnected-(J19-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 106 "Net-(IC6-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 108 "Net-(IC6-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 220.96 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J20" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -2.56 0.64 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 8.2383 3.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.7617 1.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 114 "Net-(IC7-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 201 "unconnected-(J20-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(IC7-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 202 "unconnected-(J20-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 117 "Net-(IC7-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 119 "Net-(IC7-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 281.46 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J18" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.575 1.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 8.175 3.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(IC5-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 297 "unconnected-(J18-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(IC5-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 298 "unconnected-(J18-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(IC5-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(IC5-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 251.96 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J23" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8.2067 2.2919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.5433 0.7919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -2.56 0.64 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 147 "Net-(IC10-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 205 "unconnected-(J23-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 149 "Net-(IC10-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 206 "unconnected-(J23-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(IC10-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 152 "Net-(IC10-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (footprint "Connector_TE_x6_216548-1:CONN_216548-1_TYC" (layer "B.Cu")
    (at 310.96 170.36)
    (tags "216548-1 ")
    (property "Cost" "1.76")
    (property "Digikey" "https://www.digikey.com/en/products/detail/te-connectivity-amp-connectors/216548-1/1920151")
    (property "Part" "216548-1")
    (property "Sheetfile" "MotorControl.kicad_sch")
    (property "Sheetname" "MotorControl")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J21" (at 3.175 7 180 unlocked) (layer "F.SilkS"))
    (fp_text value "216548-1" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 8 3 180 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -1.5 1 180 unlocked) (layer "B.SilkS"))
    (fp_text user "6" (at 7.874 0.24 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "1" (at -1.524 0.7919 180 unlocked) (layer "F.SilkS"))
    (fp_text user "6" (at 8.1433 3.0419 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.175 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "1" (at -1.524 0 180 unlocked) (layer "B.Fab"))
    (fp_text user "6" (at 7.874 0 180 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 125 "Net-(IC8-AOUT1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 299 "unconnected-(J21-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 127 "Net-(IC8-AOUT2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 300 "unconnected-(J21-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 128 "Net-(IC8-BOUT2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 2.54) (size 1.524 1.524) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 130 "Net-(IC8-BOUT1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -1.905 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (pad "8" thru_hole circle (at 8.255 8.89) (size 3.8608 3.8608) (drill 3.3528) (layers "*.Cu" "*.Mask"))
    (model "C:/Users/christian.saiz/Documents/0_NOAA/1_NOAA_work/1_XBT/New_Autolauncher/KiCAD_AL_libraries/3D_models/stepper_connector_216548-1.step"
      (offset (xyz 3 7.5 -18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 180))
    )
  )
  (gr_line (start 58 86) (end 356 86)
    (layer "Edge.Cuts"))
  (gr_arc (start 356 86) (mid 360.242641 87.757359) (end 362 92)
    (layer "Edge.Cuts"))
  (gr_line (start 362 92) (end 362 180)
    (layer "Edge.Cuts"))
  (gr_line (start 52 180) (end 52 92)
    (layer "Edge.Cuts"))
  (gr_arc (start 52 92) (mid 53.757359 87.757359) (end 58 86)
    (layer "Edge.Cuts"))
  (gr_line (start 356 186) (end 58 186)
    (layer "Edge.Cuts"))
  (gr_arc (start 362 180) (mid 360.242641 184.242641) (end 356 186)
    (layer "Edge.Cuts"))
  (gr_arc (start 58 186) (mid 53.757359 184.242641) (end 52 180)
    (layer "Edge.Cuts"))
  (gr_text "NOAA/AOML \nAutolauncher board V3.0\nRev-3 CJS 7-2024 " (at 326.2 180.1) (layer "F.Cu"))
  (gr_text "DIR" (at 177.25 155.25) (layer "F.SilkS"))
  (gr_text "XBT2" (at 130.5 88.5) (layer "F.SilkS"))
  (gr_text "Precision 5k" (at 319.5 113) (layer "F.SilkS"))
  (gr_text "+3V3" (at 358.25 131.5 90) (layer "F.SilkS"))
  (gr_text "B" (at 330.25 91) (layer "F.SilkS"))
  (gr_text "XBT8" (at 305.5 88.5) (layer "F.SilkS"))
  (gr_text "Open JP1 \nif powered \nfrom\nST-link" (at 176 140.5) (layer "F.SilkS"))
  (gr_text "3V3" (at 191.2 115.665) (layer "F.SilkS"))
  (gr_text "M2 M1 M0" (at 100.25 140.25) (layer "F.SilkS"))
  (gr_text "test" (at 55.6 106.2 90) (layer "F.SilkS"))
  (gr_text "TTL\nRS232" (at 228.5 144.2) (layer "F.SilkS"))
  (gr_text "Vin to ADC" (at 128.1 144.7) (layer "F.SilkS"))
  (gr_text "12V Vreg" (at 55.5 143) (layer "F.SilkS"))
  (gr_text "Mux Tx GPS(0)/UART1(1)" (at 249.4 144) (layer "F.SilkS"))
  (gr_text "GND" (at 194.3 125.4) (layer "F.SilkS"))
  (gr_text "GND" (at 161.5 128.25) (layer "F.SilkS"))
  (gr_text "SWCLK" (at 222 114.5 90) (layer "F.SilkS"))
  (gr_text "B" (at 78.5 112) (layer "F.SilkS"))
  (gr_text "Button" (at 358 119.25 90) (layer "F.SilkS"))
  (gr_text "GND" (at 358.25 145.75 90) (layer "F.SilkS"))
  (gr_text "DRV8825 Motor control" (at 104.75 126.5) (layer "F.SilkS"))
  (gr_text "XBT6" (at 254 88.5) (layer "F.SilkS"))
  (gr_text "Rx" (at 340 91) (layer "F.SilkS"))
  (gr_text "Vin" (at 85.9 136.2) (layer "F.SilkS"))
  (gr_text "5V Vreg" (at 78.5 91) (layer "F.SilkS"))
  (gr_text "A" (at 328 91) (layer "F.SilkS"))
  (gr_text "M7" (at 283.5 185) (layer "F.SilkS"))
  (gr_text "GND" (at 219.75 114.5 90) (layer "F.SilkS"))
  (gr_text "A" (at 324.8 102.2) (layer "F.SilkS"))
  (gr_text "XBT5" (at 228.5 88.5) (layer "F.SilkS"))
  (gr_text "3V3" (at 161.5 124) (layer "F.SilkS"))
  (gr_text "+5V" (at 358.25 125.75 90) (layer "F.SilkS"))
  (gr_text "to AXR ->" (at 323.2 98.6 90) (layer "F.SilkS"))
  (gr_text "Motor \ncurrent \nsense" (at 55.4 166.8) (layer "F.SilkS"))
  (gr_text "PB1 led" (at 210 150.5) (layer "F.SilkS"))
  (gr_text "SDA" (at 358.25 135.5 90) (layer "F.SilkS"))
  (gr_text "Relays \nXBT \nA&B 5-8 " (at 214.25 93.9) (layer "F.SilkS"))
  (gr_text "3V3" (at 227.25 113.5 90) (layer "F.SilkS"))
  (gr_text "SSR XBT C 5-8" (at 264.25 113) (layer "F.SilkS"))
  (gr_text "C" (at 332.5 91) (layer "F.SilkS"))
  (gr_text "5V" (at 93.5 100) (layer "F.SilkS"))
  (gr_text "3V3\nVreg" (at 161.75 120.75) (layer "F.SilkS"))
  (gr_text "XBT1" (at 105 88.5) (layer "F.SilkS"))
  (gr_text "12V" (at 84.3978 150.74) (layer "F.SilkS"))
  (gr_text "BOOT0" (at 193.9 122.4 90) (layer "F.SilkS"))
  (gr_text "eeprom" (at 232.7443 113) (layer "F.SilkS"))
  (gr_text "Vref" (at 117.25 136) (layer "F.SilkS"))
  (gr_text "STM32 UART3 3V3\nAXR UART 5V " (at 322 108.4) (layer "F.SilkS"))
  (gr_text "Microcontroller\nSTM32-F103RB" (at 205.5 122.25) (layer "F.SilkS"))
  (gr_text "B" (at 329 102.2) (layer "F.SilkS"))
  (gr_text "C" (at 78.5 115) (layer "F.SilkS"))
  (gr_text "Din" (at 61 101.6 90) (layer "F.SilkS"))
  (gr_text "M5" (at 223 185) (layer "F.SilkS"))
  (gr_text "+5V" (at 334 91) (layer "F.SilkS"))
  (gr_text "LCD & local control" (at 340 126 90) (layer "F.SilkS"))
  (gr_text "M2" (at 129 185) (layer "F.SilkS"))
  (gr_text "C" (at 333 102.2) (layer "F.SilkS"))
  (gr_text "I2C1" (at 340.25 146 90) (layer "F.SilkS"))
  (gr_text "- blue\n- nc/white\n- green\n- nc/white\n- black\n- red" (at 120 184 90) (layer "F.SilkS"))
  (gr_text "Reset" (at 178 125.75) (layer "F.SilkS"))
  (gr_text "SSR XBT C 1-4" (at 135.25 113) (layer "F.SilkS"))
  (gr_text "GND" (at 116.25 140.75) (layer "F.SilkS"))
  (gr_text "8MHZ" (at 183.5 127.8) (layer "F.SilkS"))
  (gr_text "GND" (at 57.2 101.6 90) (layer "F.SilkS"))
  (gr_text "VDA" (at 184.25 142.5) (layer "F.SilkS"))
  (gr_text "XBT3" (at 156.5 88.5) (layer "F.SilkS"))
  (gr_text "M3" (at 159 185) (layer "F.SilkS"))
  (gr_text "Relays \nXBT \nA&B 1-4 " (at 193 93.9) (layer "F.SilkS"))
  (gr_text "+5V" (at 358.25 159.15 90) (layer "F.SilkS"))
  (gr_text "Din" (at 358.25 163.15 90) (layer "F.SilkS"))
  (gr_text "to MK21" (at 69.5 115 90) (layer "F.SilkS"))
  (gr_text "M8" (at 313 185) (layer "F.SilkS"))
  (gr_text "SCL" (at 358.25 140.5 90) (layer "F.SilkS"))
  (gr_text "12V to motors" (at 73.25 173) (layer "F.SilkS"))
  (gr_text "GND" (at 358.25 167.9 90) (layer "F.SilkS"))
  (gr_text "XBT4" (at 182.5 88.5) (layer "F.SilkS"))
  (gr_text "V Im\n" (at 80.6 162.8) (layer "F.SilkS"))
  (gr_text "Tx" (at 337.75 91) (layer "F.SilkS"))
  (gr_text "+" (at 60.6 111 90) (layer "F.SilkS"))
  (gr_text "Vin/9" (at 145.75 140.5) (layer "F.SilkS"))
  (gr_text "SWDIO" (at 224.5 114.5 90) (layer "F.SilkS"))
  (gr_text "GND" (at 342.5 91) (layer "F.SilkS"))
  (gr_text "M1" (at 99.5 185) (layer "F.SilkS"))
  (gr_text "-" (at 58.2 109.6 180) (layer "F.SilkS"))
  (gr_text "GPS TTL RS232 to MUX" (at 337.1 170.6 90) (layer "F.SilkS"))
  (gr_text "ST-Link V2" (at 229.75 121.5 90) (layer "F.SilkS"))
  (gr_text "Auxiliary: GND & Calibration" (at 293.05 112.4) (layer "F.SilkS"))
  (gr_text "M4" (at 189 185) (layer "F.SilkS"))
  (gr_text "Dout" (at 64.2 101.4 90) (layer "F.SilkS"))
  (gr_text "XBT7" (at 280 88.5) (layer "F.SilkS"))
  (gr_text "A" (at 78.5 109) (layer "F.SilkS"))
  (gr_text "M6" (at 254 185) (layer "F.SilkS"))
  (gr_text "GND line to contain Tx/Rx line EMI" (at 91.75 142.75) (layer "Cmts.User"))
  (gr_text "Stepper connection\n1- RED * (A)\n2- White\n3- Black (A)\n4- White\n5- Green (B)\n6- Blue * (B)" (at 315.5 209) (layer "Cmts.User"))
  (gr_text "tx2-l2-5v relay height=7mm \ncui connector height=9.2 mm" (at 98.5 84.5) (layer "Cmts.User"))
  (gr_text "12V track min width 5A max" (at 196.5 188) (layer "Cmts.User"))
  (gr_text "track capacity:\n0.2 mm 0.7A max\n0.4 mm 1.2A max\n0.6 mm 1.6A max\n0.8 mm 2.0A max\n1.0 mm 2.3A max" (at 70.75 206.25) (layer "Cmts.User"))
  (gr_text "5V track 1.2mm >> 2.7A max" (at 72 85) (layer "Cmts.User"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 58 178) (xy 207 178))
    (height 17)
    (gr_text "149.0000 mm" (at 132.5 193.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 356 92) (xy 356 178))
    (height -11.5)
    (gr_text "86.0000 mm" (at 366.35 135 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 52 86) (xy 52 136))
    (height 5.6)
    (gr_text "50.0000 mm" (at 45.25 111 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 356 178) (xy 207 178))
    (height -17)
    (gr_text "149.0000 mm" (at 281.5 193.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 52 86)
        (xy 362 86)
        (xy 362 186)
        (xy 52 186)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 14)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 199.7 156.3)
        (xy 199.7 166.6)
        (xy 196.3 166.6)
        (xy 196.2 166.5)
        (xy 196.2 156.3)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 16)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 264.3 166.1)
        (xy 260.8 166.1)
        (xy 260.7 166)
        (xy 260.7 155.8)
        (xy 264.3 155.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 62.25 158)
        (xy 62.25 170.5)
        (xy 52 170.5)
        (xy 52 157.5)
        (xy 52 138.75)
        (xy 52 118.1)
        (xy 59.190831 118.1)
        (xy 59.25 138.75)
        (xy 65.75 138.75)
        (xy 65.75 158)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 8)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.3 156.9)
        (xy 109.7 156.9)
        (xy 109.7 167.1)
        (xy 106.3 167.1)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 12)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.7 156.4)
        (xy 139.2 156.4)
        (xy 139.2 166.7)
        (xy 135.7 166.7)
      )
    )
  )
  (zone (net 3) (net_name "+12V") (layer "F.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 74.75 94)
        (xy 74.75 91.5)
        (xy 66.5 91.5)
        (xy 66.25 91.75)
        (xy 66.25 104.75)
        (xy 69.75 104.75)
        (xy 69.75 100.5)
        (xy 69.75 94)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 18)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 323.9 155.8)
        (xy 323.9 166.1)
        (xy 320.3 166.1)
        (xy 320.3 155.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 9)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 83 89.5)
        (xy 97.5 89.5)
        (xy 97.5 86)
        (xy 83 86)
        (xy 68.75 86)
        (xy 68.75 91.25)
        (xy 75 91.25)
        (xy 75 94.337705)
        (xy 70.25 94.35)
        (xy 70.25 96.7)
        (xy 74 96.7)
        (xy 74 98.6)
        (xy 83 98.6)
      )
    )
  )
  (zone (net 1) (net_name "/+19.5V") (layer "F.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.4 121.05)
        (xy 90.5 121.05)
        (xy 90.5 134.734075)
        (xy 83.9 141.25)
        (xy 69.5 141.25)
        (xy 69.5 152.25)
        (xy 75.75 152.25)
        (xy 75.75 158)
        (xy 66.25 158)
        (xy 66.25 138.75)
        (xy 80.75 138.75)
        (xy 80.75 132.05)
        (xy 87.4 132.05)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 13)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.2 156.7)
        (xy 169.2 167)
        (xy 165.7 167)
        (xy 165.7 156.7)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 10)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 169.858327 133.9)
        (xy 167.75 135.846149)
        (xy 167.75 142)
        (xy 172.5 142)
        (xy 176.7 137.95)
        (xy 176.7 133.9)
      )
    )
  )
  (zone (net 194) (net_name "Net-(JP2-B)") (layer "F.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 62.75 167.5)
        (xy 66.75 167.5)
        (xy 66.75 170.75)
        (xy 69.75 173.75)
        (xy 79 173.75)
        (xy 79 177.25)
        (xy 68.25 177.25)
        (xy 62.75 171.75)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 17)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 294.3 155.4)
        (xy 294.3 165.6)
        (xy 290.7 165.6)
        (xy 290.7 155.4)
      )
    )
  )
  (zone (net 3) (net_name "+12V") (layer "F.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 66.75 160.75)
        (xy 66.75 163.25)
        (xy 62.75 163.25)
        (xy 62.75 158.5)
        (xy 76.25 158.5)
        (xy 76.25 151.75)
        (xy 70 151.75)
        (xy 70 145)
        (xy 72.5 145)
        (xy 72.5 144)
        (xy 74.75 144)
        (xy 74.790017 147.259983)
        (xy 86.6 147.24)
        (xy 86.6 153.8)
        (xy 78.458804 153.791196)
        (xy 78.5 160.75)
      )
    )
  )
  (zone (net 15) (net_name "Vmotor_out") (layer "F.Cu") (hatch edge 0.5)
    (priority 11)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 79.25 173.75)
        (xy 79.25 186)
        (xy 304.5 186)
        (xy 304.5 176.25)
        (xy 304 175.75)
        (xy 216 175.75)
        (xy 211.5 171.25)
        (xy 203 171.25)
        (xy 198.5 175.75)
        (xy 86.75 175.75)
        (xy 84.75 173.75)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 15)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 233.7 156)
        (xy 233.7 166.3)
        (xy 230.2 166.3)
        (xy 230.2 156)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 52 86)
        (xy 362 86)
        (xy 362 186)
        (xy 52 186)
      )
    )
  )
)
