(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+BATT")
	(net 2 "GND")
	(net 3 "unconnected-(U1-RST-Pad6)")
	(net 4 "unconnected-(U1-GND-Pad2)")
	(net 5 "Clock")
	(net 6 "+5V")
	(net 7 "unconnected-(U1-3V3-Pad5)")
	(net 8 "MOSI")
	(net 9 "unconnected-(U1-VBat-Pad1)")
	(net 10 "unconnected-(U1-SCL{slash}PC0-Pad7)")
	(net 11 "MISO")
	(net 12 "Net-(D1-K)")
	(net 13 "LED")
	(net 14 "Net-(Q1-D)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 75.75 55.25 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:light_APRS"
		(layer "F.Cu")
		(at 63.05 112.25)
		(property "Reference" "U1"
			(at -12.7 -51.8 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "light APRS v1.0"
			(at -11.3 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "3V3"
			(at 9.95 -37.95 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MOSI"
			(at 9.95 -22.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCK"
			(at 9.95 -27.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4V5 to 10V"
			(at -14.2 -52.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MISO"
			(at 9.95 -25.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SDA"
			(at 9.95 -30.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "light APRS"
			(at -13.1 -27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 9.8 -42.06 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCL"
			(at 9.85 -32.95 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at -9.95 -44.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at 9.95 -35.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "USB"
			(at -7.95 -2.06 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -9.95 -42 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -14.8 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -12.3 -45.35)
			(size 2.5 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(U1-VBat-Pad1)")
			(pinfunction "VBat")
			(pintype "power_in+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole oval
			(at -12.3 -42.81)
			(size 2.5 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(U1-GND-Pad2)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole oval
			(at 15.3 -45.35)
			(size 2.5 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+BATT")
			(pinfunction "VBat")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole oval
			(at 15.3 -42.81)
			(size 2.5 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole circle
			(at 15.4 -38.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-3V3-Pad5)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
		)
		(pad "6" thru_hole circle
			(at 15.4 -36.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(U1-RST-Pad6)")
			(pinfunction "RST")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at 15.4 -33.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U1-SCL{slash}PC0-Pad7)")
			(pinfunction "SCL/PC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole circle
			(at 15.4 -31.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "LED")
			(pinfunction "SDA/PC1")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 15.4 -28.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Clock")
			(pinfunction "SCK/PB7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 15.4 -26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "MISO")
			(pinfunction "MISO/PB6")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 15.4 -23.46)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "MOSI")
			(pinfunction "MOSI/PB5")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -11.95 -2.85)
			(size 2 2)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole circle
			(at -11.95 -48.85)
			(size 2 2)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole circle
			(at 14.85 -48.85)
			(size 2 2)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole circle
			(at 14.85 -2.85)
			(size 2 2)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "M:/KiCAD/light_APRS/Solidworks/lightAPRS.STEP"
			(offset
				(xyz 1.5 25.5 3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 82.775 49.75)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED LTST-C171TGKT"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 12 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "+BATT")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:Soldered_uSD"
		(layer "F.Cu")
		(at 81.25 98.5)
		(property "Reference" "U2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Soldered uSD"
			(at 5.5 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "Soldered uSD"
			(at 2.7 -19 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 16.8 -15.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6V (3V3 reg)"
			(at 0.25 -38.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SCLK"
			(at 15.1 -8.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MISO"
			(at 15.2 -10.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MOSI"
			(at 15.2 -12.9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 15.8 -5.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at 16 -3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 20.5 -16.35)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 20.5 -13.81)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "MOSI")
			(pinfunction "MOSI")
			(pintype "output")
		)
		(pad "3" thru_hole circle
			(at 20.5 -11.27)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "MISO")
			(pinfunction "MISO")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 20.5 -8.73)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Clock")
			(pinfunction "SCLK")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 20.5 -6.19)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 20.5 -3.6)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole circle
			(at 3 -3)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole circle
			(at 3 -35)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "M:/KiCAD/Soldered_pcb/microSD breakout 3D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 102.0375 101)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 3.4625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 95.5 104.25 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U3"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AZ1117-5.0"
			(at 0 4.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A 20V Fixed LDO Linear Regulator, 5.0V, SOT-89/SOT-223/TO-220/TO-252/TO-263"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223* SOT?89* TO?220* TO?252* TO?263*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+BATT")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 75.75 49.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "300"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(Q1-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 87.9625 101 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 3.4625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:ScienceHeads_20mm"
		(layer "F.Cu")
		(at 102.25 53.75)
		(property "Reference" "G***"
			(at -4.5 7.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 70.75 54.5 90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at 0 -2.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMN2005K"
			(at 0 2.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/DMN2056U.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4A Id, 20V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "LED")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 90)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Dave:DN_swoop_05mm"
		(layer "F.Cu")
		(at 107 88)
		(property "Reference" "G***"
			(at 2.7 2.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Dave:BAT_BH4AA-PC"
		(layer "B.Cu")
		(at 79 78 -90)
		(property "Reference" "BT1"
			(at -23.455 33.209 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "BH4AA-PC"
			(at -13 -29.25 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "E"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "MPD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "15.88mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "light_APRS_v1.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 29.75 -22.5 90)
			(layer "B.SilkS")
		)
		(fp_text user "_"
			(at 29.75 -9.25 90)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 0 -27.305 270)
			(size 2.36 2.36)
			(drill 2.36)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 27.305 270)
			(size 2.36 2.36)
			(drill 2.36)
			(layers "*.Cu" "*.Mask")
		)
		(pad "+" thru_hole oval
			(at 27.17 -22.67 270)
			(size 1.35 2.7)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+BATT")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "-" thru_hole oval
			(at 27.17 -9.97 270)
			(size 1.35 2.7)
			(drill oval 1 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "M:/KiCAD/BH4AAPC/BH4AA-PC.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(gr_arc
		(start 47 114.75)
		(mid 46.292893 114.457107)
		(end 46 113.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111 46.5)
		(mid 111.707107 46.792893)
		(end 112 47.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 112 113.75)
		(mid 111.707107 114.457107)
		(end 111 114.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 46 47.5)
		(end 46 113.75)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 46 47.5)
		(mid 46.292893 46.792893)
		(end 47 46.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111 114.75)
		(end 47 114.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111 46.5)
		(end 47 46.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112 113.75)
		(end 112 47.5)
		(layer "Edge.Cuts")
	)
	(gr_text "RAW"
		(at 73 67.25 0)
		(layer "F.SilkS")
	)
	(gr_text "U3"
		(at 95.5 109.75 0)
		(layer "F.SilkS")
	)
	(gr_text "U2"
		(at 85 81 0)
		(layer "F.SilkS")
	)
	(gr_text "25 May 2025"
		(at 110.5 113.5 90)
		(layer "F.SilkS")
	)
	(gr_text "U1"
		(at 51 86.5 0)
		(layer "F.SilkS")
	)
	(gr_text "V1.0"
		(at 108.5 113.5 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "+BATT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111 47.5) (xy 47 47.5) (xy 47 113.75) (xy 111 113.75)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111 47.5) (xy 47 47.5) (xy 47 113.75) (xy 111 113.75)
			)
		)
	)
	(embedded_fonts no)
)
