(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 38.228199 77.394999 58.444201 86.587401)
    (thickness 1.6)
    (drawings 4)
    (tracks 132)
    (zones 0)
    (modules 22)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module fh26footprints:FH26W-17S-0.3SHW (layer F.Cu) (tedit 576CF726)
    (at 45.0088 82.0928 270)
    (fp_text reference "" (at 0 0.5 270) (layer F.SilkS))
    (fp_text value FH26W-17S-0.3SHW (at 0 2.6416 270) (layer F.Fab))
    (pad 1 connect rect (at -2.3876 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 2 connect rect (at -1.778 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 3 connect rect (at -1.1684 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 4 connect rect (at -0.5588 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 5 connect rect (at 0.0508 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 6 connect rect (at 0.6604 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 7 connect rect (at 1.27 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 8 connect rect (at 1.8796 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 9 connect rect (at 2.4892 1.3716 270) (size 0.3 0.8) (layers F.Cu F.Mask))
    (pad 10 connect rect (at 2.1844 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 11 connect rect (at 1.5748 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 12 connect rect (at 0.9652 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 13 connect rect (at 0.3556 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 14 connect rect (at -0.254 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 15 connect rect (at -0.8636 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 16 connect rect (at -1.4732 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
    (pad 17 connect rect (at -2.0828 -1.524 270) (size 0.3 0.65) (layers F.Cu F.Mask))
  )
  (module transistor_footprint:TRANSISTORPAD (layer F.Cu) (tedit 576C5D42)
    (at 52.1208 82.0928)
    (fp_text reference "" (at 0 0.508) (layer F.SilkS))
    (fp_text value "TRANSISTOR PAD" (at 0 1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 3) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 49.7332 80.9752)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 49.7332 83.2104)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 49.7332 81.7372)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 49.7332 82.4484)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 54.5084 83.2104)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 54.5084 82.4484)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 54.5084 81.7372)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 54.5084 80.9752)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 50.4444 83.9724)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 53.7972 83.9724)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 51.4604 83.9724)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 52.7812 83.9724)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 50.4444 80.2132)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 51.4604 80.2132)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 52.7812 80.2132)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module transistor_footprint:WIREPAD (layer F.Cu) (tedit 576D8113)
    (at 53.7972 80.2132)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 0.5588) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
  )
  (module mountingholes:MountingHole_1.0mm_M2_no_crtyd (layer F.Cu) (tedit 57802B69)
    (at 39.878 78.8416)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_1.0mm (at -0.0508 1.3208) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module mountingholes:MountingHole_1.0mm_M2_no_crtyd (layer F.Cu) (tedit 57802B69)
    (at 39.878 85.2424)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_1.0mm (at -0.0508 1.3208) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module mountingholes:MountingHole_1.0mm_M2_no_crtyd (layer F.Cu) (tedit 57802B69)
    (at 56.9468 85.2424)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_1.0mm (at -0.0508 1.3208) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module mountingholes:MountingHole_1.0mm_M2_no_crtyd (layer F.Cu) (tedit 57802B69)
    (at 56.9468 78.8924)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_1.0mm (at -0.0508 1.3208) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 58.3692 86.5124) (end 58.3692 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.3032 86.5124) (end 58.3692 86.5124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.3032 77.47) (end 38.3032 86.5124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.3692 77.47) (end 38.3032 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
)
