(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 153)
    (zones 0)
    (modules 14)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(Q1-Pad1)")
  (net 8 /GPIO0)
  (net 9 /EN)
  (net 10 "Net-(Q2-Pad1)")
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(U1-Pad1)")
  (net 14 "Net-(U1-Pad16)")
  (net 15 "Net-(U1-Pad17)")
  (net 16 "Net-(U1-Pad18)")
  (net 17 "Net-(U1-Pad15)")
  (net 18 "Net-(U1-Pad14)")
  (net 19 "Net-(U1-Pad13)")
  (net 20 "Net-(U1-Pad10)")
  (net 21 "Net-(U1-Pad11)")
  (net 22 "Net-(U1-Pad12)")
  (net 23 "Net-(U1-Pad22)")
  (net 24 /TX)
  (net 25 /RX)
  (net 26 "Net-(U1-Pad24)")
  (net 27 /DTR)
  (net 28 /RTS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DTR)
    (add_net /EN)
    (add_net /GPIO0)
    (add_net /RTS)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.3708 80.391 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value "10 kΩ" (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /DTR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.3962 83.566 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value "10 kΩ" (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /RTS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10118194-0001lf-circle:10118194-0001lf-circle (layer F.Cu) (tedit 5981C9DE)
    (at 142.002 94.709)
    (fp_text reference J1 (at 1.63 8.1) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at 1.38 5.4) (layer F.Fab))
    (pad "" smd rect (at 2.9 2.7) (size 1.2 1.55) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.9 2.7) (size 1.2 1.55) (layers F.Cu F.Paste F.Mask))
    (pad "" thru_hole oval (at 3.5 2.7) (size 1.55 1.55) (drill oval 1.15) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -3.5 2.7) (size 1.55 1.55) (drill oval 1.15) (layers *.Cu *.Mask))
    (pad "" smd rect (at 1 2.7) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -1 2.7) (size 1.5 1.55) (layers F.Cu F.Paste F.Mask))
    (pad "" thru_hole oval (at 2.5 0) (size 1.25 1.25) (drill oval 0.85) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -2.5 0) (size 1.25 1.25) (drill oval 0.85) (layers *.Cu *.Mask))
    (pad 5 smd rect (at 1.3 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.65 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.3 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.398 83.566 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.332 80.391 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.459 90.17 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.459 86.995 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.404 86.995 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value "1 kΩ" (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 141.775 90.17)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.524) (layer F.SilkS))
    (fp_text value "22.1 kΩ" (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.404 90.17)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.524) (layer F.SilkS))
    (fp_text value "47.5 kΩ" (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 136.779 72.898 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /EN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 141.954 84.443)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 3.441) (layer F.SilkS))
    (fp_text value CP2102N-A01-GQFN24 (at 0 3.375) (layer F.Fab))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 24 smd rect (at -1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad24)"))
    (pad 23 smd rect (at -0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /DTR))
    (pad 22 smd rect (at -0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad22)"))
    (pad 21 smd rect (at 0.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /TX))
    (pad 20 smd rect (at 0.75 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /RX))
    (pad 19 smd rect (at 1.25 -1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /RTS))
    (pad 18 smd rect (at 1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at 1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at 1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at 1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at 1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at 1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad13)"))
    (pad 12 smd rect (at 1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at 0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at 0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -0.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (pad 8 smd rect (at -0.75 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 7 smd rect (at -1.25 1.95 90) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 6 smd rect (at -1.95 1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at -1.95 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at -1.95 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.95 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -1.95 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.95 -1.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mmbt2222alt1g:mmbt2222alt1g (layer F.Cu) (tedit 59244EE3)
    (at 143.0578 78.867)
    (fp_text reference Q1 (at 0.9462 1.5748) (layer F.SilkS))
    (fp_text value MMBT2222ALT1G (at 0.95 1.9) (layer F.Fab))
    (pad 3 smd rect (at 0.95 -1.9) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /GPIO0))
    (pad 2 smd rect (at 1.9 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /DTR))
    (pad 1 smd rect (at 0 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad1)"))
  )
  (module mmbt2222alt1g:mmbt2222alt1g (layer F.Cu) (tedit 59244EE3)
    (at 138.5468 78.862)
    (fp_text reference Q2 (at 0.9292 1.5036) (layer F.SilkS))
    (fp_text value MMBT2222ALT1G (at 0.95 1.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.9 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /RTS))
    (pad 3 smd rect (at 0.95 -1.9) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /EN))
  )
  (gr_text v0.2 (at 148.2725 78.74) (layer B.SilkS))
  (gr_text EN (at 136.779 75.311) (layer B.SilkS))
  (gr_text RX (at 139.3825 75.311) (layer B.SilkS))
  (gr_text TX (at 141.9225 75.311) (layer B.SilkS))
  (gr_text IO0 (at 144.399 75.311) (layer B.SilkS))
  (gr_text GND (at 147.066 75.311) (layer B.SilkS))
  (gr_line (start 149.987 70.993) (end 134.239 70.993) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.003 97.917) (end 151.003 72.009) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.239 98.933) (end 149.987 98.933) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.223 72.009) (end 133.223 97.917) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.239 97.917) (end 133.223 97.917) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.239 72.009) (end 134.239 70.993) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.987 72.009) (end 151.003 72.009) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.987 97.917) (end 149.987 98.933) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 147.066 75.311) (layer F.SilkS))
  (gr_text IO0 (at 144.399 75.311) (layer F.SilkS))
  (gr_text TX (at 141.859 75.311) (layer F.SilkS))
  (gr_text RX (at 139.319 75.311) (layer F.SilkS))
  (gr_text EN (at 136.779 75.311) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 71.755) (xy 150.3172 71.755) (xy 150.3172 98.2218) (xy 133.985 98.2218)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 71.755) (xy 150.3172 71.755) (xy 150.3172 98.2218) (xy 133.985 98.2218)
      )
    )
  )
)
