<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="11.43" y2="0" width="0" layer="20"/>
<wire x1="11.43" y1="0" x2="12.7" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="1.27" x2="11.43" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="11.43" y1="2.54" x2="10.795" y2="2.54" width="0" layer="20"/>
<wire x1="10.795" y1="2.54" x2="10.795" y2="5.08" width="0" layer="20"/>
<wire x1="10.795" y1="5.08" x2="11.43" y2="5.08" width="0" layer="20"/>
<wire x1="11.43" y1="5.08" x2="12.7" y2="6.35" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="6.35" x2="12.7" y2="19.685" width="0" layer="20"/>
<wire x1="12.7" y1="19.685" x2="11.43" y2="20.955" width="0" layer="20" curve="90"/>
<wire x1="11.43" y1="20.955" x2="10.795" y2="20.955" width="0" layer="20"/>
<wire x1="10.795" y1="20.955" x2="10.795" y2="26.035" width="0" layer="20"/>
<wire x1="10.795" y1="26.035" x2="11.43" y2="26.035" width="0" layer="20"/>
<wire x1="11.43" y1="26.035" x2="12.7" y2="27.305" width="0" layer="20" curve="90"/>
<wire x1="12.7" y1="27.305" x2="11.43" y2="28.575" width="0" layer="20" curve="90"/>
<wire x1="11.43" y1="28.575" x2="1.27" y2="28.575" width="0" layer="20"/>
<wire x1="1.27" y1="28.575" x2="0" y2="27.305" width="0" layer="20" curve="90"/>
<wire x1="0" y1="27.305" x2="1.27" y2="26.035" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="26.035" x2="1.905" y2="26.035" width="0" layer="20"/>
<wire x1="1.905" y1="26.035" x2="1.905" y2="20.955" width="0" layer="20"/>
<wire x1="1.905" y1="20.955" x2="1.27" y2="20.955" width="0" layer="20"/>
<wire x1="1.27" y1="20.955" x2="0" y2="19.685" width="0" layer="20" curve="90"/>
<wire x1="0" y1="19.685" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="1.27" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="5.08" x2="1.905" y2="5.08" width="0" layer="20"/>
<wire x1="1.905" y1="5.08" x2="1.905" y2="2.54" width="0" layer="20"/>
<wire x1="1.905" y1="2.54" x2="1.27" y2="2.54" width="0" layer="20"/>
<wire x1="1.27" y1="2.54" x2="0" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<text>SSR6-Tr ADPT</text>
<text>ANTBIAS</text>
<text>1</text>
<text>2</text>
<text>9</text>
<text>10</text>
</plain>
<libraries>
<library name="Dan_Con">
<description>Dan Contract Library.</description>
<packages>
<package name="WIREPAD040">
</package>
<package name="SMD0805">
</package>
<package name="CPL-SOCKET-SAMTEC-10PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TXD" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="RXD" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="PWR" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="PPS1" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="GND" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="BATT" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="PPS2" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="RTCMIN" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="ANT-B" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="GND1" library="Dan_Con" package="WIREPAD040" value="WIREPAD40MILL">
<attribute name="NAME"/>
</element>
<element name="J1" library="Dan_Con" package="SMD0805" value="000">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="Dan_Con" package="CPL-SOCKET-SAMTEC-10PIN" value="CPL-SOCKET-SAMTEC-10PIN"/>
</elements>
<signals>
<signal name="TXD">
<contactref element="TXD" pad="P$1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="RXD" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="PWR">
<contactref element="PWR" pad="P$1"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="PPS1">
<contactref element="PPS1" pad="P$1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="BATT">
<contactref element="BATT" pad="P$1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="PPS2">
<contactref element="PPS2" pad="P$1"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="RTCM">
<contactref element="RTCMIN" pad="P$1"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="ANTBIAS">
<contactref element="ANT-B" pad="P$1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="GND1" pad="P$1"/>
<contactref element="J2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
