(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 16)
    (no_connects 0)
    (area 142.799999 103.429999 166.445001 135.330001)
    (thickness 1.6)
    (drawings 15)
    (tracks 48)
    (zones 0)
    (modules 7)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +8V)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(P1-Pad2)")
  (net 5 "Net-(P1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +8V)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer F.Cu) (tedit 0)
    (at 147.32 125.73 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value "Amphenol FCI 68016-106HLF" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.00mm (layer F.Cu) (tedit 5813DD05)
    (at 164.465 126.015 180)
    (descr "Through hole pin header, 2x08, 2.00mm pitch, double row")
    (tags "pin header double row")
    (fp_text reference P3 (at 0 -5 180) (layer F.SilkS) hide)
    (fp_text value "3M 151216-7422-RB" (at 0 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +8V))
    (pad 3 thru_hole circle (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad3)"))
    (pad 7 thru_hole circle (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +8V))
    (pad 11 thru_hole circle (at 0 10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 15 thru_hole circle (at 0 14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 4 thru_hole circle (at 2 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 6 thru_hole circle (at 2 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 2 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 2 8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 12 thru_hole circle (at 2 10 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 2 12 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole circle (at 2 14 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 154.94 122.555)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 7805MS (at 0 -4.318) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 1 +8V))
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 152.4 118.11 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 3.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 +8V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 157.48 118.03 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 3.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 5813DD0E)
    (at 147.32 130.81 90)
    (fp_text reference P2 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (net 1 +8V))
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer F.Cu) (tedit 5813DD11)
    (at 147.32 107.95)
    (fp_text reference P4 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 1.27 5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 2.49936) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text 8V (at 150.495 127) (layer B.SilkS))
  (gr_text GND (at 151.765 111.125) (layer B.SilkS))
  (gr_text B (at 144.78 113.03) (layer B.SilkS))
  (gr_text O (at 144.78 120.65) (layer B.SilkS))
  (gr_text Y (at 144.78 123.19) (layer B.SilkS))
  (gr_text GND (at 151.765 111.125) (layer F.SilkS))
  (gr_text 8V (at 150.495 127) (layer F.SilkS))
  (gr_line (start 151.765 109.855) (end 151.765 107.95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.765 128.27) (end 151.765 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.32 130.81) (end 151.765 130.81) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.32 107.95) (end 142.875 107.95) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.765 109.855) (end 166.37 109.855) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.875 130.81) (end 142.875 107.95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 128.27) (end 151.765 128.27) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 109.855) (end 166.37 128.27) (layer Edge.Cuts) (width 0.15))
)
