(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 213)
    (no_connects 2)
    (area 148.678572 98.098955 231 137.25124)
    (thickness 1.6)
    (drawings 25)
    (tracks 448)
    (zones 0)
    (modules 108)
    (nets 111)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory pihat_gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C4-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(C8-Pad1)")
  (net 5 "Net-(C11-Pad1)")
  (net 6 NRST)
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C18-Pad2)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 COS_LED)
  (net 12 "Net-(D3-Pad2)")
  (net 13 PTT_LED)
  (net 14 "Net-(D4-Pad2)")
  (net 15 DMR_LED)
  (net 16 "Net-(D5-Pad2)")
  (net 17 DSTAR_LED)
  (net 18 "Net-(D6-Pad2)")
  (net 19 P25_LED)
  (net 20 "Net-(D7-Pad2)")
  (net 21 YSF_LED)
  (net 22 RF)
  (net 23 SWDIO)
  (net 24 TXD)
  (net 25 RXD)
  (net 26 DISP_TXD)
  (net 27 DISP_RXD)
  (net 28 "Net-(R5-Pad1)")
  (net 29 BOOT0)
  (net 30 CLKOUT)
  (net 31 "Net-(R12-Pad2)")
  (net 32 DATAIN)
  (net 33 DATAOUT)
  (net 34 "Net-(U2-Pad14)")
  (net 35 "Net-(U2-Pad15)")
  (net 36 "Net-(U2-Pad16)")
  (net 37 "Net-(U2-Pad17)")
  (net 38 SLE)
  (net 39 SDATA)
  (net 40 SREAD)
  (net 41 SCLK)
  (net 42 "Net-(U2-Pad33)")
  (net 43 SDA)
  (net 44 SCL)
  (net 45 "Net-(X1-Pad1)")
  (net 46 "Net-(PI1-Pad2)")
  (net 47 "Net-(PI1-Pad3)")
  (net 48 "Net-(PI1-Pad4)")
  (net 49 "Net-(PI1-Pad5)")
  (net 50 "Net-(PI1-Pad7)")
  (net 51 "Net-(PI1-Pad11)")
  (net 52 "Net-(PI1-Pad12)")
  (net 53 "Net-(PI1-Pad13)")
  (net 54 "Net-(PI1-Pad15)")
  (net 55 "Net-(PI1-Pad16)")
  (net 56 "Net-(PI1-Pad18)")
  (net 57 "Net-(PI1-Pad19)")
  (net 58 "Net-(PI1-Pad21)")
  (net 59 "Net-(PI1-Pad22)")
  (net 60 "Net-(PI1-Pad24)")
  (net 61 "Net-(PI1-Pad26)")
  (net 62 "Net-(PI1-Pad27)")
  (net 63 "Net-(PI1-Pad28)")
  (net 64 "Net-(PI1-Pad29)")
  (net 65 "Net-(PI1-Pad31)")
  (net 66 "Net-(PI1-Pad32)")
  (net 67 "Net-(PI1-Pad33)")
  (net 68 "Net-(PI1-Pad35)")
  (net 69 "Net-(PI1-Pad36)")
  (net 70 "Net-(C1-Pad1)")
  (net 71 "Net-(C4-Pad2)")
  (net 72 "Net-(C5-Pad1)")
  (net 73 "Net-(C6-Pad1)")
  (net 74 "Net-(C10-Pad1)")
  (net 75 "Net-(C11-Pad2)")
  (net 76 "Net-(C12-Pad1)")
  (net 77 "Net-(C13-Pad1)")
  (net 78 "Net-(C14-Pad1)")
  (net 79 "Net-(C15-Pad2)")
  (net 80 "Net-(C20-Pad2)")
  (net 81 "Net-(C21-Pad2)")
  (net 82 "Net-(C23-Pad2)")
  (net 83 "Net-(R2-Pad1)")
  (net 84 "Net-(R10-Pad2)")
  (net 85 "Net-(R11-Pad2)")
  (net 86 "Net-(U1-Pad13)")
  (net 87 "Net-(U1-Pad14)")
  (net 88 "Net-(U1-Pad15)")
  (net 89 "Net-(U1-Pad16)")
  (net 90 "Net-(U1-Pad17)")
  (net 91 "Net-(U1-Pad18)")
  (net 92 "Net-(U1-Pad20)")
  (net 93 "Net-(U1-Pad21)")
  (net 94 "Net-(U1-Pad23)")
  (net 95 "Net-(U1-Pad30)")
  (net 96 "Net-(U1-Pad33)")
  (net 97 "Net-(U1-Pad37)")
  (net 98 "Net-(U1-Pad38)")
  (net 99 "Net-(U1-Pad44)")
  (net 100 "Net-(U1-Pad46)")
  (net 101 "Net-(U2-Pad2)")
  (net 102 "Net-(U2-Pad4)")
  (net 103 "Net-(U2-Pad10)")
  (net 104 "Net-(U2-Pad11)")
  (net 105 "Net-(U2-Pad29)")
  (net 106 "Net-(U2-Pad32)")
  (net 107 BOOT_GPIO)
  (net 108 CE)
  (net 109 SWCLK)
  (net 110 "Net-(U2-Pad46)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net BOOT0)
    (add_net BOOT_GPIO)
    (add_net CE)
    (add_net CLKOUT)
    (add_net COS_LED)
    (add_net DATAIN)
    (add_net DATAOUT)
    (add_net DISP_RXD)
    (add_net DISP_TXD)
    (add_net DMR_LED)
    (add_net DSTAR_LED)
    (add_net GND)
    (add_net NRST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(PI1-Pad11)")
    (add_net "Net-(PI1-Pad12)")
    (add_net "Net-(PI1-Pad13)")
    (add_net "Net-(PI1-Pad15)")
    (add_net "Net-(PI1-Pad16)")
    (add_net "Net-(PI1-Pad18)")
    (add_net "Net-(PI1-Pad19)")
    (add_net "Net-(PI1-Pad2)")
    (add_net "Net-(PI1-Pad21)")
    (add_net "Net-(PI1-Pad22)")
    (add_net "Net-(PI1-Pad24)")
    (add_net "Net-(PI1-Pad26)")
    (add_net "Net-(PI1-Pad27)")
    (add_net "Net-(PI1-Pad28)")
    (add_net "Net-(PI1-Pad29)")
    (add_net "Net-(PI1-Pad3)")
    (add_net "Net-(PI1-Pad31)")
    (add_net "Net-(PI1-Pad32)")
    (add_net "Net-(PI1-Pad33)")
    (add_net "Net-(PI1-Pad35)")
    (add_net "Net-(PI1-Pad36)")
    (add_net "Net-(PI1-Pad4)")
    (add_net "Net-(PI1-Pad5)")
    (add_net "Net-(PI1-Pad7)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(X1-Pad1)")
    (add_net P25_LED)
    (add_net PTT_LED)
    (add_net RF)
    (add_net RXD)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net SDATA)
    (add_net SLE)
    (add_net SREAD)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TXD)
    (add_net YSF_LED)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 191.15 118.8)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 197.6 127.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 202.45 127.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 202.4 123)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 197.65 123.1)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 591D7170)
    (at 216.95918 109.237121)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 591D716A)
    (at 216.95918 132.239361)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 591D7164)
    (at 158.95 132.25)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 591D715B)
    (at 158.95 109.25)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module OPENHARDWARE:OSHWLOGO0.3IN (layer F.Cu) (tedit 0)
    (at 161 128.4)
    (descr "OSHW LOGO")
    (tags "Open Source Hardware Logo")
    (fp_text reference G*** (at 0 7.27964) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -7.27964) (layer F.SilkS) hide)
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 184.75 120.15)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 170.8 123.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 165.75 125.65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 165.55 124.35)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 168.75 123.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 167.35 121.85)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 202.6 112.95)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 196.3 112.8)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 181.35 116.6)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 176.6 116.7)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 165.45 120.55)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 166.55 121.05)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 165.1 123.1)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 167.1 126.15)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 168.8 127.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 167.85 122.95)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 169.85 123.5)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 170.65 126.15)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 179.75 130.3)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 190.6 127.75)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 208.85 119.65)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 212.55 129.35)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 207.05 127.55)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 207.55 124.9)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 199.95 125.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 182.6 126.25)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 180.9 126.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 179.1 126.2)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 182.55 124.85)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 180.9 124.85)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 179.15 124.85)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 182.45 123.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 180.85 123.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4711)
    (at 168.75 125.4 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.45 -0.05 360) (layer F.SilkS))
    (fp_text value 6p8 (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D49C5)
    (at 172.6 121)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -1.6 0) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D49DE)
    (at 172.6 119.75)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -1.6 0) (layer F.SilkS))
    (fp_text value 220p (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4706)
    (at 172.6 123.65 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.65 -0.05 180) (layer F.SilkS))
    (fp_text value 10p (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4718)
    (at 172.6 124.85 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at -1.65 0 180) (layer F.SilkS))
    (fp_text value 4p7 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4CC8)
    (at 172.6 127.4 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value 6p8 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C4697)
    (at 173.6 130.55 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4B2D)
    (at 172.6 118.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 1.55 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D47C5)
    (at 175 121.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -0.1 -0.9 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C463E)
    (at 176.25 130.55 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -0.95 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4C38)
    (at 175 118.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -1.85 0 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4D2C)
    (at 178.7 116.45 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 2 0 90) (layer F.SilkS))
    (fp_text value 470p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4D2F)
    (at 180.05 116.45 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 1.95 0 90) (layer F.SilkS))
    (fp_text value 15n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4D23)
    (at 181.3 118.7 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 1.9 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4BF2)
    (at 182.65 116.4 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at -2.05 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C2AEE)
    (at 205.5 133.5 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at -1.8 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4B80)
    (at 183.85 116.4 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 2.05 0.05 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C41E2)
    (at 186.6 119.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at -2.05 0 180) (layer F.SilkS))
    (fp_text value 22p (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A5C)
    (at 190.85 116.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at -0.05 -1 270) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C3FF6)
    (at 186.6 125.55 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A84)
    (at 195 133.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0.1 -1 90) (layer F.SilkS))
    (fp_text value 20p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C402B)
    (at 186.6 124.15 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at -1.85 0 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591C2AE9)
    (at 204 133.5 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at 1.8 0 90) (layer F.SilkS))
    (fp_text value 20p (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C23-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A8D)
    (at 193.04 128.05 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 0 -1.038 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A77)
    (at 206 121 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C25 (at 1.95 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 591D4A71)
    (at 196.7 118.25 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at -0.05 -1.2 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C222C)
    (at 213.233 113.1777)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value green (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C222F)
    (at 213.233 114.4477)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value yellow (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 COS_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C2232)
    (at 213.233 115.7177)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value red (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 PTT_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C2238)
    (at 213.233 116.9877)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value yellow (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 DMR_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C2245)
    (at 213.233 118.2577)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value green (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 DSTAR_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C2248)
    (at 213.233 120.8277)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value red (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 P25_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 591C224B)
    (at 213.233 119.5477)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at -2.54 0) (layer F.SilkS) hide)
    (fp_text value amber (at 0 1.4) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 YSF_LED))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4729)
    (at 167.15 124.85)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L1 (at 0 -1.1) (layer F.SilkS))
    (fp_text value 22n (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 RF))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D46FB)
    (at 170.3 124.85)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L2 (at 0 -1.1) (layer F.SilkS))
    (fp_text value 20n (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C4778)
    (at 172.6 122.35 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L3 (at 1.35 0 180) (layer F.SilkS))
    (fp_text value 13n (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C4750)
    (at 172.6 126.1)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference L4 (at 1.35 0) (layer F.SilkS))
    (fp_text value 27n (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 591D4A6C)
    (at 199.136 114.808 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value BOOT0 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 BOOT_GPIO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 591C27BD)
    (at 210.42 127 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value DISPLAY (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 DISP_TXD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 DISP_RXD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 591D5CFC)
    (at 160.6 121.65)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference P3 (at 0 -2.45) (layer F.SilkS))
    (fp_text value SMA (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 22 RF))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 591C27C0)
    (at 210.5 123.5 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value STLINK (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 SWDIO))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 SWCLK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module pizero:RPI-Zero-RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL (layer F.Cu) (tedit 591D684D)
    (at 155.4607 135.736941)
    (descr "RASPBERRY PI BOARD MODEL B+, FULL OUTLINE WITH POSITION OF BIG CONNECTORS & DRILL HOLES")
    (tags "RASPBERRY PI BOARD MODEL B+, FULL OUTLINE WITH POSITION OF BIG CONNECTORS & DRILL HOLES")
    (attr virtual)
    (fp_text reference PI1 (at 10.4393 -26.586941) (layer F.SilkS) hide)
    (fp_text value RPI-ZERO (at 13.3393 -26.586941) (layer F.SilkS) hide)
    (fp_text user 1 (at 8.5598 -22.88032) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 8.3693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 8.3693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 46 "Net-(PI1-Pad2)"))
    (pad 3 thru_hole circle (at 10.9093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 47 "Net-(PI1-Pad3)"))
    (pad 4 thru_hole circle (at 10.9093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 48 "Net-(PI1-Pad4)"))
    (pad 5 thru_hole circle (at 13.4493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 49 "Net-(PI1-Pad5)"))
    (pad 6 thru_hole circle (at 13.4493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 15.9893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 50 "Net-(PI1-Pad7)"))
    (pad 8 thru_hole circle (at 15.9893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 25 RXD))
    (pad 9 thru_hole circle (at 18.5293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 18.5293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 24 TXD))
    (pad 11 thru_hole circle (at 21.0693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 51 "Net-(PI1-Pad11)"))
    (pad 12 thru_hole circle (at 21.0693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 52 "Net-(PI1-Pad12)"))
    (pad 13 thru_hole circle (at 23.6093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 53 "Net-(PI1-Pad13)"))
    (pad 14 thru_hole circle (at 23.6093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 26.1493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 54 "Net-(PI1-Pad15)"))
    (pad 16 thru_hole circle (at 26.1493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 55 "Net-(PI1-Pad16)"))
    (pad 17 thru_hole circle (at 28.6893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 3 +3V3))
    (pad 18 thru_hole circle (at 28.6893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 56 "Net-(PI1-Pad18)"))
    (pad 19 thru_hole circle (at 31.2293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 57 "Net-(PI1-Pad19)"))
    (pad 20 thru_hole circle (at 31.2293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at 33.7693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 58 "Net-(PI1-Pad21)"))
    (pad 22 thru_hole circle (at 33.7693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 59 "Net-(PI1-Pad22)"))
    (pad 23 thru_hole circle (at 36.3093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 36.3093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 60 "Net-(PI1-Pad24)"))
    (pad 25 thru_hole circle (at 38.8493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 26 thru_hole circle (at 38.8493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 61 "Net-(PI1-Pad26)"))
    (pad 27 thru_hole circle (at 41.3893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 62 "Net-(PI1-Pad27)"))
    (pad 28 thru_hole circle (at 41.3893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 63 "Net-(PI1-Pad28)"))
    (pad 29 thru_hole circle (at 43.9293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 64 "Net-(PI1-Pad29)"))
    (pad 30 thru_hole circle (at 43.9293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at 46.4693 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 65 "Net-(PI1-Pad31)"))
    (pad 32 thru_hole circle (at 46.4693 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 66 "Net-(PI1-Pad32)"))
    (pad 33 thru_hole circle (at 49.0093 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 67 "Net-(PI1-Pad33)"))
    (pad 34 thru_hole circle (at 49.0093 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 35 thru_hole circle (at 51.5493 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 68 "Net-(PI1-Pad35)"))
    (pad 36 thru_hole circle (at 51.5493 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 69 "Net-(PI1-Pad36)"))
    (pad 37 thru_hole circle (at 54.0893 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 38 thru_hole circle (at 54.0893 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 107 BOOT_GPIO))
    (pad 39 thru_hole circle (at 56.6293 -25.22982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 56.6293 -27.76982) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Paste *.Mask)
      (net 6 NRST))
    (pad "" np_thru_hole circle (at 3.49758 -3.49758) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.49758 -26.49982) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 61.49848 -3.49758) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 61.49848 -26.49982) (size 2.74828 2.74828) (drill 2.74828) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4A94)
    (at 193.04 126.05 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -0.01 1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 BOOT0))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 BOOT_GPIO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C46CC)
    (at 171.85 130.55 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 1k1 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C4676)
    (at 174.95 130.55 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -1.65 0 270) (layer F.SilkS))
    (fp_text value 3k8 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4AF8)
    (at 175 119.75 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -1.35 0 180) (layer F.SilkS))
    (fp_text value 3R9 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4D28)
    (at 178.7 118.7 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -1.55 0 90) (layer F.SilkS))
    (fp_text value 560 (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591D4D1F)
    (at 180.05 118.7 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -1.55 -0.55 90) (layer F.SilkS))
    (fp_text value 270 (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2AFE)
    (at 207.2 133.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at -1.9 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C3F8C)
    (at 186.6 120.3 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at -1.65 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 CLKOUT))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C3FBB)
    (at 186.6 121.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at -1.7 0.05 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 DATAIN))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C4088)
    (at 186.6 122.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at -1.7 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 DATAOUT))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C220C)
    (at 215.773 113.1777 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2215)
    (at 215.773 114.4477 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2219)
    (at 215.773 115.7177 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C221C)
    (at 215.773 116.9877 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C221E)
    (at 215.773 118.2577 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2221)
    (at 215.773 120.8277 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 591C2226)
    (at 215.773 119.5477 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 591C2B05)
    (at 210.7 133.4)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -0.1 90) (layer F.SilkS) hide)
    (fp_text value SW_DIP_x01 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Housings_DFN_QFN:QFN-48-1EP_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 591D4C16)
    (at 180.79375 124.89375)
    (descr "UK Package; 48-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_48_05-08-1704.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 4.70625) (layer F.SilkS))
    (fp_text value ADF7021 (at 0 4.75) (layer F.Fab))
    (pad 1 smd rect (at -3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at -3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C11-Pad2)"))
    (pad 3 smd rect (at -3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C5-Pad1)"))
    (pad 7 smd rect (at -3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C6-Pad1)"))
    (pad 8 smd rect (at -3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R2-Pad1)"))
    (pad 9 smd rect (at -3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 10 smd rect (at -3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad1)"))
    (pad 11 smd rect (at -3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C10-Pad1)"))
    (pad 12 smd rect (at -3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -2.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -2.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -0.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at -0.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 0.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 0.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 1.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 1.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 2.25 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 2.75 3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 CE))
    (pad 25 smd rect (at 3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 SLE))
    (pad 26 smd rect (at 3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 SDATA))
    (pad 27 smd rect (at 3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 SREAD))
    (pad 28 smd rect (at 3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 SCLK))
    (pad 29 smd rect (at 3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 30 smd rect (at 3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C20-Pad2)"))
    (pad 32 smd rect (at 3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 33 smd rect (at 3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R12-Pad2)"))
    (pad 35 smd rect (at 3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R11-Pad2)"))
    (pad 36 smd rect (at 3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R10-Pad2)"))
    (pad 37 smd rect (at 2.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 2.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 1.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C18-Pad2)"))
    (pad 40 smd rect (at 1.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 41 smd rect (at 0.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C15-Pad2)"))
    (pad 42 smd rect (at 0.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C14-Pad1)"))
    (pad 43 smd rect (at -0.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 44 smd rect (at -0.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U1-Pad44)"))
    (pad 45 smd rect (at -1.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 46 smd rect (at -1.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at -2.25 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -3.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 49 smd rect (at 1.93125 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 1.93125 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.64375 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.64375 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -0.64375) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -1.93125 -1.93125) (size 1.2875 1.2875) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 200 125 90)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -0.102 180) (layer F.SilkS))
    (fp_text value STM32F103C8T6 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 CE))
    (pad 4 smd rect (at -4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C21-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C23-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 NRST))
    (pad 8 smd rect (at -4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 10 smd rect (at -4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at -4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 DISP_TXD))
    (pad 13 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 DISP_RXD))
    (pad 14 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 P25_LED))
    (pad 19 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 YSF_LED))
    (pad 20 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 SDA))
    (pad 22 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 23 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 25 smd rect (at 4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 DSTAR_LED))
    (pad 26 smd rect (at 4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 DMR_LED))
    (pad 27 smd rect (at 4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 PTT_LED))
    (pad 28 smd rect (at 4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 COS_LED))
    (pad 29 smd rect (at 4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U2-Pad29)"))
    (pad 30 smd rect (at 4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 TXD))
    (pad 31 smd rect (at 4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 RXD))
    (pad 32 smd rect (at 4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U2-Pad32)"))
    (pad 33 smd rect (at 4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad33)"))
    (pad 34 smd rect (at 4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 109 SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 CLKOUT))
    (pad 39 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 DATAIN))
    (pad 40 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 DATAOUT))
    (pad 41 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 SCLK))
    (pad 42 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 SDATA))
    (pad 43 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 SREAD))
    (pad 44 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 SLE))
    (pad 46 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U2-Pad46)"))
    (pad 47 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm (layer F.Cu) (tedit 591D4BA2)
    (at 186.75 116 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0 2.15 180) (layer F.SilkS))
    (fp_text value TCXO (at 0 2.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(X1-Pad1)"))
    (pad 2 smd rect (at 1.1 0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C18-Pad1)"))
    (pad 4 smd rect (at -1.1 -0.85 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_3225-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C)
    (at 199.45 133)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3 http://www.abracon.com/Resonators/abm3.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0.05 -0.1 90) (layer F.SilkS))
    (fp_text value 8MHz (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.05 0) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 2.05 0) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MMDVM:VIA-0.6mm (layer F.Cu) (tedit 591D5D86)
    (at 179.15 123.45)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (dimension 30.2 (width 0.3) (layer Dwgs.User)
    (gr_text "30,200 mm" (at 224.5 120.65 270) (layer Dwgs.User))
    (feature1 (pts (xy 213.15 135.75) (xy 225.85 135.75)))
    (feature2 (pts (xy 213.15 105.55) (xy 225.85 105.55)))
    (crossbar (pts (xy 223.15 105.55) (xy 223.15 135.75)))
    (arrow1a (pts (xy 223.15 135.75) (xy 222.563579 134.623496)))
    (arrow1b (pts (xy 223.15 135.75) (xy 223.736421 134.623496)))
    (arrow2a (pts (xy 223.15 105.55) (xy 222.563579 106.676504)))
    (arrow2b (pts (xy 223.15 105.55) (xy 223.736421 106.676504)))
  )
  (dimension 65.150173 (width 0.3) (layer Dwgs.User)
    (gr_text "65,150 mm" (at 187.82895 99.523951 0.1319163736) (layer Dwgs.User))
    (feature1 (pts (xy 220.45 119.45) (xy 220.400842 98.098955)))
    (feature2 (pts (xy 155.3 119.6) (xy 155.250842 98.248955)))
    (crossbar (pts (xy 155.257058 100.948948) (xy 220.407058 100.798948)))
    (arrow1a (pts (xy 220.407058 100.798948) (xy 219.281907 101.387961)))
    (arrow1b (pts (xy 220.407058 100.798948) (xy 219.279207 100.215122)))
    (arrow2a (pts (xy 155.257058 100.948948) (xy 156.384909 101.532774)))
    (arrow2b (pts (xy 155.257058 100.948948) (xy 156.382209 100.359935)))
  )
  (gr_arc (start 158.45 132.7) (end 158.45 135.7) (angle 88.09085647) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.449993 108.599583) (end 155.449993 108.599583) (angle 89.04515875) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.45 132.85) (end 155.45 108.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.6 135.7) (end 158.5 135.7) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 217.6 132.8) (end 220.5 132.8) (angle 89.06080905) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 220.5 108.45) (end 220.5 132.75) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 217.55 108.55) (end 217.55 105.6) (angle 88.12212255) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.4 105.6) (end 217.55 105.6) (layer Edge.Cuts) (width 0.15))
  (gr_text "(c) 2017 DB9MAT CC-BY-NC-SA\nRevision 1" (at 162.56 114.808) (layer F.SilkS))
  (gr_text "MMDVM_HS Pi Hat\n" (at 162.4 113.2) (layer F.SilkS))
  (gr_text Boot (at 196.75 114.7 90) (layer F.SilkS))
  (gr_text DFU (at 204.1 112.55) (layer F.SilkS))
  (gr_text Normal (at 199.9 112.55) (layer F.SilkS))
  (gr_text STLink (at 208.3 123.6 90) (layer F.SilkS))
  (gr_text Reset (at 210.65 131.35) (layer F.SilkS))
  (gr_text Display (at 208.25 126.95 90) (layer F.SilkS))
  (gr_text YSF (at 218.35 120.85) (layer F.SilkS))
  (gr_text P25 (at 218.35 119.55) (layer F.SilkS))
  (gr_text D* (at 217.7796 118.2704) (layer F.SilkS))
  (gr_text DMR (at 218.44 116.9877) (layer F.SilkS))
  (gr_text PTT (at 218.186 115.7177) (layer F.SilkS))
  (gr_text COS (at 218.313 114.4477) (layer F.SilkS))
  (gr_text PWR (at 218.44 113.1777) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.25 105.65) (xy 220.6 105.65) (xy 220.6 135.95) (xy 155.25 135.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.25 105.65) (xy 220.6 105.65) (xy 220.6 135.95) (xy 155.25 135.9)
      )
    )
  )
)
