(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 0)
    (no_connects 0)
    (area 114.862 57.064 142.313 112.465001)
    (thickness 1.6)
    (drawings 5)
    (tracks 53)
    (zones 0)
    (modules 8)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 1.7272)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7DF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Pin_Headers:Pin_Header_Straight_1x14 (layer F.Cu) (tedit 5D334B04)
    (at 128.016 74.295)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 1.524 -9.144) (layer F.SilkS) hide)
    (fp_text value "" (at 6.35 -14.986) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 6 thru_hole rect (at 0 12.7) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 7 thru_hole rect (at 0 15.24) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 8 thru_hole rect (at 0 17.78) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 9 thru_hole rect (at 0 20.32) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 thru_hole rect (at 0 22.86) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 thru_hole rect (at 0 25.4) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 thru_hole rect (at 0 27.94) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 13 thru_hole rect (at 0 30.48) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 14 thru_hole rect (at 0 33.02) (size 1.27 1.27) (drill 0.254 (offset -0.381 -0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module Pin_Headers:Pin_Header_Straight_1x14 (layer F.Cu) (tedit 5D334A62)
    (at 128.016 73.025)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 1.524 -9.144) (layer F.SilkS) hide)
    (fp_text value "" (at 6.35 -14.986) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 6 thru_hole rect (at 0 12.7) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 7 thru_hole rect (at 0 15.24) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 8 thru_hole rect (at 0 17.78) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 9 thru_hole rect (at 0 20.32) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 thru_hole rect (at 0 22.86) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 thru_hole rect (at 0 25.4) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 thru_hole rect (at 0 27.94) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 13 thru_hole rect (at 0 30.48) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 14 thru_hole rect (at 0 33.02) (size 1.27 1.27) (drill 0.254 (offset -0.381 0.381)) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module Pin_Headers:Pin_Header_Straight_1x14 (layer F.Cu) (tedit 5D2FBE9F)
    (at 127 73.66)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 1.524 -9.144) (layer F.SilkS) hide)
    (fp_text value "" (at 6.35 -14.986) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer B.Cu) (tedit 5D2E8558)
    (at 132.08 87.63 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference "" (at -19.685 -10.033 360) (layer B.SilkS) hide)
    (fp_text value "" (at -16.764 4.064 360) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (pad d thru_hole circle (at 22.86 0 270) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5CCB726F)
    (at 130.302 80.772)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at -14.478 -10.414) (layer F.SilkS) hide)
    (fp_text value "" (at -4.826 -18.288) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5D2E8B75)
    (at 137.668 82.296)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "" (at 0 3.2) (layer F.Fab) hide)
  )
  (module Potentiometers:Potentiometer_Trimmer-EVM3E (layer F.Cu) (tedit 5CCE3D6A)
    (at 131.064 75.184 180)
    (descr http://www.comkey.in/sites/default/files/attachments/EVM3ESX50B15.pdf)
    (tags "trimmer smd")
    (attr smd)
    (fp_text reference "" (at 0 3.835 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.785 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 1.6 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 1.6 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 -1.65 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5CCB726F)
    (at 129.54 110.49)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at -14.478 -10.414) (layer F.SilkS) hide)
    (fp_text value "" (at -4.826 -18.288) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask))
  )
  (gr_text "pi2hd44780  mincepi" (at 129.794 97.282 90) (layer F.SilkS))
  (gr_line (start 127 111.76) (end 127 72.39) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 133.35 111.76) (end 127 111.76) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 133.35 72.39) (end 133.35 111.76) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 127 72.39) (end 133.35 72.39) (angle 90) (layer Edge.Cuts) (width 0.0254))
)
