(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 59)
    (tracks 307)
    (zones 0)
    (modules 50)
    (nets 50)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.25)
    (via_size 0.7)
    (via_drill 0.3302)
    (via_min_size 0.7)
    (via_min_drill 0.3302)
    (uvia_size 0.7)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.2)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.1)
    (pad_size 0.9 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.055)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 -BATT)
  (net 2 "Net-(C101-Pad1)")
  (net 3 +3V3)
  (net 4 +5V)
  (net 5 +BATT)
  (net 6 "Net-(C108-Pad1)")
  (net 7 "Net-(C109-Pad1)")
  (net 8 "Net-(C112-Pad1)")
  (net 9 "Net-(D101-Pad1)")
  (net 10 "Net-(D102-Pad2)")
  (net 11 "Net-(D105-Pad2)")
  (net 12 A1)
  (net 13 RESET)
  (net 14 MISO)
  (net 15 MOSI)
  (net 16 SCK)
  (net 17 D8)
  (net 18 D7)
  (net 19 "Net-(R101-Pad1)")
  (net 20 "Net-(R102-Pad2)")
  (net 21 D13)
  (net 22 A2)
  (net 23 A3)
  (net 24 "Net-(J101-Pad4)")
  (net 25 "Net-(J101-Pad3)")
  (net 26 "Net-(J101-Pad2)")
  (net 27 "Net-(MOD101-Pad8)")
  (net 28 A5)
  (net 29 A4)
  (net 30 A0)
  (net 31 "Net-(U101-Pad33)")
  (net 32 D5)
  (net 33 D10)
  (net 34 D9)
  (net 35 D6)
  (net 36 D12)
  (net 37 D4)
  (net 38 "Net-(U101-Pad22)")
  (net 39 D1)
  (net 40 D0)
  (net 41 D11)
  (net 42 "Net-(U101-Pad8)")
  (net 43 D2_SDA)
  (net 44 D3_SCL)
  (net 45 "Net-(J102-Pad3)")
  (net 46 "Net-(C116-Pad2)")
  (net 47 "Net-(F101-Pad2)")
  (net 48 UD+)
  (net 49 UD-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.7)
    (via_drill 0.3302)
    (uvia_dia 0.7)
    (uvia_drill 0.3302)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.2)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net -BATT)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net D0)
    (add_net D1)
    (add_net D10)
    (add_net D11)
    (add_net D12)
    (add_net D13)
    (add_net D2_SDA)
    (add_net D3_SCL)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C108-Pad1)")
    (add_net "Net-(C109-Pad1)")
    (add_net "Net-(C112-Pad1)")
    (add_net "Net-(C116-Pad2)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(D105-Pad2)")
    (add_net "Net-(F101-Pad2)")
    (add_net "Net-(J101-Pad2)")
    (add_net "Net-(J101-Pad3)")
    (add_net "Net-(J101-Pad4)")
    (add_net "Net-(J102-Pad3)")
    (add_net "Net-(MOD101-Pad8)")
    (add_net "Net-(R101-Pad1)")
    (add_net "Net-(R102-Pad2)")
    (add_net "Net-(U101-Pad22)")
    (add_net "Net-(U101-Pad33)")
    (add_net "Net-(U101-Pad8)")
    (add_net RESET)
    (add_net SCK)
    (add_net UD+)
    (add_net UD-)
  )
  (module Airic_Lenz:Fiducial (layer F.Cu) (tedit 54469298)
    (at 114.3 50.292)
    (fp_text reference FID102 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 -2.54) (layer F.SilkS) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 1) (clearance 1))
  )
  (module Airic_Lenz:Fiducial (layer F.Cu) (tedit 54469298)
    (at 126.746 105.664)
    (fp_text reference FID101 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 -2.54) (layer F.SilkS) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 1) (clearance 1))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 123.19 96.012 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R111 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 UD-))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J101-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 124.714 96.012 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R110 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(J101-Pad3)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 UD+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52C)
    (at 119.38 107.823)
    (descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F101 (at 3.311 0.127) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 47 "Net-(F101-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 118.999 72.136)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C116 (at 0 1.27) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C116-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Airic_Lenz:NRF24L01 SMD Module" locked (layer F.Cu) (tedit 5CEE8570)
    (at 123.6 80.2 90)
    (fp_text reference MOD101 (at -6.8 -16.2 180) (layer F.SilkS))
    (fp_text value nRF24L01 (at -4.5 -11) (layer F.Fab))
    (fp_text user 3V3 (at -4.445 -1.5) (layer F.SilkS))
    (fp_text user GND (at -3.175 -1.5) (layer F.SilkS))
    (fp_text user CE (at -1.905 -1.5) (layer F.SilkS))
    (fp_text user CSN (at -0.69 -1.5) (layer F.SilkS))
    (fp_text user SCK (at 0.635 -1.5) (layer F.SilkS))
    (fp_text user MOSI (at 1.905 -1.5) (layer F.SilkS))
    (fp_text user MISO (at 3.12 -1.5) (layer F.SilkS))
    (fp_text user IRQ (at 4.39 -1.5) (layer F.SilkS))
    (pad 1 smd roundrect (at -4.445 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 3 +3V3))
    (pad 2 smd roundrect (at -3.175 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 1 -BATT))
    (pad 3 smd roundrect (at -1.905 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 34 D9))
    (pad 4 smd roundrect (at -0.635 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 17 D8))
    (pad 5 smd roundrect (at 0.635 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 16 SCK))
    (pad 6 smd roundrect (at 1.905 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 15 MOSI))
    (pad 7 smd roundrect (at 3.175 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 14 MISO))
    (pad 8 smd roundrect (at 4.445 0.254 90) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4)
      (net 27 "Net-(MOD101-Pad8)"))
    (pad 9 smd roundrect (at 5.715 -11.5 180) (size 0.9 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.4))
  )
  (module Airic_Lenz:AiricLenz_LOGO_15mm (layer F.Cu) (tedit 0)
    (at 126.619 89.408)
    (fp_text reference Logo101 (at 0 1.75006) (layer F.SilkS) hide)
    (fp_text value Airic_Lenz_Logo (at 0 -1.75006) (layer F.SilkS) hide)
  )
  (module Airic_Lenz:PinHeader_02x1 (layer F.Cu) (tedit 5BD5BD31)
    (at 129.54 53.975 180)
    (fp_text reference J106 (at 0.508 1.905) (layer F.SilkS) hide)
    (fp_text value Conn_Trigger (at 1.27 -1.905) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 D4))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 -BATT))
  )
  (module Airic_Lenz:PinHeader_03x1 (layer F.Cu) (tedit 5CDC47C8)
    (at 106.68 53.975)
    (fp_text reference J104 (at 0 2.032) (layer F.SilkS))
    (fp_text value Conn_Hall (at 2.54 -1.905) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 A1))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 -BATT))
  )
  (module Airic_Lenz:Micro_Switch_SSSS212-11 (layer F.Cu) (tedit 5CF03142)
    (at 112.141 109.855 334)
    (fp_text reference J102 (at 0 -1.7 154) (layer F.SilkS))
    (fp_text value Conn_Switch (at 0 -7.62 154) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 2.5 0 334) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(J102-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 0 334) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 +BATT))
    (pad 1 thru_hole roundrect (at -2.5 0 334) (size 1.6 1.524) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C101-Pad1)"))
  )
  (module Airic_Lenz:PinHeader_04x1 (layer F.Cu) (tedit 590B73BE)
    (at 134.62 61.595 90)
    (fp_text reference J103 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3.81 -1.905 90) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 D2_SDA))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 D3_SCL))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 -BATT))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 127.889 84.709)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C115 (at -0.127 1.397) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 109.982 64.262)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C114 (at -3.3655 0.0635) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 A3))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 118.74 64.4 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U101 (at 5.98 5.974 unlocked) (layer F.SilkS))
    (fp_text value ATMEGA32U4 (at 0 7.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 44 smd rect (at -4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 43 smd rect (at -3.2 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 42 smd rect (at -2.4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C112-Pad1)"))
    (pad 41 smd rect (at -1.6 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 A5))
    (pad 40 smd rect (at -0.8 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 A4))
    (pad 39 smd rect (at 0 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 A3))
    (pad 38 smd rect (at 0.8 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 A2))
    (pad 37 smd rect (at 1.6 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 A1))
    (pad 36 smd rect (at 2.4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 A0))
    (pad 35 smd rect (at 3.2 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 34 smd rect (at 4 -5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 33 smd rect (at 5.7 -4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U101-Pad33)"))
    (pad 32 smd rect (at 5.7 -3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 D13))
    (pad 31 smd rect (at 5.7 -2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 D5))
    (pad 30 smd rect (at 5.7 -1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 D10))
    (pad 29 smd rect (at 5.7 -0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 D9))
    (pad 28 smd rect (at 5.7 0 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 D8))
    (pad 27 smd rect (at 5.7 0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 D6))
    (pad 26 smd rect (at 5.7 1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 D12))
    (pad 25 smd rect (at 5.7 2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 D4))
    (pad 24 smd rect (at 5.7 3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 23 smd rect (at 5.7 4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 22 smd rect (at 4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U101-Pad22)"))
    (pad 21 smd rect (at 3.2 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 D1))
    (pad 20 smd rect (at 2.4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 D0))
    (pad 19 smd rect (at 1.6 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 D2_SDA))
    (pad 18 smd rect (at 0.8 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 D3_SCL))
    (pad 17 smd rect (at 0 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C108-Pad1)"))
    (pad 16 smd rect (at -0.8 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C109-Pad1)"))
    (pad 15 smd rect (at -1.6 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 14 smd rect (at -2.4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 13 smd rect (at -3.2 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 RESET))
    (pad 12 smd rect (at -4 5.7 180) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 D11))
    (pad 11 smd rect (at -5.7 4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 MISO))
    (pad 10 smd rect (at -5.7 3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 MOSI))
    (pad 9 smd rect (at -5.7 2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 SCK))
    (pad 8 smd rect (at -5.7 1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U101-Pad8)"))
    (pad 7 smd rect (at -5.7 0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 6 smd rect (at -5.7 0 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C116-Pad2)"))
    (pad 5 smd rect (at -5.7 -0.8 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 4 smd rect (at -5.7 -1.6 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 UD+))
    (pad 3 smd rect (at -5.7 -2.4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 UD-))
    (pad 2 smd rect (at -5.7 -3.2 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -5.7 -4 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 D7))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Airic_Lenz:USB_Micro_B_Würth (layer F.Cu) (tedit 5BD5E54D)
    (at 121.77644 115.594389 349)
    (fp_text reference J101 (at 0 -5.5 169) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 0.7 169) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 2.075 -3.9 349) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.075 -3.9 349) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad 6 smd roundrect (at 3.95 -1.45 349) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.053)
      (net 1 -BATT))
    (pad 6 smd roundrect (at 1.2 -1.45 349) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.053)
      (net 1 -BATT))
    (pad 6 smd roundrect (at -1.2 -1.45 349) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.053)
      (net 1 -BATT))
    (pad 6 smd roundrect (at -3.95 -1.45 79) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.053)
      (net 1 -BATT))
    (pad 5 smd roundrect (at 1.3 -4.125 349) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 4 smd roundrect (at 0.65 -4.125 349) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(J101-Pad4)"))
    (pad 3 smd roundrect (at 0 -4.125 349) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(J101-Pad3)"))
    (pad 2 smd roundrect (at -0.65 -4.125 349) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J101-Pad2)"))
    (pad 1 smd roundrect (at -1.3 -4.125 349) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(F101-Pad2)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.step
      (offset (xyz 0 2.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 114.173 72.136 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C113 (at -0.381 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_5032-4Pin_5.0x3.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 127.94 64.516 270)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y101 (at 0 -2.616 90) (layer F.SilkS))
    (fp_text value Crystal_GND24 (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -1.65 -1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 3 smd rect (at 1.65 -1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C109-Pad1)"))
    (pad 2 smd rect (at 1.65 1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 1 smd rect (at -1.65 1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C108-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.5 1.3 1.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5A0AB76C)
    (at 117.094 100.711 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U102 (at 0 2.286) (layer F.SilkS))
    (fp_text value MCP73831-2-OT (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R102-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +BATT))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R101-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Airic_Lenz:Testpoint (layer F.Cu) (tedit 54F6FFC9)
    (at 128.27 100.838)
    (fp_text reference TP103 (at 0 1.7) (layer F.SilkS) hide)
    (fp_text value TESTPOINT (at 0 -2) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Mask)
      (net 1 -BATT))
  )
  (module Airic_Lenz:Testpoint (layer F.Cu) (tedit 54F6FFC9)
    (at 133.35 100.838)
    (fp_text reference TP102 (at 0 1.7) (layer F.SilkS) hide)
    (fp_text value TESTPOINT (at 0 -2) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Mask)
      (net 4 +5V))
  )
  (module Airic_Lenz:Testpoint (layer F.Cu) (tedit 54F6FFC9)
    (at 130.81 100.838)
    (fp_text reference TP101 (at 0 1.7) (layer F.SilkS) hide)
    (fp_text value TESTPOINT (at 0 -2) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.1 1.1) (layers F.Cu F.Mask)
      (net 3 +3V3))
  )
  (module Package_TO_SOT_SMD:SOT-89-3_Handsoldering (layer F.Cu) (tedit 5A02FF57)
    (at 109.855 95.123 90)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference REG101 (at 0.127 3.175 90) (layer F.SilkS))
    (fp_text value NJU7200 (at 0.5 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0.38 0) (layer F.Fab))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 1.98 0) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad1)"))
    (pad 3 smd rect (at -1.98 1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1.98 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad1)"))
    (pad 1 smd rect (at -1.98 -1.5) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.982 65.786)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R109 (at -3.302 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 A3))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.982 67.31 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R108 (at 3.302 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 A3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.982 62.738)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R107 (at -3.302 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 A2))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.982 61.214 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R106 (at 3.302 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 A2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 117.094 55.118)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R105 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D105-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 D13))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 117.094 53.594 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R104 (at 0.014 1.27) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D102-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 128.016 71.374)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R103 (at 0 1.397) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 114.427 103.4415)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R102 (at -0.4445 1.3335) (layer F.SilkS))
    (fp_text value 2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R102-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 119.38 103.886)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R101 (at 3.08 0) (layer F.SilkS))
    (fp_text value 470 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D101-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R101-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Airic_Lenz:Flat-Header-6_with_Holes (layer F.Cu) (tedit 5BF3FE3B)
    (at 135.8 84.22 90)
    (fp_text reference J105 (at 6.35 -2.286 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at 6.35 2.54 90) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 13 RESET))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 14 MISO))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 15 MOSI))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 16 SCK))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.1 1.1) (drill 1) (layers *.Cu *.Mask)
      (net 1 -BATT))
    (pad 6 smd roundrect (at 12.7 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 3 +3V3))
    (pad 5 smd roundrect (at 10.16 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 13 RESET))
    (pad 4 smd roundrect (at 7.62 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 14 MISO))
    (pad 3 smd roundrect (at 5.08 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 15 MOSI))
    (pad 2 smd roundrect (at 2.54 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 16 SCK))
    (pad 1 smd roundrect (at 0 0 90) (size 1.6 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 1 -BATT))
  )
  (module Airic_Lenz:PinHeader_02x1 (layer F.Cu) (tedit 5BD5BD31)
    (at 129.54 93.472 270)
    (fp_text reference J102 (at 0.508 1.905 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 1.27 -1.905 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 -BATT))
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 120.65 55.118 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D105 (at -3.302 0) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D105-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 120.65 53.594 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D102 (at 0 1.27) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D102-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 119.38 105.41 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D101 (at -3.08 0 180) (layer F.SilkS))
    (fp_text value LED_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D101-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 109.982 68.834 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C112 (at 3.302 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C112-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 120.65 56.642 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C111 (at -3.302 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 109.982 58.166 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C110 (at 3.302 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128.016 68.326 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C109 (at -3.302 0) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C109-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128.016 60.706)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C108 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 20pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C108-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128.016 69.85)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C107 (at 3.302 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 109.982 70.358 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C106 (at 3.302 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 109.982 59.69 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C105 (at 3.302 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 120.65 100.711 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C104 (at -2.286 0.508 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.538 100.711 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C103 (at -2.286 -0.508 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 111.379 100.711 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C102 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 108.331 100.711 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C101 (at 3.048 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C101-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Airic_Lenz:WEEE_LOGO_15mm (layer B.Cu) (tedit 54F6FF1C)
    (at 126.873 83.312 180)
    (fp_text reference G*** (at 0.254 7.874 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -4.064 180) (layer B.SilkS) hide)
  )
  (gr_text "ESK8 Remote Rev3" (at 120.65 49.911) (layer B.SilkS))
  (gr_text TRG (at 127 52.324 90) (layer F.SilkS))
  (gr_text GND (at 129.54 52.324 90) (layer F.SilkS))
  (gr_text 3V (at 134.112 71.501) (layer F.SilkS))
  (gr_text "RESET\n" (at 134.112 74.041) (layer F.SilkS))
  (gr_text "MISO\n" (at 134.112 76.581) (layer F.SilkS))
  (gr_text MOSI (at 134.112 79.121) (layer F.SilkS))
  (gr_text SCK (at 134.112 81.661) (layer F.SilkS))
  (gr_text GND (at 134.112 84.328) (layer F.SilkS))
  (gr_text HALL (at 109.22 52.324 90) (layer F.SilkS))
  (gr_text GND (at 106.68 52.324 90) (layer F.SilkS))
  (gr_text 3V (at 111.76 52.324 90) (layer F.SilkS))
  (gr_text GND (at 133.096 61.595) (layer F.SilkS))
  (gr_text "3V\n" (at 133.096 59.055) (layer F.SilkS))
  (gr_text "SCL\n" (at 133.096 56.515) (layer F.SilkS))
  (gr_text SDA (at 132.334 52.578 90) (layer F.SilkS))
  (gr_text GND (at 128.143 102.87) (layer F.SilkS))
  (gr_text 5V (at 133.223 102.87) (layer F.SilkS))
  (gr_text "3V\n" (at 130.683 102.87) (layer F.SilkS))
  (gr_text "+BAT-\n" (at 131.826 94.742 90) (layer F.SilkS))
  (gr_arc (start 133.141912 110.415752) (end 135.23656 105.438559) (angle -110.5720106) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.494913 116.591273) (end 127.746081 110.203584) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 118.773438 115.166878) (xy 121.384173 115.84997) (xy 124.566464 116.482244) (xy 127.494913 116.591273)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 116.84668 114.625824) (xy 117.484318 114.817297) (xy 118.128684 114.998181) (xy 118.773438 115.166878)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 108.527496 111.109153) (xy 111.297974 112.849198) (xy 114.815194 114.017807) (xy 116.84668 114.625824)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 106.633305 109.710747) (xy 107.185653 110.19652) (xy 107.812635 110.660173) (xy 108.527496 111.109153)) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.113526 108.09415) (end 106.633305 109.710747) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 107.070902 106.827518) (xy 107.011482 106.667733) (xy 106.931874 106.516198) (xy 106.834019 106.376605)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 107.186203 107.323645) (xy 107.169071 107.154032) (xy 107.130323 106.987303) (xy 107.070902 106.827518)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 107.113526 108.09415) (xy 107.187686 107.844502) (xy 107.212375 107.582756) (xy 107.186203 107.323645)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 105.50193 103.442539) (xy 105.848518 104.658724) (xy 106.276813 105.581736) (xy 106.834019 106.376605)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 104.569342 92.457221) (xy 104.497027 98.146692) (xy 104.904549 101.346319) (xy 105.50193 103.442539)) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.569632 92.434343) (end 104.569342 92.457221) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 104.599448 90.026719) (xy 104.589953 90.830586) (xy 104.57981 91.633467) (xy 104.569632 92.434343)) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.517339 90.026719) (end 104.599448 90.026719) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.517339 88.426719) (end 105.517339 90.026719) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.632785 86.826719) (end 105.517339 86.826719) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 104.638219 79.047156) (xy 104.663665 81.613395) (xy 104.655425 84.21808) (xy 104.632785 86.826719)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 103.680797 63.60625) (xy 104.455022 68.113271) (xy 104.598897 75.081471) (xy 104.638219 79.047156)) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.680797 49.523382) (end 103.680797 63.60625) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.180797 49.523382) (end 105.080797 48.02672) (angle -86.17744627) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.136227 48.02672) (end 105.080797 48.02672) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.498033 48.897844) (xy 136.573562 49.061399) (xy 136.619012 49.23723) (xy 136.632201 49.416899)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.189905 48.459123) (xy 136.318125 48.585671) (xy 136.422504 48.734289) (xy 136.498033 48.897844)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 135.705702 48.139024) (xy 135.886401 48.213179) (xy 136.050888 48.321918) (xy 136.189905 48.459123)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 135.136227 48.02672) (xy 135.331549 48.02672) (xy 135.525004 48.06487) (xy 135.705702 48.139024)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 137.525592 79.746379) (xy 137.588865 69.782683) (xy 137.365158 59.401219) (xy 136.632201 49.416899)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 137.433669 86.829685) (xy 137.479565 84.458811) (xy 137.510671 82.096091) (xy 137.525592 79.746379)) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.500638 86.829685) (end 137.433669 86.829685) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.500638 88.429685) (end 136.500638 86.829685) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.362977 90.029685) (end 136.500638 90.029685) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 137.299376 92.409537) (xy 137.322117 91.615709) (xy 137.343334 90.822365) (xy 137.362977 90.029685)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.617873 104.631427) (xy 136.992719 101.381219) (xy 137.160714 97.251981) (xy 137.299376 92.409545)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 135.569171 105.515328) (xy 135.454722 105.50899) (xy 135.34221 105.483022) (xy 135.23656 105.438559)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 135.908224 105.475751) (xy 135.798311 105.508277) (xy 135.68362 105.521665) (xy 135.569171 105.515328)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.617873 104.631427) (xy 136.602955 104.760785) (xy 136.562912 104.885991) (xy 136.5 105)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.251023 105.296227) (xy 136.149537 105.377815) (xy 136.033086 105.4388) (xy 135.908224 105.475751)) (layer Edge.Cuts) (width 0.15))
  (gr_curve (pts (xy 136.5 105) (xy 136.437088 105.114008) (xy 136.352508 105.214639) (xy 136.251023 105.296227)) (layer Edge.Cuts) (width 0.15))
  (gr_text SW (at 108.966 106.045) (layer F.SilkS))
  (zone (net 1) (net_name -BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 50 30) (xy 150 30) (xy 150 130) (xy 50 130)
      )
    )
  )
  (zone (net 1) (net_name -BATT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 35) (xy 145 35) (xy 145 125) (xy 55 125)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.3) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 114.3 59.944) (xy 123.19 59.944) (xy 123.19 68.834) (xy 114.3 68.834)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.267 73.152) (xy 112.776 73.152) (xy 113.157 73.533) (xy 113.157 87.122) (xy 104.267 87.122)
      )
    )
  )
  (zone (net 5) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 123.952 95.758) (xy 124.714 97.028) (xy 125.984 95.758)
      )
    )
  )
)
