(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 62)
    (no_connects 0)
    (area 57.952857 54.559999 255.277714 200.486)
    (thickness 1.6)
    (drawings 60)
    (tracks 132)
    (zones 0)
    (modules 41)
    (nets 22)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 62.23 105.41)
    (grid_origin 62.23 105.41)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00020_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 /PulseOutput)
  (net 5 +5V)
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(J2-Pad1)")
  (net 9 "Net-(J3-Pad1)")
  (net 10 "Net-(Q1-Pad1)")
  (net 11 "Net-(R4-Pad2)")
  (net 12 "Net-(Q2-Pad3)")
  (net 13 "Net-(Q1-Pad3)")
  (net 14 "Net-(Q3-Pad2)")
  (net 15 "Net-(Q3-Pad1)")
  (net 16 "Net-(C4-Pad1)")
  (net 17 "Net-(Q2-Pad2)")
  (net 18 "Net-(Q4-Pad3)")
  (net 19 "Net-(Q5-Pad3)")
  (net 20 "Net-(R9-Pad1)")
  (net 21 "Net-(R11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PulseOutput)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R9-Pad1)")
  )
  (net_class Narrow ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (net_class Wide ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad2)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A0E154F)
    (at 184.2008 100.1776)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A0E154F)
    (at 184.2008 59.8678)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A0E154F)
    (at 67.564 100.5586)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 5A0CE689)
    (at 183.43 70.31 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at -1.3434 2.7266 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 2.746 2.7266 90) (layer F.SilkS))
    (fp_text user %R (at -1.318 2.7266 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 5A0CDA00)
    (at 112.73 79.21)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 4.7 -0.6) (layer F.SilkS))
    (fp_text value 10n (at 5.1 1) (layer F.SilkS))
    (fp_text user %R (at 4.6942 -0.597) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 5A0CDA0B)
    (at 77.1906 97.917 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 2.5 -2.8 180) (layer F.SilkS))
    (fp_text value 1n (at -1.7 -2.7 180) (layer F.SilkS))
    (fp_text user %R (at 2.4778 -2.8006 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 5A0CD9A7)
    (at 132.23 85.21 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at 3 2.6 450) (layer F.SilkS))
    (fp_text value 220pF (at -1.25 2.65 450) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P12.70mm_Horizontal placed (layer F.Cu) (tedit 59C18802)
    (at 110.73 74.21 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 9.1046 -2.5742 180) (layer F.SilkS))
    (fp_text value 1N4937 (at 4.1008 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P12.70mm_Horizontal placed (layer F.Cu) (tedit 59DE8240)
    (at 84.836 90.424 270)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 10.16 2.54 270) (layer F.SilkS))
    (fp_text value 1N914 (at 5.588 2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide placed (layer F.Cu) (tedit 59E6929E)
    (at 96.012 78.994 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -2.5908 0.381 360) (layer F.SilkS))
    (fp_text value JN3303 (at -4.318 -1.2954 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide placed (layer F.Cu) (tedit 5A0CCFF2)
    (at 160.43 76.31)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at -2.2 2.3 90) (layer F.SilkS))
    (fp_text value 2N3906 (at -2.2 -2.4 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal placed (layer F.Cu) (tedit 59E69325)
    (at 150.876 94.996 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single")
    (fp_text reference RV1 (at 3.556 3.81 180) (layer F.SilkS))
    (fp_text value "500k POT" (at -2.0066 3.81 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /PulseOutput))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal placed (layer F.Cu) (tedit 59C18016)
    (at 125.476 96.012 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single")
    (fp_text reference RV2 (at -6.858 -3.048 180) (layer F.SilkS))
    (fp_text value "10Ω POT" (at -8.89 -4.826 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R9-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket placed (layer F.Cu) (tedit 5A0CD92C)
    (at 97.79 88.646)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at -0.46 -2.536) (layer F.SilkS))
    (fp_text value LM555N (at 3.81 10.01) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q5-Pad3)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59DE8232)
    (at 79.756 84.836 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R1 (at -3.556 1.524 180) (layer F.SilkS))
    (fp_text value 100k (at -4.318 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(Q5-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C1801A)
    (at 117.83 74.21)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R2 (at -0.254 -3.048) (layer F.SilkS))
    (fp_text value 4.7M (at 4.2932 -2.9884) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5A0CD4DF)
    (at 146.53 75.81)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R3 (at 1.6 2.9) (layer F.SilkS))
    (fp_text value 1k (at 4.8 2.9) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(Q4-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F8C)
    (at 113.23 85.21 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R4 (at 4.572 -2.794 270) (layer F.SilkS))
    (fp_text value 330 (at 0.508 -2.794 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F55)
    (at 90.424 95.25 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R5 (at 4.572 -3.048 270) (layer F.SilkS))
    (fp_text value 1k (at 1.778 -3.048 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(R4-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5A0CD19C)
    (at 146.63 83.31)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R6 (at -0.6 2.9) (layer F.SilkS))
    (fp_text value 100 (at 2.54 2.86) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(Q4-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(Q2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F95)
    (at 158.73 83.31 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R7 (at 4.574 2.901 270) (layer F.SilkS))
    (fp_text value 100 (at 1.399 2.901 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /PulseOutput))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5A0CCF44)
    (at 137.93 95.41 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R8 (at -0.7 -3.1 90) (layer F.SilkS))
    (fp_text value 100k (at 2.9 -3.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(C4-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 59E68D18)
    (at 140.33 86.41 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 7.112 -3.556 360) (layer F.SilkS))
    (fp_text value 2N3904 (at 7.112 1.27 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C4-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Q4-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17FEF)
    (at 122.63 88.91 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R9 (at -0.0154 3.0238 90) (layer F.SilkS))
    (fp_text value 15 (at 4.064 3.048 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(R9-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 59C18020)
    (at 158.73 97.61 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C5 (at 1.6278 -2.3822 270) (layer F.SilkS))
    (fp_text value 1uF (at -1.9028 -2.3822 270) (layer F.SilkS))
    (fp_text user %R (at 1.6278 -2.3568 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /PulseOutput))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5A0CDA04)
    (at 105.156 83.312)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C6 (at -1.6256 2.4892) (layer F.SilkS))
    (fp_text value 1uF (at 2.1844 2.4892) (layer F.SilkS))
    (fp_text user %R (at -1.6256 2.4892) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P7.62mm_Vertical (layer F.Cu) (tedit 59E692AF)
    (at 76.962 76.962)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=7.62mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 7.62mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference L1 (at 0 -3.048) (layer F.SilkS))
    (fp_text value 10mH (at 6.096 -3.048) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 7.62 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P7.62mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A0CD668)
    (at 167.73 86.41)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at -0.5 -4 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 4.4 -4 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal (layer F.Cu) (tedit 59E68CCF)
    (at 166.878 94.996 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single")
    (fp_text reference RV3 (at 3.556 -8.636 180) (layer F.SilkS))
    (fp_text value "10Ω POT" (at -3.048 -8.636 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5A0CD5ED)
    (at 173.23 77.11)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U2 (at -2.5 -2.8) (layer F.SilkS))
    (fp_text value LMV321 (at 1.8 -2.8) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /PulseOutput))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q3-Pad2)"))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 5A0CC99D)
    (at 183.33 83.61 90)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at -3.8 0 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at -0.1 18.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Connections_Bridges:WireConnection_1.50mmDrill (layer F.Cu) (tedit 5A0CCE28)
    (at 129.53 72.11)
    (descr "WireConnection with 1.5mm drill")
    (fp_text reference J3 (at 3.6422 3.8868 90) (layer F.SilkS))
    (fp_text value GM_Tube (at 3.5914 -0.8122 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask)
      (net 16 "Net-(C4-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A0CD426)
    (at 113.53 99.61 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q5 (at -0.2 -3.9 270) (layer F.SilkS))
    (fp_text value 2N3904 (at 4.2 -3.9 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q5-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5A0CDAEF)
    (at 80.03 90.51 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R10 (at 5.0492 -3.216 180) (layer F.SilkS))
    (fp_text value 220k (at 0.7312 -3.216 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5A0CCD3D)
    (at 176.03 99.01 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R11 (at -0.685 2.9892 90) (layer F.SilkS))
    (fp_text value 15 (at 3.0996 2.9638 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:GM_tube_ziptie_mounts (layer F.Cu) (tedit 5A0E224B)
    (at 90.73 69.51 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference FuseHolder1 (at 7.62 -2.66 90) (layer Cmts.User) hide)
    (fp_text value ZipTie (at 4.8 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 9.74 0 90) (size 6 6) (drill oval 4) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomFootprints:GM_tube_ziptie_mounts (layer F.Cu) (tedit 5A0E2261)
    (at 149.43 69.51 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference FuseHolder1 (at 7.62 -2.66 90) (layer Cmts.User) hide)
    (fp_text value ZipTie (at 5 0.1 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 9.74 0 90) (size 6 6) (drill 4) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module KNEK-TEK_logo:KNEK-TEK_logo_11mm (layer F.Cu) (tedit 0)
    (at 175.0822 66.294)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:OSHW-Logo_7.5x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 184.15 92.5068)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_7.5x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A0E154F)
    (at 67.564 60.071)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module CustomFootprints:USB_Micro-B_big_holes_for_OSHpark (layer F.Cu) (tedit 5A0E269E)
    (at 66.7004 79.5528 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 -3.24 270) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 5.01 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5 -1.35) (size 1.397 1.397) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.5 -1.35) (size 1.397 1.397) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.5 1.35) (size 1.5494 1.5494) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.5 1.35) (size 1.5494 1.5494) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text 5V (at 71.7296 83.2866) (layer F.SilkS))
  (gr_text "Design files available at:\nhttps://github.com/Erik-k/StarJar" (at 119.3038 63.2206) (layer B.SilkS))
  (gr_text GND (at 68.961 90.805) (layer F.SilkS))
  (gr_text GND (at 142.5956 88.4428) (layer F.SilkS))
  (gr_text "K'NEK-TEK Star Jar v1.2\nNov 2017" (at 175.387 57.785) (layer F.Fab))
  (gr_text "LED Current Limiting" (at 166.878 91.694) (layer F.SilkS))
  (gr_text GND (at 113.538 103.378) (layer F.SilkS))
  (gr_text GND (at 143.9064 95.332) (layer F.SilkS))
  (dimension 127 (width 0.3) (layer F.SilkS)
    (gr_text "5.0000 in" (at 125.73 111.078) (layer F.SilkS))
    (feature1 (pts (xy 62.23 108.966) (xy 62.23 112.428)))
    (feature2 (pts (xy 189.23 108.966) (xy 189.23 112.428)))
    (crossbar (pts (xy 189.23 109.728) (xy 62.23 109.728)))
    (arrow1a (pts (xy 62.23 109.728) (xy 63.356504 109.141579)))
    (arrow1b (pts (xy 62.23 109.728) (xy 63.356504 110.314421)))
    (arrow2a (pts (xy 189.23 109.728) (xy 188.103496 109.141579)))
    (arrow2b (pts (xy 189.23 109.728) (xy 188.103496 110.314421)))
  )
  (dimension 50.8 (width 0.3) (layer F.SilkS)
    (gr_text "2.0000 in" (at 193.882 80.01 270) (layer F.SilkS))
    (feature1 (pts (xy 191.008 105.41) (xy 195.232 105.41)))
    (feature2 (pts (xy 191.008 54.61) (xy 195.232 54.61)))
    (crossbar (pts (xy 192.532 54.61) (xy 192.532 105.41)))
    (arrow1a (pts (xy 192.532 105.41) (xy 191.945579 104.283496)))
    (arrow1b (pts (xy 192.532 105.41) (xy 193.118421 104.283496)))
    (arrow2a (pts (xy 192.532 54.61) (xy 191.945579 55.736504)))
    (arrow2b (pts (xy 192.532 54.61) (xy 193.118421 55.736504)))
  )
  (gr_text "HIGH VOLTAGE ZONE - 400V+" (at 119.126 57.277) (layer F.SilkS))
  (gr_text - (at 186.69 87.122) (layer F.SilkS))
  (gr_text + (at 186.944 74.422) (layer F.SilkS))
  (gr_text 1.2 (at 253.492 198.882) (layer F.Fab))
  (gr_text "November 2017" (at 200.152 198.882) (layer F.Fab))
  (gr_text "Star Jar" (at 175.514 195.326) (layer F.Fab))
  (gr_text "K'NEK-TEK Star Jar v1.2\nNov 2017" (at 175.387 57.785) (layer F.SilkS))
  (gr_text "HV Tuning" (at 134.62 102.87) (layer F.SilkS))
  (gr_text "Pulse Length Control" (at 150.876 103.378) (layer F.SilkS))
  (gr_line (start 62.23 54.61) (end 62.23 105.41) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 54.61) (end 62.23 54.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 105.41) (end 189.23 54.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 62.23 105.41) (end 189.23 105.41) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.214 104.648) (xy 62.992 104.648) (xy 62.992 55.626) (xy 188.214 55.626)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.992 55.626) (xy 62.992 104.648) (xy 188.214 104.648) (xy 188.214 55.626)
      )
    )
  )
)
