(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 10)
    (no_connects 0)
    (area 125.908999 90.856999 151.713001 107.771001)
    (thickness 1.6)
    (drawings 10)
    (tracks 32)
    (zones 0)
    (modules 4)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 C)
  (net 2 A)
  (net 3 B)
  (net 4 GND)
  (net 5 "Net-(P1-Pad2)")
  (net 6 "Net-(P2-Pad2)")
  (net 7 "Net-(P3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad2)")
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.15)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A)
    (add_net B)
    (add_net C)
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 58771648)
    (at 131.064 92.964 270)
    (fp_text reference J1 (at 6.51002 3.79476 270) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312 270) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 1.905 270) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 C))
    (pad 7 thru_hole circle (at 3.81 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 C))
    (pad 6 thru_hole circle (at 4.826 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 A))
    (pad 4 thru_hole circle (at 6.858 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 B))
    (pad 2 thru_hole circle (at 8.89 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 5.842 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 B))
    (pad 3 thru_hole circle (at 7.874 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 A))
    (pad 1 thru_hole circle (at 9.906 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad "" thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58772177)
    (at 144.78 101.6 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference A (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 A))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58772181)
    (at 144.78 99.06 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference B (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 B))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58772185)
    (at 144.78 96.52 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference C (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 C))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "FRC2168\nRJ45->3xPWM\nv0.1" (at 139.8905 99.2505 90) (layer B.SilkS))
  (gr_text Sig (at 144.907 92.9005 90) (layer F.SilkS))
  (gr_text Gnd (at 150.0505 92.9005 90) (layer F.SilkS))
  (gr_text 3xPWM (at 147.574 106.299) (layer F.SilkS))
  (gr_line (start 136.398 90.932) (end 125.984 90.932) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.638 90.932) (end 136.398 90.932) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.638 92.71) (end 151.638 90.932) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.638 107.696) (end 151.638 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.984 107.696) (end 151.638 107.696) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.984 90.932) (end 125.984 107.696) (angle 90) (layer Edge.Cuts) (width 0.15))
)
