(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 20)
    (no_connects 0)
    (area 41.58359 97.13366 124.535001 171.725843)
    (thickness 1.6)
    (drawings 18)
    (tracks 75)
    (zones 0)
    (modules 26)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(J1-Pad11)")
  (net 7 "Net-(J1-Pad12)")
  (net 8 "Net-(J1-Pad10)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad8)")
  (net 11 "Net-(J1-Pad5)")
  (net 12 "Net-(J1-Pad6)")
  (net 13 "Net-(J1-Pad7)")
  (net 14 +3V3)
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J1-Pad13)")
  (net 17 "Net-(J1-Pad14)")
  (net 18 "Net-(J1-Pad15)")
  (net 19 "Net-(J1-Pad16)")
  (net 20 "Net-(J2-Pad11)")
  (net 21 "Net-(J2-Pad12)")
  (net 22 "Net-(J2-Pad10)")
  (net 23 "Net-(J2-Pad9)")
  (net 24 "Net-(J2-Pad8)")
  (net 25 "Net-(J2-Pad5)")
  (net 26 "Net-(J2-Pad6)")
  (net 27 "Net-(J2-Pad7)")
  (net 28 "Net-(J2-Pad4)")
  (net 29 "Net-(J2-Pad3)")
  (net 30 "Net-(J2-Pad2)")
  (net 31 "Net-(J2-Pad1)")
  (net 32 "Net-(U1-Pad1)")
  (net 33 "Net-(U1-Pad5)")
  (net 34 "Net-(U2-Pad1)")
  (net 35 "Net-(U2-Pad2)")
  (net 36 "Net-(U2-Pad3)")
  (net 37 "Net-(U2-Pad4)")
  (net 38 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C5B66B5)
    (at 68.58 127)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C5B6666)
    (at 71.12 132.08)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED2 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C5B6680)
    (at 66.04 132.08)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED3 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C5B6652)
    (at 68.58 137.16)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED4 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit_FeatherWing:Conn_PinHeader_1x16 (layer F.Cu) (tedit 5C5B5EB4)
    (at 78.74 127 270)
    (fp_text reference J1 (at 0 0.508 450) (layer F.Fab))
    (fp_text value CONN_01X16 (at 0 -0.508 270) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0 450) (layer Eco1.User))
    (pad 11 thru_hole circle (at 6.35 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 8.89 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad12)"))
    (pad 10 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at 1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at -1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad8)"))
    (pad 5 thru_hole circle (at -8.89 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -6.35 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 4 thru_hole circle (at -11.43 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -13.97 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -16.51 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 1 thru_hole rect (at -19.05 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
    (pad 13 thru_hole circle (at 11.43 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad13)"))
    (pad 14 thru_hole circle (at 13.97 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 16.51 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad15)"))
    (pad 16 thru_hole circle (at 19.05 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad16)"))
  )
  (module Adafruit_FeatherWing:Conn_PinHeader_1x12 (layer F.Cu) (tedit 5C5B5EA9)
    (at 99.06 132.08 270)
    (fp_text reference J2 (at 0 0.6 450) (layer F.Fab))
    (fp_text value CONN_01X12 (at 0 -0.5 270) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0 450) (layer Eco1.User))
    (pad 11 thru_hole circle (at 11.43 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 13.97 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad12)"))
    (pad 10 thru_hole circle (at 8.89 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad10)"))
    (pad 9 thru_hole circle (at 6.35 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad9)"))
    (pad 8 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad8)"))
    (pad 5 thru_hole circle (at -3.81 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at -1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 1.27 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad7)"))
    (pad 4 thru_hole circle (at -6.35 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad4)"))
    (pad 3 thru_hole circle (at -8.89 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at -11.43 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at -13.97 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad1)"))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C5B6A07)
    (at 63.5 137.16 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C5B68EF)
    (at 55.88 116.84)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad6)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C5B6909)
    (at 66.04 116.84)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C5B690F)
    (at 55.88 121.92)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad8)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C5B6915)
    (at 66.04 121.92)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C5B6A01)
    (at 58.42 132.08)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference SW1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Button (at 0 7.62) (layer Cmts.User) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C5B6974)
    (at 104.14 134.62 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33 180) (layer Cmts.User))
    (fp_text value NXP-9DOF_JP1 (at 0 15.03 180) (layer Cmts.User) hide)
    (fp_text user %R (at 0 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad12)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5C5B5E92)
    (at 116.84 132.08 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference U2 (at 0 -2.33 180) (layer Cmts.User))
    (fp_text value NXP-9DOF_JP2 (at 0 9.95 180) (layer Cmts.User) hide)
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C5B69F9)
    (at 71.12 144.78)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "Hole 2" (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C5B69F3)
    (at 109.22 144.78)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "Hole 3" (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C5B6C83)
    (at 71.12 109.22)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "Hole 1" (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Design:Try_1 (layer B.Cu) (tedit 0)
    (at 75.184 134.112 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Design:Try_2 (layer B.Cu) (tedit 5C65CD8A)
    (at 94.615 108.585)
    (fp_text reference G*** (at 0 0) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0) (layer Cmts.User) hide)
  )
  (module Design:Try_4 (layer F.Cu) (tedit 5C65CE97)
    (at 109.728 142.494)
    (fp_text reference G*** (at 0 0) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0) (layer Cmts.User) hide)
  )
  (module Design:Try_4 (layer F.Cu) (tedit 0)
    (at 73.152 145.288 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module Design:Try_4 (layer F.Cu) (tedit 0)
    (at 70.358 111.252 180)
    (fp_text reference G*** (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer F.SilkS) hide)
  )
  (module Design:Try_5 (layer F.Cu) (tedit 5C65D025)
    (at 88.9 107.95 90)
    (fp_text reference G*** (at 0 0 90) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer Cmts.User) hide)
  )
  (module Design:Try_5 (layer F.Cu) (tedit 5C65D016)
    (at 88.9 149.86 90)
    (fp_text reference G*** (at 0 0 90) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer Cmts.User) hide)
  )
  (module Design:Try_3 (layer F.Cu) (tedit 5C65D084)
    (at 88.9 129.54 90)
    (fp_text reference G*** (at 0 0 90) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer Cmts.User) hide)
  )
  (module Design:Try_5 (layer F.Cu) (tedit 5C65D0B1)
    (at 111.76 128.27)
    (fp_text reference G*** (at 0 0) (layer Cmts.User) hide)
    (fp_text value LOGO (at 0.75 0) (layer Cmts.User) hide)
  )
  (gr_text 2019 (at 123.48 139.66 90) (layer B.SilkS))
  (gr_text "Design: Francisco Botello & Alan G." (at 121.88 128.37 90) (layer B.SilkS))
  (gr_text 10kohm (at 60.96 133.35 90) (layer F.SilkS))
  (gr_text 220ohm (at 69.85 119.38) (layer F.SilkS))
  (gr_text 220ohm (at 59.69 119.38) (layer F.SilkS))
  (gr_text 220ohm (at 69.85 114.3) (layer F.SilkS))
  (gr_text 220ohm (at 59.69 114.3) (layer F.SilkS))
  (gr_line (start 101.6 114.3) (end 124.46 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 154.94) (end 53.34 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 114.3) (end 76.2 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 142.24) (end 53.34 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 154.94) (end 76.2 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 142.24) (end 101.6 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 114.3) (end 124.46 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 101.6) (end 101.6 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 101.6) (end 101.6 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "FEATHER M0 WiFi" (at 82.55 128.27 90) (layer F.SilkS))
  (gr_text "NXP 9-DOF" (at 107.95 128.27 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.33 115.57) (xy 123.19 115.57) (xy 123.19 140.97) (xy 101.6 153.67) (xy 76.2 153.67)
        (xy 54.61 140.97) (xy 54.61 114.3) (xy 76.2 102.87) (xy 100.33 102.87)
      )
    )
  )
)
