(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 72)
    (no_connects 0)
    (area 129.464999 78.664999 161.365001 134.985)
    (thickness 1.6)
    (drawings 11)
    (tracks 160)
    (zones 0)
    (modules 8)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /PC-CTS#)
  (net 3 /VCC)
  (net 4 /PC-TXD)
  (net 5 /PC-RXD)
  (net 6 /PC-RTS#)
  (net 7 /TGT-1)
  (net 8 /TGT-2)
  (net 9 /TGT-3)
  (net 10 /TGT-4)
  (net 11 /TGT-5)
  (net 12 /TGT-6)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /PC-CTS#)
    (add_net /PC-RTS#)
    (add_net /PC-RXD)
    (add_net /PC-TXD)
    (add_net /TGT-1)
    (add_net /TGT-2)
    (add_net /TGT-3)
    (add_net /TGT-4)
    (add_net /TGT-5)
    (add_net /TGT-6)
    (add_net /VCC)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 locked (layer F.Cu) (tedit 588BACEC)
    (at 133.35 105.41 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -3.81 1.27 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD11)
    (at 154.94 92.71 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD1D)
    (at 154.94 100.33 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /PC-CTS#))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD20)
    (at 154.94 107.95 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VCC))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD23)
    (at 154.94 115.57 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /PC-TXD))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD28)
    (at 154.94 123.19 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /PC-RXD))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06 (layer F.Cu) (tedit 588BAD2B)
    (at 154.94 130.81 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /PC-RTS#))
    (pad 12 thru_hole oval (at 12.7 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 588BAD17)
    (at 154.94 85.09 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /TGT-1))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /TGT-2))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /TGT-3))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /TGT-4))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /TGT-5))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /TGT-6))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_line (start 129.54 134.62) (end 161.29 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 78.74) (end 129.54 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 134.62) (end 129.54 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 78.74) (end 161.29 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "6 5 4 3 2 1" (at 148.59 81.28) (layer F.SilkS))
  (gr_text RTS# (at 139.7 130.81) (layer F.SilkS))
  (gr_text RX (at 139.7 123.19) (layer F.SilkS))
  (gr_text TX (at 139.7 115.57) (layer F.SilkS))
  (gr_text VCC (at 139.7 107.95) (layer F.SilkS))
  (gr_text CTS# (at 139.7 100.33) (layer F.SilkS))
  (gr_text GND (at 139.7 92.71) (layer F.SilkS))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 133.35) (xy 130.81 133.35) (xy 130.81 80.01) (xy 160.02 80.01)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 133.35) (xy 130.81 133.35) (xy 130.81 80.01) (xy 160.02 80.01)
      )
    )
  )
)
