(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "COM3")
  (net 2 "SEG8")
  (net 3 "SEG9")
  (net 4 "SEG10")
  (net 5 "SEG11")
  (net 6 "SEG12")
  (net 7 "SEG13")
  (net 8 "SEG14")
  (net 9 "SEG15")
  (net 10 "SEG16")
  (net 11 "COM2")
  (net 12 "COM1")
  (net 13 "SEG19")
  (net 14 "SEG20")
  (net 15 "SEG21")
  (net 16 "SEG22")
  (net 17 "SEG23")
  (net 18 "SEG24")
  (net 19 "SEG25")
  (net 20 "SEG26")
  (net 21 "SEG27")
  (net 22 "SEG28")
  (net 23 "SEG29")
  (net 24 "COM0")
  (net 25 "+9V")
  (net 26 "GND")
  (net 27 "+3V3")
  (net 28 "V_9V")
  (net 29 "Net-(LS1-Pad1)")
  (net 30 "Net-(LS1-Pad2)")
  (net 31 "Net-(Q1-Pad1)")
  (net 32 "Net-(Q2-Pad3)")
  (net 33 "SHIFT_SW")
  (net 34 "MINMX_SW")
  (net 35 "RANGE_SW")
  (net 36 "HOLD_SW")
  (net 37 "BKLT_SW")
  (net 38 "BEEP_SW")
  (net 39 "REL_SW")
  (net 40 "HZ_SW")
  (net 41 "BKLT")
  (net 42 "BPR")
  (net 43 "unconnected-(J3-Pad2)")
  (net 44 "Net-(J1-Pad1)")
  (net 45 "unconnected-(J3-Pad3)")
  (net 46 "unconnected-(J3-Pad4)")
  (net 47 "unconnected-(J3-Pad5)")
  (net 48 "unconnected-(J3-Pad6)")
  (net 49 "unconnected-(J3-Pad7)")
  (net 50 "unconnected-(J3-Pad8)")
  (net 51 "unconnected-(J3-Pad9)")
  (net 52 "unconnected-(J3-Pad19)")
  (net 53 "unconnected-(J3-Pad22)")
  (net 54 "unconnected-(J3-Pad34)")
  (net 55 "unconnected-(J3-Pad35)")
  (net 56 "unconnected-(J3-Pad37)")
  (net 57 "unconnected-(J3-Pad38)")
  (net 58 "I2C_SDA")
  (net 59 "I2C_SCL")
  (net 60 "Net-(U3-Pad11)")
  (net 61 "Net-(D1-Pad2)")
  (net 62 "Net-(BT1-Pad1)")
  (net 63 "unconnected-(U4-Pad19)")
  (net 64 "unconnected-(U4-Pad20)")
  (net 65 "unconnected-(U4-Pad22)")
  (net 66 "Net-(D3-Pad2)")
  (net 67 "Net-(U4-Pad7)")
  (net 68 "Net-(U4-Pad8)")
  (net 69 "UART_DTR")
  (net 70 "RESET")
  (net 71 "unconnected-(J3-Pad39)")
  (net 72 "UART_RX")
  (net 73 "UART_TX")
  (net 74 "SPI_MISO")
  (net 75 "SPI_SCK")
  (net 76 "SPI_MOSI")
  (net 77 "Net-(Q3-Pad3)")
  (net 78 "Net-(R13-Pad2)")
  (net 79 "unconnected-(J4-Pad2)")
  (net 80 "Net-(C7-Pad1)")
  (net 81 "Net-(C7-Pad2)")
  (net 82 "unconnected-(U6-Pad1)")
  (net 83 "RTC_INT")
  (net 84 "VLCD")
  (net 85 "Net-(JP1-Pad3)")
  (net 86 "Net-(D4-Pad1)")
  (net 87 "STAT_LED")
  (net 88 "Net-(R22-Pad2)")
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 71.9375 148.1498)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "AO3401A" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J1-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.946 69.168)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -2.4892 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.6312 149.5552 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "RESET") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(R22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 116.6876 129.8232 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.6924) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "V_9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 77.3096 140.4404 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:Symbol_Barrel_Polarity" (layer "F.Cu")
    (tedit 62A933B0)
    (at 79.756 150.5978)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Symbol_Barrel_Polarity" (at 0 2) (layer "F.Fab"))
    (fp_text user "+" (at 3 0 unlocked) (layer "F.SilkS"))
    (fp_text user "-" (at -3 0 unlocked) (layer "F.SilkS"))
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 108.833332 103.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW8" (at -3.688668 0 unlocked) (layer "F.SilkS"))
    (fp_text value "REL" (at 0 -2.9592 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 39 "REL_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.2484 122.6096 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.5616 0 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 113.5888 113.9736 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 2.1628 -2.8956) (layer "F.SilkS"))
    (fp_text value "ICSP" (at 0.4648 -3.7592) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "SPI_MISO") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "+3V3") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "SPI_SCK") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "SPI_MOSI") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "RESET") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 133.35 130.7884 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.6256) (layer "F.Fab"))
    (fp_text value "PWR" (at 0 -1.7488) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 77.5 146.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 2.5908 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.9528 63.326 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 1.5988 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.833332 90.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.5908 0.008) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "RANGE_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.2056 58.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "475K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(LS1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.946 71.0476)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2.4892 0) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.3556 151.2532)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 2.9972 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.5916 63.326 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.5988 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "I2C_SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.5 100.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 3.2004 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "HZ_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tedit 5A02F146)
    (at 125.73 121.0856 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 6.4148) (layer "F.SilkS"))
    (fp_text value "ATmega328P-A" (at 0 6.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "BKLT") (pinfunction "PD3") (pintype "bidirectional"))
    (pad "2" smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "STAT_LED") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "3" smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "VCC") (pintype "passive"))
    (pad "7" smd rect (at -4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(U4-Pad7)") (pinfunction "XTAL1/PB6") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(U4-Pad8)") (pinfunction "XTAL2/PB7") (pintype "bidirectional"))
    (pad "9" smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "HOLD_SW") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "10" smd rect (at -2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "RANGE_SW") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "11" smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "MINMX_SW") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "12" smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "SHIFT_SW") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "13" smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "HZ_SW") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "REL_SW") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "15" smd rect (at 2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "SPI_MOSI") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "SPI_MISO") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "17" smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "SPI_SCK") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "18" smd rect (at 4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "AVCC") (pintype "power_in"))
    (pad "19" smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "unconnected-(U4-Pad19)") (pinfunction "ADC6") (pintype "input"))
    (pad "20" smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "unconnected-(U4-Pad20)") (pinfunction "AREF") (pintype "passive+no_connect"))
    (pad "21" smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "22" smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "unconnected-(U4-Pad22)") (pinfunction "ADC7") (pintype "input"))
    (pad "23" smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "BEEP_SW") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "24" smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "BKLT_SW") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "25" smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "BPR") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "26" smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "V_9V") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "27" smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "I2C_SDA") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "28" smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "I2C_SCL") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "29" smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "RESET") (pinfunction "~{RESET}/PC6") (pintype "bidirectional"))
    (pad "30" smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "UART_RX") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "31" smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "UART_TX") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "32" smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "RTC_INT") (pinfunction "PD2") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 80.2132 73.0288)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "BPR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (tedit 0)
    (at 128.778 55.978991)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at -0.0508 -5.9436) (layer "F.Fab"))
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 125 143)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 0.0188 -6.4712) (layer "F.SilkS"))
    (fp_text value "DS3231M" (at 0 6.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "unconnected-(U6-Pad1)") (pinfunction "32KHZ") (pintype "open_collector+no_connect"))
    (pad "2" smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "RTC_INT") (pinfunction "~{INT}/SQW") (pintype "open_collector"))
    (pad "4" smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(R22-Pad2)") (pinfunction "~{RST}") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "7" smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "8" smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "9" smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "10" smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "11" smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "12" smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "13" smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(BT1-Pad1)") (pinfunction "VBAT") (pintype "power_in"))
    (pad "15" smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "I2C_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "I2C_SCL") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 80.2132 70.1332 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at -2.9972 0) (layer "F.SilkS"))
    (fp_text value "AO3400A" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "BPR") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(Q2-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_LCD" (layer "F.Cu")
    (tedit 639BC4BA)
    (at 100 65)
    (descr "Fluke 87V Multimeter LCD")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at -17.526 -21.082 unlocked) (layer "F.Fab"))
    (fp_text value "LCD" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 19 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 1 "COM3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 17 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 43 "unconnected-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" smd rect (at 15 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 45 "unconnected-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" smd rect (at 13 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 46 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 11 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 47 "unconnected-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" smd rect (at 9 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 48 "unconnected-(J3-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" smd rect (at 7 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 49 "unconnected-(J3-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" smd rect (at 5 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 50 "unconnected-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (pad "9" smd rect (at 3 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 51 "unconnected-(J3-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" smd rect (at 1 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 2 "SEG8") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at -1 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 3 "SEG9") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at -3 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 4 "SEG10") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at -5 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 5 "SEG11") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at -7 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 6 "SEG12") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at -9 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 7 "SEG13") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at -11 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 8 "SEG14") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at -13 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 9 "SEG15") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at -15 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 10 "SEG16") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at -17 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 52 "unconnected-(J3-Pad19)") (pinfunction "Pin_19") (pintype "passive+no_connect"))
    (pad "20" smd rect (at -19 -18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 11 "COM2") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at -19 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 12 "COM1") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at -17 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 53 "unconnected-(J3-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" smd rect (at -15 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 13 "SEG19") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at -13 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 14 "SEG20") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at -11 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 15 "SEG21") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at -9 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 16 "SEG22") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at -7 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 17 "SEG23") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at -5 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 18 "SEG24") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at -3 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 19 "SEG25") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at -1 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 20 "SEG26") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 1 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 21 "SEG27") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 3 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 22 "SEG28") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 5 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 23 "SEG29") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 7 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 54 "unconnected-(J3-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" smd rect (at 9 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 55 "unconnected-(J3-Pad35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "36" smd rect (at 11 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 24 "COM0") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 13 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 56 "unconnected-(J3-Pad37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "38" smd rect (at 15 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 57 "unconnected-(J3-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" smd rect (at 17 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 71 "unconnected-(J3-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" smd rect (at 19 18.25) (size 1 2.5) (layers "F.Cu" "F.Mask")
      (net 24 "COM0") (pinfunction "Pin_40") (pintype "passive"))
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 73.5 103.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW6" (at -3.97 0 unlocked) (layer "F.SilkS"))
    (fp_text value "BKLT" (at -0.0076 -2.9592 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 37 "BKLT_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.166666 100.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 2.6416 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "BEEP_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 70.041 70.1332 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at 2.731 0 90) (layer "F.SilkS"))
    (fp_text value "AO3400A" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "BKLT") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(Q3-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.1548 61.44 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 2.5908 0) (layer "F.SilkS"))
    (fp_text value "470pF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 117.8152 156.0576 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "RTC_BATT" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(BT1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C756B4C)
    (at 115.1128 67.5231)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0.0016 -2.118) (layer "F.SilkS"))
    (fp_text value "CONTRAST_SEL" (at 0 2) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 26 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 84 "VLCD") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 85 "Net-(JP1-Pad3)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 126.5 93.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW5" (at -3.802 -0.0052 unlocked) (layer "F.SilkS"))
    (fp_text value "HOLD" (at 0.008 -3.0024 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 36 "HOLD_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "fluke-87v-clock:BAT_1056" (layer "F.Cu")
    (tedit 63A7B0BB)
    (at 78.5 124 45)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "BT1" (at -5.938848 -8.521202 45) (layer "F.SilkS"))
    (fp_text value "Battery_Cell" (at -4.42 9.134999 45) (layer "F.Fab"))
    (fp_text user "+" (at -8.89 -2.794 45 unlocked) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -3.75 0 45) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.75 0 45) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "1" smd rect (at -7.95 0 225) (size 3.6 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect (at 7.85 0 225) (size 3.6 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "-") (pintype "passive"))
    (model "C:/Users/mikek/Documents/PCB/fluke-87v-clock/keystone-PN1056.STEP"
      (offset (xyz 0 -1.2 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "fluke-87v-clock:LED_3020" (layer "F.Cu")
    (tedit 639BE403)
    (at 64.75 65 90)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 2.8716 -0.0254 unlocked) (layer "F.SilkS"))
    (fp_text value "5973902507F" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.2 0 90) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667)
      (net 86 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.2 0 90) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1666666667)
      (net 25 "+9V") (pinfunction "A") (pintype "passive"))
    (model "C:/Users/mikek/Documents/PCB/fluke-87v-clock/QBLP676.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 82 164.5 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0.0078 -2.6328) (layer "F.SilkS"))
    (fp_text value "9V" (at -2.7608 -0.4484 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.8324 63.326 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 1.5988 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical" (layer "F.Cu")
    (tedit 5C165D15)
    (at 69.5 116.75 45)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at -0.067599 -2.74216 45 unlocked) (layer "F.SilkS"))
    (fp_text value "CONTRAST_ADJ" (at 0 2.5 45) (layer "F.Fab"))
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 45) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd rect (at -1.8 -1 45) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.45 0 45) (size 1.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(JP1-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.8 1 45) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/mikek/Documents/PCB/fluke-87v-clock/TC33X-2-104E.STEP"
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 125.0696 155.1724)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at -2.4384 -3.5852) (layer "F.SilkS"))
    (fp_text value "CAT24C256" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "I2C_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "I2C_SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "WP") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 73.5 93.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at -3.9192 0 unlocked) (layer "F.SilkS"))
    (fp_text value "SHIFT" (at -0.0076 -3.0024 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 33 "SHIFT_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.84 121.0856 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 133.35 128.858 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 1.6256) (layer "F.Fab"))
    (fp_text value "STAT" (at 0 1.604) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_GCT_DCJ200-10-A_Horizontal" (layer "F.Cu")
    (tedit 606193C0)
    (at 71 152.8)
    (descr "Barrel jack connector (5.5 mm outer diameter, 2.05 inner diameter ), https://gct.co/files/drawings/dcj200-10.pdf")
    (tags "connector barrel jack")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 7.0796 2.8512) (layer "F.SilkS"))
    (fp_text value "9V" (at 0 15.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 4.6 2) (drill oval 3.6 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6.3) (size 4.2 2) (drill oval 3.2 1) (layers *.Cu *.Mask)
      (net 26 "GND") (pintype "passive") (zone_connect 1) (thermal_width 0.381))
    (pad "3" thru_hole oval (at 4.8 2.9) (size 2 4.2) (drill oval 1 3.2) (layers *.Cu *.Mask)
      (net 26 "GND") (pintype "passive") (zone_connect 1) (thermal_width 0.381))
    (model "C:/Users/mikek/Documents/PCB/fluke-87v-clock/DCJ200-10-A-K1-K--3DModel-STEP-56544.STEP"
      (offset (xyz 0 -7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 67.0988 140.4404 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.712 63.326 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.5988 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "I2C_SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 91.166666 93.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at -3.829334 -0.0052 unlocked) (layer "F.SilkS"))
    (fp_text value "MINMX" (at 0 -3.0024 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 34 "MINMX_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "fluke-87v-clock:SSOP-A32" (layer "F.Cu")
    (tedit 639BEBF2)
    (at 99 65 -90)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -8.4088 0.0416) (layer "F.SilkS"))
    (fp_text value "BU91796FS" (at 0 -6.6 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -6 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "SEG11") (pinfunction "SEG2") (pintype "output"))
    (pad "2" smd roundrect (at -5.2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "SEG10") (pinfunction "SEG3") (pintype "output"))
    (pad "3" smd roundrect (at -4.4 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "SEG12") (pinfunction "SEG4") (pintype "output"))
    (pad "4" smd roundrect (at -3.6 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "SEG13") (pinfunction "SEG5") (pintype "output"))
    (pad "5" smd roundrect (at -2.8 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "SEG14") (pinfunction "SEG6") (pintype "output"))
    (pad "6" smd roundrect (at -2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "SEG15") (pinfunction "SEG7") (pintype "output"))
    (pad "7" smd roundrect (at -1.2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "SEG16") (pinfunction "SEG8") (pintype "output"))
    (pad "8" smd roundrect (at -0.4 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "SEG19") (pinfunction "SEG9") (pintype "output"))
    (pad "9" smd roundrect (at 0.4 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "SEG20") (pinfunction "SEG10") (pintype "output"))
    (pad "10" smd roundrect (at 1.2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "SEG21") (pinfunction "SEG11") (pintype "output"))
    (pad "11" smd roundrect (at 2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "SEG22") (pinfunction "SEG12") (pintype "output"))
    (pad "12" smd roundrect (at 2.8 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "SEG23") (pinfunction "SEG13") (pintype "output"))
    (pad "13" smd roundrect (at 3.6 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "SEG27") (pinfunction "SEG14") (pintype "output"))
    (pad "14" smd roundrect (at 4.4 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "SEG26") (pinfunction "SEG15") (pintype "output"))
    (pad "15" smd roundrect (at 5.2 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "SEG25") (pinfunction "SEG16") (pintype "output"))
    (pad "16" smd roundrect (at 6 3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "SEG24") (pinfunction "SEG17") (pintype "output"))
    (pad "17" smd roundrect (at 6 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "SEG28") (pinfunction "SEG18") (pintype "output"))
    (pad "18" smd roundrect (at 5.2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "SEG29") (pinfunction "SEG19") (pintype "output"))
    (pad "19" smd roundrect (at 4.4 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "COM0") (pinfunction "COM0") (pintype "output"))
    (pad "20" smd roundrect (at 3.6 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "COM1") (pinfunction "COM1") (pintype "output"))
    (pad "21" smd roundrect (at 2.8 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "COM2") (pinfunction "COM2") (pintype "output"))
    (pad "22" smd roundrect (at 2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "COM3") (pinfunction "COM3") (pintype "output"))
    (pad "23" smd roundrect (at 1.2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "VLCD") (pinfunction "VLCD") (pintype "power_in"))
    (pad "24" smd roundrect (at 0.4 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "25" smd roundrect (at -0.4 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "26" smd roundrect (at -1.2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "TEST1") (pintype "input"))
    (pad "27" smd roundrect (at -2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "TEST2") (pintype "input"))
    (pad "28" smd roundrect (at -2.8 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pinfunction "OSCIN") (pintype "input"))
    (pad "29" smd roundrect (at -3.6 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "I2C_SCL") (pinfunction "SCL") (pintype "input"))
    (pad "30" smd roundrect (at -4.4 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "I2C_SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "31" smd roundrect (at -5.2 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "SEG9") (pinfunction "SEG0") (pintype "output"))
    (pad "32" smd roundrect (at -6 -3.6 270) (size 0.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "SEG8") (pinfunction "SEG1") (pintype "output"))
    (model "C:/Users/mikek/Documents/PCB/fluke-87v-clock/SSOP-A32_rev1.step"
      (offset (xyz -6.8 4 1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.833332 100.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.0988 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "REL_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.9736 121.0856 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 2.9172 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.104 65.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.524) (layer "F.SilkS"))
    (fp_text value "475K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.4468 130.7884 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.5456) (layer "F.SilkS"))
    (fp_text value "9K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "V_9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.5 90.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 2.6416 0.008) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "HOLD_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 91.166666 103.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW7" (at -3.829334 0 unlocked) (layer "F.SilkS"))
    (fp_text value "BEEP" (at 0 -2.9592 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 38 "BEEP_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.2472 130.7884)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -3.0988 0) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.428 112.7036 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 1.6256) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 72.2296 140.4404 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 5.334 0) (layer "F.SilkS"))
    (fp_text value "NCP1117" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (pad "2" smd rect (at 3.15 0 90) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd rect (at -3.15 2.3 90) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "+9V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.5 100.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 2.794 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "BKLT_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.4468 128.858)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.4516) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "V_9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Rotary_Dial" (layer "F.Cu")
    (tedit 63A63037)
    (at 100 141.25)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 -15.875 unlocked) (layer "F.Fab"))
    (fp_text value "ROT_DIAL" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 0) (size 7 7) (drill 6.2) (layers *.Cu *.Mask))
    (pad "1" smd custom (at -13.5 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 31 "Net-(Q1-Pad1)") (pinfunction "A") (pintype "passive")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start 0 0) (mid 13.5 -13.5) (end 27 0) (width 1))
      ))
    (pad "2" smd circle (at 8.5 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 26 "GND") (pinfunction "B") (pintype "passive"))
    (pad "2" smd custom (at -8.5 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 26 "GND") (pinfunction "B") (pintype "passive")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start 0 0) (mid 8.5 -8.5) (end 17 0) (width 1))
      ))
  )
  (footprint "Crystal:Resonator_SMD_Murata_CSTxExxV-3Pin_3.0x1.1mm" (layer "F.Cu")
    (tedit 5D25016E)
    (at 133.23 118.6856 -90)
    (descr "SMD Resomator/Filter Murata CSTCE, https://www.murata.com/en-eu/products/productdata/8801162264606/SPEC-CSTNE16M0VH3C000R0.pdf")
    (tags "SMD SMT ceramic resonator filter")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at -3.2004 -0.0032) (layer "F.SilkS"))
    (fp_text value "8MHz" (at 0 1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 -0.05 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 0 270) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(U4-Pad8)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.2 0 270) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(U4-Pad7)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator_SMD_Murata_CSTxExxV-3Pin_3.0x1.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.3556 149.5552 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -2.9972 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "UART_DTR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.5 148.1498 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.5456 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Symbol_6.7x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 83.4644 157.7086)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "OSHW-Symbol_6.7x6mm_SilkScreen" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.0918 73.0288)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 3.0094 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "BKLT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 126.6216 160)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW10" (at -2.7712 2.3314) (layer "F.SilkS"))
    (fp_text value "RESET" (at 8.8126 2.3008 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "RESET") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "RESET") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.35 134.3406 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.5748) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "RTC_INT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 64.75 69.2188 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 3.222 0 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 86 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 77 "Net-(Q3-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.4468 136.2416 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 1.6216) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 76.486 62.71 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 5.6616) (layer "F.SilkS"))
    (fp_text value "4069" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(C7-Pad1)") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -2.54 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(LS1-Pad1)") (pintype "output"))
    (pad "3" smd roundrect (at -2.475 -1.27 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(LS1-Pad1)") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(LS1-Pad2)") (pintype "output"))
    (pad "5" smd roundrect (at -2.475 1.27 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(LS1-Pad1)") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(LS1-Pad2)") (pintype "output"))
    (pad "7" smd roundrect (at -2.475 3.81 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(Q2-Pad3)") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 3.81 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(LS1-Pad1)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(C7-Pad1)") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(C7-Pad1)") (pintype "output"))
    (pad "11" smd roundrect (at 2.475 0 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(U3-Pad11)") (pintype "input"))
    (pad "12" smd roundrect (at 2.475 -1.27 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(U3-Pad11)") (pintype "output"))
    (pad "13" smd roundrect (at 2.475 -2.54 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R13-Pad2)") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+9V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.2472 128.858)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -2.9972 0) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "STAT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 108.833332 93.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW4" (at -3.841068 -0.0052 unlocked) (layer "F.SilkS"))
    (fp_text value "RANGE" (at 0 -3.0024 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 35 "RANGE_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.166666 90.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.6416 0.008) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "MINMX_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Membrane_SW" (layer "F.Cu")
    (tedit 639BCAC3)
    (at 126.5 103.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW9" (at -3.9036 0 unlocked) (layer "F.SilkS"))
    (fp_text value "HZ" (at 0 -2.9592 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 40 "HZ_SW") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.5 3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.1333333333)
      (net 26 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 103.88 164.5 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0.924 15.5254) (layer "F.SilkS"))
    (fp_text value "UART" (at -0.8032 16.4144) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "UART_RX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "UART_TX") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "UART_DTR") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 -12.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.5 90.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.794 0.008) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "SHIFT_SW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fluke-87v-clock:Fluke_87V_Buzzer" (layer "B.Cu")
    (tedit 639BC716)
    (at 100 74.75 180)
    (property "Sheetfile" "fluke_87v_clock_v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LS1" (at 0 13.97 unlocked) (layer "B.Fab"))
    (fp_text value "Buzzer" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (pad "1" smd circle (at 0 9.5 180) (size 3.5 3.5) (layers "B.Cu" "B.Mask")
      (net 29 "Net-(LS1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" smd circle (at -11.25 -9.5 180) (size 5 5) (layers "B.Cu" "B.Mask")
      (net 30 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
    (pad "2" smd circle (at 0 -14.5 180) (size 5 5) (layers "B.Cu" "B.Mask")
      (net 30 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
    (pad "2" smd circle (at 11.25 -9.5 180) (size 5 5) (layers "B.Cu" "B.Mask")
      (net 30 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
  )
  (gr_arc (start 65.5 166.75) (mid 63.732233 166.017767) (end 63 164.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 65.5 166.75) (end 134.5 166.75) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 135 144.25) (end 136.3 144.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 77.25 47.25) (end 78.85 47.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 123 83) (end 125.125 83) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_arc (start 137 164.25) (mid 136.267767 166.017767) (end 134.5 166.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 63 51.25) (end 63 164.25) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 90 159.25) (end 91.6 159.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 69.5 44.75) (end 70.8 44.75) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 100 114.25) (end 104.35 114.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_arc (start 128 42.25) (mid 134.363961 44.886039) (end 137 51.25) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 130.5 44.75) (end 131.8 44.75) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 64.75 77.75) (end 65.875 77.75) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 122.75 47.25) (end 124.35 47.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 72 42.25) (end 128 42.25) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 63 51.25) (mid 65.636039 44.886039) (end 72 42.25) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 77 83) (end 79.125 83) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 137 51.25) (end 137 164.25) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 64.75 52.25) (end 65.875 52.25) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "REV. 1A 12/25/2022" (at 64.6 96 -90) (layer "F.Cu"))
  (gr_text "miekush" (at 135.4 96 90) (layer "F.Cu"))
  (gr_text "SEG15" (at 87 48.75 90) (layer "F.SilkS"))
  (gr_text "TX" (at 114.04 162.7336 90) (layer "F.SilkS"))
  (gr_text "SEG22" (at 91 81.25 90) (layer "F.SilkS"))
  (gr_text "NC" (at 117 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG9" (at 99 48.75 90) (layer "F.SilkS"))
  (gr_text "RST" (at 118.6688 117.094 90) (layer "F.SilkS"))
  (gr_text "github.com/miekush" (at 83.3628 112.3442) (layer "F.SilkS"))
  (gr_text "COM1" (at 81 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG23" (at 93 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG17" (at 83 48.75 90) (layer "F.SilkS"))
  (gr_text "3V3" (at 108.96 162.7336 90) (layer "F.SilkS"))
  (gr_text "3V3" (at 113.5888 108.3564 90) (layer "F.SilkS"))
  (gr_text "SEG11" (at 95 48.75 90) (layer "F.SilkS"))
  (gr_text "COM3" (at 119 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG30" (at 107 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG32" (at 113 81.25 90) (layer "F.SilkS"))
  (gr_text "CR1220" (at 68.2244 131.7498) (layer "F.SilkS"))
  (gr_text "SEG8" (at 101 48.75 90) (layer "F.SilkS"))
  (gr_text "GND" (at 103.88 162.7336 90) (layer "F.SilkS"))
  (gr_text "SEG12" (at 93 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG3" (at 111 48.75 90) (layer "F.SilkS"))
  (gr_text "VLCD" (at 115.1652 70.1295) (layer "F.SilkS"))
  (gr_text "VBAT" (at 116.5452 153.5684) (layer "F.SilkS"))
  (gr_text "COM0" (at 119 81.25 90) (layer "F.SilkS"))
  (gr_text "-" (at 117.8152 158.242) (layer "F.SilkS"))
  (gr_text "SEG16" (at 85 48.75 90) (layer "F.SilkS"))
  (gr_text "RX" (at 111.5 162.7336 90) (layer "F.SilkS"))
  (gr_text "SEG25" (at 97 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG18" (at 83 81.25 90) (layer "F.SilkS"))
  (gr_text "DTR" (at 116.58 162.7336 90) (layer "F.SilkS"))
  (gr_text "SEG19" (at 85 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG10" (at 97 48.75 90) (layer "F.SilkS"))
  (gr_text "ADJ" (at 118.9244 67.5387) (layer "F.SilkS"))
  (gr_text "SEG33" (at 115 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG24" (at 95 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG2" (at 113 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG20" (at 87 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG7" (at 103 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG26" (at 99 81.25 90) (layer "F.SilkS"))
  (gr_text "Fluke 87V\nAlarm Clock" (at 101.219 161.7218) (layer "F.SilkS"))
  (gr_text "SEG1" (at 115 48.75 90) (layer "F.SilkS"))
  (gr_text "GND" (at 111.152 67.5387) (layer "F.SilkS"))
  (gr_text "SEG0" (at 117 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG28" (at 103 81.25 90) (layer "F.SilkS"))
  (gr_text "By: Mike Kushnerik" (at 101.3206 164.719) (layer "F.SilkS"))
  (gr_text "GND" (at 118.6688 109.8296 90) (layer "F.SilkS"))
  (gr_text "SEG21" (at 89 81.25 90) (layer "F.SilkS"))
  (gr_text "COM2" (at 81 48.75 90) (layer "F.SilkS"))
  (gr_text "MOSI" (at 116.1288 108.0008 90) (layer "F.SilkS"))
  (gr_text "+" (at 115.1736 158.242) (layer "F.SilkS"))
  (gr_text "MISO" (at 113.5888 117.4496 90) (layer "F.SilkS"))
  (gr_text "SEG13" (at 91 48.75 90) (layer "F.SilkS"))
  (gr_text "SCK" (at 116.1288 117.1448 90) (layer "F.SilkS"))
  (gr_text "SEG5" (at 107 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG31" (at 109 81.25 90) (layer "F.SilkS"))
  (gr_text "VLCD" (at 70.6628 113.03 315) (layer "F.SilkS"))
  (gr_text "SEG27" (at 101 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG29" (at 105 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG4" (at 109 48.75 90) (layer "F.SilkS"))
  (gr_text "COM0" (at 111 81.25 90) (layer "F.SilkS"))
  (gr_text "SEG14" (at 89 48.75 90) (layer "F.SilkS"))
  (gr_text "SEG6" (at 105 48.75 90) (layer "F.SilkS"))
  (zone (net 26) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 137.668 167.212)
        (xy 62.484 167.212)
        (xy 62.484 41.736)
        (xy 137.668 41.736)
      )
    )
  )
)
