(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 53)
    (zones 0)
    (modules 12)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.508)
    (zone_clearance 0.381)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(BOB-12009-PadHV4)")
  (net 5 "Net-(BOB-12009-PadHV3)")
  (net 6 "Net-(BOB-12009-PadHV2)")
  (net 7 "Net-(BOB-12009-PadHV1)")
  (net 8 "Net-(BOB-12009-PadLV4)")
  (net 9 "Net-(BOB-12009-PadLV3)")
  (net 10 "Net-(BOB-12009-PadLV2)")
  (net 11 "Net-(BOB-12009-PadLV1)")
  (net_class Default "This is the default net class."
    (clearance 0.508)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net "Net-(BOB-12009-PadHV1)")
    (add_net "Net-(BOB-12009-PadHV2)")
    (add_net "Net-(BOB-12009-PadHV3)")
    (add_net "Net-(BOB-12009-PadHV4)")
    (add_net "Net-(BOB-12009-PadLV1)")
    (add_net "Net-(BOB-12009-PadLV2)")
    (add_net "Net-(BOB-12009-PadLV3)")
    (add_net "Net-(BOB-12009-PadLV4)")
  )
  (net_class 5v ""
    (clearance 1.016)
    (trace_width 1.016)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class GDN-LV ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class GND ""
    (clearance 0.508)
    (trace_width 1.016)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "NodeMCU Git:NodeMCU_Amica_R2" (layer F.Cu) (tedit 5A22F9CB)
    (at 84.836 42.672)
    (descr "Through-hole-mounted NodeMCU 0.9")
    (tags nodemcu)
    (fp_text reference U1 (at 11.43 12.68) (layer F.SilkS))
    (fp_text value NodeMCU_Amica_R2 (at 11.43 45.085) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0.75 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22 39.38) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.8 39.38) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 22.86 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(BOB-12009-PadLV1)"))
    (pad 27 thru_hole oval (at 22.86 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(BOB-12009-PadLV3)"))
    (pad 28 thru_hole oval (at 22.86 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(BOB-12009-PadLV2)"))
    (pad 20 thru_hole oval (at 22.86 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at 22.86 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at 22.86 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole oval (at 22.86 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 22.86 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 24 thru_hole oval (at 22.86 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 26 thru_hole oval (at 22.86 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(BOB-12009-PadLV4)"))
    (pad 25 thru_hole oval (at 22.86 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 19 thru_hole oval (at 22.86 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 22.86 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 18 thru_hole oval (at 22.86 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole oval (at 22.86 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (module kicad-lib:CONV_BOB-12009 (layer B.Cu) (tedit 6197CB09)
    (at 96.012 59.944 180)
    (fp_text reference BOB-12009 (at -3.325 9.135) (layer B.SilkS))
    (fp_text value BOB-12009 (at 2.39 -9.135) (layer B.Fab))
    (pad HV4 thru_hole circle (at 5.08 -6.35 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(BOB-12009-PadHV4)"))
    (pad HV3 thru_hole circle (at 5.08 -3.81 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(BOB-12009-PadHV3)"))
    (pad GND_1 thru_hole circle (at 5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad HV thru_hole circle (at 5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad HV2 thru_hole circle (at 5.08 3.81 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(BOB-12009-PadHV2)"))
    (pad HV1 thru_hole rect (at 5.08 6.35 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(BOB-12009-PadHV1)"))
    (pad LV4 thru_hole circle (at -5.08 -6.35 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(BOB-12009-PadLV4)"))
    (pad LV3 thru_hole circle (at -5.08 -3.81 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(BOB-12009-PadLV3)"))
    (pad GND_2 thru_hole circle (at -5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad LV thru_hole circle (at -5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad LV2 thru_hole circle (at -5.08 3.81 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(BOB-12009-PadLV2)"))
    (pad LV1 thru_hole rect (at -5.08 6.35 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(BOB-12009-PadLV1)"))
  )
  (module TerminalBlock_Philmore:TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EAF)
    (at 118.872 76.2 90)
    (descr "Terminal Block Philmore , 3 pins, pitch 5mm, size 15x10.2mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Philmore")
    (tags "THT Terminal Block Philmore  pitch 5mm size 15x10.2mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference D4-GPIO2 (at 5 3.048 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 6.46 90) (layer F.Fab))
    (fp_text user %R (at 5 2.8 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(BOB-12009-PadHV4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Philmore:TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EAF)
    (at 72.644 76.2 90)
    (descr "Terminal Block Philmore , 3 pins, pitch 5mm, size 15x10.2mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Philmore")
    (tags "THT Terminal Block Philmore  pitch 5mm size 15x10.2mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference D3-GPIO0 (at 4.572 -3.556 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 6.46 90) (layer F.Fab))
    (fp_text user %R (at 5 2.8 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(BOB-12009-PadHV3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Philmore:TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EAF)
    (at 118.872 53.34 90)
    (descr "Terminal Block Philmore , 3 pins, pitch 5mm, size 15x10.2mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Philmore")
    (tags "THT Terminal Block Philmore  pitch 5mm size 15x10.2mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference D2-GPIO4 (at 5.08 3.048 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 6.46 90) (layer F.Fab))
    (fp_text user %R (at 5 2.8 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(BOB-12009-PadHV2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Philmore:TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EAF)
    (at 72.944 53.34 90)
    (descr "Terminal Block Philmore , 3 pins, pitch 5mm, size 15x10.2mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Philmore")
    (tags "THT Terminal Block Philmore  pitch 5mm size 15x10.2mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference D1-GPIO5 (at 5.08 -4.064 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 6.46 90) (layer F.Fab))
    (fp_text user %R (at 5 2.8 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(BOB-12009-PadHV1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB133_1x03_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 77.216 88.392)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 77.216 32.512)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 115.316 88.392)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 115.316 32.512)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 102.616 28.956)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.25) (layer F.SilkS))
    (fp_text value C (at 2.5 6.25) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Philmore:TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EAF)
    (at 85.852 28.656)
    (descr "Terminal Block Philmore , 2 pins, pitch 5mm, size 10x10.2mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.philmore-datak.com/mc/Page%20197.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Philmore")
    (tags "THT Terminal Block Philmore  pitch 5mm size 10x10.2mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference 5VIn1 (at 2.5 -5.86) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.5 6.46) (layer F.Fab))
    (fp_text user %R (at 2.5 2.8) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 123.444 23.368) (end 125.476 23.368) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 123.444 89.408) (end 123.444 91.44) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 69.596 89.408) (end 67.564 89.408) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 69.596 23.368) (end 69.596 21.336) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "WLED 4-channel - 5v\nv1.0.0 - Nov 2021\nnico@nmac.com.ar" (at 96.52 86.36) (layer F.SilkS))
  (gr_text "NodeMCU\nAmica\nESP8266\n\nQué pasó,\nmuchachito?" (at 96.52 44.196) (layer F.SilkS))
  (gr_line (start 67.564 23.368) (end 67.564 89.408) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.444 21.336) (end 69.596 21.336) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.476 89.408) (end 125.476 23.368) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 69.596 91.44) (end 123.444 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_text 3v (at 103.632 58.928) (layer B.SilkS))
  (gr_text 5v (at 88.392 58.928) (layer B.SilkS))
  (gr_text Vin (at 87.884 78.232) (layer F.SilkS))
  (gr_text "GND\n\n\nData\n\n\n5v" (at 78.232 48.768) (layer F.SilkS))
  (gr_text "GND\n\n\nData\n\n\n5v" (at 78.232 71.628) (layer F.SilkS))
  (gr_text "GND\n\n\nData\n\n\n5v" (at 113.792 71.628) (layer F.SilkS))
  (gr_text "GND\n\n\nData\n\n\n5v" (at 113.792 49.276) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 121.158 87.376) (xy 69.342 87.376) (xy 69.85 24.384) (xy 121.666 24.384)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 121.412 87.376) (xy 69.088 87.376) (xy 69.596 24.384) (xy 121.92 24.384)
      )
    )
  )
)
