<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="77.14" y1="0" x2="77.14" y2="27.93" width="0" layer="20"/>
<hole x="3.81" y="25.4" drill="3.2"/>
<hole x="74.93" y="25.4" drill="3.2"/>
<wire x1="1.27" y1="0" x2="77.14" y2="0" width="0.4064" layer="20"/>
<wire x1="77.14" y1="0" x2="77.47" y2="0" width="0.4064" layer="20"/>
<wire x1="77.47" y1="0" x2="77.47" y2="27.94" width="0.4064" layer="20"/>
<wire x1="77.47" y1="27.94" x2="1.27" y2="27.94" width="0.4064" layer="20"/>
<wire x1="1.27" y1="27.94" x2="1.27" y2="0" width="0.4064" layer="20"/>
<text>ARDUINO
MINI-PRO</text>
<text>GY-521</text>
<text>+</text>
<text>THIS END UP -----&gt;</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>PVN012-
89751</text>
<text>PVN012-
89751</text>
<text>LED</text>
<text>FROM
PET2</text>
<hole x="74.93" y="2.54" drill="3.2"/>
<hole x="3.81" y="2.54" drill="3.2"/>
<text>PET2+ Companion Board v7
EKChess 4/5/2017</text>
<text>+ EVENT1 -</text>
<text>+ EVENT2 -</text>
<text>- BAT +</text>
<text>  PYRO
+EVENT1-</text>
<text>  PYRO
+EVENT2-</text>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="chesslib">
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="1727010">
</package>
<package name="GY-521_HOR">
<description>GY-5
21 BREAKOUT BOARD

MPU6050 6 axis accelerometer and gyroscope moption tracking device containing a Digital Motion Porcessor (DMP) from InvenSense.  Breakout board allows 5V input and I2C communication with microprocessors.</description>
</package>
<package name="ARDUINO_MINI_PRO_ALT">
</package>
</packages>
</library>
<library name="con-phoenix-3.81">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt; Grid 3.81 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1727036">
<description>&lt;b&gt;MKDS 1/ 4-3,81&lt;/b&gt;&lt;p&gt;
Source: http://eshop.phoenixcontact.de</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-03">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="led" package="CHIP-LED0805" value="GREEN"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="560"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="560"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="220"/>
<element name="U$2" library="chesslib" package="DIL06" value="PVN012PVF"/>
<element name="U$3" library="chesslib" package="DIL06" value="PVN012PVF"/>
<element name="EVENT_IN" library="con-phoenix-3.81" package="1727036" value="1727036">
<attribute name="MPN" value="1727036"/>
<attribute name="OC_NEWARK" value="71C4114"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="OC_FARNELL" value="3704592"/>
</element>
<element name="EVENT_OUT" library="con-phoenix-3.81" package="1727036" value="1727036">
<attribute name="MPN" value="1727036"/>
<attribute name="OC_NEWARK" value="71C4114"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="OC_FARNELL" value="3704592"/>
</element>
<element name="U$1" library="chesslib" package="1727010" value="MKDS_1/2-3.81"/>
<element name="U$4" library="chesslib" package="GY-521_HOR" value="GY-521">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="chesslib" package="ARDUINO_MINI_PRO_ALT" value="ARDUINO_MINI_PRO_ALT"/>
<element name="SW1" library="special" package="EDG-03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$9">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="EVENT_1_IN-">
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="4"/>
<contactref element="EVENT_IN" pad="1"/>
</signal>
<signal name="EVENT_2_IN-">
<contactref element="U$3" pad="6"/>
<contactref element="U$3" pad="4"/>
<contactref element="EVENT_IN" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$3" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$5" pad="GND1"/>
<contactref element="U$4" pad="AD0"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="EVENT_1_OUT-">
<contactref element="U$2" pad="5"/>
<contactref element="EVENT_OUT" pad="4"/>
</signal>
<signal name="RAW">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$5" pad="RAW"/>
</signal>
<signal name="EVENT2_OUT-">
<contactref element="U$3" pad="5"/>
<contactref element="EVENT_OUT" pad="2"/>
</signal>
<signal name="EVENT1_OUT+">
<contactref element="EVENT_IN" pad="2"/>
<contactref element="EVENT_OUT" pad="3"/>
</signal>
<signal name="EVENT2_OUT+">
<contactref element="EVENT_IN" pad="4"/>
<contactref element="EVENT_OUT" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$5" pad="7"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$5" pad="8"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$5" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="INT">
<contactref element="U$5" pad="2"/>
<contactref element="U$4" pad="INT"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="SDA"/>
<contactref element="U$5" pad="A4"/>
</signal>
<signal name="N$5">
<contactref element="U$4" pad="SCL"/>
<contactref element="U$5" pad="A5"/>
</signal>
<signal name="N$6">
<contactref element="U$4" pad="VCC"/>
<contactref element="U$5" pad="VCC"/>
</signal>
<signal name="N$8">
<contactref element="U$5" pad="3"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$5" pad="4"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$5" pad="5"/>
<contactref element="SW1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
