(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 210)
    (zones 0)
    (modules 18)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/"))
  )
  (net 0 "")
  (net 1 MONO_AUDIO)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 VCC)
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 STROBE)
  (net 9 D0)
  (net 10 D1)
  (net 11 D2)
  (net 12 D3)
  (net 13 D4)
  (net 14 D5)
  (net 15 D6)
  (net 16 D7)
  (net 17 "Net-(J3-Pad10)")
  (net 18 "Net-(J3-Pad11)")
  (net 19 "Net-(J3-Pad12)")
  (net 20 "Net-(J3-Pad13)")
  (net 21 "Net-(J3-Pad15)")
  (net 22 "Net-(J3-Pad16)")
  (net 23 "Net-(J3-Pad17)")
  (net 24 "Net-(R3-Pad1)")
  (net 25 "Net-(R4-Pad1)")
  (net 26 Vo)
  (net 27 "Net-(U1-Pad9)")
  (net 28 "Net-(U1-Pad18)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net MONO_AUDIO)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad9)")
    (add_net STROBE)
    (add_net Vo)
  )
  (net_class pwr ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (module Capacitor_SMD:CP_Elec_4x5.3 (layer F.Cu) (tedit 5BCA39CF)
    (at 82.931 143.51 90)
    (descr "SMD capacitor, aluminum electrolytic, Vishay, 4.0x5.3mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C4 (at 2.9845 2.0955) (layer F.SilkS))
    (fp_text value 47uf (at 4.4831 -0.0254 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 94.107 140.335 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 94.9325 131.3815 270)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference RV1 (at -0.1519 6.1635 90) (layer F.SilkS))
    (fp_text value R_POT (at 0 6.06 90) (layer F.Fab))
    (fp_text user %R (at 0 2) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 Vo))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 Vo))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 100 131.191 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J2 (at 0.1138 -2.1719 90) (layer F.SilkS))
    (fp_text value Right (at -0.0005 -2.21 90) (layer F.Fab))
    (fp_text user %R (at 0 1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 107.0102 131.191 270)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J1 (at 2.0701 -0.8128 180) (layer F.SilkS))
    (fp_text value Left (at 0.0127 -1.5748 90) (layer F.Fab))
    (fp_text user %R (at 0 1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 108.077 140.589)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C1 (at 3.429 -0.0381) (layer F.SilkS))
    (fp_text value 10uf (at 0.5715 -1.5494) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 MONO_AUDIO))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 108.5215 144.907)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C2 (at 3.4798 -0.0254) (layer F.SilkS))
    (fp_text value 10uf (at 0.127 1.905) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.4375 0) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 101.346 134.5565 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -1.905 1.778 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 3.937 0.127 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.521 136.779)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -3.1115 0.8255 180) (layer F.SilkS))
    (fp_text value 0.1uf (at -3.937 -0.0635) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-25_Male_EdgeMount_P2.77mm (layer F.Cu) (tedit 59FEDEE2)
    (at 98.298 149.0345)
    (descr "25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm")
    (attr smd)
    (fp_text reference J3 (at 14.9225 -2.7305) (layer F.SilkS))
    (fp_text value DB25_Male (at 0 16.69) (layer F.Fab))
    (fp_text user %R (at 0 3.39) (layer F.Fab))
    (fp_text user "PCB edge" (at -21.55 1.323333) (layer Dwgs.User))
    (pad 1 smd rect (at -16.62 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 8 STROBE))
    (pad 2 smd rect (at -13.85 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 9 D0))
    (pad 3 smd rect (at -11.08 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 10 D1))
    (pad 4 smd rect (at -8.31 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 11 D2))
    (pad 5 smd rect (at -5.54 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 12 D3))
    (pad 6 smd rect (at -2.77 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 13 D4))
    (pad 7 smd rect (at 0 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 14 D5))
    (pad 8 smd rect (at 2.77 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 15 D6))
    (pad 9 smd rect (at 5.54 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 16 D7))
    (pad 10 smd rect (at 8.31 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad10)"))
    (pad 11 smd rect (at 11.08 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad11)"))
    (pad 12 smd rect (at 13.85 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad12)"))
    (pad 13 smd rect (at 16.62 0) (size 1.846667 3.48) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad13)"))
    (pad 14 smd rect (at -15.235 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 15 smd rect (at -12.465 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J3-Pad15)"))
    (pad 16 smd rect (at -9.695 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J3-Pad16)"))
    (pad 17 smd rect (at -6.925 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J3-Pad17)"))
    (pad 18 smd rect (at -4.155 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 19 smd rect (at -1.385 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 20 smd rect (at 1.385 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 21 smd rect (at 4.155 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 6.925 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 23 smd rect (at 9.695 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 24 smd rect (at 12.465 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 25 smd rect (at 15.235 0) (size 1.846667 3.48) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Male_EdgeMount_P2.77mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 108.0008 136.6266 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -1.8034 1.5367 90) (layer F.SilkS))
    (fp_text value 1k (at -1.3589 -1.3843 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 MONO_AUDIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.4575 134.5565 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0.0635 1.524 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 MONO_AUDIO))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 86.995 142.494 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.9591 0.2921 90) (layer F.SilkS))
    (fp_text value 330 (at -3.429 -0.0635 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 107.8865 142.621)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.8702 -0.1397) (layer F.SilkS))
    (fp_text value 1K (at -2.1971 -0.0381) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 "Net-(R4-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 102.362 144.399 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.032 1.7145 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 VCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.775 144.399 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.032 1.651 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0.127 0.127 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 94.107 139.573)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -0.5715 -5.588) (layer F.SilkS))
    (fp_text value ADC0820CCN (at 0.0635 0.381) (layer F.Fab))
    (fp_text user %R (at 0.127 2.032) (layer F.Fab))
    (pad 1 smd roundrect (at -4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 Vo))
    (pad 2 smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D0))
    (pad 3 smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 D1))
    (pad 4 smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 D2))
    (pad 5 smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 D3))
    (pad 6 smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 STROBE))
    (pad 7 smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R3-Pad1)"))
    (pad 8 smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 9 smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad9)"))
    (pad 10 smd roundrect (at -4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 11 smd roundrect (at 4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 12 smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (pad 13 smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 14 smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 D4))
    (pad 15 smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 D5))
    (pad 16 smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 D6))
    (pad 17 smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 D7))
    (pad 18 smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(U1-Pad18)"))
    (pad 19 smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 20 smd roundrect (at 4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 103.759 140.081 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -0.1524 -2.4003 270) (layer F.SilkS))
    (fp_text value MCP6001U (at -0.1905 0.127 180) (layer F.Fab))
    (fp_text user %R (at 2.667 -1.524) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 Vo))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 21.082096 (width 0.15) (layer Dwgs.User)
    (gr_text "21.082 mm" (at 73.788816 140.442199 -89.82742287) (layer Dwgs.User))
    (feature1 (pts (xy 88.265 129.8575) (xy 74.470642 129.899049)))
    (feature2 (pts (xy 88.3285 150.9395) (xy 74.534142 150.981049)))
    (crossbar (pts (xy 75.12056 150.979283) (xy 75.05706 129.897283)))
    (arrow1a (pts (xy 75.05706 129.897283) (xy 75.646871 131.022015)))
    (arrow1b (pts (xy 75.05706 129.897283) (xy 74.474035 131.025548)))
    (arrow2a (pts (xy 75.12056 150.979283) (xy 75.703585 149.851018)))
    (arrow2b (pts (xy 75.12056 150.979283) (xy 74.530749 149.854551)))
  )
  (gr_text POT (at 93.0275 132.969) (layer B.SilkS))
  (gr_text "L   GND   R" (at 103.4415 132.9055) (layer B.SilkS))
  (gr_text "Open Amiga Sampler\n@echolevel\n@mnstrmnch\n@abrugsch" (at 115.824 143.383) (layer B.SilkS))
  (gr_line (start 88.2015 129.794) (end 87.071597 136.639364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.3945 129.794) (end 88.2015 129.794) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.728 136.791518) (end 108.3945 129.794) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.370106 139.7635) (end 113.410994 139.7635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3701 150.9395) (end 116.370106 139.7635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.391 150.9395) (end 116.3701 150.9395) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 113.423729 135.979674) (end 109.728 136.791518) (angle -77.41773834) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 83.312 136.017) (end 83.388199 139.827) (angle -79.45474536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.391 139.827) (end 83.388199 139.827) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.391 150.9395) (end 80.391 139.827) (layer Edge.Cuts) (width 0.1))
  (dimension 35.9156 (width 0.15) (layer Dwgs.User)
    (gr_text "35.916 mm" (at 98.4123 158.015162) (layer Dwgs.User))
    (feature1 (pts (xy 80.4545 150.9395) (xy 80.4545 157.301583)))
    (feature2 (pts (xy 116.3701 150.9395) (xy 116.3701 157.301583)))
    (crossbar (pts (xy 116.3701 156.715162) (xy 80.4545 156.715162)))
    (arrow1a (pts (xy 80.4545 156.715162) (xy 81.581004 156.128741)))
    (arrow1b (pts (xy 80.4545 156.715162) (xy 81.581004 157.301583)))
    (arrow2a (pts (xy 116.3701 156.715162) (xy 115.243596 156.128741)))
    (arrow2b (pts (xy 116.3701 156.715162) (xy 115.243596 157.301583)))
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.0775 132.2705) (xy 116.7765 133.1595) (xy 116.713 152.5905) (xy 79.756 152.4635) (xy 79.6925 133.63575)
        (xy 85.1535 131.953) (xy 86.2965 128.143) (xy 109.601 128.143)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.2845 152.7175) (xy 79.4385 152.654) (xy 79.4385 125.349) (xy 117.2845 125.4125)
      )
    )
  )
)
