(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 36)
    (no_connects 0)
    (area 76.565002 52.14 142.907143 122.080001)
    (thickness 1.6)
    (drawings 255)
    (tracks 85)
    (zones 0)
    (modules 15)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/mancio/Documents/GitHub/Volante-The-Gamepad/kicad/shield/gerber/))
  )
  (net 0 "")
  (net 1 A0)
  (net 2 GND)
  (net 3 A1)
  (net 4 A2)
  (net 5 10)
  (net 6 16)
  (net 7 14)
  (net 8 15)
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad12)")
  (net 11 9)
  (net 12 8)
  (net 13 7)
  (net 14 6)
  (net 15 5)
  (net 16 4)
  (net 17 3)
  (net 18 2)
  (net 19 0)
  (net 20 1)
  (net 21 "Net-(D1-Pad2)")
  (net 22 21)
  (net 23 "Net-(R1-Pad2)")
  (net 24 VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 0)
    (add_net 1)
    (add_net 10)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 2)
    (add_net 21)
    (add_net 3)
    (add_net 4)
    (add_net 5)
    (add_net 6)
    (add_net 7)
    (add_net 8)
    (add_net 9)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(R1-Pad2)")
    (add_net VCC)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A818582)
    (at 93.345 106.045)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer Eco1.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A818576)
    (at 133.35 106.045)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer Eco1.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A81855D)
    (at 133.35 65.405)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer Eco1.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A81920A)
    (at 117.856 106.172)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 1.25 -2.56) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.25 2.56) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 A0))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A8191FF)
    (at 117.856 99.568)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.56) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.25 2.56) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 A1))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5A830A07)
    (at 124.46 97.028)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.25 2.56) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A2))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-112-X-XX_1x12 (layer F.Cu) (tedit 590274D5)
    (at 104.26 65.34)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J1 (at -2.27 13.97 90) (layer F.SilkS))
    (fp_text value Conn_01x12_Fem_l (at 2.27 13.97 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 10))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 16))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 14))
    (pad 4 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 15))
    (pad 5 thru_hole circle (at 0 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 A0))
    (pad 6 thru_hole circle (at 0 12.7) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 A1))
    (pad 7 thru_hole circle (at 0 15.24) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 A2))
    (pad 8 thru_hole circle (at 0 17.78) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 21))
    (pad 9 thru_hole circle (at 0 20.32) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 VCC))
    (pad 10 thru_hole circle (at 0 22.86) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 0 25.4) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 0 27.94) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-112-X-XX_1x12.wrl
      (at (xyz 0 1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Samtec:SL-112-X-XX_1x12 (layer F.Cu) (tedit 590274D5)
    (at 119.5 65.34)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J2 (at -2.27 13.97 90) (layer F.SilkS))
    (fp_text value Conn_01x12_Fem_r (at 2.27 13.97 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 9))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 8))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 7))
    (pad 4 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 6))
    (pad 5 thru_hole circle (at 0 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 5))
    (pad 6 thru_hole circle (at 0 12.7) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 4))
    (pad 7 thru_hole circle (at 0 15.24) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 3))
    (pad 8 thru_hole circle (at 0 17.78) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 2))
    (pad 9 thru_hole circle (at 0 20.32) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 0 22.86) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0 25.4) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 0))
    (pad 12 thru_hole circle (at 0 27.94) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 20 1))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-112-X-XX_1x12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Samtec:SL-112-X-XX_1x12 (layer F.Cu) (tedit 5A81950B)
    (at 133.985 71.755)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J3 (at 0 31.115 90) (layer F.SilkS))
    (fp_text value Conn_01x12_Fem_b_r (at 2.27 13.97 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 9))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 8))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 7))
    (pad 4 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 6))
    (pad 5 thru_hole circle (at 0 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 5))
    (pad 6 thru_hole circle (at 0 12.7) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 4))
    (pad 7 thru_hole circle (at 0 15.24) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 3))
    (pad 8 thru_hole circle (at 0 17.78) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 2))
    (pad 9 thru_hole circle (at 0 20.32) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 0 22.86) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0 25.4) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 0))
    (pad 12 thru_hole circle (at 0 27.94) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 20 1))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-112-X-XX_1x12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A818533)
    (at 93.345 65.405)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer Eco1.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 100.076 106.68)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 124.46 105.41)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5A875DD3)
    (at 107.188 97.028 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value "100 Ohm" (at 5.08 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 VCC))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Triwood_RM-065 (layer F.Cu) (tedit 5A875DC7)
    (at 93.472 100.584)
    (descr "Potentiometer, Trimmer, RM-065")
    (tags "Potentiometer Trimmer RM-065")
    (fp_text reference R2 (at -2.1 -2.5 90) (layer F.SilkS))
    (fp_text value "2 kOhm" (at 7.5 -2.5 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.5 -5.04) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Triwood_RM-065.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-110-X-XX_1x10 (layer F.Cu) (tedit 5B1A9328)
    (at 99.06 68.072)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J4 (at -2.54 24.892 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Fem_b_l (at 2.27 11.43 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 VCC))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 10))
    (pad 3 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 16))
    (pad 4 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 14))
    (pad 5 thru_hole circle (at 0 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 15))
    (pad 6 thru_hole circle (at 0 12.7) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 A0))
    (pad 7 thru_hole circle (at 0 15.24) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 A1))
    (pad 8 thru_hole circle (at 0 17.78) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 A2))
    (pad 9 thru_hole circle (at 0 20.32) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 21))
    (pad 10 thru_hole circle (at 0 22.86) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-110-X-XX_1x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VCC (at 99.314 64.262 90) (layer F.SilkS))
  (gr_text "USB HID\n  device\nPlug \n  and \n    Play\nSmall \n  and \n    Cute\n      :)" (at 112.014 82.042) (layer B.SilkS))
  (gr_text Volante (at 111.76 68.58) (layer B.SilkS))
  (gr_text "Play your simulation \ngames with " (at 111.76 63.5) (layer B.SilkS))
  (dimension 15.24 (width 0.3) (layer Eco1.User)
    (gr_text "15.240 mm" (at 111.87938 56.50104) (layer Eco1.User))
    (feature1 (pts (xy 119.49938 65.33896) (xy 119.49938 55.15104)))
    (feature2 (pts (xy 104.25938 65.33896) (xy 104.25938 55.15104)))
    (crossbar (pts (xy 104.25938 57.85104) (xy 119.49938 57.85104)))
    (arrow1a (pts (xy 119.49938 57.85104) (xy 118.372876 58.437461)))
    (arrow1b (pts (xy 119.49938 57.85104) (xy 118.372876 57.264619)))
    (arrow2a (pts (xy 104.25938 57.85104) (xy 105.385884 58.437461)))
    (arrow2b (pts (xy 104.25938 57.85104) (xy 105.385884 57.264619)))
  )
  (gr_text "24 pin DIP 600" (at 112.268 53.34) (layer Eco1.User))
  (gr_text 1 (at 131.445 99.695) (layer F.SilkS))
  (gr_text 0 (at 131.445 97.155) (layer F.SilkS))
  (gr_text GND (at 130.175 94.615) (layer F.SilkS))
  (gr_text GND (at 130.175 92.075) (layer F.SilkS))
  (gr_text 2 (at 130.81 89.535) (layer F.SilkS))
  (gr_text 3 (at 130.81 86.995) (layer F.SilkS))
  (gr_text 4 (at 130.81 84.455) (layer F.SilkS))
  (gr_text 5 (at 130.81 81.915) (layer F.SilkS))
  (gr_text 6 (at 130.81 79.375) (layer F.SilkS))
  (gr_text 7 (at 130.81 76.835) (layer F.SilkS))
  (gr_text 8 (at 130.81 74.295) (layer F.SilkS))
  (gr_text 9 (at 130.81 71.755) (layer F.SilkS))
  (gr_text GND (at 95.25 90.932) (layer F.SilkS))
  (gr_text 21 (at 95.758 88.392) (layer F.SilkS))
  (gr_text A2 (at 95.758 85.852) (layer F.SilkS))
  (gr_text A1 (at 95.758 83.312) (layer F.SilkS))
  (gr_text A0 (at 95.758 80.772) (layer F.SilkS))
  (gr_text 15 (at 95.758 78.232) (layer F.SilkS))
  (gr_text 14 (at 95.758 75.692) (layer F.SilkS))
  (gr_text 16 (at 95.758 73.152) (layer F.SilkS))
  (gr_text 10 (at 95.758 70.612) (layer F.SilkS))
  (gr_text "Insert here your" (at 109.855 78.74 90) (layer F.SilkS))
  (gr_text "Arduino Pro Micro Leonardo" (at 113.03 78.105 90) (layer F.SilkS))
  (gr_text "By Andrea Mancini" (at 126.365 82.55 90) (layer F.SilkS))
  (gr_text "Volante The Gamepad" (at 123.825 78.74 90) (layer F.SilkS))
  (gr_line (start 137.795 110.49) (end 88.9 110.49) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.795 60.96) (end 137.795 110.49) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.9 60.96) (end 137.795 60.96) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.9 110.49) (end 88.9 60.96) (angle 90) (layer Edge.Cuts) (width 0.2))
  (dimension 48.895 (width 0.3) (layer Eco1.User)
    (gr_text "50 mm" (at 113.3475 120.73) (layer Eco1.User))
    (feature1 (pts (xy 137.795 110.49) (xy 137.795 122.08)))
    (feature2 (pts (xy 88.9 110.49) (xy 88.9 122.08)))
    (crossbar (pts (xy 88.9 119.38) (xy 137.795 119.38)))
    (arrow1a (pts (xy 137.795 119.38) (xy 136.668496 119.966421)))
    (arrow1b (pts (xy 137.795 119.38) (xy 136.668496 118.793579)))
    (arrow2a (pts (xy 88.9 119.38) (xy 90.026504 119.966421)))
    (arrow2b (pts (xy 88.9 119.38) (xy 90.026504 118.793579)))
  )
  (dimension 49.53 (width 0.3) (layer Eco1.User)
    (gr_text "50 mm" (at 80.565001 85.725 270) (layer Eco1.User))
    (feature1 (pts (xy 85.725 110.49) (xy 79.215001 110.49)))
    (feature2 (pts (xy 85.725 60.96) (xy 79.215001 60.96)))
    (crossbar (pts (xy 81.915001 60.96) (xy 81.915001 110.49)))
    (arrow1a (pts (xy 81.915001 110.49) (xy 81.32858 109.363496)))
    (arrow1b (pts (xy 81.915001 110.49) (xy 82.501422 109.363496)))
    (arrow2a (pts (xy 81.915001 60.96) (xy 81.32858 62.086504)))
    (arrow2b (pts (xy 81.915001 60.96) (xy 82.501422 62.086504)))
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 109.855) (xy 89.535 109.855) (xy 89.535 61.595) (xy 137.16 61.595)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 109.855) (xy 89.535 109.855) (xy 89.535 61.595) (xy 137.16 61.595)
      )
    )
  )
)
