(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 77)
    (no_connects 0)
    (area 130.9902 62.0292 156.868 81.4554)
    (thickness 1.6)
    (drawings 20)
    (tracks 432)
    (zones 0)
    (modules 39)
    (nets 24)
  )
  (page A4)
  (title_block
    (title pwrup)
    (date 2016-12-04)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.15)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VBAT)
  (net 2 GND)
  (net 3 BOOST_PGND)
  (net 4 /BOOST_VIN1)
  (net 5 +3.3V)
  (net 6 "Net-(D1-Pad1)")
  (net 7 ~PGOOD)
  (net 8 "Net-(D2-Pad1)")
  (net 9 ~CHG)
  (net 10 /BOOST_L1)
  (net 11 /BOOST_L2)
  (net 12 BOOST_EN)
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(R4-Pad1)")
  (net 15 "Net-(R5-Pad1)")
  (net 16 "Net-(R6-Pad2)")
  (net 17 CHG_OUT)
  (net 18 CHG_IN)
  (net 19 ~CE)
  (net 20 EN2)
  (net 21 EN1)
  (net 22 BOOST_IN)
  (net 23 V_ISET)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BOOST_EN)
    (add_net EN1)
    (add_net EN2)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net V_ISET)
    (add_net ~CE)
    (add_net ~CHG)
    (add_net ~PGOOD)
  )
  (net_class PWR ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net /BOOST_L1)
    (add_net /BOOST_L2)
    (add_net /BOOST_VIN1)
    (add_net BOOST_IN)
    (add_net BOOST_PGND)
    (add_net CHG_IN)
    (add_net CHG_OUT)
    (add_net GND)
    (add_net VBAT)
  )
  (module mylib:S-PVQFN-N16 (layer F.Cu) (tedit 58444A04)
    (at 140.081 70.993)
    (fp_text reference U2 (at 2.3368 1.651 90) (layer F.SilkS))
    (fp_text value bq24232 (at 0.225 3) (layer F.Fab) hide)
    (pad 17 thru_hole rect (at -0.425 0.425 90) (size 0.85 0.85) (drill 0.4) (layers *.Cu F.Mask)
      (net 2 GND))
    (pad 17 thru_hole rect (at 0.425 0.425 90) (size 0.85 0.85) (drill 0.4) (layers *.Cu F.Mask)
      (net 2 GND))
    (pad 17 thru_hole rect (at 0.425 -0.425 90) (size 0.85 0.85) (drill 0.4) (layers *.Cu F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.475 0.75 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 19 ~CE))
    (pad 3 smd rect (at -1.475 0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 VBAT))
    (pad 1 smd rect (at -1.475 -0.75 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -1.475 -0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 VBAT))
    (pad 11 smd rect (at 1.475 -0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 17 CHG_OUT))
    (pad 12 smd rect (at 1.475 -0.75 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (pad 10 smd rect (at 1.475 0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 17 CHG_OUT))
    (pad 9 smd rect (at 1.475 0.75 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 9 ~CHG))
    (pad 5 smd rect (at -0.75 1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 20 EN2))
    (pad 6 smd rect (at -0.25 1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 21 EN1))
    (pad 8 smd rect (at 0.75 1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.25 1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 7 ~PGOOD))
    (pad 14 smd rect (at 0.25 -1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad1)"))
    (pad 13 smd rect (at 0.75 -1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 18 CHG_IN))
    (pad 15 smd rect (at -0.25 -1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (pad 16 smd rect (at -0.75 -1.475) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ISET))
    (pad 17 thru_hole rect (at -0.425 -0.425 90) (size 0.85 0.85) (drill 0.4) (layers *.Cu F.Mask)
      (net 2 GND))
  )
  (module mylib:TPS63001 (layer F.Cu) (tedit 58444A14)
    (at 150.8887 71.628)
    (fp_text reference U1 (at 2.5019 -0.3048 90) (layer F.SilkS))
    (fp_text value TPS63001 (at 0.2 1.8) (layer F.Fab) hide)
    (pad 11 thru_hole rect (at 0.375 0.625 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 3 BOOST_PGND))
    (pad 11 thru_hole rect (at 0.375 -0.625 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 3 BOOST_PGND))
    (pad 11 thru_hole rect (at -0.375 -0.625 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 3 BOOST_PGND))
    (pad 3 smd rect (at -1.379 0 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (pad 4 smd rect (at -1.379 0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 10 /BOOST_L1))
    (pad 2 smd rect (at -1.379 -0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 11 /BOOST_L2))
    (pad 5 smd rect (at -1.379 1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOST_IN))
    (pad 1 smd rect (at -1.379 -1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 10 smd rect (at 1.371 -1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 6 smd rect (at 1.371 1 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 12 BOOST_EN))
    (pad 9 smd rect (at 1.371 -0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (pad 7 smd rect (at 1.371 0.5 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 4 /BOOST_VIN1))
    (pad 8 smd rect (at 1.371 0 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 4 /BOOST_VIN1))
    (pad 11 thru_hole rect (at -0.375 0.625 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu F.Mask)
      (net 3 BOOST_PGND))
    (pad 11 thru_hole rect (at 0 0 90) (size 2.2 1.55) (drill 0.3) (layers *.Cu F.Mask)
      (net 3 BOOST_PGND))
    (model walter/smd_qfn/dfn10_3x3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:joiner1 (layer B.Cu) (tedit 562B21BF)
    (at 150.41118 70.51548 270)
    (descr "SMT resistor, 0402")
    (fp_text reference JP1 (at 0 0.4826 270) (layer B.SilkS) hide)
    (fp_text value JUMPER (at 0 -0.4826 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.45 0.48) (layers B.Cu)
      (net 3 BOOST_PGND))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.45 0.48) (layers B.Cu)
      (net 2 GND))
  )
  (module mylib:inductor_smd_1212 (layer F.Cu) (tedit 5843C680)
    (at 147.193 71.628 90)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at 2.286 -1.27 180) (layer F.SilkS))
    (fp_text value 2u2 (at 2.375 0.375 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.1 3) (layers F.Cu F.Paste F.Mask)
      (net 10 /BOOST_L1))
    (pad 2 smd rect (at 1.1 0 90) (size 1.1 3) (layers F.Cu F.Paste F.Mask)
      (net 11 /BOOST_L2))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:joiner1 (layer F.Cu) (tedit 562B21BF)
    (at 147.7264 74.1426 180)
    (descr "SMT resistor, 0402")
    (fp_text reference JP2 (at 0 -0.4826 180) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.45 0.48) (layers F.Cu)
      (net 17 CHG_OUT))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.45 0.48) (layers F.Cu)
      (net 22 BOOST_IN))
  )
  (module mylib:pin_socket_2m (layer F.Cu) (tedit 58441928)
    (at 135.509 70.739 270)
    (descr "Pin socket 2pin")
    (tags "CONN DEV")
    (fp_text reference BT1 (at 0 -2.159 270) (layer F.SilkS) hide)
    (fp_text value BATTERYm0 (at 0.254 -3.556 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 VBAT))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 143.002 66.548)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 CHG_IN))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 145.542 66.548)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 148.082 76.835 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 -2.159 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 BOOST_EN))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 151.3205 66.548)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3.3V))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 153.8605 66.548)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P5 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 135.509 74.549 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 ~CE))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 145.542 76.835)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P9 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 ~CHG))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 143.002 76.835)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P10 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 ~PGOOD))
  )
  (module mylib:pin_socket_1m (layer F.Cu) (tedit 58441945)
    (at 135.509 66.929 90)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P11 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 23 V_ISET))
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 5844FBCD)
    (at 151.1808 74.8792 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C1 (at -0.0254 -1.0668 360) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOST_IN))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 5844FBC6)
    (at 153.19756 74.1807 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 1.4478 0.2794 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0.6 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 /BOOST_VIN1))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 58444A79)
    (at 142.9512 68.7832 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C3 (at -1.8161 0.0762 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0.85 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 18 CHG_IN))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 58444A6D)
    (at 143.6116 71.8312 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C4 (at 0.6985 1.0414 270) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0.85 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 17 CHG_OUT))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 56CFDABC)
    (at 150.4188 68.4784 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C5 (at -1.8 0.05 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 56CFDABC)
    (at 150.4188 69.5452 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at -1.8 0.05 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0.85 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 BOOST_PGND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 58444A33)
    (at 137.3378 70.9168 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C8 (at 1.7018 -0.0508 360) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0.85 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 VBAT))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0402_mod0 (layer F.Cu) (tedit 58444980)
    (at 139.827 75.1205 90)
    (descr "SMD LED, 0402")
    (fp_text reference D1 (at 1.4097 -0.9906 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0 90) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.54864 0 90) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 ~PGOOD))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:Led_0402_mod0 (layer F.Cu) (tedit 56CFD3E3)
    (at 140.843 75.1205 90)
    (descr "SMD LED, 0402")
    (fp_text reference D2 (at -0.0625 0.8125 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0 90) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.54864 0 90) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 ~CHG))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 5844FBD1)
    (at 150.8252 73.5584)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at -1.4478 0.0254 90) (layer F.SilkS))
    (fp_text value 100R (at 0 0.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 /BOOST_VIN1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOST_IN))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A4F)
    (at 137.668 67.564 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at -1.6002 -0.0254 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A4B)
    (at 138.684 67.564 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 1.6002 0.0508 90) (layer F.SilkS))
    (fp_text value 1.8k (at 0 0.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ISET))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A42)
    (at 139.7 67.564 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at -1.6002 -0.0254 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A40)
    (at 140.716 67.564 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at -1.6002 -0.0508 270) (layer F.SilkS))
    (fp_text value 72k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A77)
    (at 143.256 69.977)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at 1.5494 -0.0381 90) (layer F.SilkS))
    (fp_text value 2k8 (at 0 0.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 56CFD031)
    (at 139.8524 77.1144 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at -0.05 -0.9 90) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444985)
    (at 140.8176 77.1144 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at 0.0508 0.9398 90) (layer F.SilkS))
    (fp_text value 1k5 (at 0 0.7 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 56CFD031)
    (at 153.6954 76.8858 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at -0.05 -0.9 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 BOOST_EN))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 584449DA)
    (at 135.636 77.089 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at -1.8034 -1.3716 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 CHG_IN))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 EN2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 584449E0)
    (at 136.652 77.089 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at -1.8034 -0.9652 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 EN2))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 584449DC)
    (at 138.684 77.089 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R12 (at -1.8034 -0.1524 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 CHG_IN))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 21 EN1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 584449DE)
    (at 137.668 77.089 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R13 (at -1.8034 -0.5588 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.7 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 21 EN1))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 56CFD031)
    (at 145.415 75.057)
    (descr "SMT resistor, 0402")
    (fp_text reference R14 (at -0.05 -0.9) (layer F.SilkS))
    (fp_text value 100k (at 0 0.7) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 ~CHG))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:r_0402_mod0 (layer F.Cu) (tedit 58444A65)
    (at 143.129 75.057 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R15 (at -0.0127 0.889 180) (layer F.SilkS))
    (fp_text value 100k (at 0 0.7 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 ~PGOOD))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 133.477 78.74) (end 155.194 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.477 65.024) (end 133.477 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.477 65.024) (end 155.194 65.024) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text V_ISET (at 135.509 65.7098) (layer F.SilkS))
  (gr_text ~CE (at 135.509 73.3552) (layer F.SilkS))
  (gr_text VBAT (at 135.509 70.7898) (layer F.SilkS))
  (gr_text GND (at 135.509 68.2498) (layer F.SilkS))
  (gr_text GND (at 152.654 66.548 90) (layer F.SilkS))
  (gr_text B_EN (at 149.352 76.835 90) (layer F.SilkS))
  (gr_text CHG (at 146.812 76.962 90) (layer F.SilkS))
  (gr_text PGOOD (at 144.272 76.962 90) (layer F.SilkS))
  (gr_text VIN (at 144.272 66.548 90) (layer F.SilkS))
  (gr_text GND (at 146.812 66.5226 90) (layer F.SilkS))
  (gr_text 3V3 (at 150.114 66.548 90) (layer F.SilkS))
  (gr_line (start 155.194 78.74) (end 155.194 65.024) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "pwrup\nrev0.01\nrel/2016-12" (at 141.5288 71.1708 180) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 78.74) (xy 133.477 78.74) (xy 133.477 65.024) (xy 155.194 65.024)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 78.74) (xy 133.477 78.74) (xy 133.477 65.024) (xy 155.194 65.024)
      )
    )
  )
)
