(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 62)
    (tracks 177)
    (zones 0)
    (modules 6)
    (nets 6)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.1524)
    (user_trace_width 0.1772)
    (user_trace_width 0.2)
    (user_trace_width 0.254)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.308 1.308)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 128.35 105)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC)
  (net 3 /D-)
  (net 4 /D+)
  (net 5 /G)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D+)
    (add_net /D-)
    (add_net /G)
    (add_net /VCC)
    (add_net GND)
  )
  (module usb_ammeter_v230:USBAMPH-UE27AC5410H (layer Top) (tedit 5FD7AF69)
    (at 125.64735 104.9986 270)
    (fp_text reference J4 (at 7.8114 2.86735) (layer F.SilkS) hide)
    (fp_text value USB-AMPH-UE27-AC (at 0 0 270) (layer F.SilkS) hide)
    (pad VCC thru_hole circle (at -3.5 -2.71 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VCC) (solder_mask_margin 0.1016))
    (pad D- thru_hole circle (at -1 -2.71 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D-) (solder_mask_margin 0.1016))
    (pad D+ thru_hole circle (at 1 -2.71 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D+) (solder_mask_margin 0.1016))
    (pad G thru_hole circle (at 3.5 -2.71 270) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.1016))
    (pad G1 thru_hole circle (at -6.57 0 270) (size 3.316 3.316) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.1016))
    (pad G2 thru_hole circle (at 6.57 0 270) (size 3.316 3.316) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.1016))
  )
  (module usb_ammeter_v230:1X02 (layer Top) (tedit 5FD7AF41)
    (at 149.77735 109.7611 90)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP2 (at -2.6162 -1.8288 -90) (layer F.SilkS) hide)
    (fp_text value PINHD-1X2 (at -2.54 3.175 -90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /VCC) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module usb_ammeter_v230:1X02 (layer Top) (tedit 5FD7AF41)
    (at 137.99 108.17 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference JP1 (at -2.6162 -1.8288 180) (layer F.SilkS) hide)
    (fp_text value PINHD-1X2 (at -2.54 3.175 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /VCC) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.1016))
  )
  (module usb_ammeter_v230:T35-2 (layer Top) (tedit 5FD7AF1C)
    (at 138.1 114.75)
    (fp_text reference J3 (at -3.5 -3.5) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x02 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 1.75 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /VCC) (solder_mask_margin 0.0635))
    (pad 2 thru_hole rect (at -1.75 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.0635))
  )
  (module usb_ammeter_v230:LG-2-PIN (layer Top) (tedit 5FD7AF90)
    (at 145.96735 100.5536 180)
    (fp_text reference J1 (at -2.54 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHEADLG (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole rect (at -3.81 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole rect (at 3.81 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 /G) (solder_mask_margin 0.1016))
  )
  (module usb_ammeter_v230:molex-47589-101-microUSB-AB (layer Top) (tedit 5FD6FE87)
    (at 178.775 105 90)
    (attr smd)
    (fp_text reference J2 (at 0.5 -4.2 90) (layer F.SilkS) hide)
    (fp_text value usb-micro-molex-sd-47589-101 (at -0.05 3.15 90) (layer F.Fab))
    (pad 9 thru_hole custom (at 4.175 0 90) (size 1 1.7) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0.475 -0.9) (xy 0.475 0.9) (xy -1.575 0.9) (xy -1.575 -0.9)) (width 0.1))
      ))
    (pad 8 thru_hole custom (at -4.175 0 90) (size 1 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 1.575 -0.9) (xy 1.575 0.9) (xy -0.475 0.9) (xy -0.475 -0.9)) (width 0.1))
      ))
    (pad 11 smd rect (at 1.15 0 90) (size 1.8 1.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1.15 0 90) (size 1.8 1.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 2.25 -3 90) (size 1.05 1.25) (drill oval 0.65 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.225 -3 90) (size 1.05 1.25) (drill oval 0.65 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.3 -2.675 90) (size 0.4 1.35) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -2.67 90) (size 0.4 1.35) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -2.675 90) (size 0.4 1.35) (layers Top F.Paste F.Mask)
      (net 4 /D+))
    (pad 2 smd rect (at -0.65 -2.675 90) (size 0.4 1.35) (layers Top F.Paste F.Mask)
      (net 3 /D-))
    (pad 1 smd rect (at -1.3 -2.675 90) (size 0.4 1.35) (layers Top F.Paste F.Mask)
      (net 2 /VCC))
  )
  (gr_text Output (at 120.3 96.72) (layer F.SilkS))
  (gr_text Input (at 177.78 99.21) (layer F.SilkS))
  (gr_text +5V (at 139.39 110.39) (layer F.SilkS))
  (gr_text Gnd (at 136.28 110.39) (layer F.SilkS))
  (gr_text "USB Ammeter V 2.30 Copyright © 2020 PL Barrett" (at 148.35 93.025) (layer F.SilkS))
  (gr_text "Thin Wire" (at 146 109.65 90) (layer F.SilkS))
  (gr_text RD (at 147.6 110.95 90) (layer F.SilkS))
  (gr_text BK (at 147.6 108.55 90) (layer F.SilkS))
  (gr_text BK (at 149.8 98.35) (layer F.SilkS))
  (gr_text BL/RD (at 142.6 98.35) (layer F.SilkS))
  (gr_line (start 116.75735 118.3336) (end 180.24485 118.3336) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.24485 118.3336) (end 180.24485 91.6736) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.24485 91.6736) (end 116.75735 91.6736) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.75735 91.6736) (end 116.75735 118.3336) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.77485 115.2586) (end 131.67985 115.2586) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.17735 114.9411) (end 175.17735 111.6661) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.17735 98.3311) (end 175.17735 95.0561) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.67985 94.7386) (end 129.77485 94.7386) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.45735 95.0561) (end 129.45735 98.3311) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.45735 111.6661) (end 129.45735 114.9411) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.67985 98.6486) (end 129.77485 98.6486) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.77485 111.3486) (end 131.67985 111.3486) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.95485 98.6486) (end 174.85985 98.6486) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.95485 111.3486) (end 174.85985 111.3486) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.63735 98.9661) (end 172.63735 111.0311) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.85985 95.0561) (end 174.85985 94.7386) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.85985 98.3311) (end 175.17735 98.3311) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.95485 98.9661) (end 172.95485 98.6486) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.85985 111.6661) (end 174.85985 111.3486) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.95485 111.0311) (end 172.63735 111.0311) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 174.85985 114.9411) (end 175.17735 114.9411) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.67985 95.0561) (end 131.99735 95.0561) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.77485 98.3311) (end 129.45735 98.3311) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.77485 95.0561) (end 129.77485 94.7386) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.77485 114.9411) (end 129.45735 114.9411) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.77485 111.6661) (end 129.77485 111.3486) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.67985 114.9411) (end 131.99735 114.9411) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.99735 95.0561) (end 131.99735 98.3311) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.67985 98.3311) (end 131.99735 98.3311) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.99735 114.9411) (end 131.99735 111.6661) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.67985 111.6661) (end 131.99735 111.6661) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.12735 95.0561) (end 156.12735 114.9411) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.85985 94.7386) (end 156.44485 94.7386) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.44485 95.0561) (end 156.44485 94.7386) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.85985 115.2586) (end 156.44485 115.2586) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.44485 114.9411) (end 156.44485 115.2586) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Current Takeoff\nThick Wire" (at 146 97.5) (layer F.SilkS))
  (gr_text "Dest    Source" (at 146.375 103.425) (layer F.SilkS))
  (gr_text "+V Gnd\nAmmeter\nPower" (at 155.65 109.75 90) (layer F.SilkS))
  (gr_text Output (at 137.86 105.51) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 182.68305 118.5368) (xy 146.08165 118.5368) (xy 146.08165 89.5554) (xy 182.68305 89.5554)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 181.73055 118.5368) (xy 146.08165 118.5368) (xy 146.075 89.55) (xy 181.75 89.55)
      )
    )
  )
  (zone (net 5) (net_name /G) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 145.425 118.5157) (xy 116.87165 118.5368) (xy 116.87165 89.5554) (xy 145.425 89.5343)
      )
    )
  )
  (zone (net 5) (net_name /G) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 145.425 118.5368) (xy 116.87165 118.5368) (xy 116.87165 89.55) (xy 145.425 89.55)
      )
    )
  )
)
