(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 348)
    (zones 0)
    (modules 25)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VIO)
  (net 3 /VDMX)
  (net 4 /DMX1GND)
  (net 5 /DMX512_1/DMXVCC)
  (net 6 /DMX512_2/DMXVCC)
  (net 7 /DMX2GND)
  (net 8 /DMX1P)
  (net 9 /DMX1N)
  (net 10 /DMX2N)
  (net 11 /DMX2P)
  (net 12 "Net-(C101-Pad1)")
  (net 13 "Net-(C102-Pad1)")
  (net 14 /IO_SDA)
  (net 15 /IO_SCL)
  (net 16 /PMOD2_TX)
  (net 17 /PMOD1_TX)
  (net 18 /PMOD1_RX)
  (net 19 /PMOD1_TXEN)
  (net 20 /PMOD2_RX)
  (net 21 /PMOD2_TXEN)
  (net 22 "Net-(H1-Pad1)")
  (net 23 "Net-(H2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DMX1GND)
    (add_net /DMX1N)
    (add_net /DMX1P)
    (add_net /DMX2GND)
    (add_net /DMX2N)
    (add_net /DMX2P)
    (add_net /DMX512_1/DMXVCC)
    (add_net /DMX512_2/DMXVCC)
    (add_net /IO_SCL)
    (add_net /IO_SDA)
    (add_net /PMOD1_RX)
    (add_net /PMOD1_TX)
    (add_net /PMOD1_TXEN)
    (add_net /PMOD2_RX)
    (add_net /PMOD2_TX)
    (add_net /PMOD2_TXEN)
    (add_net /VDMX)
    (add_net /VIO)
    (add_net GND)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(H2-Pad1)")
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 117.25172 48.98136)
    (fp_text reference X2 (at -8.10172 20.29364) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(C101-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /DMX1P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /DMX1N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 /DMX1GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Amphenol_XLR:AC5FAH (layer F.Cu) (tedit 5D91AE83)
    (at 141.25172 48.98136)
    (fp_text reference X3 (at -7.83314 20.16252) (layer F.SilkS))
    (fp_text value XLR5_Ground (at 0 -1.27) (layer F.Fab))
    (pad "" thru_hole circle (at 3.81 8.89) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -3.81 3.81) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad G thru_hole circle (at -8.25 6.98) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(C102-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 6.98 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 17.15) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 /DMX2P))
    (pad 2 thru_hole circle (at 0 13.33) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /DMX2N))
    (pad 1 thru_hole circle (at -3.81 17.15) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 /DMX2GND))
    (model ${KIPRJMOD}/Connectors_Amphenol_XLR.pretty/NC5FAH.stp
      (offset (xyz 0 0 12.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.96848 80.99298 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C303 (at -3.35702 -0.01848 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 122.37884 77.16012 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U201 (at 1.28512 6.22116 270) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /DMX512_1/DMXVCC))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DMX1GND))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DMX1P))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /DMX1N))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /DMX1N))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DMX1P))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DMX1GND))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /PMOD1_TX))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /PMOD1_TXEN))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /PMOD1_TXEN))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /PMOD1_RX))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 145.37884 77.16012 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U301 (at 1.73512 6.12116 90) (layer F.SilkS))
    (fp_text value ISO14x2 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VIO))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /PMOD2_RX))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /PMOD2_TXEN))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /PMOD2_TXEN))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /PMOD2_TX))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DMX2GND))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /DMX2P))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /DMX2N))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /DMX2N))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /DMX2P))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DMX2GND))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at -1.11252 -1.51922 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C202 (at -2.29756 -0.36524) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /DMX512_1/DMXVCC))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.40384 78.79588 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at -1.24588 -1.39616 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /VDMX))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.13476 73.82256 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C302 (at -3.39756 0.40976 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.5065 81.75752 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C203 (at -1.3208 -1.23444 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 107.8103 62.1561 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C101-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.0579 62.0418 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C102-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.275 86.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.45 -0.05 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /IO_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.275 85.35 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.45 -0.1 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /IO_SDA))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.25 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R201 (at 0.65 1.4 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DMX1P))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /DMX512_1/DMXVCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.45 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R202 (at -0.325 1.425 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DMX1P))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /DMX1N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.5375 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R203 (at -1.4625 1.425 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DMX1GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /DMX1N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.25 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R301 (at 1.05 1.375 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DMX512_2/DMXVCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DMX2P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.4 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R302 (at 0 1.425 180) (layer F.SilkS))
    (fp_text value 130R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DMX2P))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /DMX2N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.55 70.625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R303 (at -1.025 1.4 180) (layer F.SilkS))
    (fp_text value 560R (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DMX2GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /DMX2N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 112.225 80.55 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U202 (at 1 -3 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DMX512_1/DMXVCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DMX1GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_muRata_CRE1xxxxxx3C_THT (layer F.Cu) (tedit 59F5F4E9)
    (at 135.2 80.525 180)
    (descr "Isolated 1W single output DC/DC, http://power.murata.com/data/power/ncl/kdc_cre1.pdf")
    (tags "Isolated 1W single output DC/DC")
    (fp_text reference U302 (at 0.175 -2.875 180) (layer F.SilkS))
    (fp_text value CRE1S0305S3C (at 2 11) (layer F.Fab))
    (fp_text user %R (at 3 4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DMX2GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.4 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DMX512_2/DMXVCC))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_muRata_CRE1xxxxxx3C_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 134.375 85.275 270)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference X1 (at 2.5 -2.65) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 5.655 14.97 270) (layer F.Fab))
    (fp_text user %R (at 5.31 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VIO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VDMX))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /PMOD1_TX))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /PMOD2_TX))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PMOD1_RX))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PMOD2_RX))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /PMOD1_TXEN))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PMOD2_TXEN))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IO_SDA))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IO_SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 110.5 88)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 4.225 1.85) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(H1-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 148.5 88)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at -4.125 1.775) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 23 "Net-(H2-Pad1)"))
  )
  (gr_text X1 (at 118.825 86.525) (layer B.SilkS))
  (gr_text 12 (at 121.65 89.85) (layer B.SilkS))
  (gr_text 11 (at 121.575 83.1) (layer B.SilkS))
  (gr_text 2 (at 134.4 90.25) (layer B.SilkS))
  (gr_text 1 (at 134.375 83.3) (layer B.SilkS))
  (gr_text "X1 Pinout" (at 132.825 61.425) (layer B.SilkS))
  (gr_text "12: IO_SCL" (at 145.2 75.45) (layer B.SilkS))
  (gr_text "10: TXEN(X3)" (at 143.825 72.875) (layer B.SilkS))
  (gr_text "8: RX(X3)" (at 144.425 70.125) (layer B.SilkS))
  (gr_text "6: TX(X3)" (at 145.95 55.525) (layer B.SilkS))
  (gr_text "4: GND" (at 147.475 53.025) (layer B.SilkS))
  (gr_text "2: VDMX/3.3V" (at 143.725 50.9) (layer B.SilkS))
  (gr_text "11:  IO_SDA" (at 123.25 75.525) (layer B.SilkS))
  (gr_text "9: TXEN(X2)" (at 121.775 72.9) (layer B.SilkS))
  (gr_text "7: RX(X2)" (at 123.25 70.075) (layer B.SilkS))
  (gr_text "5: TX(X2)" (at 124.075 55.35) (layer B.SilkS))
  (gr_text "3: GND" (at 125.475 53.125) (layer B.SilkS))
  (gr_text "1: VIO/3.3V" (at 122.9 50.95) (layer B.SilkS))
  (gr_line (start 152.5 92) (end 106.2228 92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.5 48.9712) (end 152.5 92) (layer Edge.Cuts) (width 0.15))
  (gr_text DmxIO2-v1.0 (at 124.325 78.775) (layer B.Mask))
  (gr_text llg.cubic.org (at 145 81.475) (layer B.Mask))
  (gr_line (start 106.31932 48.9712) (end 106.3244 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.2228 48.9712) (end 106.31932 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.2228 92) (end 106.2228 48.9712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.3244 48.9712) (end 152.5 48.9712) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name /DMX1GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.31424 48.98136) (xy 106.30408 75.55484) (xy 128.6002 75.55484) (xy 128.6002 49.01184)
      )
    )
  )
  (zone (net 7) (net_name /DMX2GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.8674 49.07788) (xy 132.83184 75.67168) (xy 151.78532 75.67168) (xy 151.78532 49.01692)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.2736 77.3176) (xy 152.475 77.30762) (xy 152.5007 91.97001) (xy 106.2993 91.97999)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.2736 77.3176) (xy 152.475 77.30762) (xy 152.5007 91.97001) (xy 106.2993 91.97999)
      )
    )
  )
)
